(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "A1050"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -5.08 0 90)
		)
		(property "Value" "A1050"
			(at 1.905 0 90)
		)
		(property "Footprint" "OptoDevice:R_LDR_D6.4mm_P3.4mm_Vertical"
			(at 4.445 0 90)
		)
		(property "Datasheet" "http://cdn-reichelt.de/documents/datenblatt/A500/A106012.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "light dependent resistor"
			(at 0 0 0)
		)
		(property "ki_keywords" "light dependent photo resistor LDR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "R*LDR*D6.4*P3.4*"
			(at 0 0 0)
		)
		(symbol "A1050_0_1")
		(symbol "A1050_1_1"
			(pin passive line
				(at 0 3.81 270)
				(length 1.27)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 1.27)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "A9050"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -5.08 0 90)
		)
		(property "Value" "A9050"
			(at 1.905 0 90)
		)
		(property "Footprint" "OptoDevice:R_LDR_5.0x4.1mm_P3mm_Vertical"
			(at 4.445 0 90)
		)
		(property "Datasheet" "http://cdn-reichelt.de/documents/datenblatt/A500/A90xxxx%23PE.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "light dependent resistor"
			(at 0 0 0)
		)
		(property "ki_keywords" "light dependent photo resistor LDR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "R*LDR*5.0x4.1mm*P3mm*"
			(at 0 0 0)
		)
		(symbol "A9050_0_1")
		(symbol "A9050_1_1"
			(pin passive line
				(at 0 3.81 270)
				(length 1.27)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 1.27)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "APDS-9251-001"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "APDS-9251-001"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "OptoDevice:Broadcom_LGA-8_2x2mm_P0.5mm"
			(at 26.67 -6.35 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/doc/APDS-9251-001-DS"
			(at 0 0 0)
		)
		(property "Description" "Digital RGB, IR, and Ambient Light Sensor, 1.7-3.6V, LGA-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto ambient light sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Broadcom*LGA*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "APDS-9251-001_0_0"
			(text "ADC"
				(at -1.27 1.27 0)
			)
		)
		(symbol "APDS-9251-001_0_1")
		(symbol "APDS-9251-001_1_0")
		(symbol "APDS-9251-001_1_1"
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin power_in line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "6")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "5")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "INT")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "APDS-9301"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "APDS-9301"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "OptoDevice:Broadcom_APDS-9301"
			(at 0 11.43 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-2315EN"
			(at -7.62 8.89 0)
		)
		(property "Description" "ambient light sensor, i2c interface, 2.7-3.6V"
			(at 0 0 0)
		)
		(property "ki_keywords" "ambient light sensor i2c"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Broadcom*APDS*9301*"
			(at 0 0 0)
		)
		(symbol "APDS-9301_0_1")
		(symbol "APDS-9301_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "ADR_SEL")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "4")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "INT")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "APDS-9306"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "APDS-9306"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "OptoDevice:Broadcom_LGA-8_2x2mm_P0.53mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-4755EN"
			(at 19.05 7.62 0)
		)
		(property "Description" "Ambient Light Sensor, I2C interface, 1.7-3.6V, LGA-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto ambient light sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Broadcom*LGA*2x2mm*P0.53mm*"
			(at 0 0 0)
		)
		(symbol "APDS-9306_0_0"
			(text "ADC"
				(at -1.27 1.27 0)
			)
		)
		(symbol "APDS-9306_0_1")
		(symbol "APDS-9306_1_0")
		(symbol "APDS-9306_1_1"
			(pin no_connect line
				(at -7.62 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at -7.62 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "6")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "5")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "INT")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "APDS-9306-065"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "APDS-9306-065"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "OptoDevice:Broadcom_DFN-6_2x2mm_P0.65mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-4755EN"
			(at 19.05 7.62 0)
		)
		(property "Description" "Ambient Light Sensor, I2C interface, 1.7-3.6V, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto ambient light sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Broadcom*DFN*2x2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "APDS-9306-065_0_0"
			(text "ADC"
				(at -1.27 1.27 0)
			)
		)
		(symbol "APDS-9306-065_0_1")
		(symbol "APDS-9306-065_1_0")
		(symbol "APDS-9306-065_1_1"
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "2")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "1")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "INT")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AS7261"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 17.78 0)
		)
		(property "Value" "AS7261"
			(at -10.16 15.24 0)
		)
		(property "Footprint" "Package_LGA:AMS_LGA-20_4.7x4.5mm_P0.65mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://ams.com/documents/20143/36005/AS7261_DS000493_1-00.pdf/0e7d1f12-702e-d061-b07a-67b0b6316800"
			(at 15.24 5.08 0)
		)
		(property "Description" "Spectral Sensing Engine, 6-Channel XYZ Spectral_ID"
			(at 0 0 0)
		)
		(property "ki_keywords" "6-Channel XYZ Spectral_ID Device Electronic Shutter Smart Interface i2c uart"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AMS?LGA*4.7x4.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AS7261_0_1")
		(symbol "AS7261_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "~{RES}")
				(number "2")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "INT")
				(number "13")
			)
			(pin no_connect line
				(at -12.7 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NF")
				(number "10")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "CSN_EE")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "CSN_SD")
				(number "7")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "LED_DRV")
				(number "15")
			)
			(pin output line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "LED_IND")
				(number "18")
			)
			(pin no_connect line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NF")
				(number "19")
			)
			(pin no_connect line
				(at -10.16 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NF")
				(number "20")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "16")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin no_connect line
				(at 10.16 10.16 180)
				(length 2.54)
				(hide yes)
				(name "NF")
				(number "1")
			)
			(pin no_connect line
				(at 10.16 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "NF")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "MISO")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "MOSI")
				(number "4")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SCK")
				(number "3")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "TX/SDA_S")
				(number "12")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "RX/SCL_S")
				(number "11")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "I2C_ENB")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AS72651"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 20.32 0)
		)
		(property "Value" "AS72651"
			(at 7.62 20.32 0)
		)
		(property "Footprint" "Package_LGA:AMS_LGA-20_4.7x4.5mm_P0.65mm"
			(at 0 -27.94 0)
		)
		(property "Datasheet" "https://ams.com/documents/20143/36005/AS7265x_DS000612_1-00.pdf/08051c8a-a7f6-6231-7993-2d3fe0bf38b8"
			(at 10.16 -2.54 0)
		)
		(property "Description" "Smart 18-Channel VIS+NIR Spectral_ID Sensor with Electronic Shutter, LGA-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Smart Spectral Sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AMS?LGA*4.7x4.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AS72651_0_1")
		(symbol "AS72651_1_1"
			(pin output line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "INT")
				(number "13")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "RX/SCL_S")
				(number "11")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "TX/SDA_S")
				(number "12")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "I2C_ENB")
				(number "8")
			)
			(pin output line
				(at -12.7 0 0)
				(length 2.54)
				(name "SCL_M")
				(number "9")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SDA_M")
				(number "10")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{SLV1_RES}")
				(number "1")
			)
			(pin output line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "~{SLV2_RES}")
				(number "20")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "~{RES}")
				(number "2")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "VDD1")
				(number "17")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "16")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "VDD2")
				(number "14")
			)
			(pin no_connect line
				(at 10.16 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 10.16 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "19")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "LED_IND")
				(number "18")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "LED_DRV")
				(number "15")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "MOSI")
				(number "4")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "MISO")
				(number "5")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "SCK")
				(number "3")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "~{CS}")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AS7341DLG"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 8.255 0)
		)
		(property "Value" "AS7341DLG"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_LGA:AMS_OLGA-8_2x3.1mm_P0.8mm"
			(at 3.81 -6.35 0)
		)
		(property "Datasheet" "https://ams.com/documents/20143/36005/AS7341_DS000504_3-00.pdf"
			(at 3.81 -8.89 0)
		)
		(property "Description" "11-Channel Multi-Spectral Digital Sensor, OLGA-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "11-Channel Spectral i2c optical color"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AMS*OLGA*2x3.1mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "AS7341DLG_0_1")
		(symbol "AS7341DLG_1_1"
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "8")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "SCL")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "GPIO")
				(number "6")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "PGND")
				(number "5")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "LDR")
				(number "4")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "INT")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BP103"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "BP103"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-18-3_Lens"
			(at 5.207 -3.556 0)
		)
		(property "Datasheet" "http://www.osram-os.com/Graphics/XPic3/00101777_0.pdf/BP"
			(at 0 0 0)
		)
		(property "Description" "NPN Phototransistor"
			(at 0 0 0)
		)
		(property "ki_keywords" "npn phototransistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?18*Lens*"
			(at 0 0 0)
		)
		(symbol "BP103_0_0")
		(symbol "BP103_0_1")
		(symbol "BP103_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 5.08)
				(name "B")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BP104-SMD"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0.508 1.778 0)
		)
		(property "Value" "BP104-SMD"
			(at -1.016 -2.794 0)
		)
		(property "Footprint" "OptoDevice:Osram_BP104-SMD"
			(at 0 4.445 0)
		)
		(property "Datasheet" "https://dammedia.osram.info/media/resource/hires/osram-dam-5989350/BP%20104%20FAS_EN.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Silicon PIN Photodiode,  Area 2.2x2.2mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto photodiode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Osram*BP104*"
			(at 0 0 0)
		)
		(symbol "BP104-SMD_0_1")
		(symbol "BP104-SMD_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BPW21"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0.508 1.778 0)
		)
		(property "Value" "BPW21"
			(at -1.016 -2.794 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-5-2_Window"
			(at 0 4.445 0)
		)
		(property "Datasheet" "http://techwww.in.tu-clausthal.de/site/Dokumentation/Dioden/Fotodioden/BPW21-Fotodiode.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Silicon Photodiode for the visible spectral range, TO-5 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto photodiode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?5*Window*"
			(at 0 0 0)
		)
		(symbol "BPW21_0_1")
		(symbol "BPW21_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "K")
				(number "2")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 2.54)
				(name "A")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BPW34"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0.508 1.778 0)
		)
		(property "Value" "BPW34"
			(at -1.016 -2.794 0)
		)
		(property "Footprint" "OptoDevice:Osram_DIL2_4.3x4.65mm_P5.08mm"
			(at 0 4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/81521/bpw34.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Silicon PIN Photodiode"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto PIN photodiode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Osram*DIL2*4.3x4.65mm*P5.08*"
			(at 0 0 0)
		)
		(symbol "BPW34_0_1")
		(symbol "BPW34_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BPW40"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "BPW40"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "LED_THT:LED_D5.0mm_Clear"
			(at 12.192 -3.556 0)
		)
		(property "Datasheet" "https://www.rcscomponents.kiev.ua/datasheets/bpw40.pdf"
			(at 0 0 0)
		)
		(property "Description" "Phototransistor NPN"
			(at 0 0 0)
		)
		(property "ki_keywords" "npn phototransistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*D5.0mm*Clear*"
			(at 0 0 0)
		)
		(symbol "BPW40_0_1")
		(symbol "BPW40_1_1"
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BPW82"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0.508 1.778 0)
		)
		(property "Value" "BPW82"
			(at -1.016 -2.794 0)
		)
		(property "Footprint" "OptoDevice:Osram_BPW82"
			(at 0 4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/81529/bpw82.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Silicon PIN Photodiode with Daylight Blocking Filter"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto photo diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Osram*BPW82*"
			(at 0 0 0)
		)
		(symbol "BPW82_0_1")
		(symbol "BPW82_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BPX65"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0.508 1.778 0)
		)
		(property "Value" "BPX65"
			(at -1.016 -2.794 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-18-2_Lens"
			(at 0 4.445 0)
		)
		(property "Datasheet" "http://www.osram-os.com/Graphics/XPic1/00181579_0.pdf/BPX%2065,%20Lead%20(Pb)%20Free%20Product%20-%20RoHS%20Compliant.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Silicon PIN Photodiode, TO-18 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto PIN photo diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?18*Lens*"
			(at 0 0 0)
		)
		(symbol "BPX65_0_1")
		(symbol "BPX65_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "C12880MA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 13.97 0)
		)
		(property "Value" "C12880MA"
			(at 0 11.43 0)
		)
		(property "Footprint" "OptoDevice:Hamamatsu_C12880"
			(at -2.54 11.43 0)
		)
		(property "Datasheet" "http://www.hamamatsu.com/resources/pdf/ssd/c12880ma_kacc1226e.pdf"
			(at 0 13.97 0)
		)
		(property "Description" "Micro spectrometer 340 to 850nm resolution 15nm"
			(at 0 0 0)
		)
		(property "ki_keywords" "spectrometer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Hamamatsu*C12880*"
			(at 0 0 0)
		)
		(symbol "C12880MA_0_1")
		(symbol "C12880MA_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CLK")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "ST")
				(number "6")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin power_in line
				(at -5.08 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "CASE")
				(number "5")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "TRG")
				(number "7")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "EOS")
				(number "9")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "VIDEO")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Flir_LEPTON"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 21.59 0)
		)
		(property "Value" "Flir_LEPTON"
			(at -15.24 19.05 0)
		)
		(property "Footprint" ""
			(at -17.78 19.05 0)
		)
		(property "Datasheet" "https://cdn.sparkfun.com/datasheets/Sensors/Infrared/FLIR_Lepton_Data_Brief.pdf"
			(at -15.24 21.59 0)
		)
		(property "Description" "LWIR camera 8 to 14um 80x60 pixel"
			(at 0 0 0)
		)
		(property "ki_keywords" "LWIR camera"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*105028*1001* *105028*2011*"
			(at 0 0 0)
		)
		(symbol "Flir_LEPTON_0_1")
		(symbol "Flir_LEPTON_1_1"
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "SPI_CS_L")
				(number "14")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "SPI_CLK")
				(number "13")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "SPI_MOSI")
				(number "11")
			)
			(pin output line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "SPI_MISO")
				(number "12")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "SCL")
				(number "21")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "SDA")
				(number "22")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PWR_DWN_L")
				(number "23")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "RESET_L")
				(number "24")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "MASTER_CLK")
				(number "26")
			)
			(pin power_in line
				(at -12.7 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at -10.16 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at -7.62 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at -5.08 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "VDDC")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VDDIO")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "15")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "18")
			)
			(pin power_in line
				(at 5.08 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "20")
			)
			(pin power_in line
				(at 7.62 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "25")
			)
			(pin power_in line
				(at 10.16 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "27")
			)
			(pin power_in line
				(at 12.7 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "30")
			)
			(pin no_connect line
				(at 15.24 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "MIPI_CLK_N")
				(number "28")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "MIPI_CLK_P")
				(number "29")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "MIPI_DATA_N")
				(number "31")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "MIPI_DATA_P")
				(number "32")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "GPIO0")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "GPIO1")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "GPIO2")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "GPIO3")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISL29035"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "ISL29035"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "OptoDevice:Renesas_DFN-6_1.5x1.6mm_P0.5mm"
			(at 0 11.43 0)
		)
		(property "Datasheet" "https://www.renesas.com/us/en/document/dst/isl29035-datasheet"
			(at 0 8.89 0)
		)
		(property "Description" "ambient light sensor, i2c interface, 2.25-3.63V, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "ambient light sensor i2c"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Renesas*DFN*1.5x1.6mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ISL29035_0_1")
		(symbol "ISL29035_1_1"
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "6")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "5")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~INT")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KPS-3227"
		(pin_numbers
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 3.81 1.27 0)
		)
		(property "Value" "KPS-3227"
			(at 7.62 -1.27 0)
		)
		(property "Footprint" "OptoDevice:Kingbright_KPS-3227"
			(at 0 3.81 0)
		)
		(property "Datasheet" "https://www.kingbright.com/attachments/file/psearch/000/00/00/KPS-3227SP1C(Ver.16).pdf"
			(at 0 3.81 0)
		)
		(property "Description" "Ambient light NPN phototransistor, KPS-3227"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kingbright npn phototransistor ambient light photo sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Kingbright*KPS?3227*"
			(at 0 0 0)
		)
		(symbol "KPS-3227_1_1"
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KPS-5130"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at -4.064 10.16 0)
		)
		(property "Value" "KPS-5130"
			(at 0 -8.89 0)
		)
		(property "Footprint" "OptoDevice:Kingbright_KPS-5130"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.kingbright.com/attachments/file/psearch/000/00/20160808bak/KPS-5130PD7C(Ver.13).pdf"
			(at -1.27 0 0)
		)
		(property "Description" "RGB Colour Sensor, KPS-5130"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto photodiode RGB colour sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Kingbright*KPS?5130*"
			(at 0 0 0)
		)
		(symbol "KPS-5130_0_0"
			(text "R"
				(at 2.032 6.223 0)
			)
			(text "G"
				(at 2.159 1.27 0)
			)
			(text "B"
				(at 2.286 -3.81 0)
			)
		)
		(symbol "KPS-5130_0_1")
		(symbol "KPS-5130_1_1"
			(pin passive line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "AR")
				(number "1")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "AG")
				(number "2")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "AB")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "C")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LDR03"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -5.08 0 90)
		)
		(property "Value" "LDR03"
			(at 1.905 0 90)
		)
		(property "Footprint" "OptoDevice:R_LDR_10x8.5mm_P7.6mm_Vertical"
			(at 4.445 0 90)
		)
		(property "Datasheet" "http://www.elektronica-componenten.nl/WebRoot/StoreNL/Shops/61422969/54F1/BA0C/C664/31B9/2173/C0A8/2AB9/2AEF/LDR03IMP.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "light dependent resistor"
			(at 0 0 0)
		)
		(property "ki_keywords" "light dependent photo resistor LDR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "R*LDR*10x8.5mm*P7.6mm*"
			(at 0 0 0)
		)
		(symbol "LDR03_0_1")
		(symbol "LDR03_1_1"
			(pin passive line
				(at 0 3.81 270)
				(length 1.27)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 1.27)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LDR07"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -5.08 0 90)
		)
		(property "Value" "LDR07"
			(at 1.905 0 90)
		)
		(property "Footprint" "OptoDevice:R_LDR_5.1x4.3mm_P3.4mm_Vertical"
			(at 4.445 0 90)
		)
		(property "Datasheet" "http://www.tme.eu/de/Document/f2e3ad76a925811312d226c31da4cd7e/LDR07.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "light dependent resistor"
			(at 0 0 0)
		)
		(property "ki_keywords" "light dependent photo resistor LDR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "R*LDR*5.1x4.3mm*P3.4mm*"
			(at 0 0 0)
		)
		(symbol "LDR07_0_1")
		(symbol "LDR07_1_1"
			(pin passive line
				(at 0 3.81 270)
				(length 1.27)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 1.27)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LPT80A"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at -5.08 6.35 0)
		)
		(property "Value" "LPT80A"
			(at -8.89 -3.81 0)
		)
		(property "Footprint" "OptoDevice:Osram_LPT80A"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://www.osram-os.com/Graphics/XPic4/00209607_0.pdf/LPT%2080A.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "NPN phototransistor"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN phototransistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Osram*LPT80A*"
			(at 0 0 0)
		)
		(symbol "LPT80A_0_1")
		(symbol "LPT80A_1_1"
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "C")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTR-303ALS-01"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "LTR-303ALS-01"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "OptoDevice:Lite-On_LTR-303ALS-01"
			(at 0 11.43 0)
		)
		(property "Datasheet" "https://optoelectronics.liteon.com/upload/download/DS86-2013-0004/LTR-303ALS-01_DS_V1.pdf"
			(at -7.62 8.89 0)
		)
		(property "Description" "ambient light sensor, i2c interface, 0.01 to 64k lux, 2.4-3.6V"
			(at 0 0 0)
		)
		(property "ki_keywords" "ambient light sensor i2c"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Lite*On*LTR*303ALS*01*"
			(at 0 0 0)
		)
		(symbol "LTR-303ALS-01_0_1")
		(symbol "LTR-303ALS-01_1_1"
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "6")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SCL")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "INT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "M9960"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -5.08 0 90)
		)
		(property "Value" "M9960"
			(at 1.905 0 90)
		)
		(property "Footprint" "OptoDevice:R_LDR_5.2x5.2mm_P3.5mm_Horizontal"
			(at 4.445 0 90)
		)
		(property "Datasheet" "http://cdn-reichelt.de/documents/datenblatt/A500/M996011a_b.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "light dependent resistor"
			(at 0 0 0)
		)
		(property "ki_keywords" "light dependent photo resistor LDR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "R*LDR*5.2x5.2mm*P3.5mm*"
			(at 0 0 0)
		)
		(symbol "M9960_0_1")
		(symbol "M9960_1_1"
			(pin passive line
				(at 0 3.81 270)
				(length 1.27)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 1.27)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NOA1305"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "NOA1305"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NOA1305-D.PDF"
			(at 17.78 8.89 0)
		)
		(property "Description" "Ambient Light Sensor with I2C Interface and Dark Current Compensation"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto ambient light sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*6*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "NOA1305_0_0"
			(text "ADC"
				(at -1.143 0.381 0)
			)
			(text "CTRL"
				(at 2.794 0.254 900)
			)
		)
		(symbol "NOA1305_0_1")
		(symbol "NOA1305_1_1"
			(pin no_connect line
				(at -10.16 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin passive line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "EP")
				(number "7")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "1")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "4")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "SCL")
				(number "3")
			)
			(pin open_collector line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "INT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PMTx08Dyn"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "PMT"
			(at -8.89 26.67 0)
		)
		(property "Value" "PMTx08Dyn"
			(at 7.62 26.67 0)
		)
		(property "Footprint" ""
			(at 0 2.54 90)
		)
		(property "Datasheet" "~"
			(at 0 2.54 90)
		)
		(property "Description" "8-stage photomultiplier tube"
			(at 0 0 0)
		)
		(property "ki_keywords" "PMT 8-stage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PMT*"
			(at 0 0 0)
		)
		(symbol "PMTx08Dyn_0_1")
		(symbol "PMTx08Dyn_1_1"
			(pin passive line
				(at 0 30.48 270)
				(length 7.62)
				(name "Photocathode")
				(number "K")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 7.62)
				(name "Anode")
				(number "P")
			)
			(pin passive line
				(at 17.78 17.78 180)
				(length 7.62)
				(name "Dynode")
				(number "Dy1")
			)
			(pin passive line
				(at 17.78 12.7 180)
				(length 7.62)
				(name "Dynode")
				(number "Dy2")
			)
			(pin passive line
				(at 17.78 7.62 180)
				(length 7.62)
				(name "Dynode")
				(number "Dy3")
			)
			(pin passive line
				(at 17.78 2.54 180)
				(length 7.62)
				(name "Dynode")
				(number "Dy4")
			)
			(pin passive line
				(at 17.78 -2.54 180)
				(length 7.62)
				(name "Dynode")
				(number "Dy5")
			)
			(pin passive line
				(at 17.78 -7.62 180)
				(length 7.62)
				(name "Dynode")
				(number "Dy6")
			)
			(pin passive line
				(at 17.78 -12.7 180)
				(length 7.62)
				(name "Dynode")
				(number "Dy7")
			)
			(pin passive line
				(at 17.78 -17.78 180)
				(length 7.62)
				(name "Dynode")
				(number "Dy8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PMTx08Dyn_Shld"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "PMT"
			(at -8.89 26.67 0)
		)
		(property "Value" "PMTx08Dyn_Shld"
			(at 8.89 26.67 0)
		)
		(property "Footprint" ""
			(at 0 2.54 90)
		)
		(property "Datasheet" "~"
			(at 0 2.54 90)
		)
		(property "Description" "8-stage photomultiplier tube with electrostatic and magnetic shield"
			(at 0 0 0)
		)
		(property "ki_keywords" "PMT 8-stage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PMT*"
			(at 0 0 0)
		)
		(symbol "PMTx08Dyn_Shld_0_1")
		(symbol "PMTx08Dyn_Shld_1_1"
			(pin passive line
				(at -15.24 0 0)
				(length 5.08)
				(name "Magnetic")
				(number "M")
			)
			(pin passive line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "Electrostatic")
				(number "E")
			)
			(pin passive line
				(at 0 30.48 270)
				(length 7.62)
				(name "Photocathode")
				(number "K")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 7.62)
				(name "Anode")
				(number "P")
			)
			(pin passive line
				(at 17.78 17.78 180)
				(length 7.62)
				(name "Dynode")
				(number "Dy1")
			)
			(pin passive line
				(at 17.78 12.7 180)
				(length 7.62)
				(name "Dynode")
				(number "Dy2")
			)
			(pin passive line
				(at 17.78 7.62 180)
				(length 7.62)
				(name "Dynode")
				(number "Dy3")
			)
			(pin passive line
				(at 17.78 2.54 180)
				(length 7.62)
				(name "Dynode")
				(number "Dy4")
			)
			(pin passive line
				(at 17.78 -2.54 180)
				(length 7.62)
				(name "Dynode")
				(number "Dy5")
			)
			(pin passive line
				(at 17.78 -7.62 180)
				(length 7.62)
				(name "Dynode")
				(number "Dy6")
			)
			(pin passive line
				(at 17.78 -12.7 180)
				(length 7.62)
				(name "Dynode")
				(number "Dy7")
			)
			(pin passive line
				(at 17.78 -17.78 180)
				(length 7.62)
				(name "Dynode")
				(number "Dy8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "S13360-3025CS"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 1.778 1.778 0)
		)
		(property "Value" "S13360-3025CS"
			(at 0.254 -2.794 0)
		)
		(property "Footprint" "OptoDevice:Hamamatsu_S13360-30CS"
			(at 1.27 4.445 0)
		)
		(property "Datasheet" "http://www.hamamatsu.com/resources/pdf/ssd/s13360_series_kapd1052e.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "Multi-Pixel Photon Counter with 25µm pixel pitch"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto SiPM MPPC hamamatsu SPAD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Hamamatsu*S13360*30CS*"
			(at 0 0 0)
		)
		(symbol "S13360-3025CS_0_1")
		(symbol "S13360-3025CS_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "2")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "S5971"
		(pin_names
			(offset 0.254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 2.54 -5.08 0)
		)
		(property "Value" "S5971"
			(at 5.08 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-18-3"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.hamamatsu.com/resources/pdf/ssd/s5971_etc_kpin1025e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Si PIN Photodiode, 0.1 GHz, TO-18-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto photodiode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?18*"
			(at 0 0 0)
		)
		(symbol "S5971_0_0"
			(pin passive line
				(at 0 -7.62 90)
				(length 3.81)
				(name "C")
				(number "2")
			)
		)
		(symbol "S5971_0_1")
		(symbol "S5971_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 3.81)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 3.81)
				(name "A")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SFH203"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0.508 1.778 0)
		)
		(property "Value" "SFH203"
			(at -1.016 -2.794 0)
		)
		(property "Footprint" "LED_THT:LED_D5.0mm_IRGrey"
			(at 0 4.445 0)
		)
		(property "Datasheet" "http://www.osram-os.com/Graphics/XPic9/00101656_0.pdf/SFH%20203,%20SFH%20203%20FA,%20Lead%20(Pb)%20Free%20Product%20-%20RoHS%20Compliant.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Silicon PIN Photodiode"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto PIN photodiode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*D5.0mm*IRGrey*"
			(at 0 0 0)
		)
		(symbol "SFH203_0_1")
		(symbol "SFH203_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SFH205F"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0.508 1.778 0)
		)
		(property "Value" "SFH205F"
			(at -1.016 -2.794 0)
		)
		(property "Footprint" "OptoDevice:Osram_SFH205"
			(at 0 4.445 0)
		)
		(property "Datasheet" "http://www.osram-os.com/Graphics/XPic2/00101668_0.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Silicon PIN Photodiode with Daylight Blocking Filter"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto photo diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Osram*SFH205*"
			(at 0 0 0)
		)
		(symbol "SFH205F_0_1")
		(symbol "SFH205F_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SFH206K"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0.508 1.778 0)
		)
		(property "Value" "SFH206K"
			(at -1.016 -2.794 0)
		)
		(property "Footprint" "OptoDevice:Osram_SFH205"
			(at 0 4.445 0)
		)
		(property "Datasheet" "http://www.osram-os.com/Graphics/XPic0/00211439_0.pdf/SFH%20206%20K.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Silicon PIN Photodiode"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto PIN photodiode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Osram*SFH205*"
			(at 0 0 0)
		)
		(symbol "SFH206K_0_1")
		(symbol "SFH206K_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SFH216"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0.508 1.778 0)
		)
		(property "Value" "SFH216"
			(at -1.016 -2.794 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-18-2_Window"
			(at 0 4.445 0)
		)
		(property "Datasheet" "http://www.osram-os.com/Graphics/XPic1/00029253_0.pdf/SFH"
			(at -1.27 0 0)
		)
		(property "Description" "Silicon PIN Photodiode With Very Short Switching Time, TO-18 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto PIN photo diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?18*Window*"
			(at 0 0 0)
		)
		(symbol "SFH216_0_1")
		(symbol "SFH216_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SFH225FA"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0.508 1.778 0)
		)
		(property "Value" "SFH225FA"
			(at -1.016 -2.794 0)
		)
		(property "Footprint" "OptoDevice:Osram_SFH225"
			(at 0 4.445 0)
		)
		(property "Datasheet" "http://www.osram-os.com/Graphics/XPic0/00209685_0.pdf/SFH%20225%20FA.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Silicon PIN Photodiode with Daylight Blocking Filter"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto PIN photodiode IR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Osram*SFH225*"
			(at 0 0 0)
		)
		(symbol "SFH225FA_0_1")
		(symbol "SFH225FA_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SFH2400"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0.508 1.778 0)
		)
		(property "Value" "SFH2400"
			(at -1.016 -2.794 0)
		)
		(property "Footprint" "OptoDevice:Osram_SMD-SmartDIL"
			(at 0 4.445 0)
		)
		(property "Datasheet" "http://www.osram-os.com/Graphics/XPic5/00215665_0.pdf/SFH%202400.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Silicon PIN Photodiode, SMD package"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto photodiode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Osram*SMD*SmartDIL*"
			(at 0 0 0)
		)
		(symbol "SFH2400_0_1")
		(symbol "SFH2400_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SFH2701"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0.508 1.778 0)
		)
		(property "Value" "SFH2701"
			(at -1.016 -2.794 0)
		)
		(property "Footprint" "LED_SMD:LED_1206_3216Metric_Castellated"
			(at 0 4.445 0)
		)
		(property "Datasheet" "http://www.osram-os.com/Graphics/XPic6/00201111_0.pdf/SFH%202701.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "High Speed PIN Photodiode, SMD package"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto photodiode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*1206*"
			(at 0 0 0)
		)
		(symbol "SFH2701_0_1")
		(symbol "SFH2701_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SFH309"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "SFH309"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "LED_THT:LED_D3.0mm_Clear"
			(at 12.192 -3.556 0)
		)
		(property "Datasheet" "http://www.osram-os.com/Graphics/XPic2/00101811_0.pdf/SFH%20309,%20SFH%20309%20FA,%20Lead%20(Pb)%20Free%20Product%20-%20RoHS%20Compliant.pdf"
			(at 0 0 0)
		)
		(property "Description" "Phototransistor NPN"
			(at 0 0 0)
		)
		(property "ki_keywords" "npn phototransistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*3.0mm*Clear*"
			(at 0 0 0)
		)
		(symbol "SFH309_0_1")
		(symbol "SFH309_1_1"
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SFH3201"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 2.54 1.27 0)
		)
		(property "Value" "SFH3201"
			(at 2.54 -1.27 0)
		)
		(property "Footprint" "OptoDevice:Osram_SFH9x0x"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://dammedia.osram.info/media/resource/hires/osram-dam-2495980/SFH%203201.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Silicon NPN phototransistor, SMD-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN phototransistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Osram*SFH9x0x*"
			(at 0 0 0)
		)
		(symbol "SFH3201_0_1")
		(symbol "SFH3201_1_1"
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "C")
				(number "4")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "E")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TSL2550D"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.985 6.35 0)
		)
		(property "Value" "TSL2550D"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://ams.com/eng/content/download/250130/975613/142977"
			(at 16.51 7.62 0)
		)
		(property "Description" "Ambient Light Sensor with SMbus Interface, SO-8 interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto ambient light sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TSL2550D_0_0"
			(text "ADC"
				(at 0.127 -0.889 0)
			)
			(text "CTRL"
				(at 4.064 -1.016 900)
			)
		)
		(symbol "TSL2550D_0_1")
		(symbol "TSL2550D_1_1"
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -7.62 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "DAT")
				(number "8")
			)
			(pin input clock
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CLK")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TSL2550T"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TSL2550T"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "OptoDevice:AMS_TSL2550_SMD"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://ams.com/eng/content/download/250130/975613/142977"
			(at 19.05 7.62 0)
		)
		(property "Description" "Ambient Light Sensor with SMbus Interface, T-4 interface SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto ambient light sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AMS*TSL2550*SMD*"
			(at 0 0 0)
		)
		(symbol "TSL2550T_0_0"
			(text "ADC"
				(at 0.127 -0.889 0)
			)
			(text "CTRL"
				(at 4.064 -1.016 900)
			)
		)
		(symbol "TSL2550T_0_1")
		(symbol "TSL2550T_1_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "DAT")
				(number "4")
			)
			(pin input clock
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CLK")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TSL25911FN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "TSL25911FN"
			(at 0 -6.35 0)
		)
		(property "Footprint" "OptoDevice:AMS_TSL25911FN"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://ams.com/documents/20143/9331680/TSL2591_DS000338_7-00.pdf"
			(at 0 -11.43 0)
		)
		(property "Description" "Light to digital converter, 2.7 to 3.6V Vdd, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "ALS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AMS*TSL25911FN*"
			(at 0 0 0)
		)
		(symbol "TSL25911FN_0_0"
			(text "ADC"
				(at -0.635 0 0)
			)
		)
		(symbol "TSL25911FN_0_1")
		(symbol "TSL25911FN_1_0")
		(symbol "TSL25911FN_1_1"
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_in line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "6")
			)
			(pin input clock
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "1")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "INT")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VT93xx"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "R"
			(at -5.08 0 90)
		)
		(property "Value" "VT93xx"
			(at 1.905 0 90)
		)
		(property "Footprint" "OptoDevice:R_LDR_4.9x4.2mm_P2.54mm_Vertical"
			(at 4.445 0 90)
		)
		(property "Datasheet" "http://www.produktinfo.conrad.com/datenblaetter/125000-149999/140375-da-01-en-FOTOWIDERSTAND__VT_93_N2__THT_.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "light dependent resistor"
			(at 0 0 0)
		)
		(property "ki_keywords" "light dependent photo resistor LDR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "R*LDR*4.9x4.2mm*P2.54mm*"
			(at 0 0 0)
		)
		(symbol "VT93xx_0_1")
		(symbol "VT93xx_1_1"
			(pin passive line
				(at 0 3.81 270)
				(length 1.27)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 1.27)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "A1060"
		(extends "A1050")
		(property "Reference" "R"
			(at -5.08 0 90)
		)
		(property "Value" "A1060"
			(at 1.905 0 90)
		)
		(property "Footprint" "OptoDevice:R_LDR_D6.4mm_P3.4mm_Vertical"
			(at 4.445 0 90)
		)
		(property "Datasheet" "http://cdn-reichelt.de/documents/datenblatt/A500/A106012.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "light dependent resistor"
			(at 0 0 0)
		)
		(property "ki_keywords" "light dependent photo resistor LDR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "R*LDR*D6.4*P3.4*"
			(at 0 0 0)
		)
	)
	(symbol "A9013"
		(extends "A9050")
		(property "Reference" "R"
			(at -5.08 0 90)
		)
		(property "Value" "A9013"
			(at 1.905 0 90)
		)
		(property "Footprint" "OptoDevice:R_LDR_5.0x4.1mm_P3mm_Vertical"
			(at 4.445 0 90)
		)
		(property "Datasheet" "http://www.produktinfo.conrad.com/datenblaetter/125000-149999/145475-da-01-en-FOTOWIDERSTAND_A_9060_A_9013.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "light dependent resistor"
			(at 0 0 0)
		)
		(property "ki_keywords" "light dependent photo resistor LDR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "R*LDR*5.0x4.1mm*P3mm*"
			(at 0 0 0)
		)
	)
	(symbol "A9060"
		(extends "A9050")
		(property "Reference" "R"
			(at -5.08 0 90)
		)
		(property "Value" "A9060"
			(at 1.905 0 90)
		)
		(property "Footprint" "OptoDevice:R_LDR_5.0x4.1mm_P3mm_Vertical"
			(at 4.445 0 90)
		)
		(property "Datasheet" "http://cdn-reichelt.de/documents/datenblatt/A500/A90xxxx%23PE.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "light dependent resistor"
			(at 0 0 0)
		)
		(property "ki_keywords" "light dependent photo resistor LDR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "R*LDR*5.0x4.1mm*P3mm*"
			(at 0 0 0)
		)
	)
	(symbol "AS7262"
		(extends "AS7261")
		(property "Reference" "U"
			(at -10.16 17.78 0)
		)
		(property "Value" "AS7262"
			(at -10.16 15.24 0)
		)
		(property "Footprint" "Package_LGA:AMS_LGA-20_4.7x4.5mm_P0.65mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://ams.com/documents/20143/36005/AS7262_DS000486_5-00.pdf"
			(at 15.24 5.08 0)
		)
		(property "Description" "Spectral Sensing Engine, 6-Channel Visible Spectral_ID"
			(at 0 0 0)
		)
		(property "ki_keywords" "6-Channel Visible Spectral_ID Device Electronic Shutter Smart Interface i2c uart"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AMS?LGA*4.7x4.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AS7263"
		(extends "AS7261")
		(property "Reference" "U"
			(at -10.16 17.78 0)
		)
		(property "Value" "AS7263"
			(at -10.16 15.24 0)
		)
		(property "Footprint" "Package_LGA:AMS_LGA-20_4.7x4.5mm_P0.65mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://ams.com/documents/20143/36005/AS7263_DS000476_4-00.pdf"
			(at 15.24 5.08 0)
		)
		(property "Description" "Spectral Sensing Engine, 6-Channel NIR Spectral_ID"
			(at 0 0 0)
		)
		(property "ki_keywords" "6-Channel NIR Spectral_ID Device Electronic Shutter Smart Interface i2c uart"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AMS?LGA*4.7x4.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AS7343xDLG"
		(extends "AS7341DLG")
		(property "Reference" "U"
			(at -2.54 8.255 0)
		)
		(property "Value" "AS7343xDLG"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_LGA:AMS_OLGA-8_2x3.1mm_P0.8mm"
			(at 3.81 -6.35 0)
		)
		(property "Datasheet" "https://ams.com/documents/20143/6705498/AS7343_DS001046_6_00.pdf"
			(at 3.81 -8.89 0)
		)
		(property "Description" "14-Channel Multi-Spectral Digital Sensor including XYZ, Clear and Flicker Detection, 380 - 1000 nm,OLGA-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "14-Channel Spectral i2c optical color"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "AMS*OLGA*2x3.1mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "BP103B"
		(extends "BPW40")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "BP103B"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "LED_THT:LED_D5.0mm_Clear"
			(at 12.192 -3.556 0)
		)
		(property "Datasheet" "http://www.b-kainka.de/Daten/Sensor/bp103bf.pdf"
			(at 0 0 0)
		)
		(property "Description" "NPN phototransistor"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN phototransistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*D5.0mm*Clear*"
			(at 0 0 0)
		)
	)
	(symbol "BP103BF"
		(extends "BPW40")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "BP103BF"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "LED_THT:LED_D5.0mm_Clear"
			(at 12.192 -3.556 0)
		)
		(property "Datasheet" "http://www.b-kainka.de/Daten/Sensor/bp103bf.pdf"
			(at 0 0 0)
		)
		(property "Description" "NPN phototransistor with daylight filter"
			(at 0 0 0)
		)
		(property "ki_keywords" "IR NPN phototransistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*D5.0mm*Clear*"
			(at 0 0 0)
		)
	)
	(symbol "BP104"
		(extends "BPW34")
		(property "Reference" "D"
			(at 0.508 1.778 0)
		)
		(property "Value" "BP104"
			(at -1.016 -2.794 0)
		)
		(property "Footprint" "OptoDevice:Osram_DIL2_4.3x4.65mm_P5.08mm"
			(at 0 4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/81500/81500.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Silicon PIN Photodiode"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto PIN photodiode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Osram*DIL2*4.3x4.65mm*P5.08*"
			(at 0 0 0)
		)
	)
	(symbol "BPW34-SMD"
		(extends "BP104-SMD")
		(property "Reference" "D"
			(at 0.508 1.778 0)
		)
		(property "Value" "BPW34-SMD"
			(at -1.016 -2.794 0)
		)
		(property "Footprint" "OptoDevice:Osram_BPW34S-SMD"
			(at 0 4.445 0)
		)
		(property "Datasheet" "https://dammedia.osram.info/media/resource/hires/osram-dam-5488319/BPW%2034%20S_EN.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Silicon PIN Photodiode, Area 2.65x2.65mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto photodiode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Osram*BPW34S*"
			(at 0 0 0)
		)
	)
	(symbol "BPW42"
		(extends "SFH309")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "BPW42"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "LED_THT:LED_D3.0mm_Clear"
			(at 12.192 -3.556 0)
		)
		(property "Datasheet" "http://www.ges.cz/sheets/b/bpw42.pdf"
			(at 0 0 0)
		)
		(property "Description" "NPN phototransistor"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN phototransistor opto"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*3.0mm*Clear*"
			(at 0 0 0)
		)
	)
	(symbol "BPW85"
		(extends "SFH309")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "BPW85"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "LED_THT:LED_D3.0mm_Clear"
			(at 12.192 -3.556 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/81531/bpw85a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Silicon NPN Phototransistor, Ica = 0.8-8mA, T-1"
			(at 0 0 0)
		)
		(property "ki_keywords" "npn phototransistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*3.0mm*Clear*"
			(at 0 0 0)
		)
	)
	(symbol "BPW85A"
		(extends "SFH309")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "BPW85A"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "LED_THT:LED_D3.0mm_Clear"
			(at 12.192 -3.556 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/81531/bpw85a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Silicon NPN Phototransistor, Ica = 0.8-2.5mA, T-1"
			(at 0 0 0)
		)
		(property "ki_keywords" "npn phototransistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*3.0mm*Clear*"
			(at 0 0 0)
		)
	)
	(symbol "BPW85B"
		(extends "SFH309")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "BPW85B"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "LED_THT:LED_D3.0mm_Clear"
			(at 12.192 -3.556 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/81531/bpw85a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Silicon NPN Phototransistor, Ica = 1.5-4mA, T-1"
			(at 0 0 0)
		)
		(property "ki_keywords" "npn phototransistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*3.0mm*Clear*"
			(at 0 0 0)
		)
	)
	(symbol "BPW85C"
		(extends "SFH309")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "BPW85C"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "LED_THT:LED_D3.0mm_Clear"
			(at 12.192 -3.556 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/81531/bpw85a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Silicon NPN Phototransistor, Ica = 3-8mA, T-1"
			(at 0 0 0)
		)
		(property "ki_keywords" "npn phototransistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*3.0mm*Clear*"
			(at 0 0 0)
		)
	)
	(symbol "BPX61"
		(extends "BPW21")
		(property "Reference" "D"
			(at 0.508 1.778 0)
		)
		(property "Value" "BPX61"
			(at -1.016 -2.794 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-5-2_Window"
			(at 0 4.445 0)
		)
		(property "Datasheet" "http://www.osram-os.com/Graphics/XPic3/00101650_0.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Silicon Photodiode for the visible spectral range"
			(at 0 0 0)
		)
		(property "ki_keywords" "photodiode opto"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?5*Window*"
			(at 0 0 0)
		)
	)
	(symbol "BPY62"
		(extends "BP103")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "BPY62"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-18-3_Lens"
			(at 5.207 -3.556 0)
		)
		(property "Datasheet" "http://www.osram-os.com/Graphics/XPic9/00208595_0.pdf"
			(at 0 0 0)
		)
		(property "Description" "NPN Phototransistor"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Phototransistor opto"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?18*Lens*"
			(at 0 0 0)
		)
	)
	(symbol "S13360-3050CS"
		(extends "S13360-3025CS")
		(property "Reference" "D"
			(at 1.778 1.778 0)
		)
		(property "Value" "S13360-3050CS"
			(at 0.254 -2.794 0)
		)
		(property "Footprint" "OptoDevice:Hamamatsu_S13360-30CS"
			(at 1.27 4.445 0)
		)
		(property "Datasheet" "http://www.hamamatsu.com/resources/pdf/ssd/s13360_series_kapd1052e.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "Multi-Pixel Photon Counter with 50µm pixel pitch"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto SiPM MPPC hamamatsu SPAD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Hamamatsu*S13360*30CS*"
			(at 0 0 0)
		)
	)
	(symbol "S13360-3075CS"
		(extends "S13360-3025CS")
		(property "Reference" "D"
			(at 1.778 1.778 0)
		)
		(property "Value" "S13360-3075CS"
			(at 0.254 -2.794 0)
		)
		(property "Footprint" "OptoDevice:Hamamatsu_S13360-30CS"
			(at 1.27 4.445 0)
		)
		(property "Datasheet" "http://www.hamamatsu.com/resources/pdf/ssd/s13360_series_kapd1052e.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "Multi-Pixel Photon Counter with 75µm pixel pitch"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto SiPM MPPC hamamatsu SPAD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Hamamatsu*S13360*30CS*"
			(at 0 0 0)
		)
	)
	(symbol "S5972"
		(extends "S5971")
		(property "Reference" "D"
			(at 2.54 -5.08 0)
		)
		(property "Value" "S5972"
			(at 5.08 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-18-3"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.hamamatsu.com/resources/pdf/ssd/s5971_etc_kpin1025e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Si PIN Photodiode, 0.5 GHz, TO-18-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto photodiode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?18*"
			(at 0 0 0)
		)
	)
	(symbol "S5973"
		(extends "S5971")
		(property "Reference" "D"
			(at 2.54 -5.08 0)
		)
		(property "Value" "S5973"
			(at 5.08 5.08 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-18-3"
			(at 0 8.89 0)
		)
		(property "Datasheet" "https://www.hamamatsu.com/resources/pdf/ssd/s5971_etc_kpin1025e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Si PIN Photodiode, 1 GHz, TO-18-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto photodiode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?18*"
			(at 0 0 0)
		)
	)
	(symbol "SFH203FA"
		(extends "SFH203")
		(property "Reference" "D"
			(at 0.508 1.778 0)
		)
		(property "Value" "SFH203FA"
			(at -1.016 -2.794 0)
		)
		(property "Footprint" "LED_THT:LED_D5.0mm_IRGrey"
			(at 0 4.445 0)
		)
		(property "Datasheet" "http://www.osram-os.com/Graphics/XPic9/00101656_0.pdf/SFH%20203,%20SFH%20203%20FA,%20Lead%20(Pb)%20Free%20Product%20-%20RoHS%20Compliant.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Silicon PIN Photodiode with Daylight Blocking Filter"
			(at 0 0 0)
		)
		(property "ki_keywords" "PIN photodiode IR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*D5.0mm*IRGrey*"
			(at 0 0 0)
		)
	)
	(symbol "SFH205FA"
		(extends "SFH205F")
		(property "Reference" "D"
			(at 0.508 1.778 0)
		)
		(property "Value" "SFH205FA"
			(at -1.016 -2.794 0)
		)
		(property "Footprint" "OptoDevice:Osram_SFH205"
			(at 0 4.445 0)
		)
		(property "Datasheet" "http://www.osram-os.com/Graphics/XPic9/00101665_0.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Silicon PIN Photodiode with Daylight Blocking Filter"
			(at 0 0 0)
		)
		(property "ki_keywords" "PIN Photodiode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Osram*SFH205*"
			(at 0 0 0)
		)
	)
	(symbol "SFH235FA"
		(extends "SFH225FA")
		(property "Reference" "D"
			(at 0.508 1.778 0)
		)
		(property "Value" "SFH235FA"
			(at -1.016 -2.794 0)
		)
		(property "Footprint" "OptoDevice:Osram_SFH225"
			(at 0 4.445 0)
		)
		(property "Datasheet" "http://www.osram-os.com/Graphics/XPic3/00211469_0.pdf/SFH%20235%20FA.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Silicon PIN Photodiode with Daylight Blocking Filter"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto PIN photodiode IR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Osram*SFH225*"
			(at 0 0 0)
		)
	)
	(symbol "SFH2430"
		(extends "BP104-SMD")
		(property "Reference" "D"
			(at 0.508 1.778 0)
		)
		(property "Value" "SFH2430"
			(at -1.016 -2.794 0)
		)
		(property "Footprint" "OptoDevice:Osram_SFH2430"
			(at 0 4.445 0)
		)
		(property "Datasheet" "https://dammedia.osram.info/media/resource/hires/osram-dam-5467144/SFH%202430_EN.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Silicon Photodiode, Vf 1.2V, Area 2.65x2.65mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto photodiode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Osram*SFH2430*"
			(at 0 0 0)
		)
	)
	(symbol "SFH2440"
		(extends "BP104-SMD")
		(property "Reference" "D"
			(at 0.508 1.778 0)
		)
		(property "Value" "SFH2440"
			(at -1.016 -2.794 0)
		)
		(property "Footprint" "OptoDevice:Osram_SFH2440"
			(at 0 4.445 0)
		)
		(property "Datasheet" "https://dammedia.osram.info/media/resource/hires/osram-dam-5467146/SFH%202440_EN.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Silicon Photodiode, Vf 1V, Area 2.65x2.65mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto photodiode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Osram*SFH2440*"
			(at 0 0 0)
		)
	)
	(symbol "SFH300"
		(extends "BPW40")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "SFH300"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "LED_THT:LED_D5.0mm_Clear"
			(at 12.192 -3.556 0)
		)
		(property "Datasheet" "http://www.osram-os.com/Graphics/XPic2/00101785_0.pdf"
			(at 0 0 0)
		)
		(property "Description" "silicon NPN phototransistor"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN phototransistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*D5.0mm*Clear*"
			(at 0 0 0)
		)
	)
	(symbol "SFH320"
		(extends "SFH309")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "SFH320"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "LED_SMD:LED_PLCC-2_3.4x3.0mm_KA"
			(at 12.192 -3.556 0)
		)
		(property "Datasheet" "https://look.ams-osram.com/m/5397c5d8583a26cf/original/SFH-320.pdf"
			(at 0 0 0)
		)
		(property "Description" "Silicon NPN Phototransistor, PLCC-2"
			(at 0 0 0)
		)
		(property "ki_keywords" "npn phototransistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED?SMD:LED?PLCC?2?3.4x3.0mm?KA*"
			(at 0 0 0)
		)
	)
	(symbol "TEPT4400"
		(extends "SFH309")
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "TEPT4400"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" "LED_THT:LED_D3.0mm_Clear"
			(at 12.192 -3.556 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/81341/tept4400.pdf"
			(at 0 0 0)
		)
		(property "Description" "Ambient Light Sensor, NPN Epitaxial Planar Phototransistor, T-1"
			(at 0 0 0)
		)
		(property "ki_keywords" "npn phototransistor ambient light sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*3.0mm*Clear*"
			(at 0 0 0)
		)
	)
)
