(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "40PC015G"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "40PC015G"
			(at 6.35 6.35 0)
		)
		(property "Footprint" ""
			(at 2.54 0 0)
		)
		(property "Datasheet" "http://www.honeywellscportal.com//index.php?ci_id=138832"
			(at 2.54 0 0)
		)
		(property "Description" "Gauge pressure sensor, 0 to 15PSI, 5V supply, 0.2% accuracy, integrated signal conditioning, excellent media compatibility"
			(at 0 0 0)
		)
		(property "ki_keywords" "gage gauge pressure sensor"
			(at 0 0 0)
		)
		(symbol "40PC015G_0_1")
		(symbol "40PC015G_1_1"
			(pin no_connect line
				(at -7.62 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -5.08 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at -2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vcc")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "Vout")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BMP280"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 10.16 0)
		)
		(property "Value" "BMP280"
			(at 5.08 10.16 0)
		)
		(property "Footprint" "Package_LGA:Bosch_LGA-8_2x2.5mm_P0.65mm_ClockwisePinNumbering"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://ae-bst.resource.bosch.com/media/_tech/media/datasheets/BST-BMP280-DS001.pdf"
			(at 0 0 0)
		)
		(property "Description" "Absolute Barometric Pressure Sensor, LGA-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C, SPI, pressure, temperature, sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Bosch*LGA*2x2.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "BMP280_0_1")
		(symbol "BMP280_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SCK")
				(number "4")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SDI")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "SDO")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "CSB")
				(number "2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDDIO")
				(number "6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LPS22DF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 1.27 0)
		)
		(property "Value" "LPS22DF"
			(at -11.176 -1.27 0)
		)
		(property "Footprint" "Package_LGA:ST_HLGA-10_2x2mm_P0.5mm_LayoutBorder3x2y"
			(at -1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/lps22df.pdf"
			(at -1.27 -11.43 0)
		)
		(property "Description" "MEMS absolute pressure sensor, 260-1260 hPa, 1-200Hz ODR, 24bit, I2C/I3C/SPI interface, 2x2mm ST_HLGA-10L"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital barometer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST?HLGA*2x2mm*P0.5mm*LayoutBorder3x2y*"
			(at 0 0 0)
		)
		(symbol "LPS22DF_0_1")
		(symbol "LPS22DF_1_1"
			(pin power_in line
				(at -5.08 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "10")
			)
			(pin passive line
				(at -5.08 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at -5.08 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "Vdd_IO")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "GND_IO")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "SDA")
				(number "4")
				(alternate "SDI" input line)
				(alternate "SDI/SDO" bidirectional line)
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "SA0")
				(number "5")
				(alternate "SDO" output line)
			)
			(pin input clock
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SCL")
				(number "2")
				(alternate "SPC" input clock)
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{CS}")
				(number "6")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "INT_DRDY")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LPS25HB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 1.27 0)
		)
		(property "Value" "LPS25HB"
			(at -11.176 -1.27 0)
		)
		(property "Footprint" "Package_LGA:ST_HLGA-10_2.5x2.5mm_P0.6mm_LayoutBorder3x2y"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/lps25hb.pdf"
			(at 1.27 -13.97 0)
		)
		(property "Description" "MEMS nano pressure sensor, 260-1260 hPa, absolute digital output baromeeter, 24 bit, SPI, I2C, 0.01 hPa noise rms, ST_HLGA-10L"
			(at 0 0 0)
		)
		(property "ki_keywords" "mems absolute baromeeter spi i2c pressure"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST?HLGA*2.5x2.5mm*P0.6mm*LayoutBorder3x2y*"
			(at 0 0 0)
		)
		(symbol "LPS25HB_0_1")
		(symbol "LPS25HB_1_1"
			(pin power_in line
				(at -5.08 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "10")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "Vdd_IO")
				(number "1")
			)
			(pin passive line
				(at -2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at -2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "SDA")
				(number "4")
				(alternate "SDI" input line)
				(alternate "SDI/SDO" bidirectional line)
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "SA0")
				(number "5")
				(alternate "SDO" output line)
			)
			(pin input clock
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SCL")
				(number "2")
				(alternate "SPC" input clock)
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{CS}")
				(number "6")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "INT_DRDY")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MPL115A1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "MPL115A1"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_LGA:NXP_LGA-8_3x5mm_P1.25mm_H1.2mm"
			(at 25.4 -11.43 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MPL115A1.pdf"
			(at 0 0 0)
		)
		(property "Description" "SPI Digital Barometer"
			(at 0 0 0)
		)
		(property "ki_keywords" "spi barometer thermometer mems"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "NXP*LGA*3x5mm*P1.25mm*H1.2mm*"
			(at 0 0 0)
		)
		(symbol "MPL115A1_0_1")
		(symbol "MPL115A1_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "SCLK")
				(number "8")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 5.08)
				(name "DIN")
				(number "7")
			)
			(pin output line
				(at -12.7 0 0)
				(length 5.08)
				(name "DOUT")
				(number "6")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 5.08)
				(name "~{CS}")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "~{SHDN}")
				(number "4")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 5.08)
				(name "CAP")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MPL3115A2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "MPL3115A2"
			(at 6.35 11.43 0)
		)
		(property "Footprint" "Package_LGA:NXP_LGA-8_3x5mm_P1.25mm_H1.1mm"
			(at 25.4 -11.43 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MPL3115A2.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C precision pressure sensor with altimetry, LGA-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "pressure sensor altimetry"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "NXP*LGA*3x5mm*P1.25mm*H1.1mm*"
			(at 0 0 0)
		)
		(symbol "MPL3115A2_0_1")
		(symbol "MPL3115A2_1_1"
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SDL")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "SCL")
				(number "8")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDDIO")
				(number "4")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "INT1")
				(number "6")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "INT2")
				(number "5")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "CAP")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MPXA6115A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "MPXA6115A"
			(at 1.27 6.35 0)
		)
		(property "Footprint" ""
			(at -12.7 -8.89 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MPXA6115A.pdf"
			(at 0 15.24 0)
		)
		(property "Description" "Absolute pressure sensor, 15 to 115kPa, analog output, integrated signal conditioning, temperature compensated, SO package"
			(at 0 0 0)
		)
		(property "ki_keywords" "absolute pressure sensor"
			(at 0 0 0)
		)
		(symbol "MPXA6115A_0_1")
		(symbol "MPXA6115A_1_1"
			(pin no_connect line
				(at -7.62 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at -5.08 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "Vcc")
				(number "2")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin no_connect line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 5.08 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "Vout")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MS5525DSO"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "MS5525DSO"
			(at 8.89 11.43 0)
		)
		(property "Footprint" ""
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=MS5525DSO&DocType=DS&DocLang=English"
			(at 0 -16.51 0)
		)
		(property "Description" "Integrated Digital Pressure Sensor"
			(at 0 0 0)
		)
		(property "ki_keywords" "24bit low-power I2C SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TE?MS5525DSO*DB* TE?MS5525DSO*SB* TE?MS5525DSO*ST* TE?MS5525DSO*DH* TE?MS5525DSO*FT* TE?MS5525DSO*FB*"
			(at 0 0 0)
		)
		(symbol "MS5525DSO_0_1")
		(symbol "MS5525DSO_1_1"
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PS")
				(number "10")
			)
			(pin output line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "SDO")
				(number "5")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "SDI/SDA")
				(number "6")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "SCLK/SCL")
				(number "7")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "CSB")
				(number "8")
			)
			(pin passive line
				(at 0 12.7 270)
				(length 2.54)
				(hide yes)
				(name "SUPPLY+")
				(number "11")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "SUPPLY+")
				(number "13")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "SUPPLY-")
				(number "9")
			)
			(pin passive line
				(at 15.24 5.08 180)
				(length 2.54)
				(hide yes)
				(name "SOUT+")
				(number "12")
			)
			(pin passive line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "SOUT+")
				(number "14")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 2.54)
				(hide yes)
				(name "SOUT-")
				(number "2")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 2.54)
				(name "SOUT-")
				(number "4")
			)
			(pin passive line
				(at 15.24 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "SIN-")
				(number "1")
			)
			(pin passive line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "SIN-")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MS5607-02BA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "MS5607-02BA"
			(at 7.62 8.89 0)
		)
		(property "Footprint" "Package_LGA:LGA-8_3x5mm_P1.25mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Data+Sheet%7FMS5607-02BA03%7FB2%7Fpdf%7FEnglish%7FENG_DS_MS5607-02BA03_B2.pdf%7FCAT-BLPS0035"
			(at 0 0 0)
		)
		(property "Description" "Barometric pressure sensor, 20cm resolution, 10 to 1200 mbar, I2C and SPI interface up to 20MHz, LGA-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "pressure SPI I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LGA*3x5mm*P1.25mm*"
			(at 0 0 0)
		)
		(symbol "MS5607-02BA_0_1")
		(symbol "MS5607-02BA_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "PS")
				(number "2")
			)
			(pin output line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SDO")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "SDI/SDA")
				(number "7")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SCLK")
				(number "8")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "CSB")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "CSB")
				(number "5")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MS5837-xxBA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 11.43 0)
		)
		(property "Value" "MS5837-xxBA"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Sensor_Pressure:TE_MS5837-xxBA"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Data+Sheet%7FMS5837-30BA%7FB1%7Fpdf%7FEnglish%7FENG_DS_MS5837-30BA_B1.pdf%7FCAT-BLPS0017"
			(at 0 -2.54 0)
		)
		(property "Description" "Ultra-small, gel-filled, pressure sensor with stainless steel cap"
			(at 0 0 0)
		)
		(property "ki_keywords" "pressure sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TE_MS5837*BA*"
			(at 0 0 0)
		)
		(symbol "MS5837-xxBA_0_1")
		(symbol "MS5837-xxBA_1_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "SCL")
				(number "3")
			)
			(pin bidirectional line
				(at 7.62 0 180)
				(length 2.54)
				(name "SDA")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XGZP6897D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "XGZP6897D"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Sensor_Pressure:CFSensor_XGZP6897x"
			(at 0 0 0)
		)
		(property "Datasheet" "https://cfsensor.com/wp-content/uploads/2022/11/XGZP6897D-Pressure-Sensor-V2.7.pdf"
			(at 0 0 0)
		)
		(property "Description" "i2c differential digital, 2.5Vdc-5.5Vdc"
			(at 0 0 0)
		)
		(property "ki_keywords" "differential i2c"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*CFSensor?XGZP6897*"
			(at 0 0 0)
		)
		(symbol "XGZP6897D_0_1")
		(symbol "XGZP6897D_1_0"
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -5.08 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -5.08 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
		)
		(symbol "XGZP6897D_1_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "SCL")
				(number "7")
			)
			(pin bidirectional line
				(at 7.62 0 180)
				(length 2.54)
				(name "SDA")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XGZP6899D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "XGZP6899D"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Sensor_Pressure:CFSensor_XGZP6899x"
			(at 0 0 0)
		)
		(property "Datasheet" "https://cfsensor.com/wp-content/uploads/2022/11/XGZP6899D-Pressure-Sensor-V2.8.pdf"
			(at 0 0 0)
		)
		(property "Description" "i2c differential digital, 2.5Vdc-5.5Vdc"
			(at 0 0 0)
		)
		(property "ki_keywords" "differential i2c"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*CFSensor?XGZP6899*"
			(at 0 0 0)
		)
		(symbol "XGZP6899D_0_1")
		(symbol "XGZP6899D_1_0"
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at -5.08 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at -5.08 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
		)
		(symbol "XGZP6899D_1_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "SCL")
				(number "3")
			)
			(pin bidirectional line
				(at 7.62 0 180)
				(length 2.54)
				(name "SDA")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "40PC100G"
		(extends "40PC015G")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "40PC100G"
			(at 6.35 6.35 0)
		)
		(property "Footprint" ""
			(at 2.54 0 0)
		)
		(property "Datasheet" "http://www.honeywellscportal.com//index.php?ci_id=138832"
			(at 2.54 0 0)
		)
		(property "Description" "Gauge pressure sensor, 0 to 100PSI, 5V supply, 0.2% accuracy, integrated signal conditioning, excellent media compatibility"
			(at 0 0 0)
		)
		(property "ki_keywords" "gage gauge pressure sensor"
			(at 0 0 0)
		)
	)
	(symbol "40PC150G"
		(extends "40PC015G")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "40PC150G"
			(at 6.35 6.35 0)
		)
		(property "Footprint" ""
			(at 2.54 0 0)
		)
		(property "Datasheet" "http://www.honeywellscportal.com//index.php?ci_id=138832"
			(at 2.54 0 0)
		)
		(property "Description" "Gauge pressure sensor, 0 to 150PSI, 5V supply, 0.2% accuracy, integrated signal conditioning, excellent media compatibility"
			(at 0 0 0)
		)
		(property "ki_keywords" "gage gauge pressure sensor"
			(at 0 0 0)
		)
	)
	(symbol "40PC250G"
		(extends "40PC015G")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "40PC250G"
			(at 6.35 6.35 0)
		)
		(property "Footprint" ""
			(at 2.54 0 0)
		)
		(property "Datasheet" "http://www.honeywellscportal.com//index.php?ci_id=138832"
			(at 2.54 0 0)
		)
		(property "Description" "Gauge pressure sensor, 0 to 250PSI, 5V supply, 0.2% accuracy, integrated signal conditioning, excellent media compatibility"
			(at 0 0 0)
		)
		(property "ki_keywords" "gage gauge pressure sensor"
			(at 0 0 0)
		)
	)
	(symbol "LPS22HB"
		(extends "LPS25HB")
		(property "Reference" "U"
			(at -11.43 1.27 0)
		)
		(property "Value" "LPS22HB"
			(at -11.43 -1.27 0)
		)
		(property "Footprint" "Package_LGA:ST_HLGA-10_2x2mm_P0.5mm_LayoutBorder3x2y"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/lps22hb.pdf"
			(at 1.27 -13.97 0)
		)
		(property "Description" "MEMS nano pressure sensor, 260-1260 hPa, absolute digital output baromeeter, 24 bit, SPI, I2C, 0.0075 hPa noise rms, ST_HLGA-10L"
			(at 0 0 0)
		)
		(property "ki_keywords" "mems absolute baromeeter spi i2c pressure"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST?HLGA*2x2mm*P0.5mm*LayoutBorder3x2y*"
			(at 0 0 0)
		)
	)
	(symbol "LPS22HH"
		(extends "LPS25HB")
		(property "Reference" "U"
			(at -11.43 1.27 0)
		)
		(property "Value" "LPS22HH"
			(at -11.43 -1.27 0)
		)
		(property "Footprint" "Package_LGA:ST_HLGA-10_2x2mm_P0.5mm_LayoutBorder3x2y"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/lps22hh.pdf"
			(at 1.27 -13.97 0)
		)
		(property "Description" "MEMS nano pressure sensor, 260-1260 hPa, absolute digital output baromeeter, 24 bit, SPI, I2C, I3C, 0.65 Pa noise rms, ST_HLGA-10L"
			(at 0 0 0)
		)
		(property "ki_keywords" "mems absolute baromeeter spi i2c i3c pressure"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST?HLGA*2x2mm*P0.5mm*LayoutBorder3x2y*"
			(at 0 0 0)
		)
	)
	(symbol "MPXAZ6115A"
		(extends "MPXA6115A")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "MPXAZ6115A"
			(at 1.27 6.35 0)
		)
		(property "Footprint" ""
			(at -12.7 -8.89 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MPXA6115A.pdf"
			(at 0 15.24 0)
		)
		(property "Description" "Absolute pressure sensor, 15 to 115kPa, analog output, integrated signal conditioning, temperature compensated, media resistant gel, SO package"
			(at 0 0 0)
		)
		(property "ki_keywords" "absolute pressure sensor"
			(at 0 0 0)
		)
	)
	(symbol "MPXH6115A"
		(extends "MPXA6115A")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "MPXH6115A"
			(at 1.27 6.35 0)
		)
		(property "Footprint" ""
			(at -12.7 -8.89 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MPXA6115A.pdf"
			(at 0 15.24 0)
		)
		(property "Description" "Absolute pressure sensor, 15 to 115kPa, analog output, integrated signal conditioning, temperature compensated, SSO package"
			(at 0 0 0)
		)
		(property "ki_keywords" "absolute pressure sensor"
			(at 0 0 0)
		)
	)
	(symbol "MPXHZ6115A"
		(extends "MPXA6115A")
		(property "Reference" "U"
			(at -10.16 6.35 0)
		)
		(property "Value" "MPXHZ6115A"
			(at 1.27 6.35 0)
		)
		(property "Footprint" ""
			(at -12.7 -8.89 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MPXA6115A.pdf"
			(at 0 15.24 0)
		)
		(property "Description" "Absolute pressure sensor, 15 to 115kPa, analog output, integrated signal conditioning, temperature compensated, media resistant gel, SSO package"
			(at 0 0 0)
		)
		(property "ki_keywords" "absolute pressure sensor"
			(at 0 0 0)
		)
	)
	(symbol "MS5611-01BA"
		(extends "MS5607-02BA")
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "MS5611-01BA"
			(at 7.62 8.89 0)
		)
		(property "Footprint" "Package_LGA:LGA-8_3x5mm_P1.25mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=MS5611-01BA03&DocType=Data+Sheet&DocLang=English"
			(at 0 0 0)
		)
		(property "Description" "Barometric pressure sensor, 10cm resolution, 10 to 1200 mbar, I2C and SPI interface up to 20MHz, LGA-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "pressure SPI I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LGA*3x5mm*P1.25mm*"
			(at 0 0 0)
		)
	)
	(symbol "WSEN-PADS_2511020213301"
		(extends "LPS25HB")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "WSEN-PADS_2511020213301"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Package_LGA:ST_HLGA-10_2x2mm_P0.5mm_LayoutBorder3x2y"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.we-online.com/components/products/manual/2511020213301_WSEN-PADS%202511020213301%20Manual_rev2.2.pdf"
			(at 1.27 -8.89 0)
		)
		(property "Description" "MEMS nano pressure sensor, 260-1260 hPa, absolute digital output baromeeter, 24 bit, SPI, I2C, 0.75 Pa noise rms, ST_HLGA-10L"
			(at 0 0 0)
		)
		(property "ki_keywords" "mems absolute baromeeter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST?HLGA*2x2mm*P0.5mm*LayoutBorder3x2y*"
			(at 0 0 0)
		)
	)
)
