(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "AD7150BRMZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "AD7150BRMZ"
			(at 8.255 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 5.08 -12.7 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD7150.pdf"
			(at 5.08 -15.24 0)
		)
		(property "Description" "Capacitance to digital converter for proximity sensing, 2-channel, 12 bit, 0..13pF range, 2.7..3.6V supply, I²C interface, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Analog ADI CDC dual"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AD7150BRMZ_0_0"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SCL")
				(number "9")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "10")
			)
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "OUT1")
				(number "7")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "OUT2")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "EXC1")
				(number "6")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "CIN1")
				(number "4")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "EXC2")
				(number "5")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "CIN2")
				(number "3")
			)
		)
		(symbol "AD7150BRMZ_1_1")
		(embedded_fonts no)
	)
	(symbol "AD7151BRMZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.985 8.89 0)
		)
		(property "Value" "AD7151BRMZ"
			(at 8.255 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 5.08 -12.7 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD7151.pdf"
			(at 5.08 -15.24 0)
		)
		(property "Description" "Capacitance to digital converter for proximity sensing, 1-channel, 12 bit, 0..13pF range, 2.7..3.6V supply, I²C interface, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Analog ADI CDC single"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AD7151BRMZ_0_0"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SCL")
				(number "9")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "10")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
		)
		(symbol "AD7151BRMZ_1_0"
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "OUT")
				(number "7")
			)
			(pin no_connect line
				(at -7.62 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 7.62 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "EXC")
				(number "6")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "CIN")
				(number "4")
			)
		)
		(symbol "AD7151BRMZ_1_1")
		(embedded_fonts no)
	)
	(symbol "APDS-9160-003"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.827 9.017 0)
		)
		(property "Value" "APDS-9160-003"
			(at 0.508 9.017 0)
		)
		(property "Footprint" "OptoDevice:Broadcom_APDS-9160-003"
			(at 0 -12.573 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/APDS-9160-003-DS"
			(at 1.016 12.7 0)
		)
		(property "Description" "Proximity Sensor, I2C interface, 1.7-3.6V, LGA-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto proximity sensor avago broadcom"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Broadcom*APDS*9160*003*"
			(at 0 0 0)
		)
		(symbol "APDS-9160-003_0_0"
			(text "ADC"
				(at 0.254 -1.524 0)
			)
		)
		(symbol "APDS-9160-003_0_1")
		(symbol "APDS-9160-003_1_0")
		(symbol "APDS-9160-003_1_1"
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "SDA")
				(number "7")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "8")
			)
			(pin open_collector line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "INT")
				(number "2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "LEDA")
				(number "5")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "LEDK")
				(number "4")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "LDR")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BPR-205"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.08 0)
		)
		(property "Value" "BPR-205"
			(at 10.16 5.08 0)
		)
		(property "Footprint" "OptoDevice:Everlight_ITR8307"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ystone.com.tw/en/data/goods/IRPT/Photo%20Interrupters-Reflective%20Type.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Subminiature Reflective Optical Sensor, Darlington photo transistor, SMD-package with PCB-cutout"
			(at 0 0 0)
		)
		(property "ki_keywords" "Reflective Optical Sensor Opto"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Everlight*ITR8307*"
			(at 0 0 0)
		)
		(symbol "BPR-205_0_1")
		(symbol "BPR-205_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin open_collector line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin open_emitter line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "E")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CNY70"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "CNY70"
			(at 5.08 5.08 0)
		)
		(property "Footprint" "OptoDevice:Vishay_CNY70"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/83751/cny70.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Reflective Optical Sensor with Transistor Output"
			(at 0 0 0)
		)
		(property "ki_keywords" "Reflective Optical Sensor Opto"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*CNY70*"
			(at 0 0 0)
		)
		(symbol "CNY70_0_1")
		(symbol "CNY70_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "K")
				(number "2")
			)
			(pin open_collector line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin open_emitter line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "E")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "GP2S700HCP"
		(pin_names
			(offset 0.0254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.08 0)
		)
		(property "Value" "GP2S700HCP"
			(at 12.7 5.08 0)
		)
		(property "Footprint" "OptoDevice:Sharp_GP2S700HCP"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.sharpsde.com/fileadmin/products/Optoelectronics/Isolation%20Devices/Specs_Photointerrupter/GP2S700HCP_03Oct05_DS_D3-A02201FEN.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Reflective Optical Sensor 0.217\" (5.5mm) 4-SMD"
			(at 0 0 0)
		)
		(property "ki_keywords" "Reflective Optical Sensor Opto reflex coupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Sharp*GP2S700HCP*"
			(at 0 0 0)
		)
		(symbol "GP2S700HCP_0_1")
		(symbol "GP2S700HCP_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "A")
				(number "4")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "K")
				(number "3")
			)
			(pin open_collector line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin open_emitter line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ITR1201SR10AR"
		(pin_names
			(offset 0.0254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.08 0)
		)
		(property "Value" "ITR1201SR10AR"
			(at 15.24 5.08 0)
		)
		(property "Footprint" "OptoDevice:Everlight_ITR1201SR10AR"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.everlight.com/file/ProductFile/ITR1201SR10AR-TR.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Miniature Reflective Optical Object Sensor, SMD-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Reflective Optical Sensor Opto reflex coupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Everlight*ITR1201SR10AR*"
			(at 0 0 0)
		)
		(symbol "ITR1201SR10AR_0_1")
		(symbol "ITR1201SR10AR_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin open_collector line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin open_emitter line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ITR8307"
		(pin_names
			(offset 0.0254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "ITR8307"
			(at 7.62 5.08 0)
		)
		(property "Footprint" "OptoDevice:Everlight_ITR8307"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.everlight.com/file/ProductFile/ITR8307.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Subminiature Reflective Optical Sensor, SMD-package with PCB-cutout"
			(at 0 0 0)
		)
		(property "ki_keywords" "Reflective Optical Sensor Opto"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Everlight*ITR8307*"
			(at 0 0 0)
		)
		(symbol "ITR8307_0_1")
		(symbol "ITR8307_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin open_collector line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin open_emitter line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "E")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ITR8307-F43"
		(pin_names
			(offset 0.0254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.08 0)
		)
		(property "Value" "ITR8307-F43"
			(at 12.7 5.08 0)
		)
		(property "Footprint" "OptoDevice:Everlight_ITR8307F43"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://everlighteurope.com/index.php?controller=attachment&id_attachment=5385"
			(at 0 2.54 0)
		)
		(property "Description" "Subminiature Reflective Optical Sensor, DIP-like THT-package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Reflective Optical Sensor Opto"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Everlight*ITR8307F43*"
			(at 0 0 0)
		)
		(symbol "ITR8307-F43_0_1")
		(symbol "ITR8307-F43_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin open_collector line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin open_emitter line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "E")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ITR9608-F"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "ITR9608-F"
			(at 0 -5.08 0)
		)
		(property "Footprint" "OptoDevice:Everlight_ITR9608-F"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "https://www.everlighteurope.com/custom/files/datasheets/DRX-0000076.pdf"
			(at -1.27 6.35 0)
		)
		(property "Description" "Photointerrupter infrared LED with photo IC, -25 to +85 degree Celsius"
			(at 0 0 0)
		)
		(property "ki_keywords" "Photointerrupter opto interrupter infrared LED fast response time infrared 940nm 5mm gap"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*ITR9608*"
			(at 0 0 0)
		)
		(symbol "ITR9608-F_0_0"
			(text "A"
				(at -4.445 3.175 0)
			)
			(text "K"
				(at -4.445 -1.778 0)
			)
			(text "E"
				(at 4.445 3.175 0)
			)
			(text "C"
				(at 4.445 -1.778 0)
			)
		)
		(symbol "ITR9608-F_0_1")
		(symbol "ITR9608-F_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin open_emitter line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin open_collector line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KRC011"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.08 0)
		)
		(property "Value" "KRC011"
			(at 7.62 5.08 0)
		)
		(property "Footprint" "OptoDevice:Kingbright_KRC011_Vertical"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.kingbright.com/attachments/file/psearch/000/00/00/KRC011(Ver.15).pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Subminiature Reflective Optical Sensor"
			(at 0 0 0)
		)
		(property "ki_keywords" "Reflective Optical Sensor Opto"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Kingbright?KRC011*"
			(at 0 0 0)
		)
		(symbol "KRC011_0_1")
		(symbol "KRC011_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "K")
				(number "2")
			)
			(pin open_collector line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin open_emitter line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "E")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LDC1312"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 11.43 0)
		)
		(property "Value" "LDC1312"
			(at 6.35 11.43 0)
		)
		(property "Footprint" "Package_SON:WSON-12-1EP_4x4mm_P0.5mm_EP2.6x3mm_ThermalVias"
			(at 2.54 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ldc1312.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Inductance to digital converter, 2-channel 12-bit, WSON-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "inductance sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LDC1312_0_1")
		(symbol "LDC1312_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "CLKIN")
				(number "3")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "IN0A")
				(number "9")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "IN0B")
				(number "10")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "IN1A")
				(number "11")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "IN1B")
				(number "12")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "7")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "SD")
				(number "6")
			)
			(pin open_collector line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "INTB")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SDA")
				(number "2")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "SCL")
				(number "1")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "ADDR")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LDC1314"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 19.05 0)
		)
		(property "Value" "LDC1314"
			(at 6.35 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:WQFN-16-1EP_4x4mm_P0.5mm_EP2.6x2.6mm_ThermalVias"
			(at 7.62 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ldc1312.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Inductance to digital converter, 4-channel 12-bit, WQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "inductance sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WQFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LDC1314_0_1")
		(symbol "LDC1314_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "CLKIN")
				(number "3")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "IN0A")
				(number "9")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "IN0B")
				(number "10")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "IN1A")
				(number "11")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "IN1B")
				(number "12")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "IN2A")
				(number "13")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "IN2B")
				(number "14")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "IN3A")
				(number "15")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "IN3B")
				(number "16")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "7")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "SD")
				(number "6")
			)
			(pin open_collector line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "INTB")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "SDA")
				(number "2")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SCL")
				(number "1")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "ADDR")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LG206D"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 8.89 0)
		)
		(property "Value" "LG206D"
			(at 3.556 8.89 0)
		)
		(property "Footprint" "OptoDevice:Kodenshi_LG206D"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://kodenshi.co.jp/products/pdf/sensor/photointerrupter_ic/LG206D.pdf"
			(at -7.62 -0.127 0)
		)
		(property "Description" "Photointerrupter infrared LED with photo IC, non-inverting output, -0.5V to 17V VDD, -20 to +85 degree Celsius, LG206D"
			(at 0 0 0)
		)
		(property "ki_keywords" "Photointerrupter infrared LED with photo IC, non-inverting output, -0.5V to 17V VDD, -20 to +85 degree Celsius, LG206D"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Kodenshi?LG206D*"
			(at 0 0 0)
		)
		(symbol "LG206D_0_1")
		(symbol "LG206D_1_1"
			(pin passive line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "A")
				(number "4")
			)
			(pin passive line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "K")
				(number "5")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin open_collector line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LG206L"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 8.89 0)
		)
		(property "Value" "LG206L"
			(at 4.318 8.89 0)
		)
		(property "Footprint" "OptoDevice:Kodenshi_LG206L"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://kodenshi.co.jp/products/pdf/sensor/photointerrupter_ic/LG206L.pdf"
			(at -7.62 -0.127 0)
		)
		(property "Description" "Photointerrupter infrared LED with photo IC, inverting output, -0.5V to 17V VDD, -20 to +85 degree Celsius, LG206X"
			(at 0 0 0)
		)
		(property "ki_keywords" "Photointerrupter infrared LED with photo IC, inverting output, -0.5V to 17V VDD, -20 to +85 degree Celsius, LG206X"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Kodenshi?LG206L*"
			(at 0 0 0)
		)
		(symbol "LG206L_0_1")
		(symbol "LG206L_1_1"
			(pin passive line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "A")
				(number "4")
			)
			(pin passive line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "K")
				(number "5")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin open_collector line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "QRE1113"
		(pin_names
			(offset 0.0254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.08 0)
		)
		(property "Value" "QRE1113"
			(at 8.89 5.08 0)
		)
		(property "Footprint" "OptoDevice:OnSemi_CASE100AQ"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/QRE1113-D.PDF"
			(at 0 2.54 0)
		)
		(property "Description" "Miniature Reflective Optical Object Sensor, DIP-like THT-package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Reflective Optical Sensor Opto reflex coupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "OnSemi*CASE100AQ*"
			(at 0 0 0)
		)
		(symbol "QRE1113_0_1")
		(symbol "QRE1113_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "K")
				(number "2")
			)
			(pin open_collector line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin open_emitter line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "QRE1113GR"
		(pin_names
			(offset 0.0254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.08 0)
		)
		(property "Value" "QRE1113GR"
			(at 11.43 5.08 0)
		)
		(property "Footprint" "OptoDevice:OnSemi_CASE100CY"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/QRE1113-D.PDF"
			(at 0 2.54 0)
		)
		(property "Description" "Miniature Reflective Optical Object Sensor, SMD-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Reflective Optical Sensor Opto reflex coupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "OnSemi*CASE100CY*"
			(at 0 0 0)
		)
		(symbol "QRE1113GR_0_1")
		(symbol "QRE1113GR_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "K")
				(number "2")
			)
			(pin open_collector line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin open_emitter line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RPR-0720"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "RPR-0720"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "OptoDevice:Rohm_RPR-0720"
			(at 0 -12.573 0)
		)
		(property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/opto/optical_sensor/photosensor/rpr-0720-e.pdf"
			(at 1.016 12.7 0)
		)
		(property "Description" "Proximity Sensor, I2C interface, 2x1x0.55mm, 1-15mm, 2.5-3.6V, LGA-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto rohm"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Rohm*RPR*0720*"
			(at 0 0 0)
		)
		(symbol "RPR-0720_0_0"
			(text "ADC"
				(at 0.508 -1.524 0)
			)
		)
		(symbol "RPR-0720_0_1")
		(symbol "RPR-0720_1_0")
		(symbol "RPR-0720_1_1"
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SDA")
				(number "3")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "2")
			)
			(pin open_collector line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "INT")
				(number "4")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VCSELA")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SFH900"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "SFH900"
			(at 6.35 5.08 0)
		)
		(property "Footprint" "OptoDevice:Siemens_SFH900"
			(at 1.27 -5.08 0)
		)
		(property "Datasheet" "https://www.batronix.com/pdf/sfh900.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Miniature Light Reflection Switches"
			(at 0 0 0)
		)
		(property "ki_keywords" "Reflective Optical Sensor Opto"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Siemens*SFH900*"
			(at 0 0 0)
		)
		(symbol "SFH900_0_1")
		(symbol "SFH900_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "K")
				(number "2")
			)
			(pin open_collector line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "C")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SFH9206"
		(pin_names
			(offset 0.0254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "SFH9206"
			(at 0 5.08 0)
		)
		(property "Footprint" "OptoDevice:Osram_SFH9x0x"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.osram-os.com/Graphics/XPic6/00200860_0.pdf"
			(at -1.016 1.016 90)
		)
		(property "Description" "Reflective Opto Interrupter/Coupler, SMD-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Reflective Opto Interrupter Coupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Osram*SFH9x0x*"
			(at 0 0 0)
		)
		(symbol "SFH9206_0_1")
		(symbol "SFH9206_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "K")
				(number "6")
			)
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin open_collector line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "C")
				(number "4")
			)
			(pin open_emitter line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "E")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SG-105"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.08 0)
		)
		(property "Value" "SG-105"
			(at 8.89 5.08 0)
		)
		(property "Footprint" "OptoDevice:Kodenshi_SG105"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.kodenshi.co.jp/products/pdf/sensor/photointerrupter_ref/SG-105.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Subminiature Reflective Optical Sensor, SMD-package with PCB-cutout"
			(at 0 0 0)
		)
		(property "ki_keywords" "Reflective Optical Sensor Opto"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Kodenshi*SG105*"
			(at 0 0 0)
		)
		(symbol "SG-105_0_1")
		(symbol "SG-105_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "K")
				(number "2")
			)
			(pin open_collector line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin open_emitter line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "E")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SG-105F"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.08 0)
		)
		(property "Value" "SG-105F"
			(at 8.89 5.08 0)
		)
		(property "Footprint" "OptoDevice:Kodenshi_SG105F"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.kodenshi.co.jp/products/pdf/sensor/photointerrupter_ref/SG-105F.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Subminiature Reflective Optical Sensor, DIP-lie THT-package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Reflective Optical Sensor Opto"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Kodenshi*SG105F*"
			(at 0 0 0)
		)
		(symbol "SG-105F_0_1")
		(symbol "SG-105F_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "K")
				(number "2")
			)
			(pin open_collector line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin open_emitter line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "E")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TSSP58P38"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "TSSP58P38"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "OptoDevice:Vishay_MINICAST-3Pin"
			(at -1.27 -9.525 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/82462/tsop581.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "Photo Modules for PCM Remote Control Systems"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*MINICAST*"
			(at 0 0 0)
		)
		(symbol "TSSP58P38_0_0"
			(text "DEMOD"
				(at -3.175 0.254 900)
			)
		)
		(symbol "TSSP58P38_0_1")
		(symbol "TSSP58P38_1_1"
			(pin power_in line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "Vs")
				(number "3")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin power_in line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "GND")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BPR-105"
		(extends "ITR8307")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "BPR-105"
			(at 7.62 5.08 0)
		)
		(property "Footprint" "OptoDevice:Everlight_ITR8307"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ystone.com.tw/en/data/goods/IRPT/Photo%20Interrupters-Reflective%20Type.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Subminiature Reflective Optical Sensor, SMD-package with PCB-cutout"
			(at 0 0 0)
		)
		(property "ki_keywords" "Reflective Optical Sensor Opto"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Everlight*ITR8307*"
			(at 0 0 0)
		)
	)
	(symbol "BPR-105F"
		(extends "ITR8307-F43")
		(property "Reference" "U"
			(at -3.81 5.08 0)
		)
		(property "Value" "BPR-105F"
			(at 12.7 5.08 0)
		)
		(property "Footprint" "OptoDevice:Everlight_ITR8307F43"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.ystone.com.tw/en/data/goods/IRPT/Photo%20Interrupters-Reflective%20Type.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Subminiature Reflective Optical Sensor, DIP-like THT-package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Reflective Optical Sensor Opto"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Everlight*ITR8307F43*"
			(at 0 0 0)
		)
	)
	(symbol "ITR8307-L24-TR8"
		(extends "ITR1201SR10AR")
		(property "Reference" "U"
			(at -3.81 5.08 0)
		)
		(property "Value" "ITR8307-L24-TR8"
			(at 15.24 5.08 0)
		)
		(property "Footprint" "OptoDevice:Everlight_ITR1201SR10AR"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.everlight.com/file/ProductFile/ITR8307-L24-TR8.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Miniature Reflective Optical Object Sensor, SMD-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Reflective Optical Sensor Opto reflex coupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Everlight*ITR1201SR10AR*"
			(at 0 0 0)
		)
	)
	(symbol "ITR8307-S17-TR8"
		(extends "ITR1201SR10AR")
		(property "Reference" "U"
			(at -3.81 5.08 0)
		)
		(property "Value" "ITR8307-S17-TR8"
			(at 15.24 5.08 0)
		)
		(property "Footprint" "OptoDevice:Everlight_ITR1201SR10AR"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/szlcsc/1810010232_Everlight-Elec-ITR8307-S17-TR8-B_C81632.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Miniature Reflective Optical Object Sensor, SMD-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Reflective Optical Sensor Opto reflex coupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Everlight*ITR1201SR10AR*"
			(at 0 0 0)
		)
	)
	(symbol "LDC1612"
		(extends "LDC1312")
		(property "Reference" "U"
			(at -8.89 11.43 0)
		)
		(property "Value" "LDC1612"
			(at 6.35 11.43 0)
		)
		(property "Footprint" "Package_SON:WSON-12-1EP_4x4mm_P0.5mm_EP2.6x3mm_ThermalVias"
			(at 2.54 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ldc1612.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Inductance to digital converter, 2-channel 28-bit, WSON-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "inductance sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LDC1614"
		(extends "LDC1314")
		(property "Reference" "U"
			(at -8.89 19.05 0)
		)
		(property "Value" "LDC1614"
			(at 6.35 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:WQFN-16-1EP_4x4mm_P0.5mm_EP2.6x2.6mm_ThermalVias"
			(at 7.62 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ldc1612.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Inductance to digital converter, 4-channel 28-bit, WQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "inductance sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WQFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "SFH9201"
		(extends "SFH9206")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "SFH9201"
			(at 0 5.08 0)
		)
		(property "Footprint" "OptoDevice:Osram_SFH9x0x"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://media.digikey.com/pdf/Data%20Sheets/Osram%20PDFs/SFH_9201.pdf"
			(at -1.016 1.016 90)
		)
		(property "Description" "Reflective Opto Interrupter/Coupler, SMD-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Reflective Opto Interrupter Coupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Osram*SFH9x0x*"
			(at 0 0 0)
		)
	)
	(symbol "SFH9202"
		(extends "SFH9206")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "SFH9202"
			(at 0 5.08 0)
		)
		(property "Footprint" "OptoDevice:Osram_SFH9x0x"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.osram-os.com/Graphics/XPic0/00083379_0.pdf/SFH%209202,%20Lead%20%28Pb%29%20Free%20Product%20-%20RoHS%20Compliant.pdf"
			(at -1.016 1.016 90)
		)
		(property "Description" "Reflective Opto Interrupter/Coupler, SMD-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Reflective Opto Interrupter Coupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Osram*SFH9x0x*"
			(at 0 0 0)
		)
	)
	(symbol "SG-107"
		(extends "SG-105")
		(property "Reference" "U"
			(at -3.81 5.08 0)
		)
		(property "Value" "SG-107"
			(at 8.89 5.08 0)
		)
		(property "Footprint" "OptoDevice:Kodenshi_SG105"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.kodenshi.co.jp/products/pdf/sensor/photointerrupter_ref/SG-107.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Subminiature Reflective Optical Sensor, SMD-package with PCB-cutout"
			(at 0 0 0)
		)
		(property "ki_keywords" "Reflective Optical Sensor Opto"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Kodenshi*SG105*"
			(at 0 0 0)
		)
	)
	(symbol "SG-107F"
		(extends "SG-105F")
		(property "Reference" "U"
			(at -3.81 5.08 0)
		)
		(property "Value" "SG-107F"
			(at 8.89 5.08 0)
		)
		(property "Footprint" "OptoDevice:Kodenshi_SG105F"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.pacer.co.uk/Assets/User/1055-SG-107F.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Subminiature Reflective Optical Sensor, DIP-lie THT-package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Reflective Optical Sensor Opto"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Kodenshi*SG105F*"
			(at 0 0 0)
		)
	)
	(symbol "TSSP58038"
		(extends "TSSP58P38")
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "TSSP58038"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "OptoDevice:Vishay_MINICAST-3Pin"
			(at -1.27 -9.525 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/82476/tssp58p38.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "IR Detector for Mid Range Proximity Sensor"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR receiver proximity sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*MINICAST*"
			(at 0 0 0)
		)
	)
	(symbol "TSSP58038SS1XB"
		(extends "TSSP58P38")
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "TSSP58038SS1XB"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "OptoDevice:Vishay_MINICAST-3Pin"
			(at -1.27 -9.525 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/82740/tssp58038ss1xb.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "IR Receiver Module for Light Barrier Systems"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR receiver light barrier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*MINICAST*"
			(at 0 0 0)
		)
	)
)
