(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "AD8494"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 3.81 0)
		)
		(property "Value" "AD8494"
			(at 8.89 -3.81 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 22.86 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ad8494_8495_8496_8497.pdf"
			(at 0 0 0)
		)
		(property "Description" "Precision Thermocouple Amplifiers with Cold Junction Compensation, J-Type Thermocouple, 0 to 50C, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Thermocouple Amp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*8*"
			(at 0 0 0)
		)
		(symbol "AD8494_0_1")
		(symbol "AD8494_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "-IN")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "+IN")
				(number "8")
			)
			(pin no_connect line
				(at -5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "+Vs")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "-Vs")
				(number "3")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 3.81)
				(name "SENSE")
				(number "5")
			)
			(pin input line
				(at 2.54 -7.62 90)
				(length 5.08)
				(name "REF")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BD1020HFV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "BD1020HFV"
			(at -5.08 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:HVSOF5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://rohmfs.rohm.com/en/products/databook/datasheet/ic/sensor/temperature/bd1020hfv-e.pdf"
			(at 0 0 0)
		)
		(property "Description" "Analog Output Temperature Sensor"
			(at 0 0 0)
		)
		(property "ki_keywords" "Temperature sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HVSOF5*"
			(at 0 0 0)
		)
		(symbol "BD1020HFV_0_1")
		(symbol "BD1020HFV_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "PG")
				(number "2")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
			(pin power_in line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "GND")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DS1621"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "DS1621"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at -17.78 -8.89 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DS1621.pdf"
			(at -3.81 6.35 0)
		)
		(property "Description" "1-Wire Digital Thermometer and Thermostat, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OneWire 1-Wire 1Wire Maxim Dallas"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "DS1621_0_1")
		(symbol "DS1621_1_1"
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SDA")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "A0")
				(number "7")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "A1")
				(number "6")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "A2")
				(number "5")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V_{DD}")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "T_{OUT}")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DS1804"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 6.35 0)
		)
		(property "Value" "DS1804"
			(at 6.35 -6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/DS1804.pdf"
			(at 0 -15.24 0)
		)
		(property "Description" "Nonvolatile Trimmer Potentiometer, DIP-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "DS1804_0_1")
		(symbol "DS1804_1_1"
			(pin input line
				(at -11.43 2.54 0)
				(length 5.08)
				(name "~{INC}")
				(number "1")
			)
			(pin input line
				(at -11.43 0 0)
				(length 5.08)
				(name "U/~{D}")
				(number "2")
			)
			(pin input line
				(at -11.43 -2.54 0)
				(length 5.08)
				(name "~{CS}")
				(number "7")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V_{CC}")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 11.43 3.81 180)
				(length 5.08)
				(name "H")
				(number "3")
			)
			(pin passive line
				(at 11.43 0 180)
				(length 5.08)
				(name "W")
				(number "5")
			)
			(pin passive line
				(at 11.43 -3.81 180)
				(length 5.08)
				(name "L")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DS1822Z"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "DS1822Z"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -25.4 -6.35 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/DS1822.pdf"
			(at -3.81 6.35 0)
		)
		(property "Description" "Econo 1-Wire Digital Thermometer SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OneWire 1-Wire 1Wire Maxim Dallas"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "DS1822Z_0_1")
		(symbol "DS1822Z_1_1"
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V_{DD}")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin bidirectional line
				(at 7.62 0 180)
				(length 2.54)
				(name "DQ")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DS18B20U"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "DS18B20U"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at -24.13 -6.35 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/DS18B20.pdf"
			(at -3.81 6.35 0)
		)
		(property "Description" "Programmable Resolution 1-Wire Digital Thermometer MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OneWire 1-Wire 1Wire Maxim Dallas"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "DS18B20U_0_1")
		(symbol "DS18B20U_1_1"
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -5.08 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V_{DD}")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin bidirectional line
				(at 7.62 0 180)
				(length 2.54)
				(name "DQ")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DS28EA00"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "DS28EA00"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at -25.4 -6.35 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/DS28EA00.pdf"
			(at -6.35 6.35 0)
		)
		(property "Description" "1-Wire Digital Thermometer with Sequence Detect and PIO"
			(at 0 0 0)
		)
		(property "ki_keywords" "1Wire OneWire Maxim Dallas"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "DS28EA00_0_1")
		(symbol "DS28EA00_1_1"
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IO")
				(number "1")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "PIOB")
				(number "7")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V_{DD}")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin no_connect line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "PIOA")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KTY81"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TH"
			(at -4.445 0 90)
		)
		(property "Value" "KTY81"
			(at 3.175 0 90)
		)
		(property "Footprint" ""
			(at 5.08 0 90)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/KTY81_SER.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "KTY81 series silicon temperature sensors"
			(at 0 0 0)
		)
		(property "ki_keywords" "silicon temperature sensors"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOD?70*"
			(at 0 0 0)
		)
		(symbol "KTY81_0_1")
		(symbol "KTY81_1_1"
			(pin passive line
				(at 0 3.81 270)
				(length 1.27)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 1.27)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KTY82"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TH"
			(at -4.445 0 90)
		)
		(property "Value" "KTY82"
			(at 3.175 0 90)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 5.08 0 90)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/KTY82_SER.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "KTY82 series silicon temperature sensors, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "silicon temperature sensors"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "KTY82_0_1")
		(symbol "KTY82_1_1"
			(pin passive line
				(at 0 3.81 270)
				(length 1.27)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 1.27)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KTY83"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TH"
			(at 0 2.54 0)
		)
		(property "Value" "KTY83"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Diode_THT:D_DO-34_SOD68_P7.62mm_Horizontal"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/KTY83_SER.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "KTY83 series silicon temperature sensors, polarized, SOD68"
			(at 0 0 0)
		)
		(property "ki_keywords" "silicon temperature sensors diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DO?34*SOD68*"
			(at 0 0 0)
		)
		(symbol "KTY83_0_1")
		(symbol "KTY83_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KTY85"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TH"
			(at 0 2.54 0)
		)
		(property "Value" "KTY85"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Diode_SMD:D_MiniMELF"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.nxp.com/documents/other/SC17_GENERAL_TEMP_1996_3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "KTY85 series silicon temperature sensors, polarized, SOD80"
			(at 0 0 0)
		)
		(property "ki_keywords" "silicon temperature sensor diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOD80*"
			(at 0 0 0)
		)
		(symbol "KTY85_0_1")
		(symbol "KTY85_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM20BIM7"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LM20BIM7"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm20.pdf"
			(at 0 0 0)
		)
		(property "Description" "Precision Temperature Sensor, Accuracy at 30°C ±1.5°C to ±4°C Maximum, SC70"
			(at 0 0 0)
		)
		(property "ki_keywords" "temperature sensor thermistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?353*"
			(at 0 0 0)
		)
		(symbol "LM20BIM7_0_1")
		(symbol "LM20BIM7_1_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "GND/DIE")
				(number "2")
			)
			(pin no_connect line
				(at 5.08 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VO")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM35-D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LM35-D"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm35.pdf"
			(at 0 0 0)
		)
		(property "Description" "Precision centigrade temperature sensor, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "temperature sensor thermistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*"
			(at 0 0 0)
		)
		(symbol "LM35-D_0_1")
		(symbol "LM35-D_1_1"
			(pin no_connect line
				(at -2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "+V_{S}")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin no_connect line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 5.08 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "V_{OUT}")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM35-LP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LM35-LP"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm35.pdf"
			(at 0 0 0)
		)
		(property "Description" "Precision centigrade temperature sensor, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "temperature sensor thermistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
		(symbol "LM35-LP_0_1")
		(symbol "LM35-LP_1_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "+V_{S}")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "V_{OUT}")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM35-NEB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LM35-NEB"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm35.pdf"
			(at 0 0 0)
		)
		(property "Description" "Precision centigrade temperature sensor, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "temperature sensor thermistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
		(symbol "LM35-NEB_0_1")
		(symbol "LM35-NEB_1_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "+V_{S}")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "V_{OUT}")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM73"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 11.43 0)
		)
		(property "Value" "LM73"
			(at -12.7 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 11.43 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm73.pdf"
			(at -10.16 11.43 0)
		)
		(property "Description" "11 to 14 Bit digital temperature sensor with 2 wire interface, SOT23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital temperature sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "LM73_0_1")
		(symbol "LM73_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "SMBDAT")
				(number "6")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "SMBCLK")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V_{DD}")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "ADDR")
				(number "1")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "~{ALERT}")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM74CIM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 4.572 13.462 0)
		)
		(property "Value" "LM74CIM"
			(at 3.556 11.176 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 31.75 -4.318 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm74.pdf"
			(at 33.274 -6.604 0)
		)
		(property "Description" "12-Bit plus sign digital temperature sensor with SPI/Microwire, SOIC-8"
			(at 46.99 -8.89 0)
		)
		(property "ki_keywords" "Temperature sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC?8*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LM74CIM_0_1")
		(symbol "LM74CIM_1_1"
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SI/O")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "SC")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{CS}")
				(number "7")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V^{+}")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin no_connect line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM74CITP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.302 13.97 0)
		)
		(property "Value" "LM74CITP"
			(at 2.54 11.684 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-5_1.5855x1.6365mm_Layout3x2_P0.5mm"
			(at 42.926 -8.382 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm74.pdf"
			(at 31.75 -3.048 0)
		)
		(property "Description" "12-Bit plus sign digital temperature sensor with SPI/Microwire, DSBGA-5"
			(at 46.228 -5.842 0)
		)
		(property "ki_keywords" "Temperature sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DSBGA*1.5855x1.6365*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LM74CITP_0_1")
		(symbol "LM74CITP_1_1"
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SI/O")
				(number "A1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "SC")
				(number "A2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{CS}")
				(number "B3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V^{+}")
				(number "B1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "A3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM75C"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.604 6.35 0)
		)
		(property "Value" "LM75C"
			(at 2.032 6.35 0)
		)
		(property "Footprint" ""
			(at -2.794 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm75b.pdf"
			(at -17.018 9.525 0)
		)
		(property "Description" "Digital Temperature Sensor & Thermal Watchdog, SOIC-8 and VSSOP-8"
			(at -17.018 9.525 0)
		)
		(property "ki_keywords" "Temperature sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LM75C_0_1")
		(symbol "LM75C_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A0")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A1")
				(number "6")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "+Vs")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "1")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "2")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "O.S.")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM92CIM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "LM92CIM"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm92.pdf"
			(at 0 0 0)
		)
		(property "Description" "Digital Temperature Sensor and Thermal Window Comparator With Two-Wire (I2C) Interface, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "temperature sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LM92CIM_0_1")
		(symbol "LM92CIM_1_1"
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SDA")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A0")
				(number "7")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A1")
				(number "6")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "+Vs")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "T_CRIT_A")
				(number "3")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "INT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM94021"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.985 6.35 0)
		)
		(property "Value" "LM94021"
			(at 6.985 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:Texas_R-PDSO-G5_DCK-5"
			(at 6.35 -14.605 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm94021-q1.pdf"
			(at 6.985 -12.7 0)
		)
		(property "Description" "Analog, selectable coefficient -5.5/-8.2/-10.9/-13.6mV/°C, ±2C accuracy, 1.5-5.5V supply, -50C to +150C, SOT-323"
			(at 0 0 0)
		)
		(property "ki_keywords" "thermistor texas ti gain temperature sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas?R?PDSO?G5?DCK*"
			(at 0 0 0)
		)
		(symbol "LM94021_0_1")
		(symbol "LM94021_1_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "GS0")
				(number "1")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "GS1")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V_{DD}")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LMT01DQX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "LMT01DQX"
			(at 6.35 -6.35 0)
		)
		(property "Footprint" "Package_SON:Texas_DQX002A"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lmt01.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "0.5°C Accurate 2-Pin Digital Output Temperature Sensor With Pulse Count Interface. DQX (WSON-2) package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Digital Temperature Pulse Count "
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas?DQX*"
			(at 0 0 0)
		)
		(symbol "LMT01DQX_0_1")
		(symbol "LMT01DQX_1_1"
			(pin bidirectional line
				(at 0 7.62 270)
				(length 2.54)
				(name "VP")
				(number "1")
			)
			(pin bidirectional line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VN")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LMT01LPG"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "LMT01LPG"
			(at 6.35 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92-2"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lmt01.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "0.5°C Accurate 2-Pin Digital Output Temperature Sensor With Pulse Count Interface. TO-92-2 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "Digital Temperature Pulse Count "
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
		(symbol "LMT01LPG_0_1")
		(symbol "LMT01LPG_1_1"
			(pin bidirectional line
				(at 0 7.62 270)
				(length 2.54)
				(name "VP")
				(number "2")
			)
			(pin bidirectional line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VN")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LMT84DCK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LMT84DCK"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmt84.pdf"
			(at 0 0 0)
		)
		(property "Description" "Analog temperature sensor, NTC, 0.4C accuracy, -5.5mV/C, -50C to +150C, 1.5 to 5.5V, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "temperature sensor thermistor ntc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
		(symbol "LMT84DCK_0_1")
		(symbol "LMT84DCK_1_1"
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V_{DD}")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LMT85DCK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LMT85DCK"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmt85-q1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Analog temperature sensor, NTC, 0.3C accuracy, -8.2mV/C, -50C to +150C, 1.8 to 5.5V, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "temperature sensor thermistor ntc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
		(symbol "LMT85DCK_0_1")
		(symbol "LMT85DCK_1_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "V_{DD}")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V_{DD}")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LMT86DCK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LMT86DCK"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmt86-q1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Analog temperature sensor, NTC, 0.25C accuracy, -10.9mV/C, -50C to +150C, 2.2 to 5.5V, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "temperature sensor thermistor ntc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
		(symbol "LMT86DCK_0_1")
		(symbol "LMT86DCK_1_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "V_{DD}")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V_{DD}")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LMT87DCK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LMT87DCK"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmt87-q1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Analog temperature sensor, NTC, 0.3C accuracy, -13.6mV/C, -50C to +150C, 2.7 to 5.5V, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "temperature sensor thermistor ntc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
		(symbol "LMT87DCK_0_1")
		(symbol "LMT87DCK_1_1"
			(pin power_in line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "V_{DD}")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V_{DD}")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "V_{DD}")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC2983"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -16.51 33.02 0)
		)
		(property "Value" "LTC2983"
			(at 8.89 33.02 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -19.05 30.48 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/2983fc.pdf"
			(at 0 0 0)
		)
		(property "Description" "Multi-Sensor Temperature Measurement System, High Accuracy, LQFP-48 (7x7mm)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flexible Temperature Measurement RTD NTC Cold Junction Termocouple"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC2983_0_1")
		(symbol "LTC2983_1_1"
			(pin passive line
				(at -20.32 27.94 0)
				(length 3.81)
				(name "CH1")
				(number "16")
			)
			(pin passive line
				(at -20.32 25.4 0)
				(length 3.81)
				(name "CH2")
				(number "17")
			)
			(pin passive line
				(at -20.32 22.86 0)
				(length 3.81)
				(name "CH3")
				(number "18")
			)
			(pin passive line
				(at -20.32 20.32 0)
				(length 3.81)
				(name "CH4")
				(number "19")
			)
			(pin passive line
				(at -20.32 17.78 0)
				(length 3.81)
				(name "CH5")
				(number "20")
			)
			(pin passive line
				(at -20.32 15.24 0)
				(length 3.81)
				(name "CH6")
				(number "21")
			)
			(pin passive line
				(at -20.32 12.7 0)
				(length 3.81)
				(name "CH7")
				(number "22")
			)
			(pin passive line
				(at -20.32 10.16 0)
				(length 3.81)
				(name "CH8")
				(number "23")
			)
			(pin passive line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "CH9")
				(number "24")
			)
			(pin passive line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "CH10")
				(number "25")
			)
			(pin passive line
				(at -20.32 2.54 0)
				(length 3.81)
				(name "CH11")
				(number "26")
			)
			(pin passive line
				(at -20.32 0 0)
				(length 3.81)
				(name "CH12")
				(number "27")
			)
			(pin passive line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "CH13")
				(number "28")
			)
			(pin passive line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "CH14")
				(number "29")
			)
			(pin passive line
				(at -20.32 -7.62 0)
				(length 3.81)
				(name "CH15")
				(number "30")
			)
			(pin passive line
				(at -20.32 -10.16 0)
				(length 3.81)
				(name "CH16")
				(number "31")
			)
			(pin passive line
				(at -20.32 -12.7 0)
				(length 3.81)
				(name "CH17")
				(number "32")
			)
			(pin passive line
				(at -20.32 -15.24 0)
				(length 3.81)
				(name "CH18")
				(number "33")
			)
			(pin passive line
				(at -20.32 -17.78 0)
				(length 3.81)
				(name "CH19")
				(number "34")
			)
			(pin passive line
				(at -20.32 -20.32 0)
				(length 3.81)
				(name "CH20")
				(number "35")
			)
			(pin passive line
				(at -20.32 -25.4 0)
				(length 3.81)
				(name "COM")
				(number "36")
			)
			(pin power_in line
				(at -10.16 -33.02 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at -7.62 -33.02 90)
				(length 3.81)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at -5.08 35.56 270)
				(length 3.81)
				(name "V_{DD}")
				(number "2")
			)
			(pin power_in line
				(at -5.08 -33.02 90)
				(length 3.81)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 3.81)
				(name "V_{DD}")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -33.02 90)
				(length 3.81)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 3.81)
				(name "V_{DD}")
				(number "6")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 3.81)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 3.81)
				(name "V_{DD}")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -33.02 90)
				(length 3.81)
				(name "GND")
				(number "12")
			)
			(pin power_in line
				(at 5.08 35.56 270)
				(length 3.81)
				(name "V_{DD}")
				(number "45")
			)
			(pin power_in line
				(at 5.08 -33.02 90)
				(length 3.81)
				(name "GND")
				(number "15")
			)
			(pin power_in line
				(at 7.62 -33.02 90)
				(length 3.81)
				(name "GND")
				(number "44")
			)
			(pin no_connect line
				(at 16.51 22.86 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin passive line
				(at 20.32 27.94 180)
				(length 3.81)
				(name "Q1")
				(number "48")
			)
			(pin passive line
				(at 20.32 20.32 180)
				(length 3.81)
				(name "Q2")
				(number "47")
			)
			(pin passive line
				(at 20.32 17.78 180)
				(length 3.81)
				(name "Q3")
				(number "46")
			)
			(pin passive line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "V_{REFOUT}")
				(number "13")
			)
			(pin passive line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "V_{REFP}")
				(number "14")
			)
			(pin passive line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "V_{REF_BYP}")
				(number "11")
			)
			(pin passive line
				(at 20.32 0 180)
				(length 3.81)
				(name "LDO")
				(number "43")
			)
			(pin output line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "INTERRUPT")
				(number "37")
			)
			(pin input line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "~{RESET}")
				(number "42")
			)
			(pin tri_state line
				(at 20.32 -17.78 180)
				(length 3.81)
				(name "SDO")
				(number "39")
			)
			(pin input line
				(at 20.32 -20.32 180)
				(length 3.81)
				(name "SDI")
				(number "40")
			)
			(pin input line
				(at 20.32 -22.86 180)
				(length 3.81)
				(name "SCK")
				(number "38")
			)
			(pin input line
				(at 20.32 -25.4 180)
				(length 3.81)
				(name "~{CS}")
				(number "41")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX31820"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "MAX31820"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at -25.4 -6.35 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX31820.pdf"
			(at -3.81 6.35 0)
		)
		(property "Description" "1-Wire Ambient Temperature Sensor TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "OneWire 1-Wire 1Wire Maxim Dallas"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*92*"
			(at 0 0 0)
		)
		(symbol "MAX31820_0_1")
		(symbol "MAX31820_1_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V_{DD}")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin bidirectional line
				(at 7.62 0 180)
				(length 2.54)
				(name "DQ")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX31820PAR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "MAX31820PAR"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at -25.4 -6.35 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX31820PAR.pdf"
			(at -3.81 6.35 0)
		)
		(property "Description" "1-Wire, Parasite-Power, Ambient Temperature Sensor TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "OneWire 1-Wire 1Wire Maxim Dallas"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*92*"
			(at 0 0 0)
		)
		(symbol "MAX31820PAR_0_1")
		(symbol "MAX31820PAR_1_1"
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin bidirectional line
				(at 7.62 0 180)
				(length 2.54)
				(name "DQ")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX31826"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "MAX31826"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at -24.13 -8.89 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX31826.pdf"
			(at -5.08 -3.81 0)
		)
		(property "Description" "1-Wire Digital Temperature Sensor with 1Kb Lockable EEPROM MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "1Wire OneWire Maxim Dallas"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MAX31826_0_1")
		(symbol "MAX31826_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "AD0")
				(number "5")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "AD1")
				(number "6")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "AD2")
				(number "7")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "AD3")
				(number "8")
			)
			(pin no_connect line
				(at -7.62 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V_{DD}")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "DQ")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX31855KASA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MAX31855KASA"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -10.16 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX31855.pdf"
			(at 2.54 -12.7 0)
		)
		(property "Description" "Cold Junction K-type Thermocouple Interface, SPI, SOIC-8"
			(at 2.54 -7.62 0)
		)
		(property "ki_keywords" "Maxim"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MAX31855KASA_0_1")
		(symbol "MAX31855KASA_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "T+")
				(number "3")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "T-")
				(number "2")
			)
			(pin no_connect line
				(at -7.62 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V_{CC}")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SCK")
				(number "5")
			)
			(pin tri_state line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SO")
				(number "7")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{CS}")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX31856"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "MAX31856"
			(at 13.97 13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 3.81 -13.97 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX31856.pdf"
			(at -1.27 5.08 0)
		)
		(property "Description" "Precision Thermocouple to Digital Converter with Linearization, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Thermocouple converter serial"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*14*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MAX31856_0_1")
		(symbol "MAX31856_1_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "T+")
				(number "4")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "T-")
				(number "3")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "BIAS")
				(number "2")
			)
			(pin no_connect line
				(at -10.16 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "6")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "AVDD")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "AGND")
				(number "1")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "DVDD")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "DGND")
				(number "14")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "~{DRDY}")
				(number "7")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "~{FAULT}")
				(number "13")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{CS}")
				(number "9")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SCK")
				(number "10")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "SDO")
				(number "11")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "SDI")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX31865xAP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 19.05 0)
		)
		(property "Value" "MAX31865xAP"
			(at 10.16 19.05 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_5.3x7.2mm_P0.65mm"
			(at 3.81 -16.51 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX31865.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "RTD-to-Digital Converter, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "RTD SPI Temperature"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MAX31865xAP_0_1")
		(symbol "MAX31865xAP_1_1"
			(pin output line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "~{DRDY}")
				(number "1")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "SDI")
				(number "14")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "SCLK")
				(number "15")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "~{CS}")
				(number "16")
			)
			(pin tri_state line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "SDO")
				(number "17")
			)
			(pin no_connect line
				(at -12.7 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "DVDD")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "DGND")
				(number "18")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "19")
			)
			(pin power_out line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "BIAS")
				(number "4")
			)
			(pin input line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "REFIN+")
				(number "5")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "REFIN-")
				(number "6")
			)
			(pin passive line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "ISENSOR")
				(number "7")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 2.54)
				(name "FORCE+")
				(number "8")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "FORCE2")
				(number "9")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "RTDIN+")
				(number "10")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "RTDIN-")
				(number "11")
			)
			(pin power_out line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "FORCE-")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX31865xTP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 19.05 0)
		)
		(property "Value" "MAX31865xTP"
			(at 10.16 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:TQFN-20-1EP_5x5mm_P0.65mm_EP3.25x3.25mm"
			(at 3.81 -16.51 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX31865.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "RTD-to-Digital Converter, TQFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "RTD SPI Temperature"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFN*1EP*5x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MAX31865xTP_0_1")
		(symbol "MAX31865xTP_1_1"
			(pin output line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "~{DRDY}")
				(number "18")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "SDI")
				(number "11")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "SCLK")
				(number "12")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "~{CS}")
				(number "13")
			)
			(pin tri_state line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "SDO")
				(number "14")
			)
			(pin no_connect line
				(at -12.7 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "DVDD")
				(number "19")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "DGND")
				(number "15")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at 2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_out line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "BIAS")
				(number "1")
			)
			(pin input line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "REFIN+")
				(number "2")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "REFIN-")
				(number "3")
			)
			(pin passive line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "ISENSOR")
				(number "4")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 2.54)
				(name "FORCE+")
				(number "5")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "FORCE2")
				(number "6")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "RTDIN+")
				(number "7")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "RTDIN-")
				(number "8")
			)
			(pin power_out line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "FORCE-")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX6654"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "MAX6654"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SSOP-16_3.9x4.9mm_P0.635mm"
			(at 1.27 -15.24 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX6654.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "Remote and Local Temperature Sensor, SSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C SMBus Serial"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "MAX6654_0_1")
		(symbol "MAX6654_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "ADD0")
				(number "10")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "ADD1")
				(number "6")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "DXP")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "DXN")
				(number "4")
			)
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "Vcc")
				(number "2")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 7.62 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "~{STBY}")
				(number "15")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SMBDATA")
				(number "12")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SMBCLK")
				(number "14")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "~{ALERT}")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP9501"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 0 90)
		)
		(property "Value" "MCP9501"
			(at -3.81 0 90)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -8.89 -2.54 90)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002268B.pdf"
			(at -6.35 0 90)
		)
		(property "Description" "Temperature Switch with Selectable Hysteresis, Open-Drain, Active-Low Output (Hot Option), SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Temperature Switch sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MCP9501_0_1")
		(symbol "MCP9501_1_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 5.08 10.16 270)
				(length 2.54)
				(name "Hyst")
				(number "3")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "Out")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP9502"
		(pin_names
			(offset 0.127)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 0 90)
		)
		(property "Value" "MCP9502"
			(at -3.81 0 90)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -8.89 -2.54 90)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002268B.pdf"
			(at -6.35 0 90)
		)
		(property "Description" "Temperature Switch with Selectable Hysteresis, Push-Pull, Active-High Output (Hot Option), SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Temperature Switch sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MCP9502_0_1")
		(symbol "MCP9502_1_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 5.08 10.16 270)
				(length 2.54)
				(name "Hyst")
				(number "3")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "Out")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP9700Ax-ELT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MCP9700Ax-ELT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001942G.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low power, analog thermistor temperature sensor, ±2C accuracy, -40C to +125C, in SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "temperature sensor thermistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
		(symbol "MCP9700Ax-ELT_0_1")
		(symbol "MCP9700Ax-ELT_1_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V_{DD}")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "V_{OUT}")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP9700x-HTT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MCP9700x-HTT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/20001942g.pdf"
			(at -3.81 6.35 0)
		)
		(property "Description" "Low power, analog thermistor temperature sensor, ±4C accuracy, -40C to +150C, in SOT-23-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "temperature sensor thermistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MCP9700x-HTT_0_1")
		(symbol "MCP9700x-HTT_1_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V_{DD}")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "V_{OUT}")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP9800Ax-xOT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MCP9800Ax-xOT"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 17.78 -6.35 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/OTH/ProductDocuments/DataSheets/21909d.pdf"
			(at 0 0 0)
		)
		(property "Description" "2-Wire High-Accuracy Temperature Sensor, No Serial Bus time-out, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Temperature Sensor No Serial Bus time-out"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MCP9800Ax-xOT_0_1")
		(symbol "MCP9800Ax-xOT_1_1"
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "SCLK")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V_{DD}")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "ALERT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP9804_DFN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "MCP9804_DFN"
			(at 10.16 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.7x1.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22203b.pdf"
			(at -6.35 11.43 0)
		)
		(property "Description" "±0.25°C (±1°C) Typical (Maximum), Digital Temperature Sensor, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "temperature sensor I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MCP9804_DFN_0_1")
		(symbol "MCP9804_DFN_1_1"
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "SDA")
				(number "1")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SCL")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A0")
				(number "7")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A1")
				(number "6")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A2")
				(number "5")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V_{DD}")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "EP/GND")
				(number "9")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "Alert")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP9804_MSOP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "MCP9804_MSOP"
			(at 10.16 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22203b.pdf"
			(at -6.35 11.43 0)
		)
		(property "Description" "±0.25°C (±1°C) Typical (Maximum), Digital Temperature Sensor, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "temperature sensor I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP9804_MSOP_0_1")
		(symbol "MCP9804_MSOP_1_1"
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "SDA")
				(number "1")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SCL")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A0")
				(number "7")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A1")
				(number "6")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A2")
				(number "5")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V_{DD}")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "Alert")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP9844x-xMN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "MCP9844x-xMN"
			(at 6.35 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.36x1.46mm"
			(at -27.94 -12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005192B.pdf"
			(at -6.35 11.43 0)
		)
		(property "Description" "±1°C Accurate, 1.8V Digital Temperature Sensor, I²C, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C TWI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MCP9844x-xMN_0_1")
		(symbol "MCP9844x-xMN_1_1"
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A0")
				(number "1")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V_{DD}")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "EP/GND")
				(number "9")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "Event")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCT2075D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "PCT2075D"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_SO:SO-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCT2075.pdf"
			(at 0 0 0)
		)
		(property "Description" "NXP I2C-bus Fm+ digital temperature sensor and thermal watchdog, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "temperature sensor I2C single channel"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "PCT2075D_0_1")
		(symbol "PCT2075D_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A0")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A1")
				(number "6")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "1")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "2")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OS")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCT2075DP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "PCT2075DP"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_3x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCT2075.pdf"
			(at 0 0 0)
		)
		(property "Description" "NXP I2C-bus Fm+ digital temperature sensor and thermal watchdog, TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "temperature sensor I2C single channel"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PCT2075DP_0_1")
		(symbol "PCT2075DP_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A0")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A1")
				(number "6")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "1")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "2")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OS")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PT100"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "TH"
			(at -4.445 0 90)
		)
		(property "Value" "PT100"
			(at 3.175 0 90)
		)
		(property "Footprint" ""
			(at 0 1.27 0)
		)
		(property "Datasheet" "https://www.heraeus.com/media/media/group/doc_group/products_1/hst/sot_to/de_15/to_92_d.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "PT100 platinum temperature sensor (RTD)"
			(at 0 0 0)
		)
		(property "ki_keywords" "platinum temperature sensor RTD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92* PIN?ARRAY* bornier* Terminal?Block* SOD70* R*1206* R*0805*"
			(at 0 0 0)
		)
		(symbol "PT100_0_1")
		(symbol "PT100_1_1"
			(pin passive line
				(at 0 3.81 270)
				(length 1.27)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 1.27)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Si7050-A20"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "Si7050-A20"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6-1EP_3x3mm_P1mm_EP1.65x2.55mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/Si7050-1-3-4-5-A20.pdf"
			(at -5.08 7.62 0)
		)
		(property "Description" "I2C Temperature Sensor, ±1.0ºC, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Temperature Sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P1mm*"
			(at 0 0 0)
		)
		(symbol "Si7050-A20_0_1")
		(symbol "Si7050-A20_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "SDA")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMP100"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 6.35 0)
		)
		(property "Value" "TMP100"
			(at 12.7 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/tmp100"
			(at -1.27 0 0)
		)
		(property "Description" "Temperature Sensor with I2C/SMBus Interface, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "temperature sensor i2c smbus"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TMP100_0_1")
		(symbol "TMP100_1_1"
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SDA")
				(number "6")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "ADD0")
				(number "5")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "ADD1")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMP101"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 10.795 0)
		)
		(property "Value" "TMP101"
			(at -2.54 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tmp101.pdf"
			(at 1.27 -11.43 0)
		)
		(property "Description" "Digital Temperature Sensor with I2C/SMBus Interface, ±2°C, one-shot conversion, alert, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital temperature sensor i2c smbus"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TMP101_0_1")
		(symbol "TMP101_1_1"
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SDA")
				(number "6")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "ADD0")
				(number "5")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V+")
				(number "4")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "ALERT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMP102xxDRL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 10.795 0)
		)
		(property "Value" "TMP102xxDRL"
			(at -2.54 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-563"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tmp102.pdf"
			(at 1.27 -11.43 0)
		)
		(property "Description" "Digital Temperature Sensor, ±3°C, low-Power, SMBus, 12 bit, Two-Wire Serial Interface, SOT-563"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital temperature sensor i2c smbus"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?563*"
			(at 0 0 0)
		)
		(symbol "TMP102xxDRL_0_1")
		(symbol "TMP102xxDRL_1_1"
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SDA")
				(number "6")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "ADD0")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "ALERT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMP1075D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TMP1075D"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_SO:SO-8_3.9x4.9mm_P1.27mm"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/tmp1075"
			(at 0 0 0)
		)
		(property "Description" "I2C-bus digital temperature sensor and thermal watchdog, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "temperature sensor I2C single channel"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TMP1075D_0_1")
		(symbol "TMP1075D_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A0")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A1")
				(number "6")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "1")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "2")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "ALERT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMP1075DGK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TMP1075DGK"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 0 -6.985 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/tmp1075"
			(at 0 0 0)
		)
		(property "Description" "I2C-bus digital temperature sensor and thermal watchdog, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "temperature sensor I2C single channel"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TMP1075DGK_0_1")
		(symbol "TMP1075DGK_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A0")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A1")
				(number "6")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "1")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "2")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "ALERT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMP1075DSG"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TMP1075DSG"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_SON:WSON-8-1EP_2x2mm_P0.5mm_EP0.9x1.6mm_ThermalVias"
			(at 1.905 -6.35 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/tmp1075"
			(at 0 0 0)
		)
		(property "Description" "I2C-bus digital temperature sensor and thermal watchdog, WSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "temperature sensor I2C single channel"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TMP1075DSG_0_1")
		(symbol "TMP1075DSG_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A0")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A1")
				(number "6")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "5")
			)
			(pin passive line
				(at -2.54 -7.62 90)
				(length 2.54)
				(name "EP")
				(number "9")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "1")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL")
				(number "2")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "ALERT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMP110D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 10.795 0)
		)
		(property "Value" "TMP110D"
			(at -2.54 8.89 0)
		)
		(property "Footprint" "Package_SON:Texas_X2SON-5_0.8x0.8mm_P0.48mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tmp110.pdf"
			(at 1.27 -11.43 0)
		)
		(property "Description" "Digital Temperature Sensor with I2C/SMBus Interface, +/-1° C accurate, address pin, X2SON"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital temperature sensor i2c smbus"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas?X2SON*0.8x0.8mm*P0.48mm*"
			(at 0 0 0)
		)
		(symbol "TMP110D_0_1")
		(symbol "TMP110D_1_1"
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SDA")
				(number "4")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "ADD0")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMP114"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 -10.16 0)
		)
		(property "Value" "TMP114"
			(at 2.54 -12.7 0)
		)
		(property "Footprint" "Package_BGA:Texas_PicoStar_BGA-4_0.758x0.758mm_Layout2x2_P0.4mm"
			(at -2.54 -25.4 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tmp114.pdf"
			(at 0 -27.94 0)
		)
		(property "Description" "Ultra-Small 0.76x0.76x0.15mm, 1.08..1.98V Supply, High Accuracy I2C 16-bit Digital Temperature Sensor, BGA-4"
			(at 0 -22.86 0)
		)
		(property "ki_keywords" "thermometer monitor i2c texas"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Texas*PicoStar*"
			(at 0 0 0)
		)
		(symbol "TMP114_0_1")
		(symbol "TMP114_1_1"
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SDA")
				(number "B1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "B2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V+")
				(number "A1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "A2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMP117xxYBG"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 10.795 0)
		)
		(property "Value" "TMP117xxYBG"
			(at -2.54 8.89 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-6_0.95x1.488mm_Layout2x3_P0.4mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tmp117.pdf"
			(at 1.27 -11.43 0)
		)
		(property "Description" "Digital Temperature Sensor with I2C/SMBus Interface, 16 bits, ±0.3°C, one-shot conversion, alert, nist traceable, EEPROM, DSBGA"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital temperature sensor i2c smbus"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas?DSBGA?6?0.95x1.488mm?Layout2x3?P0.4mm*"
			(at 0 0 0)
		)
		(symbol "TMP117xxYBG_0_1")
		(symbol "TMP117xxYBG_1_1"
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SDA")
				(number "A1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SCL")
				(number "A2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "ADD0")
				(number "C1")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V+")
				(number "B1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "B2")
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "ALERT")
				(number "C2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMP20AIDCK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TMP20AIDCK"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tmp20.pdf"
			(at 0 0 0)
		)
		(property "Description" "Analog thermistor temperature sensor, ±2.5C accuracy, -55C to +130C, SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "temperature sensor thermistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
		(symbol "TMP20AIDCK_0_1")
		(symbol "TMP20AIDCK_1_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V_{DD}")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "V_{OUT}")
				(number "3")
			)
			(pin no_connect line
				(at 10.16 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMP20AIDRL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TMP20AIDRL"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-563"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tmp20.pdf"
			(at -6.35 6.35 0)
		)
		(property "Description" "Analog thermistor temperature sensor, ±2.5C accuracy, -55C to +130C, SOT-563-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "temperature sensor thermistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?563*"
			(at 0 0 0)
		)
		(symbol "TMP20AIDRL_0_1")
		(symbol "TMP20AIDRL_1_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V_{DD}")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin no_connect line
				(at 7.62 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "V_{OUT}")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMP36xS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "TMP36xS"
			(at 6.35 -8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/TMP35_36_37.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low Voltage Temperature Sensor, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Temperature Sensor SOIC-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC?8*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TMP36xS_0_1")
		(symbol "TMP36xS_1_1"
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{SHUTDOWN}")
				(number "5")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "+Vs")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "V_{OUT}")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMP411"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "TMP411"
			(at 1.27 8.89 0)
		)
		(property "Footprint" ""
			(at -2.54 0 0)
		)
		(property "Datasheet" "http://www.ti.com.cn/cn/lit/ds/symlink/tmp411.pdf"
			(at -2.54 0 0)
		)
		(property "Description" "- Remote and Local TEMPERATURE SENSOR"
			(at 0 0 0)
		)
		(property "ki_keywords" "Temperature sensor remote local i2c"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TMP411_0_1")
		(symbol "TMP411_1_1"
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "D+")
				(number "2")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "D-")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V+")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SDA")
				(number "7")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SCL")
				(number "8")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{THERM}")
				(number "4")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "~{ALERT}")
				(number "6")
				(alternate "~{THERM2}" open_collector line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMP461xxRUN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "TMP461xxRUN"
			(at 2.54 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RUN0010A_WQFN-10_2x2mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tmp461.pdf"
			(at 0 0 0)
		)
		(property "Description" "Texas Instruments High-Accuracy Remote and Local Temperature Sensor with Pin-Programmable Bus Address, WQFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Temperature sensor remote I2C TI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RUN0010A*"
			(at 0 0 0)
		)
		(symbol "TMP461xxRUN_0_1")
		(symbol "TMP461xxRUN_1_1"
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SDA")
				(number "8")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SCL")
				(number "9")
			)
			(pin open_collector line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{THERM}")
				(number "4")
			)
			(pin open_collector line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{ALERT/THERM2}")
				(number "7")
				(alternate "~{ALERT}" open_collector line)
				(alternate "~{THERM2}" open_collector line)
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "A0")
				(number "5")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "A1")
				(number "10")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "D+")
				(number "2")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "D-")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMP464xxRGT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "TMP464xxRGT"
			(at 2.54 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.68x1.68mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tmp464.pdf"
			(at 0 0 0)
		)
		(property "Description" "Texas Instruments 5-Channel (4-Remote and 1-Local), High-Accuracy Temperature Sensor with Pin-Programmable Bus Address, VQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Temperature sensor remote I2C TI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TMP464xxRGT_0_1")
		(symbol "TMP464xxRGT_1_1"
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SDA")
				(number "12")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SCL")
				(number "13")
			)
			(pin open_collector line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{THERM}")
				(number "10")
			)
			(pin open_collector line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{THERM2}")
				(number "11")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "ADD")
				(number "9")
			)
			(pin no_connect line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin no_connect line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+")
				(number "14")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin no_connect line
				(at 10.16 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at 10.16 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "D1+")
				(number "6")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "D2+")
				(number "5")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "D3+")
				(number "4")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(name "D4+")
				(number "3")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "D-")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TMP468xxRGT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 16.51 0)
		)
		(property "Value" "TMP468xxRGT"
			(at 2.54 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.68x1.68mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tmp468.pdf"
			(at 0 0 0)
		)
		(property "Description" "Texas Instruments 9-Channel (8-Remote and 1-Local), High-Accuracy Temperature Sensor with Pin-Programmable Bus Address, VQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Temperature sensor remote I2C TI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TMP468xxRGT_0_1")
		(symbol "TMP468xxRGT_1_1"
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "SDA")
				(number "12")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "SCL")
				(number "13")
			)
			(pin open_collector line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "~{THERM}")
				(number "10")
			)
			(pin open_collector line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{THERM2}")
				(number "11")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "ADD")
				(number "9")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "V+")
				(number "14")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "D1+")
				(number "6")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "D2+")
				(number "5")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "D3+")
				(number "4")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "D4+")
				(number "3")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(name "D-")
				(number "7")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "D5+")
				(number "2")
			)
			(pin passive line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "D6+")
				(number "1")
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "D7+")
				(number "16")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "D8+")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TSIC206-SO8"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TSIC206-SO8"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -8.89 3.81 0)
		)
		(property "Datasheet" "https://shop.bb-sensors.com/out/media/Datasheet_Digital_Semiconductor_temperatur_sensor_TSIC.pdf"
			(at 0 0 0)
		)
		(property "Description" "Digital temperature sensor, range -50 ... +150 °C, 0.5 K accuracy, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "temperature digital"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TSIC206-SO8_0_1")
		(symbol "TSIC206-SO8_1_1"
			(pin no_connect line
				(at -5.08 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at -2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V+")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin no_connect line
				(at 2.54 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 5.08 -5.08 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "Signal")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TSIC206-TO92"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TSIC206-TO92"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at -8.89 3.81 0)
		)
		(property "Datasheet" "https://shop.bb-sensors.com/out/media/Datasheet_Digital_Semiconductor_temperatur_sensor_TSIC.pdf"
			(at 0 0 0)
		)
		(property "Description" "Digital temperature sensor, range -50 ... +150 °C, 0.5 K accuracy, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "temperature digital"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
		(symbol "TSIC206-TO92_0_1")
		(symbol "TSIC206-TO92_1_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V+")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "Signal")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD8495"
		(extends "AD8494")
		(property "Reference" "U"
			(at 5.08 3.81 0)
		)
		(property "Value" "AD8495"
			(at 8.89 -3.81 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 22.86 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ad8494_8495_8496_8497.pdf"
			(at 0 0 0)
		)
		(property "Description" "Precision Thermocouple Amplifiers with Cold Junction Compensation, K-Type Thermocouple, 0 to 50C, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Thermocouple Amp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*8*"
			(at 0 0 0)
		)
	)
	(symbol "AD8496"
		(extends "AD8494")
		(property "Reference" "U"
			(at 5.08 3.81 0)
		)
		(property "Value" "AD8496"
			(at 8.89 -3.81 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 22.86 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ad8494_8495_8496_8497.pdf"
			(at 0 0 0)
		)
		(property "Description" "Precision Thermocouple Amplifiers with Cold Junction Compensation, J-Type Thermocouple, 25 to 100C, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Thermocouple Amp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*8*"
			(at 0 0 0)
		)
	)
	(symbol "AD8497"
		(extends "AD8494")
		(property "Reference" "U"
			(at 5.08 3.81 0)
		)
		(property "Value" "AD8497"
			(at 8.89 -3.81 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 22.86 -6.35 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ad8494_8495_8496_8497.pdf"
			(at 0 0 0)
		)
		(property "Description" "Precision Thermocouple Amplifiers with Cold Junction Compensation, K-Type Thermocouple, 25 to 100C, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Thermocouple Amp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*8*"
			(at 0 0 0)
		)
	)
	(symbol "DS1621S"
		(extends "DS1621")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "DS1621S"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -17.78 -8.89 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DS1621.pdf"
			(at -3.81 6.35 0)
		)
		(property "Description" "1-Wire Digital Thermometer and Thermostat, SOIC-8 (150 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "OneWire 1-Wire 1Wire Maxim Dallas"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "DS1621V"
		(extends "DS1621")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "DS1621V"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_5.3x5.3mm_P1.27mm"
			(at -17.78 -8.89 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DS1621.pdf"
			(at -3.81 6.35 0)
		)
		(property "Description" "1-Wire Digital Thermometer and Thermostat, SOIC-8 (208 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "OneWire 1-Wire 1Wire Maxim Dallas"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*5.3x5.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "DS1821C"
		(extends "MAX31820")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "DS1821C"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at -25.4 -6.35 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/DS1821.pdf"
			(at -3.81 6.35 0)
		)
		(property "Description" "Programmable Digital Thermostat and Thermometer TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "OneWire 1Wire Maxim Dallas"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*92*"
			(at 0 0 0)
		)
	)
	(symbol "DS1822"
		(extends "MAX31820")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "DS1822"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at -25.4 -6.35 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/DS1822.pdf"
			(at -3.81 6.35 0)
		)
		(property "Description" "Econo 1-Wire Digital Thermometer TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "OneWire 1Wire Dallas Maxim"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*92*"
			(at 0 0 0)
		)
	)
	(symbol "DS1822-PAR"
		(extends "MAX31820PAR")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "DS1822-PAR"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at -25.4 -6.35 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/DS1822-PAR.pdf"
			(at -3.81 6.35 0)
		)
		(property "Description" "Econo 1-Wire Parasite-Power Digital Thermometer TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "OneWire 1Wire Maxim Dallas"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*92*"
			(at 0 0 0)
		)
	)
	(symbol "DS1825"
		(extends "MAX31826")
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "DS1825"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at -24.13 -8.89 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/DS1825.pdf"
			(at -5.08 -3.81 0)
		)
		(property "Description" "Programmable Resolution 1-Wire Digital Thermometer With 4-Bit ID MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "1Wire OneWire Maxim Dallas"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "DS18B20"
		(extends "MAX31820")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "DS18B20"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at -25.4 -6.35 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/DS18B20.pdf"
			(at -3.81 6.35 0)
		)
		(property "Description" "Programmable Resolution 1-Wire Digital Thermometer TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "OneWire 1Wire Dallas Maxim"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*92*"
			(at 0 0 0)
		)
	)
	(symbol "DS18B20-PAR"
		(extends "MAX31820PAR")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "DS18B20-PAR"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at -25.4 -6.35 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/DS18B20-PAR.pdf"
			(at -3.81 6.35 0)
		)
		(property "Description" "1-Wire Parasite-Power Digital Thermometer TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "OneWire 1Wire Maxim Dallas"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*92*"
			(at 0 0 0)
		)
	)
	(symbol "DS18B20Z"
		(extends "DS1822Z")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "DS18B20Z"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -25.4 -6.35 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/DS18B20.pdf"
			(at -3.81 6.35 0)
		)
		(property "Description" "Programmable Resolution 1-Wire Digital Thermometer SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OneWire 1Wire Maxim Dallas"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "DS18S20"
		(extends "MAX31820")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "DS18S20"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at -25.4 -6.35 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/DS18S20.pdf"
			(at -3.81 6.35 0)
		)
		(property "Description" "High-Precision 1-Wire Digital Thermometer TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "OneWire 1Wire Maxim Dallas"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*92*"
			(at 0 0 0)
		)
	)
	(symbol "DS18S20-PAR"
		(extends "MAX31820PAR")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "DS18S20-PAR"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at -25.4 -6.35 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/DS18S20-PAR.pdf"
			(at -3.81 6.35 0)
		)
		(property "Description" "1-Wire Parasite-Power Digital Thermometer TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "OneWire 1Wire Maxim Dallas"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO*92*"
			(at 0 0 0)
		)
	)
	(symbol "DS18S20Z"
		(extends "DS1822Z")
		(property "Reference" "U"
			(at -3.81 6.35 0)
		)
		(property "Value" "DS18S20Z"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -25.4 -6.35 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/DS18S20.pdf"
			(at -3.81 6.35 0)
		)
		(property "Description" "High-Precision 1-Wire Digital Thermometer SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "OneWire 1Wire Dallas Maxim"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "KT100"
		(extends "KTY81")
		(property "Reference" "TH"
			(at -4.445 0 90)
		)
		(property "Value" "KT100"
			(at 3.175 0 90)
		)
		(property "Footprint" ""
			(at 5.08 0 90)
		)
		(property "Datasheet" "http://www.b-kainka.de/Daten/Sensor/kty10.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "KTY10/KT100 series silicon temperature sensors"
			(at 0 0 0)
		)
		(property "ki_keywords" "silicon temperature sensors"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOD?70*"
			(at 0 0 0)
		)
	)
	(symbol "KTY10"
		(extends "KTY81")
		(property "Reference" "TH"
			(at -4.445 0 90)
		)
		(property "Value" "KTY10"
			(at 3.175 0 90)
		)
		(property "Footprint" ""
			(at 5.08 0 90)
		)
		(property "Datasheet" "http://www.b-kainka.de/Daten/Sensor/kty10.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "KTY10/KT100 series silicon temperature sensors"
			(at 0 0 0)
		)
		(property "ki_keywords" "silicon temperature sensors"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOD?70*"
			(at 0 0 0)
		)
	)
	(symbol "KTY84"
		(extends "KTY83")
		(property "Reference" "TH"
			(at 0 2.54 0)
		)
		(property "Value" "KTY84"
			(at 0 -3.175 0)
		)
		(property "Footprint" "Diode_THT:D_DO-34_SOD68_P7.62mm_Horizontal"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/KTY84_SER.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "KTY84 series silicon temperature sensors, polarized, SOD68"
			(at 0 0 0)
		)
		(property "ki_keywords" "silicon temperature sensor diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DO?34*SOD68*"
			(at 0 0 0)
		)
	)
	(symbol "LM20CIM7"
		(extends "LM20BIM7")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LM20CIM7"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm20.pdf"
			(at 0 0 0)
		)
		(property "Description" "Precision Temperature Sensor, Accuracy at 30°C ±4°C to ±5°C Maximum, SC70"
			(at 0 0 0)
		)
		(property "ki_keywords" "temperature sensor thermistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?353*"
			(at 0 0 0)
		)
	)
	(symbol "LM73-1"
		(extends "LM73")
		(property "Reference" "U"
			(at -12.7 11.43 0)
		)
		(property "Value" "LM73-1"
			(at -12.7 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 11.43 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm73.pdf"
			(at -10.16 11.43 0)
		)
		(property "Description" "11 to 14 Bit digital temperature sensor with 2 wire interface, SOT23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital temperature sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "LM75B"
		(extends "LM75C")
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "LM75B"
			(at 0 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm75b.pdf"
			(at 0 0 0)
		)
		(property "Description" "Digital Temperature Sensor & Thermal Watchdog with LP on I2C and bus fault timeout, SOIC-8 and VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Temperature sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX31855EASA"
		(extends "MAX31855KASA")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MAX31855EASA"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -10.16 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX31855.pdf"
			(at 2.54 -12.7 0)
		)
		(property "Description" "Cold Junction E-type Thermocouple Interface, SPI, SOIC-8"
			(at 2.54 -7.62 0)
		)
		(property "ki_keywords" "Maxim"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX31855JASA"
		(extends "MAX31855KASA")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MAX31855JASA"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -10.16 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX31855.pdf"
			(at 2.54 -12.7 0)
		)
		(property "Description" "Cold Junction J-type Thermocouple Interface, SPI, SOIC-8"
			(at 2.54 -7.62 0)
		)
		(property "ki_keywords" "Maxim"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX31855NASA"
		(extends "MAX31855KASA")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MAX31855NASA"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -10.16 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX31855.pdf"
			(at 2.54 -12.7 0)
		)
		(property "Description" "Cold Junction N-type Thermocouple Interface, SPI, SOIC-8"
			(at 2.54 -7.62 0)
		)
		(property "ki_keywords" "Maxim"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX31855RASA"
		(extends "MAX31855KASA")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MAX31855RASA"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -10.16 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX31855.pdf"
			(at 2.54 -12.7 0)
		)
		(property "Description" "Cold Junction R-type Thermocouple Interface, SPI, SOIC-8"
			(at 2.54 -7.62 0)
		)
		(property "ki_keywords" "Maxim"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX31855SASA"
		(extends "MAX31855KASA")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MAX31855SASA"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -10.16 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX31855.pdf"
			(at 2.54 -12.7 0)
		)
		(property "Description" "Cold Junction S-type Thermocouple Interface, SPI, SOIC-8"
			(at 2.54 -7.62 0)
		)
		(property "ki_keywords" "Maxim"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX31855TASA"
		(extends "MAX31855KASA")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MAX31855TASA"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -10.16 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX31855.pdf"
			(at 2.54 -12.7 0)
		)
		(property "Description" "Cold Junction T-type Thermocouple Interface, SPI, SOIC-8"
			(at 2.54 -7.62 0)
		)
		(property "ki_keywords" "Maxim"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP9503"
		(extends "MCP9501")
		(property "Reference" "U"
			(at -6.35 0 90)
		)
		(property "Value" "MCP9503"
			(at -3.81 0 90)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -8.89 -2.54 90)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002268B.pdf"
			(at -6.35 0 90)
		)
		(property "Description" "Temperature Switch with Selectable Hysteresis, Open-Drain, Active-Low Output (Cold Option), SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Temperature Switch sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP9504"
		(extends "MCP9502")
		(property "Reference" "U"
			(at -6.35 0 90)
		)
		(property "Value" "MCP9504"
			(at -3.81 0 90)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at -8.89 -2.54 90)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002268B.pdf"
			(at -6.35 0 90)
		)
		(property "Description" "Temperature Switch with Selectable Hysteresis, Push-Pull, Active-High Output (Cold Option), SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Temperature Switch sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP9700Ax-ETT"
		(extends "MCP9700x-HTT")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MCP9700Ax-ETT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/20001942g.pdf"
			(at -3.81 6.35 0)
		)
		(property "Description" "Low power, analog thermistor temperature sensor, ±2C accuracy, -40C to +125C, in SOT-23-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "temperature sensor thermistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP9700Ax-HLT"
		(extends "MCP9700Ax-ELT")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MCP9700Ax-HLT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/20001942g.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low power, analog thermistor temperature sensor, ±2C accuracy, -40C to +150C, in SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "temperature sensor thermistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "MCP9700Ax-HTT"
		(extends "MCP9700x-HTT")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MCP9700Ax-HTT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/20001942g.pdf"
			(at -3.81 6.35 0)
		)
		(property "Description" "Low power, analog thermistor temperature sensor, ±2C accuracy, -40C to +150C, in SOT-23-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "temperature sensor thermistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP9700x-ELT"
		(extends "MCP9700Ax-ELT")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MCP9700x-ELT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/20001942g.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low power, analog thermistor temperature sensor, ±4C accuracy, -40C to +125C, in SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "temperature sensor thermistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "MCP9700x-ETT"
		(extends "MCP9700x-HTT")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MCP9700x-ETT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/20001942g.pdf"
			(at -3.81 6.35 0)
		)
		(property "Description" "Low power, analog thermistor temperature sensor, ±4C accuracy, -40C to +125C, in SOT-23-3"
			(at 0 0 0)
		)
		(property "ki_keywords" "temperature sensor thermistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP9700x-HLT"
		(extends "MCP9700Ax-ELT")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MCP9700x-HLT"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/20001942g.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low power, analog thermistor temperature sensor, ±4C accuracy, -40C to +150C, in SC-70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "temperature sensor thermistor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
	)
	(symbol "MCP9802Ax-xOT"
		(extends "MCP9800Ax-xOT")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "MCP9802Ax-xOT"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 17.78 -6.35 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/OTH/ProductDocuments/DataSheets/21909d.pdf"
			(at 0 0 0)
		)
		(property "Description" "2-Wire High-Accuracy Temperature Sensor, Serial Bus time-out 35 ms, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Temperature Sensor Serial Bus time-out"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "MCP9808_DFN"
		(extends "MCP9804_DFN")
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "MCP9808_DFN"
			(at 10.16 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.7x1.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MCP9808-0.5C-Maximum-Accuracy-Digital-Temperature-Sensor-Data-Sheet-DS20005095B.pdf"
			(at -6.35 11.43 0)
		)
		(property "Description" "±0.25°C (±0.5°C) Typical (Maximum), Digital Temperature Sensor, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "temperature sensor I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP9808_MSOP"
		(extends "MCP9804_MSOP")
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "MCP9808_MSOP"
			(at 10.16 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22203b.pdf"
			(at -6.35 11.43 0)
		)
		(property "Description" "±0.25°C (±0.5°C) Typical (Maximum), Digital Temperature Sensor, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "temperature sensor I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PT1000"
		(extends "PT100")
		(property "Reference" "TH"
			(at -4.445 0 90)
		)
		(property "Value" "PT1000"
			(at 3.175 0 90)
		)
		(property "Footprint" ""
			(at 0 1.27 0)
		)
		(property "Datasheet" "https://www.heraeus.com/media/media/group/doc_group/products_1/hst/sot_to/de_15/to_92_d.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "PT1000 platinum temperature sensor (RTD)"
			(at 0 0 0)
		)
		(property "ki_keywords" "platinum temperature sensor RTD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92* PIN?ARRAY* bornier* Terminal?Block* SOD70* R*1206* R*0805*"
			(at 0 0 0)
		)
	)
	(symbol "PT500"
		(extends "PT100")
		(property "Reference" "TH"
			(at -4.445 0 90)
		)
		(property "Value" "PT500"
			(at 3.175 0 90)
		)
		(property "Footprint" ""
			(at 0 1.27 0)
		)
		(property "Datasheet" "https://www.heraeus.com/media/media/group/doc_group/products_1/hst/sot_to/de_15/to_92_d.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "PT500 platinum temperature sensor (RTD)"
			(at 0 0 0)
		)
		(property "ki_keywords" "platinum temperature sensor RTD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92* PIN?ARRAY* bornier* Terminal?Block* SOD70* R*1206* R*0805*"
			(at 0 0 0)
		)
	)
	(symbol "Si7051-A20"
		(extends "Si7050-A20")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "Si7051-A20"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6-1EP_3x3mm_P1mm_EP1.65x2.55mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/Si7050-1-3-4-5-A20.pdf"
			(at -5.08 7.62 0)
		)
		(property "Description" "I2C Temperature Sensor, ±0.1ºC, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Temperature Sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P1mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si7053-A20"
		(extends "Si7050-A20")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "Si7053-A20"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6-1EP_3x3mm_P1mm_EP1.65x2.55mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/Si7050-1-3-4-5-A20.pdf"
			(at -5.08 7.62 0)
		)
		(property "Description" "I2C Temperature Sensor, ±0.3ºC, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Temperature Sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P1mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si7054-A20"
		(extends "Si7050-A20")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "Si7054-A20"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6-1EP_3x3mm_P1mm_EP1.65x2.55mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/Si7050-1-3-4-5-A20.pdf"
			(at -5.08 7.62 0)
		)
		(property "Description" "I2C Temperature Sensor, ±0.4ºC, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Temperature Sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P1mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si7055-A20"
		(extends "Si7050-A20")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "Si7055-A20"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6-1EP_3x3mm_P1mm_EP1.65x2.55mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/Si7050-1-3-4-5-A20.pdf"
			(at -5.08 7.62 0)
		)
		(property "Description" "I2C Temperature Sensor, ±0.5ºC, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Temperature Sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P1mm*"
			(at 0 0 0)
		)
	)
	(symbol "TC1047AxNB"
		(extends "MCP9700x-HTT")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TC1047AxNB"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21498D.pdf"
			(at -3.81 6.35 0)
		)
		(property "Description" "Precision Temperature-to-Voltage Converter, 10mV/ºC, -40ºC to +125ºC, ±2.0ºC (max), 2.5V to 5.5V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "temperature sensor analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TC1047xNB"
		(extends "MCP9700x-HTT")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TC1047xNB"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21498D.pdf"
			(at -3.81 6.35 0)
		)
		(property "Description" "Precision Temperature-to-Voltage Converter, 10mV/ºC, -40ºC to +125ºC, ±2.0ºC (max), 2.7V to 4.4V, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "temperature sensor analog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TMP112xxDRL"
		(extends "TMP102xxDRL")
		(property "Reference" "U"
			(at -2.54 10.795 0)
		)
		(property "Value" "TMP112xxDRL"
			(at -2.54 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-563"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tmp112.pdf"
			(at 1.27 -11.43 0)
		)
		(property "Description" "Digital Temperature Sensor with I2C/SMBus/Two-wire Interface, 12 bits, ±1°C, one-shot conversion, alert, nist traceable, SOT-563"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital temperature sensor i2c smbus two-wire nist"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?563*"
			(at 0 0 0)
		)
	)
	(symbol "TMP116xxDRV"
		(extends "TMP102xxDRL")
		(property "Reference" "U"
			(at -2.54 10.795 0)
		)
		(property "Value" "TMP116xxDRV"
			(at -2.54 8.89 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tmp116.pdf"
			(at 1.27 -11.43 0)
		)
		(property "Description" "Digital Temperature Sensor with I2C/SMBus Interface, 16 bits, ±0.3°C,  one-shot conversion, alert, nist traceable, EEPROM, WSON"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital temperature sensor i2c smbus nist"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP?2x2mm?P0.65mm?EP1x1.6mm*"
			(at 0 0 0)
		)
	)
	(symbol "TMP117xxDRV"
		(extends "TMP102xxDRL")
		(property "Reference" "U"
			(at -2.54 10.795 0)
		)
		(property "Value" "TMP117xxDRV"
			(at -2.54 8.89 0)
		)
		(property "Footprint" "Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tmp117.pdf"
			(at 1.27 -11.43 0)
		)
		(property "Description" "Digital Temperature Sensor with I2C/SMBus Interface, 16 bits, ±0.3°C, one-shot conversion, alert, nist traceable, EEPROM, WSON"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital temperature sensor i2c smbus nist"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WSON*1EP?2x2mm?P0.65mm?EP1x1.6mm*"
			(at 0 0 0)
		)
	)
	(symbol "TMP119AIYBGR"
		(extends "TMP117xxYBG")
		(property "Reference" "U"
			(at -2.54 10.795 0)
		)
		(property "Value" "TMP119AIYBGR"
			(at -2.54 8.89 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-6_0.95x1.488mm_Layout2x3_P0.4mm"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tmp119.pdf"
			(at 1.27 -11.43 0)
		)
		(property "Description" "Ultra-High Accuracy, Low-Power, Digital Temperature Sensor With SMBus and I2C-Compatible Interface, DSBGA-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital temperature sensor i2c smbus"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas?DSBGA?6?0.95x1.488mm?Layout2x3?P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "TSIC306-SO8"
		(extends "TSIC206-SO8")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TSIC306-SO8"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -8.89 3.81 0)
		)
		(property "Datasheet" "https://shop.bb-sensors.com/out/media/Datasheet_Digital_Semiconductor_temperatur_sensor_TSIC.pdf"
			(at 0 0 0)
		)
		(property "Description" "Digital temperature sensor, range -50 ... +150 °C, 0.3 K accuracy, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "temperature digital"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TSIC306-TO92"
		(extends "TSIC206-TO92")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TSIC306-TO92"
			(at 1.27 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at -8.89 3.81 0)
		)
		(property "Datasheet" "https://shop.bb-sensors.com/out/media/Datasheet_Digital_Semiconductor_temperatur_sensor_TSIC.pdf"
			(at 0 0 0)
		)
		(property "Description" "Digital temperature sensor, range -50 ... +150 °C, 0.3 K accuracy, TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "temperature digital"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*"
			(at 0 0 0)
		)
	)
)
