(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "AT42QT1010-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 8.255 0)
		)
		(property "Value" "AT42QT1010-M"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_2x2mm_P0.5mm_EP0.9x1.5mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001946A.pdf"
			(at 6.858 13.97 0)
		)
		(property "Description" "Single-key Touch Sensor, UDFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Touch QTouch Sensor Key"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AT42QT1010-M_0_1")
		(symbol "AT42QT1010-M_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SYNC")
				(number "6")
			)
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "9")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SNSK")
				(number "1")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SNS")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT42QT1010-TSHR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 8.255 0)
		)
		(property "Value" "AT42QT1010-TSHR"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001946A.pdf"
			(at 6.858 13.97 0)
		)
		(property "Description" "Single-key Touch Sensor, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Touch QTouch Sensor Key"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "AT42QT1010-TSHR_0_1")
		(symbol "AT42QT1010-TSHR_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SYNC")
				(number "6")
			)
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SNSK")
				(number "3")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SNS")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT42QT1012-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 8.89 0)
		)
		(property "Value" "AT42QT1012-M"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_2x2mm_P0.5mm_EP0.9x1.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001948A.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Key Touch Sensor IC, UDFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Touch QTouch Sensor Key"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AT42QT1012-M_0_1")
		(symbol "AT42QT1012-M_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "TIME")
				(number "6")
			)
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "OUT")
				(number "5")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "9")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SNSK")
				(number "1")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SNS")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT42QT1012-T"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 8.89 0)
		)
		(property "Value" "AT42QT1012-T"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001948A.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single-Key Touch Sensor IC, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Touch QTouch Sensor Key"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "AT42QT1012-T_0_1")
		(symbol "AT42QT1012-T_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "TIME")
				(number "6")
			)
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SNSK")
				(number "3")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SNS")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT42QT1040-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 19.05 0)
		)
		(property "Value" "AT42QT1040-M"
			(at -2.54 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-20-1EP_3x3mm_P0.45mm_EP1.55x1.55mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-9524-AT42-QTouch-BSW-AT42QT1040_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "Four-key Touch Sensor IC, VQFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Touch QTouch Sensor Key"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.45mm*"
			(at 0 0 0)
		)
		(symbol "AT42QT1040-M_0_1")
		(symbol "AT42QT1040-M_1_1"
			(pin open_collector line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{OUT0}")
				(number "11")
			)
			(pin open_collector line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{OUT1}")
				(number "12")
			)
			(pin open_collector line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "~{OUT2}")
				(number "14")
			)
			(pin open_collector line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "~{OUT3}")
				(number "13")
			)
			(pin no_connect line
				(at -7.62 12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -7.62 10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at -7.62 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at -7.62 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "19")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "9")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "21")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
			(pin passive line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "SNSK0")
				(number "4")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "SNSK1")
				(number "2")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SNSK2")
				(number "20")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SNSK3")
				(number "15")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SNS0")
				(number "5")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "SNS1")
				(number "3")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "SNS2")
				(number "1")
			)
			(pin passive line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "SNS3")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT42QT1050-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 16.51 0)
		)
		(property "Value" "AT42QT1050-M"
			(at -2.54 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-20-1EP_3x3mm_P0.45mm_EP1.55x1.55mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-9707-AT42-QTouch-BSW-AT42QT1050_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "Five-Key Touch Sensor, VQFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Touch QTouch Sensor Key"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.45mm*"
			(at 0 0 0)
		)
		(symbol "AT42QT1050-M_0_1")
		(symbol "AT42QT1050-M_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "SCL")
				(number "15")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SDA")
				(number "12")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{RESET}")
				(number "13")
			)
			(pin open_collector line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{CHANGE}")
				(number "14")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "ADDR_SEL")
				(number "11")
			)
			(pin no_connect line
				(at -7.62 10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -7.62 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at -7.62 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -7.62 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "21")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
			(pin no_connect line
				(at 7.62 10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at 7.62 7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin no_connect line
				(at 7.62 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "19")
			)
			(pin no_connect line
				(at 7.62 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "KEY0")
				(number "4")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "KEY1")
				(number "3")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "KEY2")
				(number "1")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "KEY3")
				(number "17")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "KEY4")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT42QT1050-U"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 16.51 0)
		)
		(property "Value" "AT42QT1050-U"
			(at -2.54 13.97 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-12_1.403x1.555mm_Layout6x4_P0.4mm_Stagger"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-9707-AT42-QTouch-BSW-AT42QT1050_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "Five-Key Touch Sensor, WLCSP-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "Touch QTouch Sensor Key"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*1.403x1.555mm*Layout6x4*P0.4mm*Stagger*"
			(at 0 0 0)
		)
		(symbol "AT42QT1050-U_0_1")
		(symbol "AT42QT1050-U_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "SCL")
				(number "C3")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SDA")
				(number "C5")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{RESET}")
				(number "D4")
			)
			(pin open_collector line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{CHANGE}")
				(number "D2")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "ADDR_SEL")
				(number "D6")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "B6")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "B4")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "KEY0")
				(number "A3")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "KEY1")
				(number "A5")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "KEY2")
				(number "A1")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "KEY3")
				(number "C1")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "KEY4")
				(number "B2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT42QT1060-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 21.59 0)
		)
		(property "Value" "AT42QT1060-M"
			(at -2.54 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-28-1EP_4x4mm_P0.45mm_EP2.4x2.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-9505-AT42-QTouch-BSW-AT42QT1060_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "Six-Key Touch Sensor IC, VQFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Touch QTouch Sensor Key"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*4x4mm*P0.45mm*"
			(at 0 0 0)
		)
		(symbol "AT42QT1060-M_0_1")
		(symbol "AT42QT1060-M_1_1"
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "SDA")
				(number "23")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "SCL")
				(number "24")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{RST}")
				(number "25")
			)
			(pin open_collector line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~{CHG}")
				(number "22")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "IO0")
				(number "19")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IO1")
				(number "20")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "IO2")
				(number "21")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "IO3")
				(number "26")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "IO4")
				(number "27")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "IO5")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "IO6")
				(number "6")
			)
			(pin passive line
				(at 0 20.32 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "16")
			)
			(pin passive line
				(at 0 20.32 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "29")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin passive line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "SNS0")
				(number "10")
			)
			(pin passive line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "SNS1")
				(number "11")
			)
			(pin passive line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "SNS2")
				(number "12")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "SNS3")
				(number "13")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SNS4")
				(number "14")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SNS5")
				(number "15")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SNS0K")
				(number "28")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "SNS1K")
				(number "1")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "SNS2K")
				(number "2")
			)
			(pin passive line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "SNS3K")
				(number "7")
			)
			(pin passive line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "SNS4K")
				(number "8")
			)
			(pin passive line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "SNS5K")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT42QT1070-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 16.51 0)
		)
		(property "Value" "AT42QT1070-M"
			(at -2.54 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-20-1EP_3x3mm_P0.45mm_EP1.55x1.55mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-9596-AT42-QTouch-BSW-AT42QT1070_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "Seven-key Touch Sensor IC, VQFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Touch QTouch Sensor Key"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.45mm*"
			(at 0 0 0)
		)
		(symbol "AT42QT1070-M_0_1")
		(symbol "AT42QT1070-M_1_1"
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "SDA/OUT0")
				(number "12")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "SCL/OUT3")
				(number "15")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "~{RESET}")
				(number "13")
			)
			(pin open_collector line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "~{CHANGE}/OUT4")
				(number "14")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "MODE")
				(number "11")
			)
			(pin no_connect line
				(at -10.16 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -7.62 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at -5.08 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "21")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
			(pin no_connect line
				(at 5.08 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin no_connect line
				(at 7.62 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "19")
			)
			(pin no_connect line
				(at 10.16 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin passive line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "KEY0")
				(number "5")
			)
			(pin passive line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "KEY1")
				(number "4")
			)
			(pin passive line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "KEY2")
				(number "3")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 2.54)
				(name "KEY3")
				(number "2")
			)
			(pin passive line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "KEY4")
				(number "1")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "OUT1/KEY5")
				(number "17")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "OUT2/KEY6")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT42QT1070-S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 16.51 0)
		)
		(property "Value" "AT42QT1070-S"
			(at -2.54 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-9596-AT42-QTouch-BSW-AT42QT1070_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "Seven-key Touch Sensor IC, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Touch QTouch Sensor Key"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AT42QT1070-S_0_1")
		(symbol "AT42QT1070-S_1_1"
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "SDA/OUT0")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "SCL/OUT3")
				(number "6")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "~{RESET}")
				(number "4")
			)
			(pin open_collector line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "~{CHANGE}/OUT4")
				(number "5")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "MODE")
				(number "2")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "14")
			)
			(pin passive line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "KEY0")
				(number "13")
			)
			(pin passive line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "KEY1")
				(number "12")
			)
			(pin passive line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "KEY2")
				(number "11")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 2.54)
				(name "KEY3")
				(number "10")
			)
			(pin passive line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "KEY4")
				(number "9")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "OUT1/KEY5")
				(number "8")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "OUT2/KEY6")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT42QT1110-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 39.37 0)
		)
		(property "Value" "AT42QT1110-M"
			(at -2.54 36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-9520-AT42-QTouch-BSW-AT42QT1110_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "11-Key Touch Sensor IC, VQFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Touch QTouch Sensor Key"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AT42QT1110-M_0_1")
		(symbol "AT42QT1110-M_1_1"
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "MOSI")
				(number "15")
			)
			(pin output line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "MISO")
				(number "16")
			)
			(pin input line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "SCK")
				(number "17")
			)
			(pin input line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "~{SS}")
				(number "14")
			)
			(pin open_collector line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "~{CHANGE}")
				(number "28")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "~{RESET}")
				(number "29")
			)
			(pin passive line
				(at 0 38.1 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "18")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "21")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin passive line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "SNS0K")
				(number "1")
			)
			(pin passive line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "SNS1K")
				(number "3")
			)
			(pin passive line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "SNS2K")
				(number "6")
			)
			(pin passive line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "SNS3K")
				(number "9")
			)
			(pin passive line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "SNS4K")
				(number "11")
			)
			(pin passive line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "SNS5K")
				(number "13")
			)
			(pin passive line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "SNS6K")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "DETECT0/SNS7K")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "DETECT3/SNS8K")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "DETECT5/SNS9K")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "SYNC/SNS10K")
				(number "31")
			)
			(pin passive line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "SNS0")
				(number "32")
			)
			(pin passive line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "SNS1")
				(number "2")
			)
			(pin passive line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "SNS2")
				(number "7")
			)
			(pin passive line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "SNS3")
				(number "8")
			)
			(pin passive line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "SNS4")
				(number "10")
			)
			(pin passive line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "SNS5")
				(number "12")
			)
			(pin passive line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "SNS6")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "DETECT1/SNS7")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "DETECT2/SNS8")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "DETECT4/SNS9")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "DETECT6/SNS10")
				(number "30")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CAP1206-x-AIA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 12.7 0)
		)
		(property "Value" "CAP1206-x-AIA"
			(at 8.89 12.7 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-10-1EP_3x3mm_P0.5mm_EP1.55x2.48mm"
			(at 0 24.13 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/00001567B.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "6-Channel Capacitive Touch Sensor, DFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "6 Channel Capacitive Touch Sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "CAP1206-x-AIA_0_1")
		(symbol "CAP1206-x-AIA_1_1"
			(pin passive line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "CS1")
				(number "1")
			)
			(pin passive line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "CS2")
				(number "10")
			)
			(pin passive line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "CS3")
				(number "9")
			)
			(pin passive line
				(at -15.24 0 0)
				(length 3.81)
				(name "CS4")
				(number "8")
			)
			(pin passive line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "CS5")
				(number "7")
			)
			(pin passive line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "CS6")
				(number "6")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 3.81)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 3.81)
				(name "GND")
				(number "11")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "SMCLK")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "SMDATA")
				(number "3")
			)
			(pin open_collector line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "ALERT#")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CAP1206-x-SL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 12.7 0)
		)
		(property "Value" "CAP1206-x-SL"
			(at 8.89 12.7 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 24.13 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/00001567B.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "6-Channel Capacitive Touch Sensor, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "6 Channel Capacitive Touch Sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC?14*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "CAP1206-x-SL_0_1")
		(symbol "CAP1206-x-SL_1_1"
			(pin passive line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "CS1")
				(number "2")
			)
			(pin passive line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "CS2")
				(number "13")
			)
			(pin passive line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "CS3")
				(number "12")
			)
			(pin passive line
				(at -15.24 0 0)
				(length 3.81)
				(name "CS4")
				(number "11")
			)
			(pin passive line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "CS5")
				(number "10")
			)
			(pin passive line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "CS6")
				(number "9")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 3.81)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 3.81)
				(name "GND")
				(number "8")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "SMCLK")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "SMDATA")
				(number "4")
			)
			(pin open_collector line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "ALERT#")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CY8CMBR3002"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "CY8CMBR3002"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.cypress.com/?docID=49119"
			(at 0 0 0)
		)
		(property "Description" "CapSense Controller, 2 Sensors, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Touch Sensor 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "CY8CMBR3002_0_1")
		(symbol "CY8CMBR3002_1_1"
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "CS0")
				(number "7")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CS1")
				(number "6")
			)
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "GPO0")
				(number "8")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "GPO1")
				(number "1")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "CMOD")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CY8CMBR3102"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "CY8CMBR3102"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.cypress.com/?docID=49119"
			(at 0 0 0)
		)
		(property "Description" "CapSense Controller, 2 Sensors, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Touch Sensor 2ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "CY8CMBR3102_0_1")
		(symbol "CY8CMBR3102_1_1"
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "CS0")
				(number "7")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CS1")
				(number "6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "SDA")
				(number "8")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SCL")
				(number "1")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "CMOD")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CY8CMBR3106S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 24.13 0)
		)
		(property "Value" "CY8CMBR3106S"
			(at 1.27 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 -30.48 0)
		)
		(property "Datasheet" "http://www.cypress.com/?docID=49119"
			(at 0 0 0)
		)
		(property "Description" "CapSense Controller, 16 Sensors w/ Slider, QFN-24+EP"
			(at 0 0 0)
		)
		(property "ki_keywords" "Touch Sensor 16ch Slider"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "CY8CMBR3106S_0_1")
		(symbol "CY8CMBR3106S_1_1"
			(pin passive line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "CS0")
				(number "1")
			)
			(pin passive line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "CS1")
				(number "2")
			)
			(pin passive line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "CS2")
				(number "3")
			)
			(pin passive line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "CS3")
				(number "4")
			)
			(pin passive line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "CS4")
				(number "20")
			)
			(pin passive line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "CS5")
				(number "19")
			)
			(pin passive line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "CS11")
				(number "14")
			)
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "CS12")
				(number "15")
			)
			(pin passive line
				(at -12.7 0 0)
				(length 2.54)
				(name "CS13")
				(number "16")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "CS14")
				(number "17")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "CS15")
				(number "18")
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "SLD10")
				(number "9")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "SLD11")
				(number "10")
			)
			(pin passive line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "SLD12")
				(number "11")
			)
			(pin passive line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "SLD13")
				(number "12")
			)
			(pin passive line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "SLD14")
				(number "13")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
			(pin passive line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "EP")
				(number "25")
			)
			(pin passive line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "VCC")
				(number "6")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "SDA")
				(number "21")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "SCL")
				(number "22")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "~{XRES}")
				(number "24")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "~{HI}")
				(number "23")
			)
			(pin passive line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "CMOD")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CY8CMBR3108"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 13.97 0)
		)
		(property "Value" "CY8CMBR3108"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP1.8x1.8mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "http://www.cypress.com/?docID=49119"
			(at 0 0 0)
		)
		(property "Description" "CapSense Controller, 8 Sensors, QFN-16+EP"
			(at 0 0 0)
		)
		(property "ki_keywords" "Touch Sensor 8ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "CY8CMBR3108_0_1")
		(symbol "CY8CMBR3108_1_1"
			(pin passive line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "CS0")
				(number "1")
			)
			(pin passive line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "CS1")
				(number "2")
			)
			(pin passive line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "CS2")
				(number "12")
			)
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "CS3")
				(number "13")
			)
			(pin passive line
				(at -12.7 0 0)
				(length 2.54)
				(name "CS4")
				(number "8")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "CS5")
				(number "9")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "CS6")
				(number "10")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "CS7")
				(number "11")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDDIO")
				(number "5")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(name "EP")
				(number "17")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "SDA")
				(number "14")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SCL")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "~{HI}")
				(number "16")
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "CMOD")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CY8CMBR3110"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "CY8CMBR3110"
			(at 1.27 16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://www.cypress.com/?docID=49119"
			(at 0 0 0)
		)
		(property "Description" "CapSense Controller, 10 Sensors, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Touch Sensor 10ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "CY8CMBR3110_0_1")
		(symbol "CY8CMBR3110_1_1"
			(pin passive line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "CS0")
				(number "3")
			)
			(pin passive line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "CS1")
				(number "4")
			)
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "CS2")
				(number "13")
			)
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "CS3")
				(number "15")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CS4")
				(number "16")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "CS5")
				(number "9")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "CS6")
				(number "10")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "CS7")
				(number "11")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "CS8")
				(number "12")
			)
			(pin passive line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "CS9")
				(number "14")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
			(pin passive line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "VCC")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "SDA")
				(number "1")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SCL")
				(number "2")
			)
			(pin passive line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "CMOD")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CY8CMBR3116"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 24.13 0)
		)
		(property "Value" "CY8CMBR3116"
			(at 1.27 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 -29.21 0)
		)
		(property "Datasheet" "http://www.cypress.com/?docID=49119"
			(at 0 0 0)
		)
		(property "Description" "CapSense Controller, 16 Sensors, QFN-24+EP"
			(at 0 0 0)
		)
		(property "ki_keywords" "Touch Sensor 16ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "CY8CMBR3116_0_1")
		(symbol "CY8CMBR3116_1_1"
			(pin passive line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "CS0")
				(number "1")
			)
			(pin passive line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "CS1")
				(number "2")
			)
			(pin passive line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "CS2")
				(number "3")
			)
			(pin passive line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "CS3")
				(number "4")
			)
			(pin passive line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "CS4")
				(number "20")
			)
			(pin passive line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "CS5")
				(number "19")
			)
			(pin passive line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "CS6")
				(number "18")
			)
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "CS7")
				(number "17")
			)
			(pin passive line
				(at -12.7 0 0)
				(length 2.54)
				(name "CS8")
				(number "16")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "CS9")
				(number "15")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "CS10")
				(number "14")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "CS11")
				(number "13")
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "CS12")
				(number "12")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "CS13")
				(number "11")
			)
			(pin passive line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "CS14")
				(number "10")
			)
			(pin passive line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "CS15")
				(number "9")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
			(pin passive line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "EP")
				(number "25")
			)
			(pin passive line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "VCC")
				(number "6")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "SDA")
				(number "21")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "SCL")
				(number "22")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "~{XRES}")
				(number "24")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "~{HI}")
				(number "23")
			)
			(pin passive line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "CMOD")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MPR121QR2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 19.05 0)
		)
		(property "Value" "MPR121QR2"
			(at 6.35 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:UQFN-20_3x3mm_P0.4mm"
			(at 0 -19.05 0)
		)
		(property "Datasheet" "https://resurgentsemi.com/wp-content/uploads/2018/09/MPR121_rev5-Resurgent.pdf?d453f8&d453f8"
			(at -11.43 -7.62 0)
		)
		(property "Description" "12ch Touch Sensor controller, UQFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Touch Sensor 12ch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UQFN*3x3mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "MPR121QR2_0_1")
		(symbol "MPR121QR2_1_1"
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "SDA")
				(number "3")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "SCL")
				(number "2")
			)
			(pin open_collector line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "~{IRQ}")
				(number "1")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "ADDR")
				(number "4")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "REXT")
				(number "7")
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "VREG")
				(number "5")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "6")
			)
			(pin passive line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "ELE0")
				(number "8")
			)
			(pin passive line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "ELE1")
				(number "9")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "ELE2")
				(number "10")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "ELE3")
				(number "11")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "LED0/ELE4")
				(number "12")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "LED1/ELE5")
				(number "13")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(name "LED2/ELE6")
				(number "14")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "LED3/ELE7")
				(number "15")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "LED4/ELE8")
				(number "16")
			)
			(pin passive line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "LED5/ELE9")
				(number "17")
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "LED6/ELE10")
				(number "18")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "LED7/ELE11")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCA8886"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 -8.89 0)
		)
		(property "Value" "PCA8886"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at -2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/PCA8886.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "Dual capacitive touch/proximity switch with auto-calibration, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP capacitive touch sensor auto-calibration"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PCA8886_0_1")
		(symbol "PCA8886_1_1"
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "IN1")
				(number "1")
			)
			(pin power_out line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VDD(int)1")
				(number "16")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD1")
				(number "13")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS1")
				(number "4")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "TYPE1")
				(number "2")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUT1")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CPC1")
				(number "3")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "CLIN1")
				(number "15")
			)
		)
		(symbol "PCA8886_2_1"
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "IN2")
				(number "5")
			)
			(pin power_out line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VDD(int)2")
				(number "12")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD2")
				(number "9")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS2")
				(number "8")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "TYPE2")
				(number "6")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUT2")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CPC2")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "CLIN2")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCF8883"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 -8.89 0)
		)
		(property "Value" "PCF8883"
			(at 1.27 8.89 0)
		)
		(property "Footprint" ""
			(at -2.54 -8.89 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/PCF8883.pdf"
			(at 0 -3.81 0)
		)
		(property "Description" "Capacitive touch/proximity switch with auto-calibration, SOIC-8/WLCSP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP capacitive touch sensor auto-calibration"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* NXP*WLCSP*PCF8883*"
			(at 0 0 0)
		)
		(symbol "PCF8883_0_1")
		(symbol "PCF8883_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin power_out line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VDD(int)")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "TYPE")
				(number "2")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "CPC")
				(number "3")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "CLIN")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT42QT1011-M"
		(extends "AT42QT1010-M")
		(property "Reference" "U"
			(at -2.54 8.255 0)
		)
		(property "Value" "AT42QT1011-M"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_2x2mm_P0.5mm_EP0.9x1.5mm"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001947A.pdf"
			(at 6.858 13.97 0)
		)
		(property "Description" "Single-key Touch Sensor, UDFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Touch QTouch Sensor Key"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "AT42QT1011-TSHR"
		(extends "AT42QT1010-TSHR")
		(property "Reference" "U"
			(at -2.54 8.255 0)
		)
		(property "Value" "AT42QT1011-TSHR"
			(at -2.54 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001947A.pdf"
			(at 6.858 13.97 0)
		)
		(property "Description" "Single-key Touch Sensor, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Touch QTouch Sensor Key"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
)
