(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "0"
		(power)
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "#GND"
			(at 0 -5.08 0)
		)
		(property "Value" "0"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#subsec_Circuit_elements__device"
			(at 0 -10.16 0)
		)
		(property "Description" "0V reference potential for simulation"
			(at 0 -7.62 0)
		)
		(property "ki_keywords" "simulation"
			(at 0 0 0)
		)
		(symbol "0_0_1")
		(symbol "0_1_1"
			(pin power_in line
				(at 0 0 0)
				(length 0)
				(name "~")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BSOURCE"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "B"
			(at 2.54 2.54 0)
		)
		(property "Value" "BSOURCE"
			(at 2.54 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#sec_Non_linear_Dependent_Sources"
			(at 0 -16.51 0)
		)
		(property "Description" "Arbitrary behavioral voltage or current source for simulation only"
			(at 0 0 0)
		)
		(property "Sim.Device" "SPICE"
			(at 0 0 0)
		)
		(property "Sim.Params" "type=\"B\" model=\"v=1\""
			(at 2.54 -2.54 0)
		)
		(property "ki_keywords" "simulation dependent"
			(at 0 0 0)
		)
		(symbol "BSOURCE_0_1")
		(symbol "BSOURCE_1_1"
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "N+")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "N-")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "D"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "D"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#cha_DIODEs"
			(at 0 0 0)
		)
		(property "Description" "Diode for simulation or PCB"
			(at 0 0 0)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
		)
		(property "Sim.Params" "rs=50m cjo=10p"
			(at 0 0 0)
		)
		(property "ki_keywords" "simulation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO-???* *_Diode_* *SingleDiode* D_*"
			(at 0 0 0)
		)
		(symbol "D_0_1")
		(symbol "D_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ESOURCE"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "E"
			(at 2.54 2.54 0)
		)
		(property "Value" "ESOURCE"
			(at 2.54 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#subsec_Exxxx__Linear_Voltage_Controlled"
			(at 0 16.51 0)
		)
		(property "Description" "Voltage-controlled voltage source symbol for simulation only"
			(at 0 0 0)
		)
		(property "Sim.Device" "SPICE"
			(at 0 0 0)
		)
		(property "Sim.Params" "type=\"E\" model=\"1\""
			(at 2.54 -2.54 0)
		)
		(property "ki_keywords" "simulation vcvs dependent"
			(at 0 0 0)
		)
		(symbol "ESOURCE_0_1")
		(symbol "ESOURCE_1_1"
			(text "V"
				(at -5.08 0 0)
			)
			(pin input line
				(at -5.08 5.08 270)
				(length 2.54)
				(name "C+")
				(number "3")
			)
			(pin input line
				(at -5.08 -5.08 90)
				(length 2.54)
				(name "C-")
				(number "4")
			)
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "N+")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "N-")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "GSOURCE"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "G"
			(at 2.54 2.54 0)
		)
		(property "Value" "GSOURCE"
			(at 2.54 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#subsec_Gxxxx__Linear_Voltage_Controlled"
			(at 0 19.05 0)
		)
		(property "Description" "Voltage-controlled current source symbol for simulation only"
			(at 0 0 0)
		)
		(property "Sim.Device" "SPICE"
			(at 0 0 0)
		)
		(property "Sim.Params" "type=\"G\" model=\"1\""
			(at 2.54 -2.54 0)
		)
		(property "ki_keywords" "simulation vccs dependent"
			(at 0 0 0)
		)
		(symbol "GSOURCE_0_1")
		(symbol "GSOURCE_1_1"
			(text "V"
				(at -5.08 0 0)
			)
			(pin input line
				(at -5.08 5.08 270)
				(length 2.54)
				(name "C+")
				(number "3")
			)
			(pin input line
				(at -5.08 -5.08 90)
				(length 2.54)
				(name "C-")
				(number "4")
			)
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "N+")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "N-")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IAM"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "I"
			(at 2.54 2.54 0)
		)
		(property "Value" "IAM"
			(at 2.54 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#sec_Independent_Sources_for"
			(at 0 0 0)
		)
		(property "Description" "Current source, AM"
			(at 0 0 0)
		)
		(property "Sim.Pins" "1=1 2=2"
			(at 0 0 0)
		)
		(property "Sim.Device" "SPICE"
			(at 0 0 0)
		)
		(property "Sim.Params" "type=\"I\" model=\"am(1 0 1k 100k 1n)\" lib=\"\""
			(at 2.54 -2.54 0)
		)
		(property "ki_keywords" "simulation amplitude modulated"
			(at 0 0 0)
		)
		(symbol "IAM_0_0")
		(symbol "IAM_0_1")
		(symbol "IAM_1_1"
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IBIS_DEVICE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U?"
			(at 6.35 0.635 0)
		)
		(property "Value" "IBIS_DEVICE"
			(at 6.35 -1.905 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://ibis.org"
			(at 1.27 6.35 0)
		)
		(property "Description" "Device model for IBIS files. Pin 3 can be used to monitor the die potential"
			(at 0 0 0)
		)
		(property "Ibis_Pin" ""
			(at 0 0 0)
		)
		(property "Ibis_Model" ""
			(at 0 0 0)
		)
		(property "Sim.Device" "IBIS"
			(at 0 0 0)
		)
		(property "Sim.Type" "IBISDEVICE"
			(at 0 0 0)
		)
		(property "Sim.Pins" "1=1 2=2"
			(at 0 0 0)
		)
		(property "ki_keywords" "Simulation IBIS"
			(at 0 0 0)
		)
		(symbol "IBIS_DEVICE_0_1")
		(symbol "IBIS_DEVICE_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "")
				(number "2")
			)
			(pin power_in line
				(at 0 -5.08 90)
				(length 2.54)
				(name "REF")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IBIS_DEVICE_DIFF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U?"
			(at 6.35 0.635 0)
		)
		(property "Value" "IBIS_DEVICE_DIFF"
			(at 6.35 -1.905 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://ibis.org"
			(at 1.27 6.35 0)
		)
		(property "Description" "Device model for IBIS files. Pin 3 can be used to monitor the die potential"
			(at 0 0 0)
		)
		(property "Sim_Name" ""
			(at 0 0 0)
		)
		(property "Sim_Library" ""
			(at 0 0 0)
		)
		(property "Ibis_Pin" ""
			(at 0 0 0)
		)
		(property "Sim.Device" "IBIS"
			(at 0 0 0)
		)
		(property "Sim.Type" "IBISDRIVERDC"
			(at 0 0 0)
		)
		(property "Sim.Pins" "1=1 2=2 3=3"
			(at 0 0 0)
		)
		(property "Ibis_Diff" "1"
			(at 0 0 0)
		)
		(property "ki_keywords" "Simulation IBIS"
			(at 0 0 0)
		)
		(symbol "IBIS_DEVICE_DIFF_0_1")
		(symbol "IBIS_DEVICE_DIFF_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "3")
			)
			(pin power_in line
				(at 0 -5.08 90)
				(length 2.54)
				(name "REF")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IBIS_DRIVER"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U?"
			(at 0 8.89 0)
		)
		(property "Value" "IBIS_DRIVER"
			(at 0 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://ibis.org"
			(at 0 6.35 0)
		)
		(property "Description" "Driver model for IBIS files."
			(at 0 0 0)
		)
		(property "Sim_Name" ""
			(at 0 0 0)
		)
		(property "Sim_Library" ""
			(at 0 0 0)
		)
		(property "Ibis_Pin" ""
			(at 0 0 0)
		)
		(property "Ibis_Model" ""
			(at 0 0 0)
		)
		(property "Sim.Device" "IBIS"
			(at 0 0 0)
		)
		(property "Sim.Type" "IBISDRIVERDC"
			(at 0 0 0)
		)
		(property "Sim.Pins" "1=1 2=2"
			(at 0 0 0)
		)
		(property "ki_keywords" "Simulation IBIS"
			(at 0 0 0)
		)
		(symbol "IBIS_DRIVER_0_1")
		(symbol "IBIS_DRIVER_1_1"
			(pin power_in line
				(at 0 -5.08 90)
				(length 2.54)
				(name "REF")
				(number "1")
			)
			(pin bidirectional line
				(at 7.62 0 180)
				(length 2.54)
				(name "")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IBIS_DRIVER_DIFF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U?"
			(at 0 8.89 0)
		)
		(property "Value" "IBIS_DRIVER_DIFF"
			(at 0 6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://ibis.org"
			(at 0 6.35 0)
		)
		(property "Description" "Driver model for IBIS files. Pin 3 can be used to monitor the die potential."
			(at 0 0 0)
		)
		(property "Sim_Name" ""
			(at 0 0 0)
		)
		(property "Sim_Library" ""
			(at 0 0 0)
		)
		(property "Ibis_Pin" ""
			(at 0 0 0)
		)
		(property "Ibis_Model" ""
			(at 0 0 0)
		)
		(property "Ibis_Diff" "1"
			(at 0 0 0)
		)
		(property "Sim.Device" "IBIS"
			(at 0 0 0)
		)
		(property "Sim.Type" "IBISDRIVERDC"
			(at 0 0 0)
		)
		(property "Sim.Pins" "1=1 2=2 3=3"
			(at 0 0 0)
		)
		(property "ki_keywords" "Simulation IBIS"
			(at 0 0 0)
		)
		(symbol "IBIS_DRIVER_DIFF_0_1")
		(symbol "IBIS_DRIVER_DIFF_1_1"
			(pin power_in line
				(at 0 -5.08 90)
				(length 2.54)
				(name "REF")
				(number "1")
			)
			(pin bidirectional line
				(at 7.62 2.54 180)
				(length 3.81)
				(name "+")
				(number "2")
			)
			(pin bidirectional line
				(at 7.62 -2.54 180)
				(length 3.81)
				(name "-")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IDC"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "I"
			(at 2.54 2.54 0)
		)
		(property "Value" "1"
			(at 2.54 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#sec_Independent_Sources_for"
			(at 0 0 0)
		)
		(property "Description" "Current source, DC"
			(at 0 0 0)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 0)
		)
		(property "Sim.Type" "DC"
			(at 0 0 0)
		)
		(property "Sim.Device" "I"
			(at 0 0 0)
		)
		(property "ki_keywords" "simulation"
			(at 0 0 0)
		)
		(symbol "IDC_0_0")
		(symbol "IDC_0_1")
		(symbol "IDC_1_1"
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IEXP"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "I"
			(at 2.54 2.54 0)
		)
		(property "Value" "IEXP"
			(at 2.54 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#sec_Independent_Sources_for"
			(at 0 0 0)
		)
		(property "Description" "Current source, exponential"
			(at 0 0 0)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 0)
		)
		(property "Sim.Type" "EXP"
			(at 0 0 0)
		)
		(property "Sim.Device" "I"
			(at 0 0 0)
		)
		(property "Sim.Params" "y1=0 y2=1 td1=2n tau1=30n td2=60n tau2=40n"
			(at 2.54 -2.54 0)
		)
		(property "ki_keywords" "simulation"
			(at 0 0 0)
		)
		(symbol "IEXP_0_0")
		(symbol "IEXP_0_1")
		(symbol "IEXP_1_1"
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IPULSE"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "I"
			(at 2.54 2.54 0)
		)
		(property "Value" "IPULSE"
			(at 2.54 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#sec_Independent_Sources_for"
			(at 0 0 0)
		)
		(property "Description" "Current source, pulse"
			(at 0 0 0)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 0)
		)
		(property "Sim.Device" "I"
			(at 0 0 0)
		)
		(property "Sim.Type" "PULSE"
			(at 0 0 0)
		)
		(property "Sim.Params" "y1=0 y2=1 td=2n tr=2n tf=2n tw=50n per=100n"
			(at 2.54 -2.54 0)
		)
		(property "ki_keywords" "simulation"
			(at 0 0 0)
		)
		(symbol "IPULSE_0_0")
		(symbol "IPULSE_0_1")
		(symbol "IPULSE_1_1"
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IPWL"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "I"
			(at 2.54 2.54 0)
		)
		(property "Value" "IPWL"
			(at 2.54 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#sec_Independent_Sources_for"
			(at 0 0 0)
		)
		(property "Description" "Current source, piece-wise linear"
			(at 0 0 0)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 0)
		)
		(property "Sim.Device" "I"
			(at 0 0 0)
		)
		(property "Sim.Params" "pwl=\"0 -1 50n -1 51n 0 97n 1 171n -1 200n -1\""
			(at 2.54 -2.54 0)
		)
		(property "Sim.Type" "PWL"
			(at 0 0 0)
		)
		(property "ki_keywords" "simulation"
			(at 0 0 0)
		)
		(symbol "IPWL_0_0")
		(symbol "IPWL_0_1")
		(symbol "IPWL_1_1"
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISFFM"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "I"
			(at 2.54 2.54 0)
		)
		(property "Value" "ISFFM"
			(at 2.54 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#sec_Independent_Sources_for"
			(at 0 0 0)
		)
		(property "Description" "Current source, single-frequency FM"
			(at 0 0 0)
		)
		(property "Sim.Pins" "1=1 2=2"
			(at 0 0 0)
		)
		(property "Sim.Device" "SPICE"
			(at 0 0 0)
		)
		(property "Sim.Params" "type=\"I\" model=\"sffm(0 1 100k 5 1k)\" lib=\"\""
			(at 2.54 -2.54 0)
		)
		(property "ki_keywords" "simulation frequency modulated"
			(at 0 0 0)
		)
		(symbol "ISFFM_0_1")
		(symbol "ISFFM_1_1"
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISIN"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "I"
			(at 2.54 2.54 0)
		)
		(property "Value" "ISIN"
			(at 2.54 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#sec_Independent_Sources_for"
			(at 0 0 0)
		)
		(property "Description" "Current source, sinusoidal"
			(at 0 0 0)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 0)
		)
		(property "Sim.Params" "dc=0 ampl=1 f=1k ac=1"
			(at 2.54 -2.54 0)
		)
		(property "Sim.Device" "I"
			(at 0 0 0)
		)
		(property "Sim.Type" "SIN"
			(at 0 0 0)
		)
		(property "ki_keywords" "simulation"
			(at 0 0 0)
		)
		(symbol "ISIN_0_0")
		(symbol "ISIN_0_1")
		(symbol "ISIN_1_1"
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ITRNOISE"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "I"
			(at 2.54 2.54 0)
		)
		(property "Value" "ITRNOISE"
			(at 2.54 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#subsec_Transient_noise_source"
			(at 0 0 0)
		)
		(property "Description" "Current source, transient noise"
			(at 0 0 0)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 0)
		)
		(property "Sim.Device" "I"
			(at 0 0 0)
		)
		(property "Sim.Params" "rms=20n dt=500p ac=0 ph=0"
			(at 2.54 -2.54 0)
		)
		(property "Sim.Type" "WHITENOISE"
			(at 0 0 0)
		)
		(property "ki_keywords" "simulation"
			(at 0 0 0)
		)
		(symbol "ITRNOISE_0_1")
		(symbol "ITRNOISE_1_1"
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ITRRANDOM"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "I"
			(at 2.54 2.54 0)
		)
		(property "Value" "ITRRANDOM"
			(at 2.54 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#subsec_Random_voltage_source"
			(at 0 0 0)
		)
		(property "Description" "Current source, random noise"
			(at 0 0 0)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 0)
		)
		(property "Sim.Device" "I"
			(at 0 0 0)
		)
		(property "Sim.Params" "ts=1u td=0 range=1 offset=0"
			(at 2.54 -2.54 0)
		)
		(property "Sim.Type" "RANDUNIFORM"
			(at 0 0 0)
		)
		(property "ki_keywords" "simulation"
			(at 0 0 0)
		)
		(symbol "ITRRANDOM_0_1")
		(symbol "ITRRANDOM_1_1"
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NJFET"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "NJFET"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#cha_JFETs"
			(at 0 0 0)
		)
		(property "Description" "N-JFET transistor, for simulation only"
			(at 0 0 0)
		)
		(property "Sim.Device" "NJFET"
			(at 0 0 0)
		)
		(property "Sim.Type" "SHICHMANHODGES"
			(at 0 0 0)
		)
		(property "Sim.Pins" "1=D 2=G 3=S"
			(at 0 0 0)
		)
		(property "ki_keywords" "transistor NJFET N-JFET"
			(at 0 0 0)
		)
		(symbol "NJFET_0_1")
		(symbol "NJFET_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 5.334)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NMOS"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "NMOS"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#cha_MOSFETs"
			(at 0 -12.7 0)
		)
		(property "Description" "N-MOSFET transistor, drain/source/gate"
			(at 0 0 0)
		)
		(property "Sim.Device" "NMOS"
			(at 0 -17.145 0)
		)
		(property "Sim.Type" "VDMOS"
			(at 0 -19.05 0)
		)
		(property "Sim.Pins" "1=D 2=G 3=S"
			(at 0 -15.24 0)
		)
		(property "ki_keywords" "transistor NMOS N-MOS N-MOSFET simulation"
			(at 0 0 0)
		)
		(symbol "NMOS_0_1")
		(symbol "NMOS_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NMOS_Substrate"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 6.985 1.27 0)
		)
		(property "Value" "NMOS_Substrate"
			(at 6.985 -1.27 0)
		)
		(property "Footprint" ""
			(at 29.845 0 0)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#cha_MOSFETs"
			(at 0 -19.05 0)
		)
		(property "Description" "N-channel MOSFET symbol with substrate (bulk) pin"
			(at 0 0 0)
		)
		(property "Sim.Device" "NMOS"
			(at 0 -16.51 0)
		)
		(property "Sim.Type" "MOS1"
			(at 0 -14.605 0)
		)
		(property "Sim.Pins" "1=D 2=G 3=S 4=B"
			(at 0 -12.7 0)
		)
		(property "ki_keywords" "mosfet nmos simulation"
			(at 0 0 0)
		)
		(symbol "NMOS_Substrate_0_1")
		(symbol "NMOS_Substrate_1_1"
			(pin input line
				(at -3.81 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
			(pin input line
				(at 5.08 -5.08 90)
				(length 2.54)
				(name "Bulk")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NPN"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at -2.54 7.62 0)
		)
		(property "Value" "NPN"
			(at -2.54 5.08 0)
		)
		(property "Footprint" ""
			(at 63.5 0 0)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#cha_BJTs"
			(at 63.5 0 0)
		)
		(property "Description" "Bipolar transistor symbol for simulation only, substrate tied to the emitter"
			(at 0 0 0)
		)
		(property "Sim.Device" "NPN"
			(at 0 0 0)
		)
		(property "Sim.Type" "GUMMELPOON"
			(at 0 0 0)
		)
		(property "Sim.Pins" "1=C 2=B 3=E"
			(at 0 0 0)
		)
		(property "ki_keywords" "simulation"
			(at 0 0 0)
		)
		(symbol "NPN_0_1")
		(symbol "NPN_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "2")
			)
			(pin open_collector line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "1")
			)
			(pin open_emitter line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NPN_Substrate"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 4.445 4.445 0)
		)
		(property "Value" "NPN_Substrate"
			(at 4.445 1.905 0)
		)
		(property "Footprint" ""
			(at 63.5 0 0)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#cha_BJTs"
			(at 63.5 0 0)
		)
		(property "Description" "Bipolar transistor symbol for simulation only, with substrate pin"
			(at 0 0 0)
		)
		(property "Sim.Device" "NPN"
			(at 0 0 0)
		)
		(property "Sim.Type" "GUMMELPOON"
			(at 0 0 0)
		)
		(property "Sim.Pins" "1=C 2=B 3=E"
			(at 0 0 0)
		)
		(property "ki_keywords" "simulation"
			(at 0 0 0)
		)
		(symbol "NPN_Substrate_0_1")
		(symbol "NPN_Substrate_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "2")
			)
			(pin open_collector line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "1")
			)
			(pin open_emitter line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "Substrate")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "OPAMP"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 3.175 0)
		)
		(property "Value" "${SIM.PARAMS}"
			(at 3.81 -3.175 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#sec__SUBCKT_Subcircuits"
			(at 0 0 0)
		)
		(property "Description" "Operational amplifier, single"
			(at 0 0 0)
		)
		(property "Sim.Pins" "1=in+ 2=in- 3=vcc 4=vee 5=out"
			(at 0 0 0)
		)
		(property "Sim.Device" "SUBCKT"
			(at 0 0 0)
		)
		(property "Sim.Library" "${KICAD8_SYMBOL_DIR}/Simulation_SPICE.sp"
			(at 0 0 0)
		)
		(property "Sim.Name" "kicad_builtin_opamp"
			(at 0 0 0)
		)
		(property "ki_keywords" "simulation"
			(at 0 0 0)
		)
		(symbol "OPAMP_0_1")
		(symbol "OPAMP_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "V+")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "V-")
				(number "4")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PJFET"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "PJFET"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#cha_JFETs"
			(at 0 0 0)
		)
		(property "Description" "P-JFET transistor, for simulation only"
			(at 0 0 0)
		)
		(property "Sim.Device" "PJFET"
			(at 0 0 0)
		)
		(property "Sim.Type" "SHICHMANHODGES"
			(at 0 0 0)
		)
		(property "Sim.Pins" "1=D 2=G 3=S"
			(at 0 0 0)
		)
		(property "ki_keywords" "transistor PJFET P-JFET"
			(at 0 0 0)
		)
		(symbol "PJFET_0_1")
		(symbol "PJFET_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 5.334)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PMOS"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.27 0)
		)
		(property "Value" "PMOS"
			(at 5.08 -1.27 0)
		)
		(property "Footprint" ""
			(at 5.08 2.54 0)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#cha_MOSFETs"
			(at 0 -12.7 0)
		)
		(property "Description" "P-MOSFET transistor, drain/source/gate"
			(at 0 0 0)
		)
		(property "Sim.Device" "PMOS"
			(at 0 -17.145 0)
		)
		(property "Sim.Type" "VDMOS"
			(at 0 -19.05 0)
		)
		(property "Sim.Pins" "1=D 2=G 3=S"
			(at 0 -15.24 0)
		)
		(property "ki_keywords" "transistor PMOS P-MOS P-MOSFET simulation"
			(at 0 0 0)
		)
		(symbol "PMOS_0_1")
		(symbol "PMOS_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PMOS_Substrate"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 6.35 1.27 0)
		)
		(property "Value" "PMOS_Substrate"
			(at 6.35 -1.27 0)
		)
		(property "Footprint" ""
			(at 40.64 0 0)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#cha_MOSFETs"
			(at 0 -17.78 0)
		)
		(property "Description" "P-channel MOSFET symbol with substrate (bulk) pin"
			(at 0 0 0)
		)
		(property "Sim.Device" "PMOS"
			(at 0 -13.97 0)
		)
		(property "Sim.Type" "MOS1"
			(at 0 -15.875 0)
		)
		(property "Sim.Pins" "1=D 2=G 3=S 4=B"
			(at 0 -12.065 0)
		)
		(property "ki_keywords" "mosfet pmos simulation"
			(at 0 0 0)
		)
		(symbol "PMOS_Substrate_0_1")
		(symbol "PMOS_Substrate_1_1"
			(pin input line
				(at -3.81 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin passive line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "S")
				(number "3")
			)
			(pin input line
				(at 5.08 -5.08 90)
				(length 2.54)
				(name "Bulk")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PNP"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at -2.54 7.62 0)
		)
		(property "Value" "PNP"
			(at -2.54 5.08 0)
		)
		(property "Footprint" ""
			(at 35.56 0 0)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#cha_BJTs"
			(at 35.56 0 0)
		)
		(property "Description" "Bipolar transistor symbol for simulation only, substrate tied to the emitter"
			(at 0 0 0)
		)
		(property "Sim.Device" "PNP"
			(at 0 0 0)
		)
		(property "Sim.Type" "GUMMELPOON"
			(at 0 0 0)
		)
		(property "Sim.Pins" "1=C 2=B 3=E"
			(at 0 0 0)
		)
		(property "ki_keywords" "simulation"
			(at 0 0 0)
		)
		(symbol "PNP_0_1")
		(symbol "PNP_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "2")
			)
			(pin open_collector line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "1")
			)
			(pin open_emitter line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PNP_Substrate"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 4.445 4.445 0)
		)
		(property "Value" "PNP_Substrate"
			(at 4.445 2.54 0)
		)
		(property "Footprint" ""
			(at 35.56 0 0)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#cha_BJTs"
			(at 35.56 0 0)
		)
		(property "Description" "Bipolar transistor symbol for simulation only, with substrate pin"
			(at 0 0 0)
		)
		(property "Sim.Device" "PNP"
			(at 0 0 0)
		)
		(property "Sim.Type" "GUMMELPOON"
			(at 0 0 0)
		)
		(property "Sim.Pins" "1=C 2=B 3=E"
			(at 0 0 0)
		)
		(property "ki_keywords" "simulation"
			(at 0 0 0)
		)
		(symbol "PNP_Substrate_0_1")
		(symbol "PNP_Substrate_1_1"
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "2")
			)
			(pin open_collector line
				(at 2.54 5.08 270)
				(length 2.54)
				(name "C")
				(number "1")
			)
			(pin open_emitter line
				(at 2.54 -5.08 90)
				(length 2.54)
				(name "E")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "Substrate")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SWITCH"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "S"
			(at 2.54 2.54 0)
		)
		(property "Value" "SWITCH"
			(at 2.54 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#subsec_Switches"
			(at 0 16.51 0)
		)
		(property "Description" "Voltage controlled switch symbol for simulation only"
			(at 0 0 0)
		)
		(property "Sim.Device" "SW"
			(at 0 0 0)
		)
		(property "Sim.Type" "V"
			(at 0 0 0)
		)
		(property "Sim.Params" "thr=0 ron=1"
			(at 2.54 -2.54 0)
		)
		(property "Sim.Pins" "1=no+ 2=no- 3=ctrl+ 4=ctrl-"
			(at 0 13.97 0)
		)
		(property "ki_keywords" "simulation"
			(at 0 0 0)
		)
		(symbol "SWITCH_0_1")
		(symbol "SWITCH_1_1"
			(text "V"
				(at -5.08 0 0)
			)
			(pin input line
				(at -5.08 5.08 270)
				(length 2.54)
				(name "C+")
				(number "3")
			)
			(pin input line
				(at -5.08 -5.08 90)
				(length 2.54)
				(name "C-")
				(number "4")
			)
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "N+")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "N-")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLINE"
		(pin_numbers
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom no)
		(on_board no)
		(property "Reference" "T"
			(at 0 7.62 0)
		)
		(property "Value" "TLINE"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#sec_Lossless_Transmission_Lines"
			(at 0 5.08 0)
		)
		(property "Description" "Lossless transmission line, for simulation only"
			(at 0 0 0)
		)
		(property "Sim.Device" "TLINE"
			(at 0 0 0)
		)
		(property "Sim.Pins" "1=1+ 2=1- 3=2+ 4=2-"
			(at 0 0 0)
		)
		(property "Sim.Params" "z0=50 td=10n"
			(at 0 2.54 0)
		)
		(property "ki_keywords" "lossless transmission line characteristic impedance"
			(at 0 0 0)
		)
		(symbol "TLINE_0_1")
		(symbol "TLINE_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "")
				(number "1")
			)
			(pin passive line
				(at -5.08 -2.54 90)
				(length 1.27)
				(name "")
				(number "2")
			)
			(pin passive line
				(at 5.08 -2.54 90)
				(length 1.27)
				(name "")
				(number "4")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VAM"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "V"
			(at 2.54 2.54 0)
		)
		(property "Value" "VAM"
			(at 2.54 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#sec_Independent_Sources_for"
			(at 0 0 0)
		)
		(property "Description" "Voltage source, AM"
			(at 0 0 0)
		)
		(property "Sim.Pins" "1=1 2=2"
			(at 0 0 0)
		)
		(property "Sim.Device" "SPICE"
			(at 0 0 0)
		)
		(property "Sim.Params" "type=\"V\" model=\"am(1 0 1k 100k 1n)\" lib=\"\""
			(at 2.54 -2.54 0)
		)
		(property "ki_keywords" "simulation amplitude modulated"
			(at 0 0 0)
		)
		(symbol "VAM_0_0"
			(text "+"
				(at 0 1.905 0)
			)
		)
		(symbol "VAM_0_1")
		(symbol "VAM_1_1"
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VDC"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "V"
			(at 2.54 2.54 0)
		)
		(property "Value" "1"
			(at 2.54 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#sec_Independent_Sources_for"
			(at 0 0 0)
		)
		(property "Description" "Voltage source, DC"
			(at 0 0 0)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 0)
		)
		(property "Sim.Type" "DC"
			(at 0 0 0)
		)
		(property "Sim.Device" "V"
			(at 0 0 0)
		)
		(property "ki_keywords" "simulation"
			(at 0 0 0)
		)
		(symbol "VDC_0_0"
			(text "+"
				(at 0 1.905 0)
			)
		)
		(symbol "VDC_0_1")
		(symbol "VDC_1_1"
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VEXP"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "V"
			(at 2.54 2.54 0)
		)
		(property "Value" "VEXP"
			(at 2.54 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#sec_Independent_Sources_for"
			(at 0 0 0)
		)
		(property "Description" "Voltage source, exponential"
			(at 0 0 0)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 0)
		)
		(property "Sim.Type" "EXP"
			(at 0 0 0)
		)
		(property "Sim.Device" "V"
			(at 0 0 0)
		)
		(property "Sim.Params" "y1=0 y2=1 td1=2n tau1=30n td2=60n tau2=40n"
			(at 2.54 -2.54 0)
		)
		(property "ki_keywords" "simulation"
			(at 0 0 0)
		)
		(symbol "VEXP_0_0"
			(text "+"
				(at 0 1.905 0)
			)
		)
		(symbol "VEXP_0_1")
		(symbol "VEXP_1_1"
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VOLTMETER_DIFF"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.0254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom no)
		(on_board no)
		(property "Reference" "MES?"
			(at -10.16 0 0)
		)
		(property "Value" "VOLTMETER_DIFF"
			(at -19.05 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 2.54 90)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#sec__SUBCKT_Subcircuits"
			(at 0 2.54 90)
		)
		(property "Description" "Differential voltmeter for simulation. The sensed differential voltage can be measured on the third terminal as a single-ended voltage"
			(at 0 0 0)
		)
		(property "Sim.Name" "kicad_builtin_vdiff"
			(at 0 0 0)
		)
		(property "Sim.Device" "SUBCKT"
			(at 0 0 0)
		)
		(property "Sim.Pins" "1=1 2=2 3=3"
			(at 0 0 0)
		)
		(property "Sim.Params" ""
			(at 0 0 0)
		)
		(property "Sim.Library" "${KICAD8_SYMBOL_DIR}/Simulation_SPICE.sp"
			(at 0 0 0)
		)
		(property "ki_keywords" "voltmeter differential vdiff"
			(at 0 0 0)
		)
		(symbol "VOLTMETER_DIFF_0_0"
			(text "V"
				(at 0 0 0)
			)
		)
		(symbol "VOLTMETER_DIFF_0_1")
		(symbol "VOLTMETER_DIFF_1_1"
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "+")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "-")
				(number "2")
			)
			(pin output line
				(at 5.08 0 180)
				(length 2.54)
				(name "out")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VPULSE"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "V"
			(at 2.54 2.54 0)
		)
		(property "Value" "VPULSE"
			(at 2.54 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#sec_Independent_Sources_for"
			(at 0 0 0)
		)
		(property "Description" "Voltage source, pulse"
			(at 0 0 0)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 0)
		)
		(property "Sim.Type" "PULSE"
			(at 0 0 0)
		)
		(property "Sim.Device" "V"
			(at 0 0 0)
		)
		(property "Sim.Params" "y1=0 y2=1 td=2n tr=2n tf=2n tw=50n per=100n"
			(at 2.54 -2.54 0)
		)
		(property "ki_keywords" "simulation"
			(at 0 0 0)
		)
		(symbol "VPULSE_0_0"
			(text "+"
				(at 0 1.905 0)
			)
		)
		(symbol "VPULSE_0_1")
		(symbol "VPULSE_1_1"
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VPWL"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "V"
			(at 2.54 2.54 0)
		)
		(property "Value" "VPWL"
			(at 2.54 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#sec_Independent_Sources_for"
			(at 0 0 0)
		)
		(property "Description" "Voltage source, piece-wise linear"
			(at 0 0 0)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 0)
		)
		(property "Sim.Device" "V"
			(at 0 0 0)
		)
		(property "Sim.Params" "pwl=\"0 -1 50n -1 51n 0 97n 1 171n -1 200n -1\""
			(at 2.54 -2.54 0)
		)
		(property "Sim.Type" "PWL"
			(at 0 0 0)
		)
		(property "ki_keywords" "simulation"
			(at 0 0 0)
		)
		(symbol "VPWL_0_0"
			(text "+"
				(at 0 1.905 0)
			)
		)
		(symbol "VPWL_0_1")
		(symbol "VPWL_1_1"
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VSFFM"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "V"
			(at 2.54 2.54 0)
		)
		(property "Value" "VSFFM"
			(at 2.54 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#sec_Independent_Sources_for"
			(at 0 0 0)
		)
		(property "Description" "Voltage source, single-frequency FM"
			(at 0 0 0)
		)
		(property "Sim.Pins" "1=1 2=2"
			(at 0 0 0)
		)
		(property "Sim.Device" "SPICE"
			(at 0 0 0)
		)
		(property "Sim.Params" "type=\"V\" model=\"sffm(0 1 100k 5 1k)\" lib=\"\""
			(at 2.54 -2.54 0)
		)
		(property "ki_keywords" "simulation frequency modulated"
			(at 0 0 0)
		)
		(symbol "VSFFM_0_0"
			(text "+"
				(at 0 1.905 0)
			)
		)
		(symbol "VSFFM_0_1")
		(symbol "VSFFM_1_1"
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VSIN"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "V"
			(at 2.54 2.54 0)
		)
		(property "Value" "VSIN"
			(at 2.54 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#sec_Independent_Sources_for"
			(at 0 0 0)
		)
		(property "Description" "Voltage source, sinusoidal"
			(at 0 0 0)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 0)
		)
		(property "Sim.Params" "dc=0 ampl=1 f=1k ac=1"
			(at 2.54 -2.54 0)
		)
		(property "Sim.Type" "SIN"
			(at 0 0 0)
		)
		(property "Sim.Device" "V"
			(at 0 0 0)
		)
		(property "ki_keywords" "simulation ac vac"
			(at 0 0 0)
		)
		(symbol "VSIN_0_0"
			(text "+"
				(at 0 1.905 0)
			)
		)
		(symbol "VSIN_0_1")
		(symbol "VSIN_1_1"
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VTRNOISE"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "V"
			(at 2.54 2.54 0)
		)
		(property "Value" "VTRNOISE"
			(at 2.54 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#subsec_Transient_noise_source"
			(at 0 0 0)
		)
		(property "Description" "Voltage source, transient noise"
			(at 0 0 0)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 0)
		)
		(property "Sim.Params" "rms=20n dt=500p ac=0 ph=0"
			(at 2.54 -2.54 0)
		)
		(property "Sim.Device" "V"
			(at 0 0 0)
		)
		(property "Sim.Type" "WHITENOISE"
			(at 0 0 0)
		)
		(property "ki_keywords" "simulation"
			(at 0 0 0)
		)
		(symbol "VTRNOISE_0_0"
			(text "+"
				(at 0 1.905 0)
			)
		)
		(symbol "VTRNOISE_0_1")
		(symbol "VTRNOISE_1_1"
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VTRRANDOM"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "V"
			(at 2.54 2.54 0)
		)
		(property "Value" "VTRRANDOM"
			(at 2.54 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#subsec_Random_voltage_source"
			(at 0 0 0)
		)
		(property "Description" "Voltage source, random noise"
			(at 0 0 0)
		)
		(property "Sim.Pins" "1=+ 2=-"
			(at 0 0 0)
		)
		(property "Sim.Params" "ts=1u td=0 range=1 offset=0"
			(at 2.54 -2.54 0)
		)
		(property "Sim.Type" "RANDUNIFORM"
			(at 0 0 0)
		)
		(property "Sim.Device" "V"
			(at 0 0 0)
		)
		(property "ki_keywords" "simulation"
			(at 0 0 0)
		)
		(symbol "VTRRANDOM_0_0"
			(text "+"
				(at 0 1.905 0)
			)
		)
		(symbol "VTRRANDOM_0_1")
		(symbol "VTRRANDOM_1_1"
			(pin passive line
				(at 0 5.08 270)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
)
