(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "SW_Coded"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 7.62 0)
		)
		(property "Value" "SW_Coded"
			(at 0 -7.62 0)
		)
		(property "Footprint" ""
			(at -1.016 0 0)
		)
		(property "Datasheet" "~"
			(at 0 -10.16 0)
		)
		(property "Description" "Rotary switch, 4-bit encoding"
			(at 0 0 0)
		)
		(property "ki_keywords" "rotary hex"
			(at 0 0 0)
		)
		(symbol "SW_Coded_0_1")
		(symbol "SW_Coded_1_1"
			(pin passive line
				(at 10.16 5.08 180)
				(length 3.81)
				(name "CM")
				(number "1")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 3.81)
				(name "D0")
				(number "2")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 3.81)
				(name "D1")
				(number "3")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 3.81)
				(name "D2")
				(number "4")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 3.81)
				(name "D3")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_Coded_SH-7010"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at -7.62 8.89 0)
		)
		(property "Value" "SW_Coded_SH-7010"
			(at -7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at -7.62 -11.43 0)
		)
		(property "Datasheet" "https://www.nidec-copal-electronics.com/e/catalog/switch/sh-7000.pdf"
			(at 0 0 0)
		)
		(property "Description" "Rotary switch, 4-bit encoding, 10 positions, Real code"
			(at 0 0 0)
		)
		(property "ki_keywords" "rotary bcd Real"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nidec*Copal*SH*7010*"
			(at 0 0 0)
		)
		(symbol "SW_Coded_SH-7010_0_0"
			(text "5"
				(at -5.715 0 900)
			)
			(text "6"
				(at -4.6228 3.3528 540)
			)
			(text "4"
				(at -4.6228 -3.3528 1260)
			)
			(text "7"
				(at -1.778 5.4356 180)
			)
			(text "3"
				(at -1.778 -5.4356 1620)
			)
			(text "8"
				(at 1.778 5.4356 3420)
			)
			(text "2"
				(at 1.778 -5.4356 1980)
			)
			(text "9"
				(at 4.6228 3.3528 3060)
			)
			(text "1"
				(at 4.6228 -3.3528 2340)
			)
			(text "0"
				(at 5.715 0 2700)
			)
		)
		(symbol "SW_Coded_SH-7010_0_1")
		(symbol "SW_Coded_SH-7010_1_1"
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "C")
				(number "C")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "8")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_Coded_SH-7040"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at -7.62 8.89 0)
		)
		(property "Value" "SW_Coded_SH-7040"
			(at -7.62 -8.89 0)
		)
		(property "Footprint" "Button_Switch_SMD:Nidec_Copal_SH-7040B"
			(at -7.62 -11.43 0)
		)
		(property "Datasheet" "https://www.nidec-copal-electronics.com/e/catalog/switch/sh-7000.pdf"
			(at 0 0 0)
		)
		(property "Description" "Rotary switch, 4-bit encoding, 10 positions, Gray code"
			(at 0 0 0)
		)
		(property "ki_keywords" "rotary bcd Gray"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nidec*Copal*SH*7040*"
			(at 0 0 0)
		)
		(symbol "SW_Coded_SH-7040_0_0"
			(text "5"
				(at -5.715 0 900)
			)
			(text "6"
				(at -4.6228 3.3528 540)
			)
			(text "4"
				(at -4.6228 -3.3528 1260)
			)
			(text "7"
				(at -1.778 5.4356 180)
			)
			(text "3"
				(at -1.778 -5.4356 1620)
			)
			(text "8"
				(at 1.778 5.4356 3420)
			)
			(text "2"
				(at 1.778 -5.4356 1980)
			)
			(text "9"
				(at 4.6228 3.3528 3060)
			)
			(text "1"
				(at 4.6228 -3.3528 2340)
			)
			(text "0"
				(at 5.715 0 2700)
			)
		)
		(symbol "SW_Coded_SH-7040_0_1")
		(symbol "SW_Coded_SH-7040_1_1"
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "C")
				(number "C")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "8")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_Coded_SH-7050"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at -7.62 8.89 0)
		)
		(property "Value" "SW_Coded_SH-7050"
			(at -7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at -7.62 -11.43 0)
		)
		(property "Datasheet" "https://www.nidec-copal-electronics.com/e/catalog/switch/sh-7000.pdf"
			(at 0 0 0)
		)
		(property "Description" "Rotary switch, 4-bit encoding, 16 positions, Real code"
			(at 0 0 0)
		)
		(property "ki_keywords" "rotary hex Real"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nidec*Copal*SH*7010*"
			(at 0 0 0)
		)
		(symbol "SW_Coded_SH-7050_0_0"
			(text "8"
				(at -5.715 0 900)
			)
			(text "9"
				(at -5.2832 2.1844 675)
			)
			(text "7"
				(at -5.2832 -2.1844 1125)
			)
			(text "A"
				(at -4.0386 4.0386 450)
			)
			(text "6"
				(at -4.0386 -4.0386 1350)
			)
			(text "B"
				(at -2.1844 5.2832 225)
			)
			(text "5"
				(at -2.1844 -5.2832 1575)
			)
			(text "C"
				(at 0 5.715 0)
			)
			(text "4"
				(at 0 -5.715 1800)
			)
			(text "D"
				(at 2.1844 5.2832 3375)
			)
			(text "3"
				(at 2.1844 -5.2832 2025)
			)
			(text "E"
				(at 4.0386 4.0386 3150)
			)
			(text "2"
				(at 4.0386 -4.0386 2250)
			)
			(text "F"
				(at 5.2832 2.1844 2925)
			)
			(text "1"
				(at 5.2832 -2.1844 2475)
			)
			(text "0"
				(at 5.715 0 2700)
			)
		)
		(symbol "SW_Coded_SH-7050_0_1")
		(symbol "SW_Coded_SH-7050_1_1"
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "C")
				(number "C")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "8")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_Coded_SH-7080"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at -7.62 8.89 0)
		)
		(property "Value" "SW_Coded_SH-7080"
			(at -7.62 -8.89 0)
		)
		(property "Footprint" "Button_Switch_SMD:Nidec_Copal_SH-7040B"
			(at -7.62 -11.43 0)
		)
		(property "Datasheet" "https://www.nidec-copal-electronics.com/e/catalog/switch/sh-7000.pdf"
			(at 0 0 0)
		)
		(property "Description" "Rotary switch, 4-bit encoding, 16 positions, Gray code"
			(at 0 0 0)
		)
		(property "ki_keywords" "rotary hex Gray"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nidec*Copal*SH*7040*"
			(at 0 0 0)
		)
		(symbol "SW_Coded_SH-7080_0_0"
			(text "8"
				(at -5.715 0 900)
			)
			(text "9"
				(at -5.2832 2.1844 675)
			)
			(text "7"
				(at -5.2832 -2.1844 1125)
			)
			(text "A"
				(at -4.0386 4.0386 450)
			)
			(text "6"
				(at -4.0386 -4.0386 1350)
			)
			(text "B"
				(at -2.1844 5.2832 225)
			)
			(text "5"
				(at -2.1844 -5.2832 1575)
			)
			(text "C"
				(at 0 5.715 0)
			)
			(text "4"
				(at 0 -5.715 1800)
			)
			(text "D"
				(at 2.1844 5.2832 3375)
			)
			(text "3"
				(at 2.1844 -5.2832 2025)
			)
			(text "E"
				(at 4.0386 4.0386 3150)
			)
			(text "2"
				(at 4.0386 -4.0386 2250)
			)
			(text "F"
				(at 5.2832 2.1844 2925)
			)
			(text "1"
				(at 5.2832 -2.1844 2475)
			)
			(text "0"
				(at 5.715 0 2700)
			)
		)
		(symbol "SW_Coded_SH-7080_0_1")
		(symbol "SW_Coded_SH-7080_1_1"
			(pin passive line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "C")
				(number "C")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "8")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_DIP_x01"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 3.81 0)
		)
		(property "Value" "SW_DIP_x01"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "1x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol"
			(at 0 0 0)
		)
		(property "ki_keywords" "dip switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SW?DIP?x1*"
			(at 0 0 0)
		)
		(symbol "SW_DIP_x01_0_0")
		(symbol "SW_DIP_x01_0_1")
		(symbol "SW_DIP_x01_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 5.08)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 5.08)
				(name "~")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_DIP_x02"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 6.35 0)
		)
		(property "Value" "SW_DIP_x02"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "2x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol"
			(at 0 0 0)
		)
		(property "ki_keywords" "dip switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SW?DIP?x2*"
			(at 0 0 0)
		)
		(symbol "SW_DIP_x02_0_0")
		(symbol "SW_DIP_x02_0_1")
		(symbol "SW_DIP_x02_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 5.08)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 5.08)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 5.08)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 5.08)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_DIP_x03"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 6.35 0)
		)
		(property "Value" "SW_DIP_x03"
			(at 0 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 -2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 -2.54 0)
		)
		(property "Description" "3x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol"
			(at 0 0 0)
		)
		(property "ki_keywords" "dip switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SW?DIP?x3*"
			(at 0 0 0)
		)
		(symbol "SW_DIP_x03_0_0")
		(symbol "SW_DIP_x03_0_1")
		(symbol "SW_DIP_x03_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 5.08)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 5.08)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 5.08)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 5.08)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 5.08)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 5.08)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_DIP_x04"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 8.89 0)
		)
		(property "Value" "SW_DIP_x04"
			(at 0 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "4x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol"
			(at 0 0 0)
		)
		(property "ki_keywords" "dip switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SW?DIP?x4*"
			(at 0 0 0)
		)
		(symbol "SW_DIP_x04_0_0")
		(symbol "SW_DIP_x04_0_1")
		(symbol "SW_DIP_x04_1_1"
			(pin passive line
				(at -7.62 5.08 0)
				(length 5.08)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 5.08)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 5.08)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 5.08)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 5.08)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 5.08)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 5.08)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 5.08)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_DIP_x05"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 8.89 0)
		)
		(property "Value" "SW_DIP_x05"
			(at 0 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "5x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol"
			(at 0 0 0)
		)
		(property "ki_keywords" "dip switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SW?DIP?x5*"
			(at 0 0 0)
		)
		(symbol "SW_DIP_x05_0_0")
		(symbol "SW_DIP_x05_0_1")
		(symbol "SW_DIP_x05_1_1"
			(pin passive line
				(at -7.62 5.08 0)
				(length 5.08)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 5.08)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 5.08)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 5.08)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 5.08)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 5.08)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 5.08)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 5.08)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 5.08)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 5.08)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_DIP_x06"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 11.43 0)
		)
		(property "Value" "SW_DIP_x06"
			(at 0 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "6x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol"
			(at 0 0 0)
		)
		(property "ki_keywords" "dip switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SW?DIP?x6*"
			(at 0 0 0)
		)
		(symbol "SW_DIP_x06_0_0")
		(symbol "SW_DIP_x06_0_1")
		(symbol "SW_DIP_x06_1_1"
			(pin passive line
				(at -7.62 7.62 0)
				(length 5.08)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 5.08)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 5.08)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 5.08)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 5.08)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 5.08)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 5.08)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 5.08)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 5.08)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 5.08)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 5.08)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 5.08)
				(name "~")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_DIP_x07"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 11.43 0)
		)
		(property "Value" "SW_DIP_x07"
			(at 0 -11.43 0)
		)
		(property "Footprint" ""
			(at 0 -2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 -2.54 0)
		)
		(property "Description" "7x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol"
			(at 0 0 0)
		)
		(property "ki_keywords" "dip switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SW?DIP?x7*"
			(at 0 0 0)
		)
		(symbol "SW_DIP_x07_0_0")
		(symbol "SW_DIP_x07_0_1")
		(symbol "SW_DIP_x07_1_1"
			(pin passive line
				(at -7.62 7.62 0)
				(length 5.08)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 5.08)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 5.08)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 5.08)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 5.08)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 5.08)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 5.08)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 5.08)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 5.08)
				(name "~")
				(number "13")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 5.08)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 5.08)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 5.08)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 5.08)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 5.08)
				(name "~")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_DIP_x08"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 13.97 0)
		)
		(property "Value" "SW_DIP_x08"
			(at 0 -11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "8x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol"
			(at 0 0 0)
		)
		(property "ki_keywords" "dip switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SW?DIP?x8*"
			(at 0 0 0)
		)
		(symbol "SW_DIP_x08_0_0")
		(symbol "SW_DIP_x08_0_1")
		(symbol "SW_DIP_x08_1_1"
			(pin passive line
				(at -7.62 10.16 0)
				(length 5.08)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 7.62 0)
				(length 5.08)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 5.08)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 5.08)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 5.08)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 5.08)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 5.08)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 5.08)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 5.08)
				(name "~")
				(number "16")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 5.08)
				(name "~")
				(number "15")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 5.08)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 5.08)
				(name "~")
				(number "13")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 5.08)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 5.08)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 5.08)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 5.08)
				(name "~")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_DIP_x09"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 13.97 0)
		)
		(property "Value" "SW_DIP_x09"
			(at 0 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "9x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol"
			(at 0 0 0)
		)
		(property "ki_keywords" "dip switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SW?DIP?x9*"
			(at 0 0 0)
		)
		(symbol "SW_DIP_x09_0_0")
		(symbol "SW_DIP_x09_0_1")
		(symbol "SW_DIP_x09_1_1"
			(pin passive line
				(at -7.62 10.16 0)
				(length 5.08)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 7.62 0)
				(length 5.08)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 5.08)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 5.08)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 5.08)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 5.08)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 5.08)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 5.08)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at -7.62 -10.16 0)
				(length 5.08)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 5.08)
				(name "~")
				(number "18")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 5.08)
				(name "~")
				(number "17")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 5.08)
				(name "~")
				(number "16")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 5.08)
				(name "~")
				(number "15")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 5.08)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 5.08)
				(name "~")
				(number "13")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 5.08)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 5.08)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 5.08)
				(name "~")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_DIP_x10"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 16.51 0)
		)
		(property "Value" "SW_DIP_x10"
			(at 0 -13.97 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "10x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol"
			(at 0 0 0)
		)
		(property "ki_keywords" "dip switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SW?DIP?x10*"
			(at 0 0 0)
		)
		(symbol "SW_DIP_x10_0_0")
		(symbol "SW_DIP_x10_0_1")
		(symbol "SW_DIP_x10_1_1"
			(pin passive line
				(at -7.62 12.7 0)
				(length 5.08)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 10.16 0)
				(length 5.08)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -7.62 7.62 0)
				(length 5.08)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 5.08)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 5.08)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 5.08)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 5.08)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 5.08)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 5.08)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at -7.62 -10.16 0)
				(length 5.08)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 5.08)
				(name "~")
				(number "20")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 5.08)
				(name "~")
				(number "19")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 5.08)
				(name "~")
				(number "18")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 5.08)
				(name "~")
				(number "17")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 5.08)
				(name "~")
				(number "16")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 5.08)
				(name "~")
				(number "15")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 5.08)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 5.08)
				(name "~")
				(number "13")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 5.08)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 5.08)
				(name "~")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_DIP_x11"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 16.51 0)
		)
		(property "Value" "SW_DIP_x11"
			(at 0 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 -2.54 0)
		)
		(property "Datasheet" "~"
			(at 0 -2.54 0)
		)
		(property "Description" "11x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol"
			(at 0 0 0)
		)
		(property "ki_keywords" "dip switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SW?DIP?x11*"
			(at 0 0 0)
		)
		(symbol "SW_DIP_x11_0_0")
		(symbol "SW_DIP_x11_0_1")
		(symbol "SW_DIP_x11_1_1"
			(pin passive line
				(at -7.62 12.7 0)
				(length 5.08)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 10.16 0)
				(length 5.08)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -7.62 7.62 0)
				(length 5.08)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 5.08)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 5.08)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 5.08)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 5.08)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 5.08)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 5.08)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at -7.62 -10.16 0)
				(length 5.08)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at -7.62 -12.7 0)
				(length 5.08)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 5.08)
				(name "~")
				(number "22")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 5.08)
				(name "~")
				(number "21")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 5.08)
				(name "~")
				(number "20")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 5.08)
				(name "~")
				(number "19")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 5.08)
				(name "~")
				(number "18")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 5.08)
				(name "~")
				(number "17")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 5.08)
				(name "~")
				(number "16")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 5.08)
				(name "~")
				(number "15")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 5.08)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 5.08)
				(name "~")
				(number "13")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 5.08)
				(name "~")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_DIP_x12"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 19.05 0)
		)
		(property "Value" "SW_DIP_x12"
			(at 0 -16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "12x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol"
			(at 0 0 0)
		)
		(property "ki_keywords" "dip switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SW?DIP?x12*"
			(at 0 0 0)
		)
		(symbol "SW_DIP_x12_0_0")
		(symbol "SW_DIP_x12_1_1"
			(pin passive line
				(at -7.62 15.24 0)
				(length 5.08)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 12.7 0)
				(length 5.08)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -7.62 10.16 0)
				(length 5.08)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -7.62 7.62 0)
				(length 5.08)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 5.08)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 5.08)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 5.08)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 5.08)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 5.08)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 5.08)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at -7.62 -10.16 0)
				(length 5.08)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at -7.62 -12.7 0)
				(length 5.08)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 7.62 15.24 180)
				(length 5.08)
				(name "~")
				(number "24")
			)
			(pin passive line
				(at 7.62 12.7 180)
				(length 5.08)
				(name "~")
				(number "23")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 5.08)
				(name "~")
				(number "22")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 5.08)
				(name "~")
				(number "21")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 5.08)
				(name "~")
				(number "20")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 5.08)
				(name "~")
				(number "19")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 5.08)
				(name "~")
				(number "18")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 5.08)
				(name "~")
				(number "17")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 5.08)
				(name "~")
				(number "16")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 5.08)
				(name "~")
				(number "15")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 5.08)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 -12.7 180)
				(length 5.08)
				(name "~")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_DP3T"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 5.08 0)
		)
		(property "Value" "SW_DP3T"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at -15.875 4.445 0)
		)
		(property "Datasheet" "~"
			(at -15.875 4.445 0)
		)
		(property "Description" "Switch, three position, dual pole triple throw, 3 position switch, SP3T"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch dp3t ON-ON-ON"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SW* DP3T*"
			(at 0 0 0)
		)
		(symbol "SW_DP3T_0_1")
		(symbol "SW_DP3T_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "4")
				(number "4")
			)
		)
		(symbol "SW_DP3T_2_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "7")
				(number "7")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "5")
				(number "5")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "6")
				(number "6")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "8")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_DPDT_x2"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 5.08 0)
		)
		(property "Value" "SW_DPDT_x2"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Switch, dual pole double throw, separate symbols"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch dual-pole double-throw DPDT spdt ON-ON"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SW*DPDT*"
			(at 0 0 0)
		)
		(symbol "SW_DPDT_x2_0_0")
		(symbol "SW_DPDT_x2_0_1")
		(symbol "SW_DPDT_x2_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "2")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "C")
				(number "3")
			)
		)
		(symbol "SW_DPDT_x2_2_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "5")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "A")
				(number "4")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "C")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_DPST"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 6.35 0)
		)
		(property "Value" "SW_DPST"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Double Pole Single Throw (DPST) Switch"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch dual double-pole single-throw OFF-ON"
			(at 0 0 0)
		)
		(symbol "SW_DPST_0_0")
		(symbol "SW_DPST_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_DPST_Temperature"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 7.62 0)
		)
		(property "Value" "SW_DPST_Temperature"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Double Pole Single Throw (DPST) Switch, temperature dependent"
			(at 0 0 0)
		)
		(property "ki_keywords" "temperature switch dual double-pole single-throw OFF-ON"
			(at 0 0 0)
		)
		(symbol "SW_DPST_Temperature_0_0")
		(symbol "SW_DPST_Temperature_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_DPST_x2"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 3.175 0)
		)
		(property "Value" "SW_DPST_x2"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Single Pole Single Throw (SPST) switch, separate symbol"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch lever"
			(at 0 0 0)
		)
		(symbol "SW_DPST_x2_0_0")
		(symbol "SW_DPST_x2_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "B")
				(number "2")
			)
		)
		(symbol "SW_DPST_x2_2_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "B")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_E3_SA3216"
		(pin_names
			(offset 0.0254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 1.27 8.89 0)
		)
		(property "Value" "SW_E3_SA3216"
			(at 7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 2.54 0)
		)
		(property "Datasheet" "http://www.e3-keys.com/files/SA%20Technical%20Datasheet%20v2.0.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Push button switch with LCD screen"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch normally-open pushbutton push-button LCD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SW?PUSH?LCD?E3?SAxxxx*"
			(at 0 0 0)
		)
		(symbol "SW_E3_SA3216_0_0"
			(text "LCD"
				(at 0 2.54 0)
			)
		)
		(symbol "SW_E3_SA3216_0_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "CLK")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "DAT")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "5V")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
		)
		(symbol "SW_E3_SA3216_1_1"
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SW1")
				(number "5")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SW2")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_MEC_5E"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0.635 5.715 0)
		)
		(property "Value" "SW_MEC_5E"
			(at 0 -3.175 0)
		)
		(property "Footprint" ""
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://www.apem.com/int/index.php?controller=attachment&id_attachment=1371"
			(at 0 7.62 0)
		)
		(property "Description" "MEC 5E single pole normally-open tactile switch"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch normally-open pushbutton push-button"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SW*MEC*5G*"
			(at 0 0 0)
		)
		(symbol "SW_MEC_5E_0_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "A")
				(number "4")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_MEC_5G"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 1.27 2.54 0)
		)
		(property "Value" "SW_MEC_5G"
			(at 0 -1.524 0)
		)
		(property "Footprint" ""
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.apem.com/int/index.php?controller=attachment&id_attachment=488"
			(at 0 5.08 0)
		)
		(property "Description" "MEC 5G single pole normally-open tactile switch"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch normally-open pushbutton push-button"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SW*MEC*5G*"
			(at 0 0 0)
		)
		(symbol "SW_MEC_5G_0_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "B")
				(number "3")
			)
		)
		(symbol "SW_MEC_5G_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "A")
				(number "2")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "B")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_MEC_5G_2LED"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 10.16 0)
		)
		(property "Value" "SW_MEC_5G_2LED"
			(at 0 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 10.16 0)
		)
		(property "Datasheet" "http://www.apem.com/int/index.php?controller=attachment&id_attachment=488"
			(at 1.27 -11.43 0)
		)
		(property "Description" "MEC 5G single pole normally-open illuminated tactile switch with two LEDs"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch normally-open pushbutton push-button LED"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SW*MEC*5G*"
			(at 0 0 0)
		)
		(symbol "SW_MEC_5G_2LED_0_0")
		(symbol "SW_MEC_5G_2LED_0_1"
			(pin passive line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "A")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "K")
				(number "3")
			)
		)
		(symbol "SW_MEC_5G_2LED_1_1")
		(embedded_fonts no)
	)
	(symbol "SW_MEC_5G_LED"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 7.62 0)
		)
		(property "Value" "SW_MEC_5G_LED"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://www.apem.com/int/index.php?controller=attachment&id_attachment=488"
			(at 0 -6.35 0)
		)
		(property "Description" "MEC 5G single pole normally-open illuminated tactile switch"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch normally-open pushbutton push-button LED"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SW*MEC*5G*"
			(at 0 0 0)
		)
		(symbol "SW_MEC_5G_LED_0_0")
		(symbol "SW_MEC_5G_LED_0_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "A")
				(number "4")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "3")
			)
		)
		(symbol "SW_MEC_5G_LED_1_1")
		(embedded_fonts no)
	)
	(symbol "SW_NKK_GW12LJPCF"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 10.16 0)
		)
		(property "Value" "SW_NKK_GW12LJPCF"
			(at 0 -10.16 0)
		)
		(property "Footprint" "Button_Switch_THT:SW_NKK_GW12LJP"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.nkkswitches.com/pdf/gwillum.pdf"
			(at 0 -15.24 0)
		)
		(property "Description" "Switch, single pole double throw, illuminated paddle, red and green LEDs"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch single-pole double-throw spdt ON-ON illuminated red green"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SW*NKK*GW12LJP*"
			(at 0 0 0)
		)
		(symbol "SW_NKK_GW12LJPCF_0_0"
			(text "RED"
				(at 0.889 -2.159 0)
			)
			(text "GREEN"
				(at 1.143 -7.239 0)
			)
		)
		(symbol "SW_NKK_GW12LJPCF_0_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "KR")
				(number "4")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "KG")
				(number "6")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "A")
				(number "5")
			)
		)
		(symbol "SW_NKK_GW12LJPCF_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "B")
				(number "2")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "C")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_Push"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 1.27 2.54 0)
		)
		(property "Value" "SW_Push"
			(at 0 -1.524 0)
		)
		(property "Footprint" ""
			(at 0 5.08 0)
		)
		(property "Datasheet" "~"
			(at 0 5.08 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch normally-open pushbutton push-button"
			(at 0 0 0)
		)
		(symbol "SW_Push_0_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_Push_45deg"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 3.048 1.016 0)
		)
		(property "Value" "SW_Push_45deg"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Push button switch, normally open, two pins, 45° tilted"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch normally-open pushbutton push-button"
			(at 0 0 0)
		)
		(symbol "SW_Push_45deg_0_1"
			(pin passive line
				(at -2.54 2.54 0)
				(length 0)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 2.54 -2.54 180)
				(length 0)
				(name "2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_Push_DPDT"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 10.16 0)
		)
		(property "Value" "SW_Push_DPDT"
			(at 0 -10.16 0)
		)
		(property "Footprint" ""
			(at 0 5.08 0)
		)
		(property "Datasheet" "~"
			(at 0 5.08 0)
		)
		(property "Description" "Momentary Switch, dual pole double throw"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch dual-pole double-throw spdt ON-ON"
			(at 0 0 0)
		)
		(symbol "SW_Push_DPDT_0_0")
		(symbol "SW_Push_DPDT_0_1")
		(symbol "SW_Push_DPDT_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "B")
				(number "2")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "B")
				(number "5")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "A")
				(number "4")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 2.54)
				(name "C")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_Push_Dual"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 7.62 0)
		)
		(property "Value" "SW_Push_Dual"
			(at 0 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 7.62 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Push button switch, generic, symbol, four pins"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch normally-open pushbutton push-button"
			(at 0 0 0)
		)
		(symbol "SW_Push_Dual_0_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "4")
				(number "4")
			)
		)
		(symbol "SW_Push_Dual_1_1")
		(embedded_fonts no)
	)
	(symbol "SW_Push_Dual_x2"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 1.27 2.54 0)
		)
		(property "Value" "SW_Push_Dual_x2"
			(at 0 -1.524 0)
		)
		(property "Footprint" ""
			(at 0 5.08 0)
		)
		(property "Datasheet" "~"
			(at 0 5.08 0)
		)
		(property "Description" "Push button switch, generic, separate symbols, four pins"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch normally-open pushbutton push-button"
			(at 0 0 0)
		)
		(symbol "SW_Push_Dual_x2_0_1")
		(symbol "SW_Push_Dual_x2_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "C")
				(number "1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "D")
				(number "2")
			)
		)
		(symbol "SW_Push_Dual_x2_2_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "D")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_Push_LED"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 7.62 0)
		)
		(property "Value" "SW_Push_LED"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 7.62 0)
		)
		(property "Datasheet" "~"
			(at 0 7.62 0)
		)
		(property "Description" "Push button switch with LED, generic"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch normally-open pushbutton push-button LED"
			(at 0 0 0)
		)
		(symbol "SW_Push_LED_0_0")
		(symbol "SW_Push_LED_0_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "K")
				(number "3")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "A")
				(number "4")
			)
		)
		(symbol "SW_Push_LED_1_1")
		(embedded_fonts no)
	)
	(symbol "SW_Push_Lamp"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 7.62 0)
		)
		(property "Value" "SW_Push_Lamp"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 7.62 0)
		)
		(property "Datasheet" "~"
			(at 0 7.62 0)
		)
		(property "Description" "Push button switch with Signal Lamp, generic"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch normally-open pushbutton push-button Lamp"
			(at 0 0 0)
		)
		(symbol "SW_Push_Lamp_0_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "L")
				(number "3")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "L")
				(number "4")
			)
		)
		(symbol "SW_Push_Lamp_1_1")
		(embedded_fonts no)
	)
	(symbol "SW_Push_Open"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 2.54 0)
		)
		(property "Value" "SW_Push_Open"
			(at 0 -1.905 0)
		)
		(property "Footprint" ""
			(at 0 5.08 0)
		)
		(property "Datasheet" "~"
			(at 0 5.08 0)
		)
		(property "Description" "Push button switch, push-to-open, generic, two pins"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch normally-closed pushbutton push-button"
			(at 0 0 0)
		)
		(symbol "SW_Push_Open_0_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
		)
		(symbol "SW_Push_Open_1_1"
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "B")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_Push_Open_Dual"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 3.81 0)
		)
		(property "Value" "SW_Push_Open_Dual"
			(at 0 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 5.08 0)
		)
		(property "Datasheet" "~"
			(at 0 5.08 0)
		)
		(property "Description" "Push button switch, normally closed, generic, four pins"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch normally-closed pushbutton push-button"
			(at 0 0 0)
		)
		(symbol "SW_Push_Open_Dual_0_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "4")
				(number "4")
			)
		)
		(symbol "SW_Push_Open_Dual_1_1")
		(embedded_fonts no)
	)
	(symbol "SW_Push_Open_Dual_x2"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 2.54 0)
		)
		(property "Value" "SW_Push_Open_Dual_x2"
			(at 0 -1.905 0)
		)
		(property "Footprint" ""
			(at 0 5.08 0)
		)
		(property "Datasheet" "~"
			(at 0 5.08 0)
		)
		(property "Description" "Push button switch, push-to-open, generic, two pins"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch normally-closed pushbutton push-button"
			(at 0 0 0)
		)
		(symbol "SW_Push_Open_Dual_x2_0_1")
		(symbol "SW_Push_Open_Dual_x2_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2")
				(number "2")
			)
		)
		(symbol "SW_Push_Open_Dual_x2_2_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1")
				(number "3")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_Push_SPDT"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 5.08 0)
		)
		(property "Value" "SW_Push_SPDT"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Momentary Switch, single pole double throw"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch single-pole double-throw spdt ON-ON"
			(at 0 0 0)
		)
		(symbol "SW_Push_SPDT_0_0")
		(symbol "SW_Push_SPDT_0_1")
		(symbol "SW_Push_SPDT_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "2")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "C")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_Push_Shielded"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 4.318 2.032 0)
		)
		(property "Value" "SW_Push_Shielded"
			(at 0 4.572 0)
		)
		(property "Footprint" ""
			(at 0 5.08 0)
		)
		(property "Datasheet" "~"
			(at 0 5.08 0)
		)
		(property "Description" "Generic push-button switch, two contact pins and shield pin(s)"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch normally-open pushbutton momentary"
			(at 0 0 0)
		)
		(symbol "SW_Push_Shielded_0_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2")
				(number "2")
			)
		)
		(symbol "SW_Push_Shielded_1_1"
			(pin passive line
				(at 0 -3.81 90)
				(length 2.54)
				(name "B")
				(number "SH")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_Reed"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 2.54 0)
		)
		(property "Value" "SW_Reed"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "reed switch"
			(at 0 0 0)
		)
		(property "ki_keywords" "reed magnetic switch"
			(at 0 0 0)
		)
		(symbol "SW_Reed_0_0")
		(symbol "SW_Reed_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_Reed_Opener"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 2.54 0)
		)
		(property "Value" "SW_Reed_Opener"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "reed switch, default-closed"
			(at 0 0 0)
		)
		(property "ki_keywords" "reed magnetic switch"
			(at 0 0 0)
		)
		(symbol "SW_Reed_Opener_0_0")
		(symbol "SW_Reed_Opener_0_1")
		(symbol "SW_Reed_Opener_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_Reed_SPDT"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 2.54 0)
		)
		(property "Value" "SW_Reed_SPDT"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "SPDT reed switch"
			(at 0 0 0)
		)
		(property "ki_keywords" "reed magnetic switch SPDT"
			(at 0 0 0)
		)
		(symbol "SW_Reed_SPDT_0_0")
		(symbol "SW_Reed_SPDT_0_1")
		(symbol "SW_Reed_SPDT_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "3")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_Rotary_1x12"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 17.78 0)
		)
		(property "Value" "SW_Rotary_1x12"
			(at 0 -17.78 0)
		)
		(property "Footprint" ""
			(at 0 17.78 0)
		)
		(property "Datasheet" "http://cdn-reichelt.de/documents/datenblatt/C200/DS-Serie%23LOR.pdf"
			(at 0 -20.32 0)
		)
		(property "Description" "rotary switch with 12 positions"
			(at 0 0 0)
		)
		(property "ki_keywords" "rotary switch 1x12"
			(at 0 0 0)
		)
		(symbol "SW_Rotary_1x12_0_0")
		(symbol "SW_Rotary_1x12_1_1"
			(pin passive line
				(at -15.24 0 0)
				(length 3.81)
				(name "13")
				(number "13")
			)
			(pin passive line
				(at 15.24 15.24 180)
				(length 3.81)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 15.24 12.7 180)
				(length 3.81)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 15.24 10.16 180)
				(length 3.81)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at 15.24 7.62 180)
				(length 3.81)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "5")
				(number "5")
			)
			(pin passive line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "6")
				(number "6")
			)
			(pin passive line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "7")
				(number "7")
			)
			(pin passive line
				(at 15.24 -5.08 180)
				(length 3.81)
				(name "8")
				(number "8")
			)
			(pin passive line
				(at 15.24 -7.62 180)
				(length 3.81)
				(name "9")
				(number "9")
			)
			(pin passive line
				(at 15.24 -10.16 180)
				(length 3.81)
				(name "10")
				(number "10")
			)
			(pin passive line
				(at 15.24 -12.7 180)
				(length 3.81)
				(name "11")
				(number "11")
			)
			(pin passive line
				(at 15.24 -15.24 180)
				(length 3.81)
				(name "12")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_Rotary_1x3_MP"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 6.35 0)
		)
		(property "Value" "SW_Rotary_1x3_MP"
			(at 8.89 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 -8.89 0)
		)
		(property "Datasheet" "~"
			(at 0 -11.43 0)
		)
		(property "Description" "Rotary switch 1x3, SP3T with mount point"
			(at 0 0 0)
		)
		(property "ki_keywords" "Rotary switch 1x3 SP3T"
			(at 0 0 0)
		)
		(symbol "SW_Rotary_1x3_MP_0_1")
		(symbol "SW_Rotary_1x3_MP_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "")
				(number "4")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "")
				(number "MP")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "")
				(number "1")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "")
				(number "2")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_Rotary_1x4_MP"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 7.62 0)
		)
		(property "Value" "SW_Rotary_1x4_MP"
			(at 8.89 -6.35 0)
		)
		(property "Footprint" ""
			(at 0 -10.16 0)
		)
		(property "Datasheet" "~"
			(at 0 -12.7 0)
		)
		(property "Description" "Rotary switch 1x4, SP4T with mount point"
			(at 0 0 0)
		)
		(property "ki_keywords" "Rotary switch 1x4 SP4T"
			(at 0 0 0)
		)
		(symbol "SW_Rotary_1x4_MP_0_1")
		(symbol "SW_Rotary_1x4_MP_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "")
				(number "5")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "")
				(number "MP")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "")
				(number "1")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "")
				(number "2")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "")
				(number "3")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_Rotary_1x5_MP"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 7.62 0)
		)
		(property "Value" "SW_Rotary_1x5_MP"
			(at 8.89 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 -10.16 0)
		)
		(property "Datasheet" "~"
			(at 0 -12.7 0)
		)
		(property "Description" "Rotary switch 1x5, SP5T with mount point"
			(at 0 0 0)
		)
		(property "ki_keywords" "Rotary switch 1x5 SP5T"
			(at 0 0 0)
		)
		(symbol "SW_Rotary_1x5_MP_0_1")
		(symbol "SW_Rotary_1x5_MP_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "")
				(number "6")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "")
				(number "MP")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "")
				(number "1")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "")
				(number "2")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "")
				(number "3")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "")
				(number "4")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_Rotary_1x6_MP"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 10.16 0)
		)
		(property "Value" "SW_Rotary_1x6_MP"
			(at 8.89 -7.62 0)
		)
		(property "Footprint" ""
			(at 0 -10.16 0)
		)
		(property "Datasheet" "~"
			(at 0 -12.7 0)
		)
		(property "Description" "Rotary switch 1x6, SP6T with mount point"
			(at 0 0 0)
		)
		(property "ki_keywords" "Rotary switch 1x6 SP6T"
			(at 0 0 0)
		)
		(symbol "SW_Rotary_1x6_MP_0_1")
		(symbol "SW_Rotary_1x6_MP_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "")
				(number "7")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "")
				(number "MP")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "")
				(number "1")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "")
				(number "5")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_Rotary_1x7_MP"
		(pin_names
			(offset 0.002)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 10.16 0)
		)
		(property "Value" "SW_Rotary_1x7_MP"
			(at 8.89 -10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Rotary switch 1x7, SP7T with mount point"
			(at 0 0 0)
		)
		(property "ki_keywords" "Rotary switch 1x7 SP7T"
			(at 0 0 0)
		)
		(symbol "SW_Rotary_1x7_MP_0_1")
		(symbol "SW_Rotary_1x7_MP_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "")
				(number "8")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "")
				(number "MP")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "")
				(number "1")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "")
				(number "5")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "")
				(number "6")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_Rotary_1x8_MP"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 12.7 0)
		)
		(property "Value" "SW_Rotary_1x8_MP"
			(at 10.16 -10.16 0)
		)
		(property "Footprint" ""
			(at -1.27 0 0)
		)
		(property "Datasheet" "~"
			(at -1.27 0 0)
		)
		(property "Description" "Rotary switch 1x8, SP8T with mount point"
			(at 0 0 0)
		)
		(property "ki_keywords" "Rotary switch 1x8 SP8T"
			(at 0 0 0)
		)
		(symbol "SW_Rotary_1x8_MP_0_1")
		(symbol "SW_Rotary_1x8_MP_1_1"
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "")
				(number "9")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "")
				(number "MP")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 2.54)
				(name "")
				(number "1")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "")
				(number "2")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "")
				(number "3")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "")
				(number "4")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "")
				(number "5")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "")
				(number "6")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "")
				(number "7")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_Rotary_1x9_MP"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 12.7 0)
		)
		(property "Value" "SW_Rotary_1x9_MP"
			(at 8.89 -12.7 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Rotary switch 1x8, SP8T with mount point"
			(at 0 0 0)
		)
		(property "ki_keywords" "Rotary switch 1x8 SP8T"
			(at 0 0 0)
		)
		(symbol "SW_Rotary_1x9_MP_0_1")
		(symbol "SW_Rotary_1x9_MP_1_1"
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "")
				(number "10")
			)
			(pin passive line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "")
				(number "MP")
			)
			(pin passive line
				(at 7.62 10.16 180)
				(length 2.54)
				(name "")
				(number "1")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "")
				(number "2")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "")
				(number "3")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "")
				(number "4")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "")
				(number "5")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "")
				(number "6")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "")
				(number "7")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "")
				(number "8")
			)
			(pin passive line
				(at 7.62 -10.16 180)
				(length 2.54)
				(name "")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_Rotary_2x6"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 17.78 0)
		)
		(property "Value" "SW_Rotary_2x6"
			(at 0 -17.78 0)
		)
		(property "Footprint" ""
			(at -2.54 15.24 0)
		)
		(property "Datasheet" "http://cdn-reichelt.de/documents/datenblatt/C200/DS-Serie%23LOR.pdf"
			(at 0 -20.32 0)
		)
		(property "Description" "2 rotary switch with 6 positions"
			(at 0 0 0)
		)
		(property "ki_keywords" "rotary switch 2x6"
			(at 0 0 0)
		)
		(symbol "SW_Rotary_2x6_0_0")
		(symbol "SW_Rotary_2x6_0_1")
		(symbol "SW_Rotary_2x6_1_1"
			(pin passive line
				(at -12.7 7.62 0)
				(length 3.81)
				(name "13")
				(number "13")
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 3.81)
				(name "14")
				(number "14")
			)
			(pin passive line
				(at 12.7 15.24 180)
				(length 3.81)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 12.7 12.7 180)
				(length 3.81)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 3.81)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 3.81)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 3.81)
				(name "5")
				(number "5")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 3.81)
				(name "6")
				(number "6")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 3.81)
				(name "7")
				(number "7")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 3.81)
				(name "8")
				(number "8")
			)
			(pin passive line
				(at 12.7 -7.62 180)
				(length 3.81)
				(name "9")
				(number "9")
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 3.81)
				(name "10")
				(number "10")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 3.81)
				(name "11")
				(number "11")
			)
			(pin passive line
				(at 12.7 -15.24 180)
				(length 3.81)
				(name "12")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_Rotary_3x4"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 20.32 0)
		)
		(property "Value" "SW_Rotary_3x4"
			(at 0 -17.78 0)
		)
		(property "Footprint" ""
			(at -2.54 20.32 0)
		)
		(property "Datasheet" "http://cdn-reichelt.de/documents/datenblatt/C200/DS-Serie%23LOR.pdf"
			(at 0 -20.32 0)
		)
		(property "Description" "3 rotary switches with 4 positions"
			(at 0 0 0)
		)
		(property "ki_keywords" "rotary switch 3x4"
			(at 0 0 0)
		)
		(symbol "SW_Rotary_3x4_0_0")
		(symbol "SW_Rotary_3x4_0_1")
		(symbol "SW_Rotary_3x4_1_1"
			(pin passive line
				(at -12.7 12.7 0)
				(length 3.81)
				(name "13")
				(number "13")
			)
			(pin passive line
				(at -12.7 0 0)
				(length 3.81)
				(name "14")
				(number "14")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 3.81)
				(name "15")
				(number "15")
			)
			(pin passive line
				(at 12.7 17.78 180)
				(length 3.81)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 12.7 15.24 180)
				(length 3.81)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 12.7 12.7 180)
				(length 3.81)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 3.81)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 3.81)
				(name "5")
				(number "5")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 3.81)
				(name "6")
				(number "6")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 3.81)
				(name "7")
				(number "7")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 3.81)
				(name "8")
				(number "8")
			)
			(pin passive line
				(at 12.7 -7.62 180)
				(length 3.81)
				(name "9")
				(number "9")
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 3.81)
				(name "10")
				(number "10")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 3.81)
				(name "11")
				(number "11")
			)
			(pin passive line
				(at 12.7 -15.24 180)
				(length 3.81)
				(name "12")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_Rotary_4x3"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 20.32 0)
		)
		(property "Value" "SW_Rotary_4x3"
			(at 0 -20.32 0)
		)
		(property "Footprint" ""
			(at -2.54 22.86 0)
		)
		(property "Datasheet" "http://cdn-reichelt.de/documents/datenblatt/C200/DS-Serie%23LOR.pdf"
			(at -2.54 22.86 0)
		)
		(property "Description" "4 rotary switches with 3 positions"
			(at 0 0 0)
		)
		(property "ki_keywords" "rotary switch 4x3"
			(at 0 0 0)
		)
		(symbol "SW_Rotary_4x3_0_0")
		(symbol "SW_Rotary_4x3_0_1")
		(symbol "SW_Rotary_4x3_1_1"
			(pin passive line
				(at -12.7 15.24 0)
				(length 3.81)
				(name "13")
				(number "13")
			)
			(pin passive line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "14")
				(number "14")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "15")
				(number "15")
			)
			(pin passive line
				(at -12.7 -15.24 0)
				(length 3.81)
				(name "16")
				(number "16")
			)
			(pin passive line
				(at 12.7 17.78 180)
				(length 3.81)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 12.7 15.24 180)
				(length 3.81)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 12.7 12.7 180)
				(length 3.81)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at 12.7 7.62 180)
				(length 3.81)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 3.81)
				(name "5")
				(number "5")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 3.81)
				(name "6")
				(number "6")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 3.81)
				(name "7")
				(number "7")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 3.81)
				(name "8")
				(number "8")
			)
			(pin passive line
				(at 12.7 -7.62 180)
				(length 3.81)
				(name "9")
				(number "9")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 3.81)
				(name "10")
				(number "10")
			)
			(pin passive line
				(at 12.7 -15.24 180)
				(length 3.81)
				(name "11")
				(number "11")
			)
			(pin passive line
				(at 12.7 -17.78 180)
				(length 3.81)
				(name "12")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_SP3T"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 5.08 0)
		)
		(property "Value" "SW_SP3T"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at -15.875 4.445 0)
		)
		(property "Datasheet" "~"
			(at 0 -7.62 0)
		)
		(property "Description" "Switch, three position, single pole triple throw, 3 position switch, SP3T"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch sp3t ON-ON-ON"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SW* SP3T*"
			(at 0 0 0)
		)
		(symbol "SW_SP3T_0_1")
		(symbol "SW_SP3T_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "4")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_SP3T_NR01103"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 6.35 0)
		)
		(property "Value" "SW_SP3T_NR01103"
			(at 0 -6.35 0)
		)
		(property "Footprint" "Button_Switch_THT:SW_NKK_NR01"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.nkkswitches.com/pdf/NR01%20Rotaries.pdf"
			(at 0 -11.43 0)
		)
		(property "Description" "NKK Switches NR01 Series rotary SP3T switch"
			(at 0 0 0)
		)
		(property "ki_keywords" "NR01 SP3T Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SW?NKK?NR01*"
			(at 0 0 0)
		)
		(symbol "SW_SP3T_NR01103_0_1")
		(symbol "SW_SP3T_NR01103_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "Common")
				(number "C")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "MP")
				(number "MP")
			)
			(pin no_connect line
				(at -2.54 5.08 270)
				(length 0)
				(hide yes)
				(name "")
				(number "4")
			)
			(pin no_connect line
				(at 2.54 5.08 270)
				(length 0)
				(hide yes)
				(name "")
				(number "5")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "3")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_SP4T_NR01104"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 7.62 0)
		)
		(property "Value" "SW_SP4T_NR01104"
			(at 0 -7.62 0)
		)
		(property "Footprint" "Button_Switch_THT:SW_NKK_NR01"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.nkkswitches.com/pdf/NR01%20Rotaries.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "NKK Switches NR01 Series rotary SP4T switch"
			(at 0 0 0)
		)
		(property "ki_keywords" "NR01 SP4T Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SW?NKK?NR01*"
			(at 0 0 0)
		)
		(symbol "SW_SP4T_NR01104_0_1")
		(symbol "SW_SP4T_NR01104_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "Common")
				(number "C")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "MP")
				(number "MP")
			)
			(pin no_connect line
				(at 5.08 -5.08 180)
				(length 0)
				(hide yes)
				(name "")
				(number "5")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "4")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_SP5T_NR01105"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 7.62 0)
		)
		(property "Value" "SW_SP5T_NR01105"
			(at 0 -7.62 0)
		)
		(property "Footprint" "Button_Switch_THT:SW_NKK_NR01"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.nkkswitches.com/pdf/NR01%20Rotaries.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "NKK Switches NR01 Series rotary SP5T switch"
			(at 0 0 0)
		)
		(property "ki_keywords" "NR01 SP5T Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SW?NKK?NR01*"
			(at 0 0 0)
		)
		(symbol "SW_SP5T_NR01105_0_1")
		(symbol "SW_SP5T_NR01105_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "Common")
				(number "C")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "MP")
				(number "MP")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "5")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_SPDT"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 5.08 0)
		)
		(property "Value" "SW_SPDT"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 -7.62 0)
		)
		(property "Description" "Switch, single pole double throw"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch single-pole double-throw spdt ON-ON"
			(at 0 0 0)
		)
		(symbol "SW_SPDT_0_1")
		(symbol "SW_SPDT_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "2")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "C")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_SPDT_312"
		(pin_names
			(offset 1)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 5.08 0)
		)
		(property "Value" "SW_SPDT_312"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 -10.16 0)
		)
		(property "Datasheet" "~"
			(at 0 -7.62 0)
		)
		(property "Description" "Switch, single pole double throw"
			(at 0 0 0)
		)
		(property "ki_keywords" "changeover single-pole double-throw spdt ON-ON"
			(at 0 0 0)
		)
		(symbol "SW_SPDT_312_0_1")
		(symbol "SW_SPDT_312_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "C")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_SPDT_321"
		(pin_names
			(offset 1)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 5.08 0)
		)
		(property "Value" "SW_SPDT_321"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at 0 -10.16 0)
		)
		(property "Datasheet" "~"
			(at 0 -7.62 0)
		)
		(property "Description" "Switch, single pole double throw"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch single-pole double-throw spdt ON-ON"
			(at 0 0 0)
		)
		(symbol "SW_SPDT_321_0_1")
		(symbol "SW_SPDT_321_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "2")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "C")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_SPDT_MSM"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 5.08 0)
		)
		(property "Value" "SW_SPDT_MSM"
			(at 0 -5.08 0)
		)
		(property "Footprint" ""
			(at -13.97 11.43 0)
		)
		(property "Datasheet" "~"
			(at 0 -7.62 0)
		)
		(property "Description" "Switch, single pole double throw, center OFF position"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch spdt single-pole double-throw ON-OFF-ON"
			(at 0 0 0)
		)
		(symbol "SW_SPDT_MSM_0_1")
		(symbol "SW_SPDT_MSM_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "3")
				(number "2")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "4")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_SPDT_XKB_DMx-xxxx-1"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 4.318 0)
		)
		(property "Value" "SW_SPDT_XKB_DMx-xxxx-1"
			(at 0 -5.588 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Position switch"
			(at 0 0 0)
		)
		(property "ki_keywords" "limit switch single pole double throw spdt microswitch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SW?XKB?DM??16U??1*"
			(at 0 0 0)
		)
		(symbol "SW_SPDT_XKB_DMx-xxxx-1_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "B")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_SPST"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 3.175 0)
		)
		(property "Value" "SW_SPST"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Single Pole Single Throw (SPST) switch"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch lever"
			(at 0 0 0)
		)
		(symbol "SW_SPST_0_0")
		(symbol "SW_SPST_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "B")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_SPST_LED"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 6.35 0)
		)
		(property "Value" "SW_SPST_LED"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 7.62 0)
		)
		(property "Datasheet" "~"
			(at 0 -6.35 0)
		)
		(property "Description" "Single Pole Single Throw (SPST) switch with LED, generic"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch SPST LED OFF-ON"
			(at 0 0 0)
		)
		(symbol "SW_SPST_LED_0_0")
		(symbol "SW_SPST_LED_0_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "K")
				(number "3")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "A")
				(number "4")
			)
		)
		(symbol "SW_SPST_LED_1_1")
		(embedded_fonts no)
	)
	(symbol "SW_SPST_Lamp"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 6.35 0)
		)
		(property "Value" "SW_SPST_Lamp"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 7.62 0)
		)
		(property "Datasheet" "~"
			(at 0 -6.35 0)
		)
		(property "Description" "Single Pole Single Throw (SPST) switch with signal lamp, generic"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch SPST LED OFF-ON lamp"
			(at 0 0 0)
		)
		(symbol "SW_SPST_Lamp_0_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "L")
				(number "3")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "L")
				(number "4")
			)
		)
		(symbol "SW_SPST_Lamp_1_1")
		(embedded_fonts no)
	)
	(symbol "SW_SPST_Temperature"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 5.08 0)
		)
		(property "Value" "SW_SPST_Temperature"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 -5.08 0)
		)
		(property "Description" "Single Pole Single Throw (SPST) switch, temperature dependent"
			(at 0 0 0)
		)
		(property "ki_keywords" "temperature switch"
			(at 0 0 0)
		)
		(symbol "SW_SPST_Temperature_0_0")
		(symbol "SW_SPST_Temperature_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "B")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SW_Slide_DPDT"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "SW"
			(at 0 6.858 0)
		)
		(property "Value" "SW_Slide_DPDT"
			(at 0 -8.128 0)
		)
		(property "Footprint" ""
			(at 13.97 5.08 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Slide Switch, dual pole double throw"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch dual-pole double-throw dpdt ON-ON"
			(at 0 0 0)
		)
		(symbol "SW_Slide_DPDT_0_0")
		(symbol "SW_Slide_DPDT_0_1")
		(symbol "SW_Slide_DPDT_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "B")
				(number "2")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "C")
				(number "6")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "B")
				(number "5")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "A")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CK_KMS2xxG"
		(extends "SW_Push_Shielded")
		(property "Reference" "SW"
			(at 4.318 2.032 0)
		)
		(property "Value" "CK_KMS2xxG"
			(at 0 4.572 0)
		)
		(property "Footprint" "Button_Switch_SMD:SW_SPST_CK_KMS2xxGP"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://www.ckswitches.com/media/1482/kms.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Microminiature SMT Side Actuated, 4.2 x 2.8 x 1.42mm, without pegs, with shield pin"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch normally-open pushbutton push-button"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SW*KMS2*G*"
			(at 0 0 0)
		)
	)
	(symbol "CK_KMS2xxGP"
		(extends "SW_Push_Shielded")
		(property "Reference" "SW"
			(at 4.318 2.032 0)
		)
		(property "Value" "CK_KMS2xxGP"
			(at 0 4.572 0)
		)
		(property "Footprint" "Button_Switch_SMD:SW_SPST_CK_KMS2xxGP"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://www.ckswitches.com/media/1482/kms.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Microminiature SMT Side Actuated, 4.2 x 2.8 x 1.42mm, with pegs, with shield pin"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch normally-open pushbutton push-button"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SW*KMS2*GP*"
			(at 0 0 0)
		)
	)
	(symbol "SW_Coded_SH-7030"
		(extends "SW_Coded_SH-7010")
		(property "Reference" "SW"
			(at -7.62 8.89 0)
		)
		(property "Value" "SW_Coded_SH-7030"
			(at -7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at -7.62 -11.43 0)
		)
		(property "Datasheet" "https://www.nidec-copal-electronics.com/e/catalog/switch/sh-7000.pdf"
			(at 0 0 0)
		)
		(property "Description" "Rotary switch, 4-bit encoding, 10 positions, Complementary code"
			(at 0 0 0)
		)
		(property "ki_keywords" "rotary bcd Complementary"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nidec*Copal*SH*7010*"
			(at 0 0 0)
		)
	)
	(symbol "SW_Coded_SH-7070"
		(extends "SW_Coded_SH-7050")
		(property "Reference" "SW"
			(at -7.62 8.89 0)
		)
		(property "Value" "SW_Coded_SH-7070"
			(at -7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at -7.62 -11.43 0)
		)
		(property "Datasheet" "https://www.nidec-copal-electronics.com/e/catalog/switch/sh-7000.pdf"
			(at 0 0 0)
		)
		(property "Description" "Rotary switch, 4-bit encoding, 16 positions, Complementary code"
			(at 0 0 0)
		)
		(property "ki_keywords" "rotary hex Complementary"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Nidec*Copal*SH*7010*"
			(at 0 0 0)
		)
	)
	(symbol "SW_E3_SA3624"
		(extends "SW_E3_SA3216")
		(property "Reference" "SW"
			(at 1.27 8.89 0)
		)
		(property "Value" "SW_E3_SA3624"
			(at 7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 2.54 0)
		)
		(property "Datasheet" "http://www.e3-keys.com/files/SA%20Technical%20Datasheet%20v2.0.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Push button switch with LCD screen"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch normally-open pushbutton push-button LCD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SW?PUSH?LCD?E3?SAxxxx*"
			(at 0 0 0)
		)
	)
	(symbol "SW_E3_SA6432"
		(extends "SW_E3_SA3216")
		(property "Reference" "SW"
			(at 1.27 8.89 0)
		)
		(property "Value" "SW_E3_SA6432"
			(at 7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 2.54 0)
		)
		(property "Datasheet" "http://www.e3-keys.com/files/SA%20Technical%20Datasheet%20v2.0.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Push button switch with LCD screen"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch normally-open pushbutton push-button LCD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SW?PUSH?LCD?E3?SAxxxx*"
			(at 0 0 0)
		)
	)
	(symbol "SW_MMI_Q5-100"
		(extends "SW_E3_SA3216")
		(property "Reference" "SW"
			(at 1.27 8.89 0)
		)
		(property "Value" "SW_MMI_Q5-100"
			(at 7.62 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 2.54 0)
		)
		(property "Datasheet" "http://latest.ledswitches.co.uk/media/pdf/Q5-PCB-V1-withQ5data.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Push button switch with LCD screen"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch normally-open pushbutton push-button LCD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SW?PUSH?LCD?E3?SAxxxx*"
			(at 0 0 0)
		)
	)
	(symbol "SW_Nidec_CAS-120A1"
		(extends "SW_SPDT_321")
		(property "Reference" "SW"
			(at 0 4.318 0)
		)
		(property "Value" "SW_Nidec_CAS-120A1"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Button_Switch_SMD:Nidec_Copal_CAS-120A"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.nidec-components.com/e/catalog/switch/cas.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "Switch, single pole double throw"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch single-pole double-throw spdt ON-ON"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Nidec?Copal?CAS?120A*"
			(at 0 0 0)
		)
	)
	(symbol "SW_Omron_B3FS"
		(extends "SW_Push")
		(property "Reference" "SW"
			(at 1.27 2.54 0)
		)
		(property "Value" "SW_Omron_B3FS"
			(at 0 -1.524 0)
		)
		(property "Footprint" ""
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://omronfs.omron.com/en_US/ecb/products/pdf/en-b3fs.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Omron B3FS 6x6mm single pole normally-open tactile switch"
			(at 0 0 0)
		)
		(property "ki_keywords" "switch normally-open pushbutton push-button"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SW*Omron*B3FS*"
			(at 0 0 0)
		)
	)
	(symbol "SW_Wuerth_450301014042"
		(extends "SW_SPDT_312")
		(property "Reference" "SW"
			(at 0 5.08 0)
		)
		(property "Value" "SW_Wuerth_450301014042"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Button_Switch_THT:SW_Slide-03_Wuerth-WS-SLTV_10x2.5x6.4_P2.54mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/450301014042.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "Switch slide, single pole double throw"
			(at 0 0 0)
		)
		(property "ki_keywords" "changeover single-pole opposite-side-connection double-throw spdt ON-ON"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SW*Wuerth*WS*SLTV*10x2.5x6.4*P2.54mm*"
			(at 0 0 0)
		)
	)
)
