(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "8284"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 19.05 0)
		)
		(property "Value" "8284"
			(at 2.54 19.05 0)
		)
		(property "Footprint" "Package_DIP:DIP-18_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.cpu-galaxy.at/cpu/ram%20rom%20eprom/other_intel_chips/other_intel-Dateien/D8284A_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "Clock Generator and Driver for i8086/88 Microcontrollers, PDIP-18"
			(at 0 0 0)
		)
		(property "ki_keywords" "Clock Generator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "8284_0_0")
		(symbol "8284_1_1"
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "~{RES}")
				(number "11")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "RDY1")
				(number "4")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "RDY2")
				(number "6")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~{AEN1}")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{AEN2}")
				(number "7")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{ASYNC}")
				(number "15")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "CSYNC")
				(number "1")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "F/~{C}")
				(number "13")
			)
			(pin input line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "EFI")
				(number "14")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VCC")
				(number "18")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin output line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "CLK")
				(number "8")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "READY")
				(number "5")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "RESET")
				(number "10")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "PCLK")
				(number "2")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OSC")
				(number "12")
			)
			(pin input line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "X1")
				(number "17")
			)
			(pin output line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "X2")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "82C54"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 24.13 0)
		)
		(property "Value" "82C54"
			(at 2.54 24.13 0)
		)
		(property "Footprint" "Package_DIP:DIP-24_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://download.intel.com/design/archives/periphrl/docs/23124406.pdf"
			(at -11.43 22.86 0)
		)
		(property "Description" "CHMOS Programmable Interval Timer, PDIP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Timer Counter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "82C54_0_1")
		(symbol "82C54_1_1"
			(pin bidirectional line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "D0")
				(number "8")
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "D1")
				(number "7")
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "D2")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "D3")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "D4")
				(number "4")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "D5")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "D6")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "D7")
				(number "1")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{RD}")
				(number "22")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "~{WR}")
				(number "23")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "A0")
				(number "19")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "A1")
				(number "20")
			)
			(pin input line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "~{CS}")
				(number "21")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VCC")
				(number "24")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "12")
			)
			(pin input clock
				(at 10.16 15.24 180)
				(length 2.54)
				(name "CLK0")
				(number "9")
			)
			(pin input line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "G0")
				(number "11")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "OUT0")
				(number "10")
			)
			(pin input clock
				(at 10.16 2.54 180)
				(length 2.54)
				(name "CLK1")
				(number "15")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "G1")
				(number "14")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT1")
				(number "13")
			)
			(pin input clock
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "CLK2")
				(number "18")
			)
			(pin input line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "G2")
				(number "16")
			)
			(pin output line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "OUT2")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "82C54_PLCC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 24.13 0)
		)
		(property "Value" "82C54_PLCC"
			(at 2.54 24.13 0)
		)
		(property "Footprint" "Package_LCC:PLCC-28"
			(at 2.54 0 0)
		)
		(property "Datasheet" "http://download.intel.com/design/archives/periphrl/docs/23124406.pdf"
			(at -13.97 22.86 0)
		)
		(property "Description" "CHMOS Programmable Interval Timer, PLCC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Timer Counter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PLCC?28*"
			(at 0 0 0)
		)
		(symbol "82C54_PLCC_0_1")
		(symbol "82C54_PLCC_1_1"
			(pin bidirectional line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "D0")
				(number "9")
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "D1")
				(number "8")
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "D2")
				(number "7")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "D3")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "D4")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "D5")
				(number "4")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "D6")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "D7")
				(number "2")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "~{RD}")
				(number "26")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "~{WR}")
				(number "27")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "A0")
				(number "22")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "A1")
				(number "23")
			)
			(pin input line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "~{CS}")
				(number "24")
			)
			(pin no_connect line
				(at -5.08 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -2.54 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VCC")
				(number "28")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin no_connect line
				(at 2.54 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin no_connect line
				(at 5.08 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "25")
			)
			(pin input clock
				(at 10.16 15.24 180)
				(length 2.54)
				(name "CLK0")
				(number "10")
			)
			(pin input line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "G0")
				(number "13")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "OUT0")
				(number "12")
			)
			(pin input clock
				(at 10.16 2.54 180)
				(length 2.54)
				(name "CLK1")
				(number "18")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "G1")
				(number "17")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT1")
				(number "16")
			)
			(pin input clock
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "CLK2")
				(number "21")
			)
			(pin input line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "G2")
				(number "19")
			)
			(pin output line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "OUT2")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD9513"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "AD9513"
			(at 11.43 26.67 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD9513.pdf"
			(at 0 15.24 0)
		)
		(property "Description" "800 MHz, 3 Outputs, Clock Distribution IC, Divider, Delay Adjust, LFCSP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "clock distribution LVDS CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AD9513_0_1")
		(symbol "AD9513_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "S0")
				(number "25")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "S1")
				(number "16")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "S2")
				(number "15")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "S3")
				(number "14")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "S4")
				(number "13")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "S5")
				(number "12")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "S6")
				(number "11")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "S7")
				(number "10")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "S8")
				(number "9")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "S9")
				(number "8")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "S10")
				(number "7")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "CLK")
				(number "2")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "CLKB")
				(number "3")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "SYNCB")
				(number "5")
			)
			(pin passive line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "RSET")
				(number "32")
			)
			(pin power_in line
				(at -10.16 27.94 270)
				(length 2.54)
				(name "VS")
				(number "1")
			)
			(pin power_in line
				(at -7.62 27.94 270)
				(length 2.54)
				(name "VS")
				(number "4")
			)
			(pin power_in line
				(at -5.08 27.94 270)
				(length 2.54)
				(name "VS")
				(number "17")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VS")
				(number "20")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VS")
				(number "21")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "31")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VS")
				(number "24")
			)
			(pin power_in line
				(at 5.08 27.94 270)
				(length 2.54)
				(name "VS")
				(number "26")
			)
			(pin power_in line
				(at 7.62 27.94 270)
				(length 2.54)
				(name "VS")
				(number "29")
			)
			(pin power_in line
				(at 10.16 27.94 270)
				(length 2.54)
				(name "VS")
				(number "30")
			)
			(pin power_out line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "VREF")
				(number "6")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "OUT0")
				(number "28")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "OUT0B")
				(number "27")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "OUT1")
				(number "23")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "OUT1B")
				(number "22")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "OUT2")
				(number "19")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "OUT2B")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD9514"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "AD9514"
			(at 11.43 26.67 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD9514.pdf"
			(at 0 16.51 0)
		)
		(property "Description" "1.6 GHz, 3 Outputs, Clock Distribution IC, Divider, Delay Adjust, LFCSP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "clock distribution LVPECL LVDS CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AD9514_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "S0")
				(number "25")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "S1")
				(number "16")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "S2")
				(number "15")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "S3")
				(number "14")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "S4")
				(number "13")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "S5")
				(number "12")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "S6")
				(number "11")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "S7")
				(number "10")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "S8")
				(number "9")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "S9")
				(number "8")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "S10")
				(number "7")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "CLK")
				(number "2")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "CLKB")
				(number "3")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "SYNCB")
				(number "5")
			)
			(pin passive line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "RSET")
				(number "32")
			)
			(pin power_in line
				(at -10.16 27.94 270)
				(length 2.54)
				(name "VS")
				(number "1")
			)
			(pin power_in line
				(at -7.62 27.94 270)
				(length 2.54)
				(name "VS")
				(number "4")
			)
			(pin power_in line
				(at -5.08 27.94 270)
				(length 2.54)
				(name "VS")
				(number "17")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VS")
				(number "20")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VS")
				(number "21")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "31")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VS")
				(number "24")
			)
			(pin power_in line
				(at 5.08 27.94 270)
				(length 2.54)
				(name "VS")
				(number "26")
			)
			(pin power_in line
				(at 7.62 27.94 270)
				(length 2.54)
				(name "VS")
				(number "29")
			)
			(pin power_in line
				(at 10.16 27.94 270)
				(length 2.54)
				(name "VS")
				(number "30")
			)
			(pin power_out line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "VREF")
				(number "6")
			)
			(pin open_emitter line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "OUT0")
				(number "28")
			)
			(pin open_emitter line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "OUT0B")
				(number "27")
			)
			(pin open_emitter line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "OUT1")
				(number "23")
			)
			(pin open_emitter line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "OUT1B")
				(number "22")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "OUT2")
				(number "19")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "OUT2B")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD9515"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "AD9515"
			(at 11.43 26.67 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD9515.pdf"
			(at 0 15.24 0)
		)
		(property "Description" "1.6 GHz, 2 Outputs, Clock Distribution IC, Divider, Delay Adjust, LFCSP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "clock distribution LVPECL LVDS CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AD9515_1_1"
			(pin input line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "S0")
				(number "25")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "S1")
				(number "16")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "S2")
				(number "15")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "S3")
				(number "14")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "S4")
				(number "13")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "S5")
				(number "12")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "S6")
				(number "11")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "S7")
				(number "10")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "S8")
				(number "9")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "S9")
				(number "8")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "S10")
				(number "7")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "CLK")
				(number "2")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "CLKB")
				(number "3")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "SYNCB")
				(number "5")
			)
			(pin passive line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "RSET")
				(number "32")
			)
			(pin power_in line
				(at -10.16 27.94 270)
				(length 2.54)
				(name "VS")
				(number "1")
			)
			(pin power_in line
				(at -7.62 27.94 270)
				(length 2.54)
				(name "VS")
				(number "4")
			)
			(pin power_in line
				(at -5.08 27.94 270)
				(length 2.54)
				(name "VS")
				(number "17")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VS")
				(number "20")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VS")
				(number "21")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "31")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VS")
				(number "24")
			)
			(pin power_in line
				(at 5.08 27.94 270)
				(length 2.54)
				(name "VS")
				(number "26")
			)
			(pin power_in line
				(at 7.62 27.94 270)
				(length 2.54)
				(name "VS")
				(number "29")
			)
			(pin power_in line
				(at 10.16 27.94 270)
				(length 2.54)
				(name "VS")
				(number "30")
			)
			(pin no_connect line
				(at 12.7 12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "28")
			)
			(pin no_connect line
				(at 12.7 10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "27")
			)
			(pin power_out line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "VREF")
				(number "6")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "OUT0")
				(number "23")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "OUT0B")
				(number "22")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "OUT1")
				(number "19")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "OUT1B")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CD4541BE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 15.24 0)
		)
		(property "Value" "CD4541BE"
			(at 7.62 15.24 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/cd4541b.pdf"
			(at 0 0 0)
		)
		(property "Description" "20V, Programmable Timer, PDIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "cmos"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "CD4541BE_0_0"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "R_{TC}")
				(number "1")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "C_{TC}")
				(number "2")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "R_{S}")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "MODE")
				(number "10")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "B")
				(number "13")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A")
				(number "12")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "Q/~{Q}_SELECT")
				(number "9")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "MR")
				(number "6")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "AR")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "V_{DD}")
				(number "14")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "V_{SS}")
				(number "7")
			)
			(pin no_connect line
				(at 7.62 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 7.62 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUTPUT/Q")
				(number "8")
			)
		)
		(symbol "CD4541BE_0_1")
		(embedded_fonts no)
	)
	(symbol "DS1023S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 19.05 0)
		)
		(property "Value" "DS1023S"
			(at 5.08 -21.59 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -25.4 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/DS1023.pdf"
			(at 0 -27.94 0)
		)
		(property "Description" "8-bit Programamble Delay Line / Timing Element, 5V supply, SOIC-16W package."
			(at 0 0 0)
		)
		(property "ki_keywords" "Delay Line"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*W?7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "DS1023S_1_1"
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "IN")
				(number "1")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "LE")
				(number "2")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "MS")
				(number "11")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~{P}/S")
				(number "14")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "Q/P0")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "CLK/P1")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "D/P2")
				(number "5")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "P3")
				(number "6")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "P4")
				(number "7")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "P5")
				(number "10")
			)
			(pin input line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "P6")
				(number "12")
			)
			(pin input line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "P7")
				(number "13")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "V_{CC}")
				(number "16")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "REF/PWM")
				(number "9")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUT/~{OUT}")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ICM7209"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 6.35 0)
		)
		(property "Value" "ICM7209"
			(at 8.636 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheets/320/500974_DS.pdf"
			(at 5.08 -5.08 0)
		)
		(property "Description" "Timebase generator, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Timebase generator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "ICM7209_0_1")
		(symbol "ICM7209_1_1"
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "OSC_IN")
				(number "2")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "DISABLE")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "OUT/8")
				(number "6")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "OUT/1")
				(number "5")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "OSC_OUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM555xMM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LM555xMM"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 16.51 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm555.pdf"
			(at 21.59 -10.16 0)
		)
		(property "Description" "Precision Timers, 555 compatible, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single timer 555"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LM555xMM_0_0"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
		)
		(symbol "LM555xMM_0_1")
		(symbol "LM555xMM_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "TR")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 3.81)
				(name "CV")
				(number "5")
			)
			(pin input inverted
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "R")
				(number "4")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 3.81)
				(name "Q")
				(number "3")
			)
			(pin input line
				(at 12.7 0 180)
				(length 3.81)
				(name "DIS")
				(number "7")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 3.81)
				(name "THR")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM556"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LM556"
			(at -10.16 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm556.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Timer, DIP-14/SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual timer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* TSSOP*5.3x6.2mm*P0.65mm* SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LM556_0_0"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
		)
		(symbol "LM556_0_1")
		(symbol "LM556_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "TR")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 3.81)
				(name "CV")
				(number "3")
			)
			(pin input inverted
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "R")
				(number "4")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 3.81)
				(name "Q")
				(number "5")
			)
			(pin input line
				(at 12.7 0 180)
				(length 3.81)
				(name "DIS")
				(number "1")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 3.81)
				(name "THR")
				(number "2")
			)
		)
		(symbol "LM556_2_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "TR")
				(number "8")
			)
			(pin input line
				(at -12.7 0 0)
				(length 3.81)
				(name "CV")
				(number "11")
			)
			(pin input inverted
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "R")
				(number "10")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 3.81)
				(name "Q")
				(number "9")
			)
			(pin input line
				(at 12.7 0 180)
				(length 3.81)
				(name "DIS")
				(number "13")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 3.81)
				(name "THR")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LMC555xTP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LMC555xTP"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-8_1.43x1.41mm_Layout3x3_P0.5mm"
			(at 2.54 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmc555.pdf"
			(at 0 0 0)
		)
		(property "Description" "CMOS Timer, DSBGA-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single timer 555"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DSBGA*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LMC555xTP_0_0"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "A2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "A3")
			)
		)
		(symbol "LMC555xTP_0_1")
		(symbol "LMC555xTP_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "TR")
				(number "B3")
			)
			(pin input line
				(at -12.7 0 0)
				(length 3.81)
				(name "CV")
				(number "C1")
			)
			(pin input inverted
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "R")
				(number "C2")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 3.81)
				(name "Q")
				(number "C3")
			)
			(pin input line
				(at 12.7 0 180)
				(length 3.81)
				(name "DIS")
				(number "A1")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 3.81)
				(name "THR")
				(number "B1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC6902"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "LTC6902"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 0 11.43 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/6902f.pdf"
			(at -6.35 8.89 0)
		)
		(property "Description" "Multiphase oscillator, spread spectrum frequency modulation, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "clock generator dual triple quad signal"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC6902_0_1")
		(symbol "LTC6902_1_1"
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SET")
				(number "10")
			)
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "MOD")
				(number "9")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "DIV")
				(number "2")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "PH")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V+")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUT1")
				(number "4")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT2")
				(number "5")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT3")
				(number "6")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT4")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC6909"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "LTC6909"
			(at 5.08 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-16_3x4.039mm_P0.5mm"
			(at 0 13.97 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/6909fa.pdf"
			(at -6.35 11.43 0)
		)
		(property "Description" "Multiphase oscillator, spread spectrum frequency modulation, MSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "clock generator signal"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x4.039mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC6909_0_1")
		(symbol "LTC6909_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SET")
				(number "16")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "PH0")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "PH1")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "PH2")
				(number "15")
			)
			(pin passive line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "MOD")
				(number "14")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "V+A")
				(number "1")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V+D")
				(number "13")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin tri_state line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "OUT1")
				(number "5")
			)
			(pin tri_state line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUT2")
				(number "6")
			)
			(pin tri_state line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT3")
				(number "7")
			)
			(pin tri_state line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT4")
				(number "8")
			)
			(pin tri_state line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT5")
				(number "9")
			)
			(pin tri_state line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "OUT6")
				(number "10")
			)
			(pin tri_state line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "OUT7")
				(number "11")
			)
			(pin tri_state line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "OUT8")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC6993xS6-1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "LTC6993xS6-1"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/69931234fc.pdf"
			(at 1.27 2.54 0)
		)
		(property "Description" "TimerBlox Monostable Pulse Generator (One Shot), Rising-edge input, non-retriggerable, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Timer TimerBlox monostable pulse"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT*23*"
			(at 0 0 0)
		)
		(symbol "LTC6993xS6-1_0_1")
		(symbol "LTC6993xS6-1_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 3.81)
				(name "DIV")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "TRIG")
				(number "1")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 3.81)
				(name "SET")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 3.81)
				(name "OUT")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC6994xDCB-1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LTC6994xDCB-1"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6-1EP_3x2mm_P0.5mm_EP1.65x1.35mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/699412fb.pdf"
			(at -6.35 8.89 0)
		)
		(property "Description" "TimerBlox Delay Block, Programmable, Noise Discriminator, Rising or Falling Edge, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "TimerBlox delay block noise discriminator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC6994xDCB-1_0_1")
		(symbol "LTC6994xDCB-1_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 3.81)
				(name "DIV")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "IN")
				(number "4")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 3.81)
				(name "SET")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V+")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 10.16 0 180)
				(length 3.81)
				(name "OUT")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC6994xS6-1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LTC6994xS6-1"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/699412fb.pdf"
			(at -6.35 8.89 0)
		)
		(property "Description" "TimerBlox Delay Block, Programmable, Noise Discriminator, Rising or Falling Edge, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "TimerBlox delay block noise discriminator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT*23*"
			(at 0 0 0)
		)
		(symbol "LTC6994xS6-1_0_1")
		(symbol "LTC6994xS6-1_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 3.81)
				(name "DIV")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 3.81)
				(name "IN")
				(number "1")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 3.81)
				(name "SET")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "V+")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 3.81)
				(name "OUT")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MN3101"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MN3101"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 2.54 -9.525 0)
		)
		(property "Datasheet" "http://www.experimentalistsanonymous.com/diy/Datasheets/MN3101.pdf"
			(at 2.54 -12.065 0)
		)
		(property "Description" "Clock Generator Driver/Driver for MN3000 Series BBD (bucket brigade device), -8V to -16V, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Matsushita Panasonic BBD CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MN3101_0_1")
		(symbol "MN3101_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "OX1")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "OX2")
				(number "6")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "OX3")
				(number "5")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "VGG_OUT")
				(number "8")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "CP1")
				(number "2")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "CP2")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MN3102"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "MN3102"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 2.54 -9.525 0)
		)
		(property "Datasheet" "http://www.experimentalistsanonymous.com/diy/Datasheets/MN3102.pdf"
			(at 2.54 -12.065 0)
		)
		(property "Description" "Clock Generator Driver/Driver for MN3000 Series BBD (bucket brigade device), 4V to 10V, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Matsushita Panasonic BBD CMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MN3102_0_1")
		(symbol "MN3102_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "OX1")
				(number "7")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "OX2")
				(number "6")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "OX3")
				(number "5")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 10.16 0 180)
				(length 2.54)
				(name "VGG_OUT")
				(number "8")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "CP1")
				(number "2")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "CP2")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NE555D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "NE555D"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 21.59 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ne555.pdf"
			(at 21.59 -10.16 0)
		)
		(property "Description" "Precision Timers, 555 compatible, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single timer 555"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "NE555D_0_0"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
		)
		(symbol "NE555D_0_1")
		(symbol "NE555D_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "TR")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 3.81)
				(name "CV")
				(number "5")
			)
			(pin input inverted
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "R")
				(number "4")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 3.81)
				(name "Q")
				(number "3")
			)
			(pin input line
				(at 12.7 0 180)
				(length 3.81)
				(name "DIS")
				(number "7")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 3.81)
				(name "THR")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NE555P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "NE555P"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 16.51 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ne555.pdf"
			(at 21.59 -10.16 0)
		)
		(property "Description" "Precision Timers, 555 compatible,  PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single timer 555"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "NE555P_0_0"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
		)
		(symbol "NE555P_0_1")
		(symbol "NE555P_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "TR")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 3.81)
				(name "CV")
				(number "5")
			)
			(pin input inverted
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "R")
				(number "4")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 3.81)
				(name "Q")
				(number "3")
			)
			(pin input line
				(at 12.7 0 180)
				(length 3.81)
				(name "DIS")
				(number "7")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 3.81)
				(name "THR")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NE567"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 10.795 0)
		)
		(property "Value" "NE567"
			(at -2.54 8.89 0)
		)
		(property "Footprint" ""
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm567.pdf"
			(at -7.62 0 0)
		)
		(property "Description" "Tone Decoder/Phase-Locked Loop, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "tone decoder PLL"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "NE567_0_1")
		(symbol "NE567_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "INPUT")
				(number "3")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "TIM_R")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "TIM_RC")
				(number "6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "OUTPUT")
				(number "8")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "LP_FLT_C")
				(number "2")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "OFLT_C")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PL611-01-xxxT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "PL611-01-xxxT"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PL611-01.pdf"
			(at -6.35 8.89 0)
		)
		(property "Description" "Programmable Clock, Dual Programmable Clock Outputs, Up To 200MHz, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "clock generator dual programmable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "PL611-01-xxxT_0_1")
		(symbol "PL611-01-xxxT_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "XIN,FIN")
				(number "3")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "XOUT")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CLK1")
				(number "1")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "CLK2,OE,~{PDB},FSEL")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SY58031U"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 12.7 -31.75 0)
		)
		(property "Value" "SY58031U"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm_ThermalVias"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/sy58031u.pdf"
			(at 17.78 2.54 0)
		)
		(property "Description" "1:8 CML Fanout Buffer 75fsRMS, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "CML 2.5V/3.3V differential LVPECL LVDS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "SY58031U_0_1")
		(symbol "SY58031U_1_1"
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "IN")
				(number "3")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "~{IN}")
				(number "6")
			)
			(pin passive line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "VT")
				(number "4")
			)
			(pin passive line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "VREF-AC")
				(number "5")
			)
			(pin power_in line
				(at -10.16 33.02 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at -7.62 33.02 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at -5.08 33.02 270)
				(length 2.54)
				(name "VCC")
				(number "9")
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 2.54)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VCC")
				(number "18")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "24")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 2.54 33.02 270)
				(length 2.54)
				(name "VCC")
				(number "23")
			)
			(pin power_in line
				(at 5.08 33.02 270)
				(length 2.54)
				(name "VCC")
				(number "25")
			)
			(pin power_in line
				(at 7.62 33.02 270)
				(length 2.54)
				(name "VCC")
				(number "32")
			)
			(pin output line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "Q0")
				(number "31")
			)
			(pin output line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "~{Q0}")
				(number "30")
			)
			(pin output line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "Q1")
				(number "29")
			)
			(pin output line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "~{Q1}")
				(number "28")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "Q2")
				(number "27")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "~{Q2}")
				(number "26")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "Q3")
				(number "22")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "~{Q3}")
				(number "21")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "Q4")
				(number "20")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "~{Q4}")
				(number "19")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "Q5")
				(number "15")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "~{Q5}")
				(number "14")
			)
			(pin output line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "Q6")
				(number "13")
			)
			(pin output line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "~{Q6}")
				(number "12")
			)
			(pin output line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "Q7")
				(number "11")
			)
			(pin output line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "~{Q7}")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SY58032U"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 12.7 -31.75 0)
		)
		(property "Value" "SY58032U"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm_ThermalVias"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/sy58032u.pdf"
			(at 17.78 2.54 0)
		)
		(property "Description" "1:8 LVPECL Fanout Buffer 75fsRMS, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "2.5V/3.3V differential LVPECL LVDS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "SY58032U_0_1")
		(symbol "SY58032U_1_1"
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "IN")
				(number "3")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "~{IN}")
				(number "6")
			)
			(pin passive line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "VT")
				(number "4")
			)
			(pin passive line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "VREF-AC")
				(number "5")
			)
			(pin power_in line
				(at -10.16 33.02 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at -7.62 33.02 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at -5.08 33.02 270)
				(length 2.54)
				(name "VCC")
				(number "9")
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 2.54)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VCC")
				(number "18")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "24")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 2.54 33.02 270)
				(length 2.54)
				(name "VCC")
				(number "23")
			)
			(pin power_in line
				(at 5.08 33.02 270)
				(length 2.54)
				(name "VCC")
				(number "25")
			)
			(pin power_in line
				(at 7.62 33.02 270)
				(length 2.54)
				(name "VCC")
				(number "32")
			)
			(pin open_emitter line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "Q0")
				(number "31")
			)
			(pin open_emitter line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "~{Q0}")
				(number "30")
			)
			(pin open_emitter line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "Q1")
				(number "29")
			)
			(pin open_emitter line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "~{Q1}")
				(number "28")
			)
			(pin open_emitter line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "Q2")
				(number "27")
			)
			(pin open_emitter line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "~{Q2}")
				(number "26")
			)
			(pin open_emitter line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "Q3")
				(number "22")
			)
			(pin open_emitter line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "~{Q3}")
				(number "21")
			)
			(pin open_emitter line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "Q4")
				(number "20")
			)
			(pin open_emitter line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "~{Q4}")
				(number "19")
			)
			(pin open_emitter line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "Q5")
				(number "15")
			)
			(pin open_emitter line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "~{Q5}")
				(number "14")
			)
			(pin open_emitter line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "Q6")
				(number "13")
			)
			(pin open_emitter line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "~{Q6}")
				(number "12")
			)
			(pin open_emitter line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "Q7")
				(number "11")
			)
			(pin open_emitter line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "~{Q7}")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLC555xPW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "TLC555xPW"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlc555.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single LinCMOS Timer, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "single timer 555"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TLC555xPW_0_0"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
		)
		(symbol "TLC555xPW_0_1")
		(symbol "TLC555xPW_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "TR")
				(number "3")
			)
			(pin input line
				(at -12.7 0 0)
				(length 3.81)
				(name "CONT")
				(number "8")
			)
			(pin input inverted
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "RESET")
				(number "7")
			)
			(pin no_connect line
				(at -2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -2.54 0 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at 0 5.08 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 0 0 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin no_connect line
				(at 2.54 5.08 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 2.54 0 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 3.81)
				(name "OUT")
				(number "5")
			)
			(pin input line
				(at 12.7 0 180)
				(length 3.81)
				(name "DISCH")
				(number "12")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 3.81)
				(name "THRES")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPL5010"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "TPL5010"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tpl5010.pdf"
			(at -5.08 -7.62 0)
		)
		(property "Description" "Timer, Nano Power, Watchdog, 35 nA, 100 ms to 7200 s, VDD 1.8V to 5.5V, Iout max 1mA"
			(at 0 0 0)
		)
		(property "ki_keywords" "timer watchdog nano wake done"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TPL5010_0_1")
		(symbol "TPL5010_1_1"
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "DELAY/M_RST")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin open_collector line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "~{RST}")
				(number "6")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "DONE")
				(number "4")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "WAKE")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPL5110"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "TPL5110"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tpl5110.pdf"
			(at -5.08 -10.16 0)
		)
		(property "Description" "Timer, Nano Power, Active-Low, 35 nA, 100 ms to 7200 s, VDD 1.8V to 5.5V, Iout max 1mA, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "timer active-low nano wake done"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TPL5110_0_1")
		(symbol "TPL5110_1_1"
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "EN/ONE_SHOT")
				(number "6")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "DELAY/M_DRV")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "DRV")
				(number "5")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "DONE")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPL5111"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 11.43 0)
		)
		(property "Value" "TPL5111"
			(at 6.35 11.43 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tpl5111.pdf"
			(at -41.91 3.81 0)
		)
		(property "Description" "Timer, Nano Power, Active-High, 35 nA, 100 ms to 7200 s, VDD 1.8V to 5.5V, Iout max 1mA, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "timer active-high nano wake done"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TPL5111_0_1")
		(symbol "TPL5111_1_1"
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "EN/ONE_SHOT")
				(number "6")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "DELAY/M_DRV")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "~{DRV}")
				(number "5")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "DONE")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "8253"
		(extends "82C54")
		(property "Reference" "U"
			(at -5.08 24.13 0)
		)
		(property "Value" "8253"
			(at 2.54 24.13 0)
		)
		(property "Footprint" "Package_DIP:DIP-24_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.cpcwiki.eu/imgs/e/e3/8253.pdf"
			(at -11.43 22.86 0)
		)
		(property "Description" "Programmable Interval Timer, PDIP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Timer Counter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "8254"
		(extends "82C54")
		(property "Reference" "U"
			(at -5.08 24.13 0)
		)
		(property "Value" "8254"
			(at 2.54 24.13 0)
		)
		(property "Footprint" "Package_DIP:DIP-24_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.scs.stanford.edu/10wi-cs140/pintos/specs/8254.pdf"
			(at -11.43 22.86 0)
		)
		(property "Description" "Programmable Interval Timer, PDIP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Timer Counter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "CD4541BM"
		(extends "CD4541BE")
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "CD4541BM"
			(at 0 0 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/cd4541b.pdf"
			(at 0 0 0)
		)
		(property "Description" "20V, Programmable Timer, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "cmos"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "CD4541BPW"
		(extends "CD4541BE")
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "CD4541BPW"
			(at 0 0 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/cd4541b.pdf"
			(at 0 0 0)
		)
		(property "Description" "20V, Programmable Timer, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "cmos"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ICM7555xB"
		(extends "NE555D")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "ICM7555xB"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 21.59 -10.16 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/icm7/icm7555-56.pdf"
			(at 21.59 -10.16 0)
		)
		(property "Description" "CMOS General Purpose Timer, 555 compatible, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single timer 555"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ICM7555xP"
		(extends "NE555P")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "ICM7555xP"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 16.51 -10.16 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/icm7/icm7555-56.pdf"
			(at 21.59 -10.16 0)
		)
		(property "Description" "CMOS General Purpose Timer, 555 compatible, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single timer 555"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ICM7556"
		(extends "LM556")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "ICM7556"
			(at -10.16 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/icm7/icm7555-56.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual CMOS General Purpose Timer, DIP-14/SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual timer 556"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* TSSOP*5.3x6.2mm*P0.65mm* SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM555xM"
		(extends "NE555D")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LM555xM"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 21.59 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm555.pdf"
			(at 21.59 -10.16 0)
		)
		(property "Description" "Timer, 555 compatible, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single timer 555"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LM555xN"
		(extends "NE555P")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LM555xN"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 16.51 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm555.pdf"
			(at 21.59 -10.16 0)
		)
		(property "Description" "Timer, 555 compatible, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single timer 555"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LMC555xM"
		(extends "NE555D")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LMC555xM"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 21.59 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmc555.pdf"
			(at 21.59 -10.16 0)
		)
		(property "Description" "CMOS Timer, 555 compatible, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single timer 555"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LMC555xMM"
		(extends "LM555xMM")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LMC555xMM"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 16.51 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmc555.pdf"
			(at 21.59 -10.16 0)
		)
		(property "Description" "CMOS Timer, 555 compatible, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single timer 555"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LMC555xN"
		(extends "NE555P")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LMC555xN"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 16.51 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lmc555.pdf"
			(at 21.59 -10.16 0)
		)
		(property "Description" "CMOS Timer, 555 compatible, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single timer 555"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC6993xS6-2"
		(extends "LTC6993xS6-1")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "LTC6993xS6-2"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/69931234fc.pdf"
			(at 1.27 2.54 0)
		)
		(property "Description" "TimerBlox Monostable Pulse Generator (One Shot), Rising-edge input, retriggerable, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Timer TimerBlox monostable pulse"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT*23*"
			(at 0 0 0)
		)
	)
	(symbol "LTC6993xS6-3"
		(extends "LTC6993xS6-1")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "LTC6993xS6-3"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/69931234fc.pdf"
			(at 1.27 2.54 0)
		)
		(property "Description" "TimerBlox Monostable Pulse Generator (One Shot), Falling-edge input, non-retriggerable, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Timer TimerBlox monostable pulse"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT*23*"
			(at 0 0 0)
		)
	)
	(symbol "LTC6993xS6-4"
		(extends "LTC6993xS6-1")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "LTC6993xS6-4"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/69931234fc.pdf"
			(at 1.27 2.54 0)
		)
		(property "Description" "TimerBlox Monostable Pulse Generator (One Shot), Falling-edge input, retriggerable, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Timer TimerBlox monostable pulse"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT*23*"
			(at 0 0 0)
		)
	)
	(symbol "LTC6994xDCB-2"
		(extends "LTC6994xDCB-1")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LTC6994xDCB-2"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-6-1EP_3x2mm_P0.5mm_EP1.65x1.35mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/699412fb.pdf"
			(at -6.35 8.89 0)
		)
		(property "Description" "TimerBlox Debouncer, Programmable, Noise Discriminator, Rising and Falling Edges, DFN-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "TimerBlox debouncer noise discriminator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC6994xS6-2"
		(extends "LTC6994xS6-1")
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "LTC6994xS6-2"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-6"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/699412fb.pdf"
			(at -6.35 8.89 0)
		)
		(property "Description" "TimerBlox Debouncer, Programmable, Noise Discriminator, Rising and Falling Edges, TSOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "TimerBlox debouncer noise discriminator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT*23*"
			(at 0 0 0)
		)
	)
	(symbol "MC14541BD"
		(extends "CD4541BE")
		(property "Reference" "U"
			(at -7.62 15.24 0)
		)
		(property "Value" "MC14541BD"
			(at 7.62 15.24 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/mc14541b-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "18V, Programmable Timer, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "cmos"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC14541BDT"
		(extends "CD4541BE")
		(property "Reference" "U"
			(at -7.62 15.24 0)
		)
		(property "Value" "MC14541BDT"
			(at 7.62 15.24 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/mc14541b-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "18V, Programmable Timer, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "cmos"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC1455B"
		(extends "NE555D")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "MC1455B"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 21.59 -10.16 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC1455-D.PDF"
			(at 21.59 -10.16 0)
		)
		(property "Description" "Timer, 555 compatible, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single timer 555"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC1455P"
		(extends "NE555P")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "MC1455P"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 16.51 -10.16 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC1455-D.PDF"
			(at 21.59 -10.16 0)
		)
		(property "Description" "Timer, 555 compatible, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single timer 555"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "NA555D"
		(extends "NE555D")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "NA555D"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 21.59 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ne555.pdf"
			(at 21.59 -10.16 0)
		)
		(property "Description" "Precision Timers, 555 compatible, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single timer 555"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "NA555P"
		(extends "NE555P")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "NA555P"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 16.51 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ne555.pdf"
			(at 21.59 -10.16 0)
		)
		(property "Description" "Precision Timers, 555 compatible, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single timer 555"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "NA556"
		(extends "LM556")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "NA556"
			(at -10.16 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/se556.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Precision Timers, DIP-14/SOIC-14/SSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual timer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* TSSOP*5.3x6.2mm*P0.65mm* SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "NE556"
		(extends "LM556")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "NE556"
			(at -10.16 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ne556.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Precision Timers, DIP-14/SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual timer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* TSSOP*5.3x6.2mm*P0.65mm* SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "NLV14541BD"
		(extends "CD4541BE")
		(property "Reference" "U"
			(at -7.62 15.24 0)
		)
		(property "Value" "NLV14541BD"
			(at 7.62 15.24 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/mc14541b-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "18V, Programmable Timer, AEC Q100, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "cmos"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "NLV14541BDT"
		(extends "CD4541BE")
		(property "Reference" "U"
			(at -7.62 15.24 0)
		)
		(property "Value" "NLV14541BDT"
			(at 7.62 15.24 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/mc14541b-d.pdf"
			(at 0 0 0)
		)
		(property "Description" "18V, Programmable Timer, AEC Q100, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "cmos"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "SA555D"
		(extends "NE555D")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "SA555D"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 21.59 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ne555.pdf"
			(at 21.59 -10.16 0)
		)
		(property "Description" "Precision Timers, 555 compatible, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single timer 555"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "SA555P"
		(extends "NE555P")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "SA555P"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 16.51 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ne555.pdf"
			(at 21.59 -10.16 0)
		)
		(property "Description" "Precision Timers, 555 compatible, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single timer 555"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "SA556"
		(extends "LM556")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "SA556"
			(at -10.16 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ne556.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Precision Timers, DIP-14/SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual timer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* TSSOP*5.3x6.2mm*P0.65mm* SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "SE555D"
		(extends "NE555D")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "SE555D"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 21.59 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ne555.pdf"
			(at 21.59 -10.16 0)
		)
		(property "Description" "Precision Timers, 555 compatible, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single timer 555"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "SE555P"
		(extends "NE555P")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "SE555P"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 16.51 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ne555.pdf"
			(at 21.59 -10.16 0)
		)
		(property "Description" "Precision Timers, 555 compatible, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single timer 555"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "SE556"
		(extends "LM556")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "SE556"
			(at -10.16 -8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ne556.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Precision Timers, DIP-14/SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "dual timer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* TSSOP*5.3x6.2mm*P0.65mm* SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "SE567"
		(extends "NE567")
		(property "Reference" "U"
			(at -2.54 10.795 0)
		)
		(property "Value" "SE567"
			(at -2.54 8.89 0)
		)
		(property "Footprint" ""
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm567.pdf"
			(at -7.62 0 0)
		)
		(property "Description" "Tone Decoder/Phase-Locked Loop, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "tone decoder PLL"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "SY58033U"
		(extends "SY58032U")
		(property "Reference" "U"
			(at 12.7 -31.75 0)
		)
		(property "Value" "SY58033U"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm_ThermalVias"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/sy58033u.pdf"
			(at 17.78 2.54 0)
		)
		(property "Description" "1:8 400mV LVPECL Fanout Buffer 75fsRMS, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "2.5V/3.3V differential LVPECL LVDS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLC555xD"
		(extends "NE555D")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "TLC555xD"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 21.59 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlc555.pdf"
			(at 21.59 -10.16 0)
		)
		(property "Description" "Single LinCMOS Timer, 555 compatible, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single timer 555"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLC555xP"
		(extends "NE555P")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "TLC555xP"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 16.51 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlc555.pdf"
			(at 21.59 -10.16 0)
		)
		(property "Description" "Single LinCMOS Timer, 555 compatible, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single timer 555"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLC555xPS"
		(extends "LM555xMM")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "TLC555xPS"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 16.51 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tlc555.pdf"
			(at 21.59 -10.16 0)
		)
		(property "Description" "Single LinCMOS Timer, 555 compatible, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "single timer 555"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
)
