(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "ADF4002BCPZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 12.7 16.51 0)
		)
		(property "Value" "ADF4002BCPZ"
			(at 0 0 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-20-1EP_4x4mm_P0.5mm_EP2.1x2.1mm"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADF4002.pdf"
			(at 0 0 0)
		)
		(property "Description" "400MHz Bandwidth Frequency Synthesizer, LFCSP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Analog Devices PFD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ADF4002BCPZ_0_1")
		(symbol "ADF4002BCPZ_1_1"
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "REFIN")
				(number "8")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "RFINA")
				(number "5")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "RFINB")
				(number "4")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "CLK")
				(number "12")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "DATA")
				(number "13")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "LE")
				(number "14")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "CE")
				(number "11")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "RSET")
				(number "19")
			)
			(pin power_in line
				(at -5.08 17.78 270)
				(length 2.54)
				(name "DVDD")
				(number "16")
			)
			(pin passive line
				(at -5.08 17.78 270)
				(length 2.54)
				(hide yes)
				(name "DVDD")
				(number "17")
			)
			(pin passive line
				(at -5.08 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "DGND")
				(number "10")
			)
			(pin power_in line
				(at -5.08 -17.78 90)
				(length 2.54)
				(name "DGND")
				(number "9")
			)
			(pin passive line
				(at 0 17.78 270)
				(length 2.54)
				(hide yes)
				(name "AVDD")
				(number "6")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "AVDD")
				(number "7")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "AGND")
				(number "2")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "21")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "3")
			)
			(pin power_in line
				(at 5.08 17.78 270)
				(length 2.54)
				(name "VP")
				(number "18")
			)
			(pin power_in line
				(at 5.08 -17.78 90)
				(length 2.54)
				(name "CPGND")
				(number "1")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "CP")
				(number "20")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "MUXOUT")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADF4002BRUZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 12.7 16.51 0)
		)
		(property "Value" "ADF4002BRUZ"
			(at 0 0 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADF4002.pdf"
			(at 0 0 0)
		)
		(property "Description" "400MHz Bandwidth Frequency Synthesizer, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Analog Devices PFD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADF4002BRUZ_0_1")
		(symbol "ADF4002BRUZ_1_1"
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "REFIN")
				(number "8")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "RFINA")
				(number "6")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "RFINB")
				(number "5")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "CLK")
				(number "11")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "DATA")
				(number "12")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "LE")
				(number "13")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "CE")
				(number "10")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "RSET")
				(number "1")
			)
			(pin power_in line
				(at -5.08 17.78 270)
				(length 2.54)
				(name "DVDD")
				(number "15")
			)
			(pin power_in line
				(at -5.08 -17.78 90)
				(length 2.54)
				(name "DGND")
				(number "9")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "AVDD")
				(number "7")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "AGND")
				(number "4")
			)
			(pin power_in line
				(at 5.08 17.78 270)
				(length 2.54)
				(name "VP")
				(number "16")
			)
			(pin power_in line
				(at 5.08 -17.78 90)
				(length 2.54)
				(name "CPGND")
				(number "3")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "CP")
				(number "2")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "MUXOUT")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADF4158"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "ADF4158"
			(at 0 0 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-24-1EP_4x4mm_P0.5mm_EP2.5x2.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADF4158.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.5-6.1GHz fractional-N PLL, LFCSP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "fractional-N PLL"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ADF4158_0_1")
		(symbol "ADF4158_1_1"
			(pin input line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "CE")
				(number "13")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "REFIN")
				(number "9")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "TXDATA")
				(number "12")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "CLK")
				(number "14")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "DATA")
				(number "15")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "LE")
				(number "16")
			)
			(pin passive line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "RSET")
				(number "23")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "AVDD")
				(number "6")
			)
			(pin passive line
				(at -2.54 17.78 270)
				(length 2.54)
				(hide yes)
				(name "AVDD")
				(number "7")
			)
			(pin passive line
				(at -2.54 17.78 270)
				(length 2.54)
				(hide yes)
				(name "AVDD")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "CPGND")
				(number "1")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "SDVDD")
				(number "18")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "AGND")
				(number "2")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "25")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "3")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "DVDD")
				(number "19")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "DGND")
				(number "10")
			)
			(pin power_in line
				(at 5.08 17.78 270)
				(length 2.54)
				(name "VP")
				(number "22")
			)
			(pin power_in line
				(at 5.08 -17.78 90)
				(length 2.54)
				(name "SDGND")
				(number "11")
			)
			(pin passive line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "SW2")
				(number "21")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "CP")
				(number "24")
			)
			(pin passive line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "SW1")
				(number "20")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "MUXOUT")
				(number "17")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "RFINB")
				(number "4")
			)
			(pin input line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "RFINA")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADF4351"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ADF4351"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-32-1EP_5x5mm_P0.5mm_EP3.25x3.25mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADF4351.pdf"
			(at 0 0 0)
		)
		(property "Description" "35-4400MHz fractional-N PLL, LFCSP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "fractional-N PLL"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*32*1EP*5x5mm*P0.5mm*EP3.25x3.25mm*"
			(at 0 0 0)
		)
		(symbol "ADF4351_0_1")
		(symbol "ADF4351_1_1"
			(pin input line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "CLK")
				(number "1")
			)
			(pin input line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "DATA")
				(number "2")
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "LE")
				(number "3")
			)
			(pin input line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "CE")
				(number "4")
			)
			(pin input line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PDB_RF")
				(number "26")
			)
			(pin input line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "REFIN")
				(number "29")
			)
			(pin input line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "TEMP")
				(number "19")
			)
			(pin input line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "VCOM")
				(number "23")
			)
			(pin input line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "VREF")
				(number "24")
			)
			(pin input line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "RSET")
				(number "22")
			)
			(pin power_in line
				(at -10.16 27.94 270)
				(length 2.54)
				(name "Vp")
				(number "6")
			)
			(pin power_in line
				(at -10.16 -27.94 90)
				(length 2.54)
				(name "CPGND")
				(number "8")
			)
			(pin power_in line
				(at -7.62 27.94 270)
				(length 2.54)
				(name "AVDD")
				(number "10")
			)
			(pin power_in line
				(at -7.62 -27.94 90)
				(length 2.54)
				(name "AGND")
				(number "9")
			)
			(pin power_in line
				(at -5.08 -27.94 90)
				(length 2.54)
				(name "AGNDVCO")
				(number "11")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VVCO")
				(number "16")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 2.54)
				(name "AGNDVCO")
				(number "18")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VVCO")
				(number "17")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "AGNDVCO")
				(number "21")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "DVDD")
				(number "28")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 2.54)
				(name "DGND")
				(number "27")
			)
			(pin power_in line
				(at 5.08 -27.94 90)
				(length 2.54)
				(name "SDGND")
				(number "31")
			)
			(pin power_in line
				(at 7.62 27.94 270)
				(length 2.54)
				(name "SDVDD")
				(number "32")
			)
			(pin power_in line
				(at 7.62 -27.94 90)
				(length 2.54)
				(name "EP")
				(number "33")
			)
			(pin input line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "LD")
				(number "25")
			)
			(pin output line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "MUXOUT")
				(number "30")
			)
			(pin output line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "RF_OUT_A+")
				(number "12")
			)
			(pin output line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "RF_OUT_A-")
				(number "13")
			)
			(pin output line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "RF_OUT_B+")
				(number "14")
			)
			(pin output line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "RF_OUT_B-")
				(number "15")
			)
			(pin input line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "VTUNE")
				(number "20")
			)
			(pin input line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "CPout")
				(number "7")
			)
			(pin input line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "SW")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CDCVF2505"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "CDCVF2505"
			(at 10.16 8.89 0)
		)
		(property "Footprint" ""
			(at -10.16 7.62 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/cdcvf2505.pdf"
			(at -10.16 7.62 0)
		)
		(property "Description" "Clock Phase-Lock Loop Clock Driver, 24-200MHz, 3.3V, SOIC-8/TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "pll clock driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "CDCVF2505_0_1")
		(symbol "CDCVF2505_1_1"
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "CLKIN")
				(number "1")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "CLKOUT")
				(number "8")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "1Y0")
				(number "3")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 2.54)
				(name "1Y1")
				(number "2")
			)
			(pin tri_state line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "1Y3")
				(number "7")
			)
			(pin tri_state line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "1Y2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CS2000-CP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "CS2000-CP"
			(at 7.62 13.97 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 20.32 -11.43 0)
		)
		(property "Datasheet" "https://statics.cirrus.com/pubs/proDatasheet/CS2000-CP_F3.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Fractional-N Clock Synthesizer & Clock Multiplier, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Clock Synthesizer Multiplier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "CS2000-CP_0_1")
		(symbol "CS2000-CP_1_1"
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "SDA/CDIN")
				(number "10")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "SCL/CCLK")
				(number "9")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "AD0/~{CS}")
				(number "8")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "CLK_IN")
				(number "5")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "XTI/REF_CLK")
				(number "7")
			)
			(pin output line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "XTO")
				(number "6")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VD")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "CLK_OUT")
				(number "3")
			)
			(pin output line
				(at 17.78 0 180)
				(length 2.54)
				(name "AUX_OUT")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ICS525-01R"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 36.83 0)
		)
		(property "Value" "ICS525-01R"
			(at 7.62 -36.83 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_3.9x9.9mm_P0.635mm"
			(at 0 -50.8 0)
		)
		(property "Datasheet" "https://www.idt.com/document/dst/525-01-02-datasheet"
			(at 0 0 0)
		)
		(property "Description" "User configurable clock up to 160 MHz, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Configurable clock"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x9.9mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "ICS525-01R_0_1")
		(symbol "ICS525-01R_1_1"
			(pin input line
				(at -10.16 30.48 0)
				(length 2.54)
				(name "X1/ICLK")
				(number "7")
			)
			(pin output line
				(at -10.16 27.94 0)
				(length 2.54)
				(name "X2")
				(number "8")
			)
			(pin input line
				(at -10.16 22.86 0)
				(length 2.54)
				(name "R0")
				(number "24")
			)
			(pin input line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "R1")
				(number "25")
			)
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "R2")
				(number "26")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "R3")
				(number "27")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "R4")
				(number "28")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "R5")
				(number "1")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "R6")
				(number "2")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "S0")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "S1")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "S2")
				(number "5")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "V0")
				(number "10")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "V1")
				(number "11")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "V2")
				(number "12")
			)
			(pin input line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "V3")
				(number "13")
			)
			(pin input line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "V4")
				(number "14")
			)
			(pin input line
				(at -10.16 -20.32 0)
				(length 2.54)
				(name "V5")
				(number "15")
			)
			(pin input line
				(at -10.16 -22.86 0)
				(length 2.54)
				(name "V6")
				(number "16")
			)
			(pin input line
				(at -10.16 -25.4 0)
				(length 2.54)
				(name "V7")
				(number "17")
			)
			(pin input line
				(at -10.16 -27.94 0)
				(length 2.54)
				(name "V8")
				(number "18")
			)
			(pin input line
				(at -10.16 -33.02 0)
				(length 2.54)
				(name "~{PD}")
				(number "19")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "20")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "23")
			)
			(pin tri_state line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "CLK")
				(number "21")
			)
			(pin tri_state line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "REF")
				(number "22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Si5342A-D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "Si5342A-D"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/Si5345-44-42-D-DataSheet.pdf"
			(at -2.54 25.4 0)
		)
		(property "Description" "Jitter Attenuator/Clock Multiplier, 2 channel, Fractional, 0.001-1028 MHz, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Clock Jitter Attenuator Multiplier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "Si5342A-D_0_1")
		(symbol "Si5342A-D_1_1"
			(pin input line
				(at -20.32 35.56 0)
				(length 2.54)
				(name "IN0")
				(number "43")
			)
			(pin input line
				(at -20.32 33.02 0)
				(length 2.54)
				(name "IN0b")
				(number "44")
			)
			(pin input line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "IN1")
				(number "1")
			)
			(pin input line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "IN1b")
				(number "2")
			)
			(pin input line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "IN2")
				(number "10")
			)
			(pin input line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "IN2b")
				(number "11")
			)
			(pin input line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "IN3/FB_IN")
				(number "41")
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "IN3b/FB_INb")
				(number "42")
			)
			(pin input line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "X1")
				(number "4")
			)
			(pin input line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "XA")
				(number "5")
			)
			(pin input line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "XB")
				(number "6")
			)
			(pin input line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "X2")
				(number "7")
			)
			(pin input line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "~{RST}")
				(number "17")
			)
			(pin input line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "~{OE}")
				(number "12")
			)
			(pin input line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "IN_SEL0")
				(number "3")
			)
			(pin input line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "IN_SEL1")
				(number "37")
			)
			(pin input line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "I2C_SEL")
				(number "38")
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "SDA/SDIO")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "A1/SDO")
				(number "15")
			)
			(pin input line
				(at -20.32 -33.02 0)
				(length 2.54)
				(name "SCLK")
				(number "14")
			)
			(pin input line
				(at -20.32 -35.56 0)
				(length 2.54)
				(name "A0/~{CS}")
				(number "16")
			)
			(pin power_in line
				(at -7.62 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "8")
			)
			(pin passive line
				(at -7.62 40.64 270)
				(length 2.54)
				(hide yes)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "21")
			)
			(pin passive line
				(at -5.08 40.64 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "32")
			)
			(pin passive line
				(at -5.08 40.64 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "39")
			)
			(pin passive line
				(at -5.08 40.64 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "40")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDDS")
				(number "26")
			)
			(pin passive line
				(at 0 40.64 270)
				(length 2.54)
				(hide yes)
				(name "VDDS")
				(number "29")
			)
			(pin passive line
				(at 0 40.64 270)
				(length 2.54)
				(hide yes)
				(name "VDDS")
				(number "34")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "GND")
				(number "45")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDO0")
				(number "18")
			)
			(pin power_in line
				(at 7.62 40.64 270)
				(length 2.54)
				(name "VDDO1")
				(number "23")
			)
			(pin no_connect line
				(at 17.78 -35.56 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "22")
			)
			(pin output line
				(at 20.32 35.56 180)
				(length 2.54)
				(name "OUT0")
				(number "20")
			)
			(pin output line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "OUT0b")
				(number "19")
			)
			(pin output line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "OUT1")
				(number "25")
			)
			(pin output line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "OUT1b")
				(number "24")
			)
			(pin output line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "~{LOS0}")
				(number "30")
			)
			(pin output line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "~{LOS1}")
				(number "31")
			)
			(pin output line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "~{LOS2}")
				(number "35")
			)
			(pin output line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "~{LOS3}")
				(number "36")
			)
			(pin output line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "~{LOS_XAXB}")
				(number "28")
			)
			(pin output line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "~{INTR}")
				(number "33")
			)
			(pin output line
				(at 20.32 0 180)
				(length 2.54)
				(name "~{LOL}")
				(number "27")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Si5344A-D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "Si5344A-D"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/Si5345-44-42-D-DataSheet.pdf"
			(at -2.54 25.4 0)
		)
		(property "Description" "Jitter Attenuator/Clock Multiplier, 4 channel, Fractional, 0.001-1028 MHz, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Clock Jitter Attenuator Multiplier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "Si5344A-D_0_1")
		(symbol "Si5344A-D_1_1"
			(pin input line
				(at -22.86 35.56 0)
				(length 2.54)
				(name "IN0")
				(number "43")
			)
			(pin input line
				(at -22.86 33.02 0)
				(length 2.54)
				(name "IN0b")
				(number "44")
			)
			(pin input line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "IN1")
				(number "1")
			)
			(pin input line
				(at -22.86 25.4 0)
				(length 2.54)
				(name "IN1b")
				(number "2")
			)
			(pin input line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "IN2")
				(number "10")
			)
			(pin input line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "IN2b")
				(number "11")
			)
			(pin input line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "IN3/FB_IN")
				(number "41")
			)
			(pin input line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "IN3b/FB_INb")
				(number "42")
			)
			(pin input line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "X1")
				(number "4")
			)
			(pin input line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "XA")
				(number "5")
			)
			(pin input line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "XB")
				(number "6")
			)
			(pin input line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "X2")
				(number "7")
			)
			(pin input line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "~{RST}")
				(number "17")
			)
			(pin input line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "~{OE}")
				(number "12")
			)
			(pin input line
				(at -22.86 -17.78 0)
				(length 2.54)
				(name "IN_SEL0")
				(number "3")
			)
			(pin input line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "IN_SEL1")
				(number "37")
			)
			(pin input line
				(at -22.86 -25.4 0)
				(length 2.54)
				(name "I2C_SEL")
				(number "38")
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 2.54)
				(name "SDA/SDIO")
				(number "13")
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 2.54)
				(name "A1/SDO")
				(number "15")
			)
			(pin input line
				(at -22.86 -33.02 0)
				(length 2.54)
				(name "SCLK")
				(number "14")
			)
			(pin input line
				(at -22.86 -35.56 0)
				(length 2.54)
				(name "A0/~{CS}")
				(number "16")
			)
			(pin power_in line
				(at -10.16 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "8")
			)
			(pin passive line
				(at -10.16 40.64 270)
				(length 2.54)
				(hide yes)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at -7.62 40.64 270)
				(length 2.54)
				(name "VDD")
				(number "21")
			)
			(pin passive line
				(at -7.62 40.64 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "32")
			)
			(pin passive line
				(at -7.62 40.64 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "39")
			)
			(pin passive line
				(at -7.62 40.64 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "40")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDDS")
				(number "26")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "GND")
				(number "45")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDDO0")
				(number "18")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "VDDO1")
				(number "23")
			)
			(pin power_in line
				(at 7.62 40.64 270)
				(length 2.54)
				(name "VDDO2")
				(number "29")
			)
			(pin power_in line
				(at 10.16 40.64 270)
				(length 2.54)
				(name "VDDO3")
				(number "34")
			)
			(pin no_connect line
				(at 20.32 -35.56 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "22")
			)
			(pin output line
				(at 22.86 35.56 180)
				(length 2.54)
				(name "OUT0")
				(number "20")
			)
			(pin output line
				(at 22.86 33.02 180)
				(length 2.54)
				(name "OUT0b")
				(number "19")
			)
			(pin output line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "OUT1")
				(number "25")
			)
			(pin output line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "OUT1b")
				(number "24")
			)
			(pin output line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "OUT2")
				(number "31")
			)
			(pin output line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "OUT2b")
				(number "30")
			)
			(pin output line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "OUT3")
				(number "36")
			)
			(pin output line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "OUT3b")
				(number "35")
			)
			(pin output line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "~{LOS_XAXB}")
				(number "28")
			)
			(pin output line
				(at 22.86 0 180)
				(length 2.54)
				(name "~{INTR}")
				(number "33")
			)
			(pin output line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "~{LOL}")
				(number "27")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Si5345A-D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "Si5345A-D"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.2x5.2mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/Si5345-44-42-D-DataSheet.pdf"
			(at -2.54 27.94 0)
		)
		(property "Description" "Jitter Attenuator/Clock Multiplier, 10-channel, Fractional, 0.001-1028 MHz, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Clock Jitter Attenuator Multiplier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "Si5345A-D_0_1")
		(symbol "Si5345A-D_1_1"
			(pin input line
				(at -27.94 40.64 0)
				(length 2.54)
				(name "IN0")
				(number "63")
			)
			(pin input line
				(at -27.94 38.1 0)
				(length 2.54)
				(name "IN0b")
				(number "64")
			)
			(pin input line
				(at -27.94 33.02 0)
				(length 2.54)
				(name "IN1")
				(number "1")
			)
			(pin input line
				(at -27.94 30.48 0)
				(length 2.54)
				(name "IN1b")
				(number "2")
			)
			(pin input line
				(at -27.94 25.4 0)
				(length 2.54)
				(name "IN2")
				(number "14")
			)
			(pin input line
				(at -27.94 22.86 0)
				(length 2.54)
				(name "IN2b")
				(number "15")
			)
			(pin input line
				(at -27.94 17.78 0)
				(length 2.54)
				(name "IN3/FB_IN")
				(number "61")
			)
			(pin input line
				(at -27.94 15.24 0)
				(length 2.54)
				(name "IN3b/FB_INb")
				(number "62")
			)
			(pin input line
				(at -27.94 10.16 0)
				(length 2.54)
				(name "X1")
				(number "7")
			)
			(pin input line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "XA")
				(number "8")
			)
			(pin input line
				(at -27.94 0 0)
				(length 2.54)
				(name "XB")
				(number "9")
			)
			(pin input line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "X2")
				(number "10")
			)
			(pin input line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "~{RST}")
				(number "6")
			)
			(pin input line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "~{OE}")
				(number "11")
			)
			(pin input line
				(at -27.94 -15.24 0)
				(length 2.54)
				(name "IN_SEL0")
				(number "3")
			)
			(pin input line
				(at -27.94 -17.78 0)
				(length 2.54)
				(name "IN_SEL1")
				(number "4")
			)
			(pin input line
				(at -27.94 -22.86 0)
				(length 2.54)
				(name "FINC")
				(number "48")
			)
			(pin input line
				(at -27.94 -25.4 0)
				(length 2.54)
				(name "FDEC")
				(number "25")
			)
			(pin input line
				(at -27.94 -30.48 0)
				(length 2.54)
				(name "I2C_SEL")
				(number "39")
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 2.54)
				(name "SDA/SDIO")
				(number "18")
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 2.54)
				(name "A1/SDO")
				(number "17")
			)
			(pin input line
				(at -27.94 -38.1 0)
				(length 2.54)
				(name "SCLK")
				(number "16")
			)
			(pin input line
				(at -27.94 -40.64 0)
				(length 2.54)
				(name "A0/~{CS}")
				(number "19")
			)
			(pin power_in line
				(at -15.24 45.72 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at -12.7 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin passive line
				(at -12.7 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "46")
			)
			(pin passive line
				(at -12.7 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "60")
			)
			(pin power_in line
				(at -7.62 45.72 270)
				(length 2.54)
				(name "VDDO0")
				(number "22")
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 2.54)
				(name "VDDO1")
				(number "26")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDDO2")
				(number "29")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDDO3")
				(number "33")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "GND")
				(number "65")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDDO4")
				(number "36")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VDDO5")
				(number "40")
			)
			(pin power_in line
				(at 7.62 45.72 270)
				(length 2.54)
				(name "VDDO6")
				(number "43")
			)
			(pin power_in line
				(at 10.16 45.72 270)
				(length 2.54)
				(name "VDDO7")
				(number "49")
			)
			(pin power_in line
				(at 12.7 45.72 270)
				(length 2.54)
				(name "VDDO8")
				(number "52")
			)
			(pin power_in line
				(at 15.24 45.72 270)
				(length 2.54)
				(name "VDDO9")
				(number "57")
			)
			(pin no_connect line
				(at 25.4 35.56 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 25.4 27.94 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin no_connect line
				(at 25.4 20.32 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "21")
			)
			(pin no_connect line
				(at 25.4 12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "55")
			)
			(pin no_connect line
				(at 25.4 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "56")
			)
			(pin output line
				(at 27.94 40.64 180)
				(length 2.54)
				(name "OUT0")
				(number "24")
			)
			(pin output line
				(at 27.94 38.1 180)
				(length 2.54)
				(name "OUT0b")
				(number "23")
			)
			(pin output line
				(at 27.94 33.02 180)
				(length 2.54)
				(name "OUT1")
				(number "28")
			)
			(pin output line
				(at 27.94 30.48 180)
				(length 2.54)
				(name "OUT1b")
				(number "27")
			)
			(pin output line
				(at 27.94 25.4 180)
				(length 2.54)
				(name "OUT2")
				(number "31")
			)
			(pin output line
				(at 27.94 22.86 180)
				(length 2.54)
				(name "OUT2b")
				(number "30")
			)
			(pin output line
				(at 27.94 17.78 180)
				(length 2.54)
				(name "OUT3")
				(number "35")
			)
			(pin output line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "OUT3b")
				(number "34")
			)
			(pin output line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "OUT4")
				(number "38")
			)
			(pin output line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "OUT4b")
				(number "37")
			)
			(pin output line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "OUT5")
				(number "42")
			)
			(pin output line
				(at 27.94 0 180)
				(length 2.54)
				(name "OUT5b")
				(number "41")
			)
			(pin output line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "OUT6")
				(number "45")
			)
			(pin output line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "OUT6b")
				(number "44")
			)
			(pin output line
				(at 27.94 -12.7 180)
				(length 2.54)
				(name "OUT7")
				(number "51")
			)
			(pin output line
				(at 27.94 -15.24 180)
				(length 2.54)
				(name "OUT7b")
				(number "50")
			)
			(pin output line
				(at 27.94 -20.32 180)
				(length 2.54)
				(name "OUT8")
				(number "54")
			)
			(pin output line
				(at 27.94 -22.86 180)
				(length 2.54)
				(name "OUT8b")
				(number "53")
			)
			(pin output line
				(at 27.94 -27.94 180)
				(length 2.54)
				(name "OUT9")
				(number "59")
			)
			(pin output line
				(at 27.94 -30.48 180)
				(length 2.54)
				(name "OUT9b")
				(number "58")
			)
			(pin output line
				(at 27.94 -38.1 180)
				(length 2.54)
				(name "~{INTR}")
				(number "12")
			)
			(pin output line
				(at 27.94 -40.64 180)
				(length 2.54)
				(name "~{LOL}")
				(number "47")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADF4350"
		(extends "ADF4351")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ADF4350"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-32-1EP_5x5mm_P0.5mm_EP3.25x3.25mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADF4350.pdf"
			(at 0 0 0)
		)
		(property "Description" "137.5-4400MHz fractional-N PLL, LFCSP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "fractional-N PLL"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*32*1EP*5x5mm*P0.5mm*EP3.25x3.25mm*"
			(at 0 0 0)
		)
	)
	(symbol "ICS525R-02"
		(extends "ICS525-01R")
		(property "Reference" "U"
			(at -5.08 36.83 0)
		)
		(property "Value" "ICS525R-02"
			(at 7.62 -36.83 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_3.9x9.9mm_P0.635mm"
			(at 0 -50.8 0)
		)
		(property "Datasheet" "https://www.idt.com/document/dst/525-01-02-datasheet"
			(at 0 0 0)
		)
		(property "Description" "User configurable clock up to 200 MHz, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Configurable clock"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x9.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si5342B-D"
		(extends "Si5342A-D")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "Si5342B-D"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/Si5345-44-42-D-DataSheet.pdf"
			(at -2.54 25.4 0)
		)
		(property "Description" "Jitter Attenuator/Clock Multiplier, 2 channel, Fractional, 0.001-350 MHz, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Clock Jitter Attenuator Multiplier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si5342C-D"
		(extends "Si5342A-D")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "Si5342C-D"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/Si5345-44-42-D-DataSheet.pdf"
			(at -2.54 25.4 0)
		)
		(property "Description" "Jitter Attenuator/Clock Multiplier, 2 channel, Integer, 0.001-1028 MHz, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Clock Jitter Attenuator Multiplier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si5342D-D"
		(extends "Si5342A-D")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "Si5342D-D"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/Si5345-44-42-D-DataSheet.pdf"
			(at -2.54 25.4 0)
		)
		(property "Description" "Jitter Attenuator/Clock Multiplier, 2 channel, Integer, 0.001-350 MHz, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Clock Jitter Attenuator Multiplier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si5344B-D"
		(extends "Si5344A-D")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "Si5344B-D"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/Si5345-44-42-D-DataSheet.pdf"
			(at -2.54 25.4 0)
		)
		(property "Description" "Jitter Attenuator/Clock Multiplier, 4 channel, Fractional, 0.001-350 MHz, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Clock Jitter Attenuator Multiplier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si5344C-D"
		(extends "Si5344A-D")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "Si5344C-D"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/Si5345-44-42-D-DataSheet.pdf"
			(at -2.54 25.4 0)
		)
		(property "Description" "Jitter Attenuator/Clock Multiplier, 4 channel, Integer, 0.001-1028 MHz, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Clock Jitter Attenuator Multiplier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si5344D-D"
		(extends "Si5344A-D")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "Si5344D-D"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/Si5345-44-42-D-DataSheet.pdf"
			(at -2.54 25.4 0)
		)
		(property "Description" "Jitter Attenuator/Clock Multiplier, 4 channel, Integer, 0.001-350 MHz, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Clock Jitter Attenuator Multiplier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si5345B-D"
		(extends "Si5345A-D")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "Si5345B-D"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.2x5.2mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/Si5345-44-42-D-DataSheet.pdf"
			(at -2.54 27.94 0)
		)
		(property "Description" "Jitter Attenuator/Clock Multiplier, 10-channel, Fractional, 0.001-350 MHz, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Clock Jitter Attenuator Multiplier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si5345C-D"
		(extends "Si5345A-D")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "Si5345C-D"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.2x5.2mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/Si5345-44-42-D-DataSheet.pdf"
			(at -2.54 27.94 0)
		)
		(property "Description" "Jitter Attenuator/Clock Multiplier, 10-channel, Integer, 0.001-1028 MHz, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Clock Jitter Attenuator Multiplier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si5345D-D"
		(extends "Si5345A-D")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "Si5345D-D"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.2x5.2mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/Si5345-44-42-D-DataSheet.pdf"
			(at -2.54 27.94 0)
		)
		(property "Description" "Jitter Attenuator/Clock Multiplier, 10-channel, Integer, 0.001-350 MHz, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Clock Jitter Attenuator Multiplier"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
)
