(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "AB0805"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "AB0805"
			(at 2.54 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.8x1.8mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://abracon.com/Precisiontiming/AB08X5-RTC.PDF"
			(at 0 0 0)
		)
		(property "Description" "Real-Time Clock, I2C Interface, 3 GPO, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "rtc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AB0805_0_1")
		(symbol "AB0805_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SCL")
				(number "7")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SDA")
				(number "6")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "EXTI")
				(number "10")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "WDI")
				(number "2")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "AF")
				(number "14")
			)
			(pin no_connect line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -10.16 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "VBAT")
				(number "5")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "13")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "17")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "9")
			)
			(pin no_connect line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin open_collector line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "~{TIRQ}")
				(number "12")
			)
			(pin open_collector line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "FOUT/~{IRQ}")
				(number "11")
			)
			(pin open_collector line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "~{IRQ2}")
				(number "4")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "XI")
				(number "16")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "XO")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AB0815"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "AB0815"
			(at 2.54 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.8x1.8mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://abracon.com/Precisiontiming/AB08X5-RTC.PDF"
			(at 0 0 0)
		)
		(property "Description" "Real-Time Clock, SPI Interface, 2 GPO, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "rtc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AB0815_0_1")
		(symbol "AB0815_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SCL")
				(number "7")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SDI")
				(number "9")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{CE}")
				(number "12")
			)
			(pin output line
				(at -12.7 0 0)
				(length 2.54)
				(name "SDO")
				(number "6")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "EXTI")
				(number "10")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "WDI")
				(number "2")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "AF")
				(number "14")
			)
			(pin no_connect line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -10.16 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "VBAT")
				(number "5")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "13")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "17")
			)
			(pin no_connect line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin open_collector line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "FOUT/~{IRQ}")
				(number "11")
			)
			(pin open_collector line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "~{IRQ2}")
				(number "4")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "XI")
				(number "16")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "XO")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AB1805"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "AB1805"
			(at 2.54 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.8x1.8mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://abracon.com/Precisiontiming/AB18X5-RTC.pdf"
			(at 0 0 0)
		)
		(property "Description" "Real-Time Clock, I2C Interface, 4 GPO, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "rtc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AB1805_0_1")
		(symbol "AB1805_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "~{EXTR}")
				(number "3")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SCL")
				(number "7")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SDA")
				(number "6")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "EXTI")
				(number "10")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "WDI")
				(number "2")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "AF")
				(number "14")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "VBAT")
				(number "5")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "13")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "17")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "9")
			)
			(pin open_collector line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "~{RST}")
				(number "1")
			)
			(pin open_collector line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "~{TIRQ}")
				(number "12")
			)
			(pin open_collector line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "FOUT/~{IRQ}")
				(number "11")
			)
			(pin open_collector line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "~{IRQ2}")
				(number "4")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "CLKOUT/~{IRQ3}")
				(number "8")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "XI")
				(number "16")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "XO")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AB1815"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "AB1815"
			(at 2.54 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.8x1.8mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://abracon.com/Precisiontiming/AB18X5-RTC.pdf"
			(at 0 0 0)
		)
		(property "Description" "Real-Time Clock, SPI Interface, 3 GPO, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "rtc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AB1815_0_1")
		(symbol "AB1815_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "~{EXTR}")
				(number "3")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SCL")
				(number "7")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SDI")
				(number "9")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{CE}")
				(number "12")
			)
			(pin output line
				(at -12.7 0 0)
				(length 2.54)
				(name "SDO")
				(number "6")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "EXTI")
				(number "10")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "WDI")
				(number "2")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "AF")
				(number "14")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "VBAT")
				(number "5")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "13")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "17")
			)
			(pin open_collector line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "~{RST}")
				(number "1")
			)
			(pin open_collector line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "FOUT/~{IRQ}")
				(number "11")
			)
			(pin open_collector line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "~{IRQ2}")
				(number "4")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "CLKOUT/~{IRQ3}")
				(number "8")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "XI")
				(number "16")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "XO")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BQ32000"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "BQ32000"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq32000.pdf"
			(at 0 0 0)
		)
		(property "Description" "Serial, I2C Real-time clock, Trickle charger, 3V to 3.6V VCC, -40°C to +85°C, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RTC, I2C Timekeeping Chip"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm?P1.27mm*"
			(at 0 0 0)
		)
		(symbol "BQ32000_0_1")
		(symbol "BQ32000_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "OSCI")
				(number "1")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "OSCO")
				(number "2")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VBACK")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin open_collector line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{IRQ}")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DS1302+"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "DS1302+"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DS1302.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "Trickle-Charge Timekeeping Chip, 2.0V to 5.5V VCC, 0°C to +70°C, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RTC Trickle-Charge Timekeeping Chip"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "DS1302+_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SCLK")
				(number "7")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "CE")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "X1")
				(number "2")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "X2")
				(number "3")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VCC2")
				(number "1")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC1")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "I/O")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DS1302S+"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "DS1302S+"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_5.3x5.3mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DS1302.pdf"
			(at -11.43 10.16 0)
		)
		(property "Description" "Trickle-Charge Timekeeping Chip, 2.0V to 5.5V VCC, 0°C to +70°C, SOIC-8 (208 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "RTC Trickle-Charge Timekeeping Chip"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*5.3x5.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "DS1302S+_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SCLK")
				(number "7")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "CE")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "X1")
				(number "2")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "X2")
				(number "3")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VCC2")
				(number "1")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC1")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "I/O")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DS1302Z+"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "DS1302Z+"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DS1302.pdf"
			(at 0 0 0)
		)
		(property "Description" "Trickle-Charge Timekeeping Chip, 2.0V to 5.5V VCC, 0°C to +70°C, SOIC-8 (150 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "RTC Trickle-Charge Timekeeping Chip"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm?P1.27mm*"
			(at 0 0 0)
		)
		(symbol "DS1302Z+_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SCLK")
				(number "7")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "CE")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "X1")
				(number "2")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "X2")
				(number "3")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VCC2")
				(number "1")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC1")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "I/O")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DS1307+"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "DS1307+"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DS1307.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "64 x 8, Serial, I2C Real-time clock, 4.5V to 5.5V VCC, 0°C to +70°C, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RTC, Trickle-Charge Timekeeping Chip"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "DS1307+_0_1")
		(symbol "DS1307+_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "X1")
				(number "1")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "X2")
				(number "2")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VBAT")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin open_collector line
				(at 12.7 0 180)
				(length 2.54)
				(name "SQW/OUT")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DS1307Z+"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "DS1307Z+"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DS1307.pdf"
			(at 0 0 0)
		)
		(property "Description" "64 x 8, Serial, I2C Real-time clock, 4.5V to 5.5V VCC, 0°C to +70°C, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RTC, I2C Timekeeping Chip"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm?P1.27mm*"
			(at 0 0 0)
		)
		(symbol "DS1307Z+_0_1")
		(symbol "DS1307Z+_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "X1")
				(number "1")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "X2")
				(number "2")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VBAT")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin open_collector line
				(at 12.7 0 180)
				(length 2.54)
				(name "SQW/OUT")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DS1602"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "DS1602"
			(at 7.62 8.89 0)
		)
		(property "Footprint" ""
			(at 2.54 -5.08 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DS1602.pdf"
			(at 2.54 -5.08 0)
		)
		(property "Description" "Elapsed Time Counter, -40 to +85 C, 2.5V to 5.5V VCC, DIP-8, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Elapsed Time Counter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SO*5.3x6.2mm?P1.27mm*"
			(at 0 0 0)
		)
		(symbol "DS1602_0_1")
		(symbol "DS1602_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "CLK")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "DQ")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{RST}")
				(number "1")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VBAT")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "XTAL1")
				(number "7")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "XTAL2")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DS3231M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "DS3231M"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/DS3231.pdf"
			(at 6.858 1.27 0)
		)
		(property "Description" "Extremely Accurate I2C-Integrated RTC/TCXO/Crystal SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "RTC TCXO Realtime Time Clock Crystal Oscillator I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "DS3231M_0_1")
		(symbol "DS3231M_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SCL")
				(number "16")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "15")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{RST}")
				(number "4")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VBAT")
				(number "14")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin open_collector line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "32KHZ")
				(number "1")
			)
			(pin open_collector line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "~{INT}/SQW")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DS3231MZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "DS3231MZ"
			(at 11.43 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/DS3231M.pdf"
			(at 0 -15.24 0)
		)
		(property "Description" "±5ppm, I2C Real-Time Clock SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RTC TCXO Realtime Time Clock MEMS I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "DS3231MZ_0_1")
		(symbol "DS3231MZ_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SCL")
				(number "8")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "7")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{RST}")
				(number "4")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin open_collector line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "32KHZ")
				(number "1")
			)
			(pin open_collector line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "~{INT}/SQW")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DS3232M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "DS3232M"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -12.7 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/DS3232M.pdf"
			(at 6.858 3.81 0)
		)
		(property "Description" "±5ppm, I2C Real-Time Clock with SRAM SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RTC TCXO Realtime Time Clock MEMS SRAM I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "DS3232M_0_1")
		(symbol "DS3232M_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SCL")
				(number "8")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "7")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{RST}")
				(number "4")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VBAT")
				(number "6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "32KHZ")
				(number "1")
			)
			(pin open_collector line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "~{INT}/SQW")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "M41T62Q"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "M41T62Q"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP1.8x1.8mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/m41t62.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low-power I2C RTC with alarm interrupt QFN"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C RTC Alarm interrupt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*16*1EP*3x3mm*P0.5mm*EP1.8x1.8mm*"
			(at 0 0 0)
		)
		(symbol "M41T62Q_0_1")
		(symbol "M41T62Q_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "XI")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "XO")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SCL")
				(number "10")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SDA")
				(number "9")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin passive line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "EP")
				(number "17")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{IRQ}/OUT")
				(number "11")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SQW")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP7940N-xMNY"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "MCP7940N-xMNY"
			(at 11.43 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.36x1.46mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005010F.pdf"
			(at 0 0 0)
		)
		(property "Description" "Real-Time Clock, I2C, Battery Backup, TDFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "realtime clock RTC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MCP7940N-xMNY_0_1")
		(symbol "MCP7940N-xMNY_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin open_collector line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "MFP")
				(number "7")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VBAT")
				(number "3")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "EP")
				(number "9")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "X1")
				(number "1")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "X2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP7940N-xMS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "MCP7940N-xMS"
			(at 11.43 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005010F.pdf"
			(at 0 0 0)
		)
		(property "Description" "Real-Time Clock, I2C, Battery Backup, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "realtime clock RTC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MCP7940N-xMS_0_1")
		(symbol "MCP7940N-xMS_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin open_collector line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "MFP")
				(number "7")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VBAT")
				(number "3")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "X1")
				(number "1")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "X2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCF85063ATL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "PCF85063ATL"
			(at 6.35 -8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-10-1EP_2.6x2.6mm_P0.5mm_EP1.3x2.2mm"
			(at 0 20.32 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCF85063A.pdf"
			(at 0 -20.32 0)
		)
		(property "Description" "I2C Real-Time Clock Calendar w/ Alarm, DFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "RTC I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*2.6x2.6mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PCF85063ATL_0_1")
		(symbol "PCF85063ATL_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SCL")
				(number "7")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "CLKOE")
				(number "3")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "OSCI")
				(number "1")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "OSCO")
				(number "2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "10")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin no_connect line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "~{INT}")
				(number "4")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "CLKOUT")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCF8523T"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "PCF8523T"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 20.32 -8.89 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCF8523.pdf"
			(at 0 0 0)
		)
		(property "Description" "Realtime Clock/Calendar I2C Interface, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C RTC Clock Calendar"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "PCF8523T_0_1")
		(symbol "PCF8523T_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "OSCI")
				(number "1")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "OSCO")
				(number "2")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VBAT")
				(number "3")
			)
			(pin open_collector line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{INT1}/CLKOUT")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCF8523TK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "PCF8523TK"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_SON:HVSON-8-1EP_4x4mm_P0.8mm_EP2.2x3.1mm"
			(at 20.32 -8.89 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCF8523.pdf"
			(at 0 0 0)
		)
		(property "Description" "Realtime Clock/Calendar I2C Interface, HVSON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C RTC Clock Calendar"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HVSON*1EP*4x4mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "PCF8523TK_0_1")
		(symbol "PCF8523TK_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "OSCI")
				(number "1")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "OSCO")
				(number "2")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "9")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VBAT")
				(number "3")
			)
			(pin open_collector line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{INT1}/CLKOUT")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCF8523TS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "PCF8523TS"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 20.32 -8.89 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCF8523.pdf"
			(at 0 0 0)
		)
		(property "Description" "Realtime Clock/Calendar I2C Interface, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C RTC Clock Calendar"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PCF8523TS_0_1")
		(symbol "PCF8523TS_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SCL")
				(number "11")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "10")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "OSCI")
				(number "1")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "OSCO")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "14")
			)
			(pin no_connect line
				(at -2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VBAT")
				(number "4")
			)
			(pin no_connect line
				(at 2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at 5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin open_collector line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "~{INT2}")
				(number "7")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{INT1}/CLKOUT")
				(number "13")
			)
			(pin open_collector line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CLKOUT")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCF85263AT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "PCF85263AT"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -21.59 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCF85263A.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "Tiny Real-Time Clock/calendar with alarm function, battery switch-over, time stamp input, I2C bus, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RTC battery I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "PCF85263AT_0_1")
		(symbol "PCF85263AT_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "OSCI")
				(number "1")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "OSCO")
				(number "2")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VBAT")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin open_collector line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "~{INTA}")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCF85263ATL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "PCF85263ATL"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-10-1EP_2.6x2.6mm_P0.5mm_EP1.3x2.2mm"
			(at 0 -21.59 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCF85263A.pdf"
			(at 0 -24.13 0)
		)
		(property "Description" "Tiny Real-Time Clock/calendar with alarm function, battery switch-over, time stamp input, I2C bus, DFN-10"
			(at 0 -26.67 0)
		)
		(property "ki_keywords" "RTC battery I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*2.6x2.6mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PCF85263ATL_0_1")
		(symbol "PCF85263ATL_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SCL")
				(number "7")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "6")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "OSCI")
				(number "1")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "OSCO")
				(number "2")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "10")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VBAT")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin no_connect line
				(at 10.16 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "PAD")
				(number "11")
			)
			(pin open_collector line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "~{INTA}")
				(number "9")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "CLK")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "TS")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCF85263ATT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "PCF85263ATT"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_3x3mm_P0.65mm"
			(at 0 -21.59 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCF85263A.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "Tiny Real-Time Clock/calendar with alarm function, battery switch-over, time stamp input, I2C bus, TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RTC battery I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PCF85263ATT_0_1")
		(symbol "PCF85263ATT_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "OSCI")
				(number "1")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "OSCO")
				(number "2")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VBAT")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin open_collector line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "~{INTA}")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCF85263ATT1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "PCF85263ATT1"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:TSSOP-10_3x3mm_P0.5mm"
			(at 0 -21.59 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCF85263A.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "Tiny Real-Time Clock/calendar with alarm function, battery switch-over, time stamp input, I2C bus, TSSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "RTC battery I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PCF85263ATT1_0_1")
		(symbol "PCF85263ATT1_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SCL")
				(number "7")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "6")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "OSCI")
				(number "1")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "OSCO")
				(number "2")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "10")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VBAT")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin open_collector line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "~{INTA}")
				(number "9")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "CLK")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "TS")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCF8563T"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "PCF8563T"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCF8563.pdf"
			(at 0 0 0)
		)
		(property "Description" "Realtime Clock/Calendar I2C Interface, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C RTC Clock Calendar"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "PCF8563T_0_1")
		(symbol "PCF8563T_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "OSCI")
				(number "1")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "OSCO")
				(number "2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin output clock
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "CLKO")
				(number "7")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "~{INT}")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCF8563TS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "PCF8563TS"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCF8563.pdf"
			(at 0 0 0)
		)
		(property "Description" "Realtime Clock/Calendar I2C Interface, TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C RTC Clock Calendar"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PCF8563TS_0_1")
		(symbol "PCF8563TS_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "OSCI")
				(number "1")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "OSCO")
				(number "2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin output clock
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "CLKO")
				(number "7")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "~{INT}")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RV-1805-C3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "RV-1805-C3"
			(at 7.62 8.89 0)
		)
		(property "Footprint" "Package_SON:RTC_SMD_MicroCrystal_C3_2.5x3.7mm"
			(at 25.4 -8.89 0)
		)
		(property "Datasheet" "https://www.microcrystal.com/fileadmin/Media/Products/RTC/Datasheet/RV-1805-C3.pdf"
			(at 0 0 0)
		)
		(property "Description" "Realtime Clock/Calendar I2C Interface, Extreme Low Power, MicroCrystal C3"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Power RTC I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RTC*SMD*MicroCrystal*C3*2.5x3.7mm*"
			(at 0 0 0)
		)
		(symbol "RV-1805-C3_0_1")
		(symbol "RV-1805-C3_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SCL")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "WDI")
				(number "9")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "Cap_RC")
				(number "2")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VBACKUP")
				(number "7")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "6")
			)
			(pin open_collector line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "~{RST}")
				(number "10")
			)
			(pin open_collector line
				(at 12.7 0 180)
				(length 2.54)
				(name "PSW")
				(number "8")
			)
			(pin open_collector line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CLK/~{INT}")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RV-3028-C7"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "RV-3028-C7"
			(at 7.62 8.89 0)
		)
		(property "Footprint" "Package_SON:MicroCrystal_C7_SON-8_1.5x3.2mm_P0.9mm"
			(at 25.4 -8.89 0)
		)
		(property "Datasheet" "https://www.microcrystal.com/fileadmin/Media/Products/RTC/Datasheet/RV-3028-C7.pdf"
			(at 0 0 0)
		)
		(property "Description" "Realtime Clock/Calendar I2C Interface, Extreme Low Power, 1.1 V to 5.5 V, MicroCrystal C7"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low-power RTC I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MicroCrystal*C7*1.5x3.2mm*"
			(at 0 0 0)
		)
		(symbol "RV-3028-C7_0_1")
		(symbol "RV-3028-C7_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SCL")
				(number "3")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "EVI")
				(number "8")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VBACKUP")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin open_collector line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "~{INT}")
				(number "2")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CLKOUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RV-8523-C3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "RV-8523-C3"
			(at 7.62 8.89 0)
		)
		(property "Footprint" "Package_SON:RTC_SMD_MicroCrystal_C3_2.5x3.7mm"
			(at 25.4 -8.89 0)
		)
		(property "Datasheet" "https://www.microcrystal.com/fileadmin/Media/Products/RTC/Datasheet/RV-8523-C3.pdf"
			(at 0 0 0)
		)
		(property "Description" "Realtime Clock/Calendar I2C Interface, Low Power, 1.2 V to 5.5 V, MicroCrystal C3"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Power RTC I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RTC*SMD*MicroCrystal*C3*2.5x3.7mm*"
			(at 0 0 0)
		)
		(symbol "RV-8523-C3_0_1")
		(symbol "RV-8523-C3_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SCL")
				(number "3")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "4")
			)
			(pin no_connect line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VBACKUP")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin open_collector line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "~{INT_1}")
				(number "2")
			)
			(pin open_collector line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{INT_2}")
				(number "6")
			)
			(pin open_collector line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CLKOUT")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RX8901CE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "RX8901CE"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_SON:EPSON_CE-USON-10_USON-10_3.2x2.5mm_P0.7mm"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://support.epson.biz/td/api/doc_check.php?dl=app_RX8901CE&lang=en"
			(at 48.26 -8.89 0)
		)
		(property "Description" "Realtime Clock/Calendar I2C Interface built-in crystal , SON-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C RTC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*EPSON*CE*USON*10*USON*10*3.2x2.5mm*P0.7mm*"
			(at 0 0 0)
		)
		(symbol "RX8901CE_0_1")
		(symbol "RX8901CE_1_1"
			(pin open_collector line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "~{INT}")
				(number "8")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SCL")
				(number "5")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "SDA")
				(number "7")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "V_{DD}")
				(number "1")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "V_{BAT}")
				(number "3")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin power_out line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "V_{OUT}")
				(number "2")
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "EVIN1")
				(number "6")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "EVIN2/FOE")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "FOUT/EVIN3")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BQ32002"
		(extends "BQ32000")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "BQ32002"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq32002.pdf"
			(at 0 0 0)
		)
		(property "Description" "Serial, I2C Real-time clock, 3V to 3.6V VCC, -40°C to +85°C, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RTC, I2C Timekeeping Chip"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm?P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "DS1302N+"
		(extends "DS1302+")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "DS1302N+"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DS1302.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "Trickle-Charge Timekeeping Chip, 2.0V to 5.5V VCC, -40°C to +85°C, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RTC Trickle-Charge Timekeeping Chip"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "DS1302SN+"
		(extends "DS1302S+")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "DS1302SN+"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_5.3x5.3mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DS1302.pdf"
			(at -11.43 10.16 0)
		)
		(property "Description" "Trickle-Charge Timekeeping Chip, 2.0V to 5.5V VCC, -40°C to +85°C, SOIC-8 (208 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "RTC Trickle-Charge Timekeeping Chip"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*5.3x5.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "DS1302ZN+"
		(extends "DS1302Z+")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "DS1302ZN+"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DS1302.pdf"
			(at 0 0 0)
		)
		(property "Description" "Trickle-Charge Timekeeping Chip, 2.0V to 5.5V VCC, -40°C to +85°C, SOIC-8 (150 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "RTC Trickle-Charge Timekeeping Chip"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm?P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "DS1307N+"
		(extends "DS1307+")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "DS1307N+"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DS1307.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "64 x 8, Serial, I2C Real-time clock, 4.5V to 5.5V VCC, -40°C to +85°C, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RTC, Trickle-Charge Timekeeping Chip"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "DS1307ZN+"
		(extends "DS1307Z+")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "DS1307ZN+"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/DS1307.pdf"
			(at 0 0 0)
		)
		(property "Description" "64 x 8, Serial, I2C Real-time clock, 4.5V to 5.5V VCC, -40°C to +85°C, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RTC, I2C Timekeeping Chip"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm?P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP7940N-xP"
		(extends "MCP7940N-xMS")
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "MCP7940N-xP"
			(at 11.43 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005010F.pdf"
			(at 0 0 0)
		)
		(property "Description" "Real-Time Clock, I2C, Battery Backup, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "realtime clock RTC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP7940N-xSN"
		(extends "MCP7940N-xMS")
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "MCP7940N-xSN"
			(at 11.43 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005010F.pdf"
			(at 0 0 0)
		)
		(property "Description" "Real-Time Clock, I2C, Battery Backup, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "realtime clock RTC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP7940N-xST"
		(extends "MCP7940N-xMS")
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "MCP7940N-xST"
			(at 11.43 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005010F.pdf"
			(at 0 0 0)
		)
		(property "Description" "Real-Time Clock, I2C, Battery Backup, TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "realtime clock RTC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "PCF85363ATT"
		(extends "PCF85263ATT")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "PCF85363ATT"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_3x3mm_P0.65mm"
			(at 0 -21.59 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCF85363A.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "Tiny Real-Time Clock/calendar with 64 byte RAM, alarm function, battery switch-over, time stamp input, I2C bus, TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RTC RAM battery I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PCF85363ATT1"
		(extends "PCF85263ATT1")
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "PCF85363ATT1"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:TSSOP-10_3x3mm_P0.5mm"
			(at 0 -21.59 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCF85363A.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "Tiny Real-Time Clock/calendar with 64 byte RAM, alarm function, battery switch-over, time stamp input, I2C bus, TSSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "RTC RAM battery I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
)
