(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "A2982"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "A2982"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.allegromicro.com/~/media/Files/Datasheets/A2981-2-Datasheet.ashx"
			(at -7.62 10.16 0)
		)
		(property "Description" "8-Channel Source Driver, TTL DTL, PMOS or CMOS compatible, 500mA 50V output, SOIC-20W"
			(at 0 0 0)
		)
		(property "ki_keywords" "relays solenoids lamps steppers servos LEDs"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*20W*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "A2982_0_1")
		(symbol "A2982_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "IN1")
				(number "1")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN2")
				(number "2")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN3")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN4")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IN5")
				(number "5")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "IN6")
				(number "6")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "IN7")
				(number "7")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "IN8")
				(number "8")
			)
			(pin no_connect line
				(at -2.54 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "+VS")
				(number "9")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "12")
			)
			(pin no_connect line
				(at 2.54 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin open_emitter line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "OUT1")
				(number "20")
			)
			(pin open_emitter line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUT2")
				(number "19")
			)
			(pin open_emitter line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT3")
				(number "18")
			)
			(pin open_emitter line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT4")
				(number "17")
			)
			(pin open_emitter line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT5")
				(number "16")
			)
			(pin open_emitter line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "OUT6")
				(number "15")
			)
			(pin open_emitter line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "OUT7")
				(number "14")
			)
			(pin open_emitter line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "OUT8")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC1413D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "MC1413D"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 1.27 -13.97 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MC1413-D.PDF"
			(at 2.54 -5.08 0)
		)
		(property "Description" "High Voltage, High Current Darlington Transistor Arrays, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "darlington transistor array"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MC1413D_0_1")
		(symbol "MC1413D_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "I1")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "I2")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "I3")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "I4")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "I5")
				(number "5")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "I6")
				(number "6")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "I7")
				(number "7")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "COM")
				(number "9")
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "O1")
				(number "16")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "O2")
				(number "15")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "O3")
				(number "14")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "O4")
				(number "13")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "O5")
				(number "12")
			)
			(pin open_collector line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "O6")
				(number "11")
			)
			(pin open_collector line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "O7")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN75468"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "SN75468"
			(at 0 13.97 0)
		)
		(property "Footprint" ""
			(at 1.27 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/slrs023e/slrs023e.pdf"
			(at 2.54 -5.08 0)
		)
		(property "Description" "Higher Voltage, High Current Darlington Transistor Arrays, 5V CMOS/TTL-compatible input, SOIC16/SOIC16W/DIP16"
			(at 0 0 0)
		)
		(property "ki_keywords" "darlington transistor array"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* SOIC*W*5.3x10.2mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "SN75468_0_1")
		(symbol "SN75468_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "I1")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "I2")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "I3")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "I4")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "I5")
				(number "5")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "I6")
				(number "6")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "I7")
				(number "7")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "COM")
				(number "9")
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "O1")
				(number "16")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "O2")
				(number "15")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "O3")
				(number "14")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "O4")
				(number "13")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "O5")
				(number "12")
			)
			(pin open_collector line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "O6")
				(number "11")
			)
			(pin open_collector line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "O7")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TBD62783A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TBD62783A"
			(at 1.27 11.43 0)
		)
		(property "Footprint" ""
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://toshiba.semicon-storage.com/info/docget.jsp?did=30523&prodName=TBD62783APG"
			(at -7.62 10.16 0)
		)
		(property "Description" "8-Channel Source Type Transistor Array, TTL and CMOS compatible, 500mA, 50V, DIP-18/SOP-18/SSOP-18/SOIC-18W"
			(at 0 0 0)
		)
		(property "ki_keywords" "relays solenoids lamps steppers servos LEDs"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOP*7.0x12.5mm*P1.27mm* SSOP*4.4x6.5mm*P0.65mm* SOIC*7.5x11.6mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TBD62783A_0_1")
		(symbol "TBD62783A_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "I1")
				(number "1")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "I2")
				(number "2")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "I3")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "I4")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "I5")
				(number "5")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "I6")
				(number "6")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "I7")
				(number "7")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "I8")
				(number "8")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "9")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin open_emitter line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "O1")
				(number "18")
			)
			(pin open_emitter line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "O2")
				(number "17")
			)
			(pin open_emitter line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "O3")
				(number "16")
			)
			(pin open_emitter line
				(at 10.16 0 180)
				(length 2.54)
				(name "O4")
				(number "15")
			)
			(pin open_emitter line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "O5")
				(number "14")
			)
			(pin open_emitter line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "O6")
				(number "13")
			)
			(pin open_emitter line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "O7")
				(number "12")
			)
			(pin open_emitter line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "O8")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TBD62785APG"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TBD62785APG"
			(at 8.128 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-18_W7.62mm"
			(at 18.034 -14.224 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/TBD62785APG_datasheet_en_20170530.pdf?did=58399&prodName=TBD62785APG"
			(at 63.881 -16.51 0)
		)
		(property "Description" "8-Channel Source Type Transistor Array, TTL and CMOS compatible, 500mA, 50V, DIP-18-18W"
			(at 0 0 0)
		)
		(property "ki_keywords" "relays solenoids lamps steppers servos LEDs"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "TBD62785APG_0_1")
		(symbol "TBD62785APG_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "I1")
				(number "1")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "I2")
				(number "2")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "I3")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "I4")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "I5")
				(number "5")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "I6")
				(number "6")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "I7")
				(number "7")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "I8")
				(number "8")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "9")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin open_emitter line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "O1")
				(number "18")
			)
			(pin open_emitter line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "O2")
				(number "17")
			)
			(pin open_emitter line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "O3")
				(number "16")
			)
			(pin open_emitter line
				(at 10.16 0 180)
				(length 2.54)
				(name "O4")
				(number "15")
			)
			(pin open_emitter line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "O5")
				(number "14")
			)
			(pin open_emitter line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "O6")
				(number "13")
			)
			(pin open_emitter line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "O7")
				(number "12")
			)
			(pin open_emitter line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "O8")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ULN2003"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "ULN2003"
			(at 0 13.97 0)
		)
		(property "Footprint" ""
			(at 1.27 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/uln2003a.pdf"
			(at 2.54 -5.08 0)
		)
		(property "Description" "High Voltage, High Current Darlington Transistor Arrays, SOIC16/SOIC16W/DIP16/TSSOP16"
			(at 0 0 0)
		)
		(property "ki_keywords" "darlington transistor array"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* SSOP*4.4x5.2mm*P0.65mm* TSSOP*4.4x5mm*P0.65mm* SOIC*W*5.3x10.2mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ULN2003_0_1")
		(symbol "ULN2003_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "I1")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "I2")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "I3")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "I4")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "I5")
				(number "5")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "I6")
				(number "6")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "I7")
				(number "7")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "COM")
				(number "9")
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "O1")
				(number "16")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "O2")
				(number "15")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "O3")
				(number "14")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "O4")
				(number "13")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "O5")
				(number "12")
			)
			(pin open_collector line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "O6")
				(number "11")
			)
			(pin open_collector line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "O7")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ULN2803A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 13.335 0)
		)
		(property "Value" "ULN2803A"
			(at 0 11.43 0)
		)
		(property "Footprint" ""
			(at 1.27 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/uln2803a.pdf"
			(at 2.54 -5.08 0)
		)
		(property "Description" "Darlington Transistor Arrays, SOIC18/DIP18"
			(at 0 0 0)
		)
		(property "ki_keywords" "Darlington transistor array"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*7.5x11.6mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ULN2803A_0_1")
		(symbol "ULN2803A_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "I1")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "I2")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "I3")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "I4")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "I5")
				(number "5")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "I6")
				(number "6")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "I7")
				(number "7")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "I8")
				(number "8")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "COM")
				(number "10")
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "O1")
				(number "18")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "O2")
				(number "17")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "O3")
				(number "16")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "O4")
				(number "15")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "O5")
				(number "14")
			)
			(pin open_collector line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "O6")
				(number "13")
			)
			(pin open_collector line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "O7")
				(number "12")
			)
			(pin open_collector line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "O8")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ULQ2003A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "ULQ2003A"
			(at 0 13.97 0)
		)
		(property "Footprint" ""
			(at 1.27 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/uln2003a.pdf"
			(at 2.54 -5.08 0)
		)
		(property "Description" "High Voltage, High Current Darlington Transistor Arrays, SOIC16W/TSSOP16"
			(at 0 0 0)
		)
		(property "ki_keywords" "darlington transistor array"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* SSOP*4.4x5.2mm*P0.65mm* TSSOP*4.4x5mm*P0.65mm* SOIC*W*5.3x10.2mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ULQ2003A_0_1")
		(symbol "ULQ2003A_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "I1")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "I2")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "I3")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "I4")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "I5")
				(number "5")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "I6")
				(number "6")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "I7")
				(number "7")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "COM")
				(number "9")
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "O1")
				(number "16")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "O2")
				(number "15")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "O3")
				(number "14")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "O4")
				(number "13")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "O5")
				(number "12")
			)
			(pin open_collector line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "O6")
				(number "11")
			)
			(pin open_collector line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "O7")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC1413BD"
		(extends "MC1413D")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "MC1413BD"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 1.27 -13.97 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MC1413-D.PDF"
			(at 2.54 -5.08 0)
		)
		(property "Description" "High Voltage, High Current Darlington Transistor Arrays,  TTL/CMOS-compatible, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "darlington transistor array"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC1413BP"
		(extends "MC1413D")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "MC1413BP"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 1.27 -13.97 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MC1413-D.PDF"
			(at 2.54 -5.08 0)
		)
		(property "Description" "High Voltage, High Current Darlington Transistor Arrays,  TTL/CMOS-compatible, PDIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "darlington transistor array"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC1413P"
		(extends "MC1413D")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "MC1413P"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 1.27 -13.97 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MC1413-D.PDF"
			(at 2.54 -5.08 0)
		)
		(property "Description" "High Voltage, High Current Darlington Transistor Arrays, PDIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "darlington transistor array"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "NCV1413B"
		(extends "MC1413D")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "NCV1413B"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 1.27 -13.97 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub_link/Collateral/MC1413-D.PDF"
			(at 2.54 -5.08 0)
		)
		(property "Description" "High Voltage, High Current Darlington Transistor Arrays,  TTL/CMOS-compatible, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "darlington transistor array"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "SN75469"
		(extends "SN75468")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "SN75469"
			(at 0 13.97 0)
		)
		(property "Footprint" ""
			(at 1.27 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/slrs023e/slrs023e.pdf"
			(at 2.54 -5.08 0)
		)
		(property "Description" "Higher Voltage, High Current Darlington Transistor Arrays, 6-15V CMOS/PMOS-compatible input, SOIC16/SOIC16W/DIP16"
			(at 0 0 0)
		)
		(property "ki_keywords" "darlington transistor array"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* SOIC*W*5.3x10.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TBD62785AFWG"
		(extends "TBD62785APG")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TBD62785AFWG"
			(at 8.128 11.43 0)
		)
		(property "Footprint" "Package_SO:SOP-18_7.495x11.515mm_P1.27mm"
			(at 24.13 -14.224 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/TBD62785AFWG_datasheet_en_20170530.pdf?did=58399&prodName=TBD62785AFWG"
			(at 63.881 -16.51 0)
		)
		(property "Description" "8-Channel Source Type Transistor Array, TTL and CMOS compatible, 500mA, 50V, SOP-18-18W"
			(at 0 0 0)
		)
		(property "ki_keywords" "relays solenoids lamps steppers servos LEDs"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*7.495x11.515mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ULN2002"
		(extends "ULN2003")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "ULN2002"
			(at 0 13.97 0)
		)
		(property "Footprint" ""
			(at 1.27 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/uln2003a.pdf"
			(at 2.54 -5.08 0)
		)
		(property "Description" "High Voltage, High Current Darlington Transistor Arrays, SOIC16/SOIC16W/DIP16/TSSOP16"
			(at 0 0 0)
		)
		(property "ki_keywords" "darlington transistor array"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* SSOP*4.4x5.2mm*P0.65mm* TSSOP*4.4x5mm*P0.65mm* SOIC*W*5.3x10.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ULN2002A"
		(extends "ULN2003")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "ULN2002A"
			(at 0 13.97 0)
		)
		(property "Footprint" ""
			(at 1.27 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/uln2003a.pdf"
			(at 2.54 -5.08 0)
		)
		(property "Description" "High Voltage, High Current Darlington Transistor Arrays, SOIC16/SOIC16W/DIP16/TSSOP16"
			(at 0 0 0)
		)
		(property "ki_keywords" "darlington transistor array"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* SSOP*4.4x5.2mm*P0.65mm* TSSOP*4.4x5mm*P0.65mm* SOIC*W*5.3x10.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ULN2003A"
		(extends "ULN2003")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "ULN2003A"
			(at 0 13.97 0)
		)
		(property "Footprint" ""
			(at 1.27 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/uln2003a.pdf"
			(at 2.54 -5.08 0)
		)
		(property "Description" "High Voltage, High Current Darlington Transistor Arrays, SOIC16/SOIC16W/DIP16/TSSOP16"
			(at 0 0 0)
		)
		(property "ki_keywords" "darlington transistor array"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* SSOP*4.4x5.2mm*P0.65mm* TSSOP*4.4x5mm*P0.65mm* SOIC*W*5.3x10.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ULN2004"
		(extends "ULN2003")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "ULN2004"
			(at 0 13.97 0)
		)
		(property "Footprint" ""
			(at 1.27 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/uln2003a.pdf"
			(at 2.54 -5.08 0)
		)
		(property "Description" "High Voltage, High Current Darlington Transistor Arrays, SOIC16/SOIC16W/DIP16/TSSOP16"
			(at 0 0 0)
		)
		(property "ki_keywords" "darlington transistor array"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* SSOP*4.4x5.2mm*P0.65mm* TSSOP*4.4x5mm*P0.65mm* SOIC*W*5.3x10.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ULN2004A"
		(extends "ULN2003")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "ULN2004A"
			(at 0 13.97 0)
		)
		(property "Footprint" ""
			(at 1.27 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/uln2003a.pdf"
			(at 2.54 -5.08 0)
		)
		(property "Description" "High Voltage, High Current Darlington Transistor Arrays, SOIC16/SOIC16W/DIP16/TSSOP16"
			(at 0 0 0)
		)
		(property "ki_keywords" "darlington transistor array"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* SSOP*4.4x5.2mm*P0.65mm* TSSOP*4.4x5mm*P0.65mm* SOIC*W*5.3x10.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ULN2801A"
		(extends "ULN2803A")
		(property "Reference" "U"
			(at 0 13.335 0)
		)
		(property "Value" "ULN2801A"
			(at 0 11.43 0)
		)
		(property "Footprint" ""
			(at 1.27 -16.51 0)
		)
		(property "Datasheet" "http://www.promelec.ru/pdf/1536.pdf"
			(at 2.54 -5.08 0)
		)
		(property "Description" "Darlington Transistor Arrays, SOIC18/DIP18"
			(at 0 0 0)
		)
		(property "ki_keywords" "darlington transistor array"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*7.5x11.6mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ULN2802A"
		(extends "ULN2803A")
		(property "Reference" "U"
			(at 0 13.335 0)
		)
		(property "Value" "ULN2802A"
			(at 0 11.43 0)
		)
		(property "Footprint" ""
			(at 1.27 -16.51 0)
		)
		(property "Datasheet" "http://www.promelec.ru/pdf/1536.pdf"
			(at 2.54 -5.08 0)
		)
		(property "Description" "Darlington Transistor Arrays, SOIC18/DIP18"
			(at 0 0 0)
		)
		(property "ki_keywords" "darlington transistor array"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*7.5x11.6mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ULN2804A"
		(extends "ULN2803A")
		(property "Reference" "U"
			(at 0 13.335 0)
		)
		(property "Value" "ULN2804A"
			(at 0 11.43 0)
		)
		(property "Footprint" ""
			(at 1.27 -16.51 0)
		)
		(property "Datasheet" "http://www.promelec.ru/pdf/1536.pdf"
			(at 2.54 -5.08 0)
		)
		(property "Description" "Darlington Transistor Arrays, SOIC18/DIP18"
			(at 0 0 0)
		)
		(property "ki_keywords" "darlington transistor array"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*7.5x11.6mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ULN2805A"
		(extends "ULN2803A")
		(property "Reference" "U"
			(at 0 13.335 0)
		)
		(property "Value" "ULN2805A"
			(at 0 11.43 0)
		)
		(property "Footprint" ""
			(at 1.27 -16.51 0)
		)
		(property "Datasheet" "http://www.promelec.ru/pdf/1536.pdf"
			(at 2.54 -5.08 0)
		)
		(property "Description" "Darlington Transistor Arrays, SOIC18/DIP18"
			(at 0 0 0)
		)
		(property "ki_keywords" "darlington transistor array"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*7.5x11.6mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ULQ2004A"
		(extends "ULQ2003A")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "ULQ2004A"
			(at 0 13.97 0)
		)
		(property "Footprint" ""
			(at 1.27 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/uln2003a.pdf"
			(at 2.54 -5.08 0)
		)
		(property "Description" "High Voltage, High Current Darlington Transistor Arrays, SOIC16W/TSSOP16"
			(at 0 0 0)
		)
		(property "ki_keywords" "darlington transistor array"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* SSOP*4.4x5.2mm*P0.65mm* TSSOP*4.4x5mm*P0.65mm* SOIC*W*5.3x10.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
)
