(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "BT169B"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 2.54 1.905 0)
		)
		(property "Value" "BT169B"
			(at 2.54 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 2.54 -1.905 0)
		)
		(property "Datasheet" "https://media.digikey.com/pdf/Data%20Sheets/NXP%20PDFs/BT169_Series.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.5A Ion, 200V Voff, Thyristors logic level, Silicon Controlled Rectifier (Thyristor), TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "thyristor logic level"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*Inline*Narrow*"
			(at 0 0 0)
		)
		(symbol "BT169B_0_1")
		(symbol "BT169B_1_1"
			(pin input line
				(at -3.81 -2.54 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 0 3.81 270)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 2.54)
				(name "K")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Generic_Triac_A1A2G"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 3.175 0.635 0)
		)
		(property "Value" "Generic_Triac_A1A2G"
			(at 3.175 -1.27 0)
		)
		(property "Footprint" ""
			(at 1.905 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
		)
		(property "Description" "Triode for alternating current, anode1/anode2/gate"
			(at 0 0 0)
		)
		(property "ki_keywords" "TRIAC"
			(at 0 0 0)
		)
		(symbol "Generic_Triac_A1A2G_0_1")
		(symbol "Generic_Triac_A1A2G_1_1"
			(pin input line
				(at -3.81 -2.54 0)
				(length 2.54)
				(name "G")
				(number "3")
			)
			(pin passive line
				(at 0 3.81 270)
				(length 2.54)
				(name "A2")
				(number "2")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 2.54)
				(name "A1")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Generic_Triac_A1GA2"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 3.175 0.635 0)
		)
		(property "Value" "Generic_Triac_A1GA2"
			(at 3.175 -1.27 0)
		)
		(property "Footprint" ""
			(at 1.905 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
		)
		(property "Description" "Triode for alternating current, anode1/gate/anode2"
			(at 0 0 0)
		)
		(property "ki_keywords" "TRIAC"
			(at 0 0 0)
		)
		(symbol "Generic_Triac_A1GA2_0_1")
		(symbol "Generic_Triac_A1GA2_1_1"
			(pin input line
				(at -3.81 -2.54 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 0 3.81 270)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 2.54)
				(name "A1")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Generic_Triac_A2A1G"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 3.175 0.635 0)
		)
		(property "Value" "Generic_Triac_A2A1G"
			(at 3.175 -1.27 0)
		)
		(property "Footprint" ""
			(at 1.905 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
		)
		(property "Description" "Triode for alternating current, anode2/anode1/gate"
			(at 0 0 0)
		)
		(property "ki_keywords" "TRIAC"
			(at 0 0 0)
		)
		(symbol "Generic_Triac_A2A1G_0_1")
		(symbol "Generic_Triac_A2A1G_1_1"
			(pin input line
				(at -3.81 -2.54 0)
				(length 2.54)
				(name "G")
				(number "3")
			)
			(pin passive line
				(at 0 3.81 270)
				(length 2.54)
				(name "A2")
				(number "1")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 2.54)
				(name "A1")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Generic_Triac_A2GA1"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 3.175 0.635 0)
		)
		(property "Value" "Generic_Triac_A2GA1"
			(at 3.175 -1.27 0)
		)
		(property "Footprint" ""
			(at 1.905 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
		)
		(property "Description" "Triode for alternating current, anode2/gate/anode1"
			(at 0 0 0)
		)
		(property "ki_keywords" "TRIAC"
			(at 0 0 0)
		)
		(symbol "Generic_Triac_A2GA1_0_1")
		(symbol "Generic_Triac_A2GA1_1_1"
			(pin input line
				(at -3.81 -2.54 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin passive line
				(at 0 3.81 270)
				(length 2.54)
				(name "A2")
				(number "1")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 2.54)
				(name "A1")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Generic_Triac_GA1A2"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 3.175 0.635 0)
		)
		(property "Value" "Generic_Triac_GA1A2"
			(at 3.175 -1.27 0)
		)
		(property "Footprint" ""
			(at 1.905 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
		)
		(property "Description" "Triode for alternating current, gate/anode1/anode2"
			(at 0 0 0)
		)
		(property "ki_keywords" "TRIAC"
			(at 0 0 0)
		)
		(symbol "Generic_Triac_GA1A2_0_1")
		(symbol "Generic_Triac_GA1A2_1_1"
			(pin input line
				(at -3.81 -2.54 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 0 3.81 270)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 2.54)
				(name "A1")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Generic_Triac_GA2A1"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 3.175 0.635 0)
		)
		(property "Value" "Generic_Triac_GA2A1"
			(at 3.175 -1.27 0)
		)
		(property "Footprint" ""
			(at 1.905 0.635 90)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
		)
		(property "Description" "Triode for alternating current, gate/anode2/anode1"
			(at 0 0 0)
		)
		(property "ki_keywords" "TRIAC"
			(at 0 0 0)
		)
		(symbol "Generic_Triac_GA2A1_0_1")
		(symbol "Generic_Triac_GA2A1_1_1"
			(pin input line
				(at -3.81 -2.54 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin passive line
				(at 0 3.81 270)
				(length 2.54)
				(name "A2")
				(number "2")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 2.54)
				(name "A1")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TIC106"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 2.54 1.905 0)
		)
		(property "Value" "TIC106"
			(at 2.54 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 2.54 -1.905 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheet/PowerInnovations/mXyzrtvs.pdf"
			(at 0 0 0)
		)
		(property "Description" "5A Ion, 400-800V Voff, Silicon Controlled Rectifier (Thyristor), TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "thyristor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
		(symbol "TIC106_0_1")
		(symbol "TIC106_1_1"
			(pin input line
				(at -3.81 -2.54 0)
				(length 2.54)
				(name "G")
				(number "3")
			)
			(pin passive line
				(at 0 3.81 270)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 2.54)
				(name "K")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TIC226"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "TIC226"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheet/PowerInnovations/mXuqxvy.pdf"
			(at 0 0 0)
		)
		(property "Description" "8A RMS, 400-800V Off-State Voltage, Triac, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
		(symbol "TIC226_0_1")
		(symbol "TIC226_1_1"
			(pin input line
				(at -3.81 -2.54 0)
				(length 2.54)
				(name "G")
				(number "3")
			)
			(pin passive line
				(at 0 3.81 270)
				(length 2.54)
				(name "A2")
				(number "2")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 2.54)
				(name "A1")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "X0202MN"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "Q"
			(at 2.54 1.905 0)
		)
		(property "Value" "X0202MN"
			(at 2.54 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223"
			(at 2.54 -1.905 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/x02.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.25A Ion, 600 Voff, Silicon Controlled Rectifier (Thyristor), SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "thyristor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
		(symbol "X0202MN_0_1")
		(symbol "X0202MN_1_1"
			(pin input line
				(at -3.81 -2.54 0)
				(length 2.54)
				(name "G")
				(number "3")
			)
			(pin passive line
				(at 0 3.81 270)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin passive line
				(at 0 3.81 270)
				(length 2.54)
				(hide yes)
				(name "A")
				(number "4")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 2.54)
				(name "K")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Z0103MN"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 3.175 0.635 0)
		)
		(property "Value" "Z0103MN"
			(at 3.175 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223"
			(at 19.05 -3.81 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/z01.pdf"
			(at 3.81 7.62 0)
		)
		(property "Description" "4Q Triac, 1A RMS, 600V VDRM, 3mA Igt, 7mA Ih, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Q Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*223*"
			(at 0 0 0)
		)
		(symbol "Z0103MN_0_1")
		(symbol "Z0103MN_1_1"
			(pin input line
				(at -3.81 -2.54 0)
				(length 2.54)
				(name "G")
				(number "3")
			)
			(pin passive line
				(at 0 3.81 270)
				(length 2.54)
				(name "A2")
				(number "2")
			)
			(pin passive line
				(at 0 3.81 270)
				(length 2.54)
				(hide yes)
				(name "A4")
				(number "4")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 2.54)
				(name "A1")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BT136-500"
		(extends "TIC226")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BT136-500"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.micropik.com/PDF/BT136-600.pdf"
			(at 0 0 0)
		)
		(property "Description" "4A RMS, 500V Off-State Voltage, Triac, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BT136-600"
		(extends "TIC226")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BT136-600"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.micropik.com/PDF/BT136-600.pdf"
			(at 0 0 0)
		)
		(property "Description" "4A RMS, 500V Off-State Voltage, Triac, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BT136-800"
		(extends "TIC226")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BT136-800"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.micropik.com/PDF/BT136-600.pdf"
			(at 0 0 0)
		)
		(property "Description" "4A RMS, 800V Off-State Voltage, Triac, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BT138-600"
		(extends "TIC226")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BT138-600"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BT138_SER_D_E.pdf"
			(at 0 0 0)
		)
		(property "Description" "12A RMS, 600V Off-State Voltage, Triac, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BT138-800"
		(extends "TIC226")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BT138-800"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BT138_SER_D_E.pdf"
			(at 0 0 0)
		)
		(property "Description" "12A RMS, 800V Off-State Voltage, Triac, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BT139-600"
		(extends "TIC226")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BT139-600"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.rapidonline.com/pdf/47-3240.pdf"
			(at 0 0 0)
		)
		(property "Description" "16A RMS, 600V Off-State Voltage, 4Q Triac, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BT169D"
		(extends "BT169B")
		(property "Reference" "Q"
			(at 2.54 1.905 0)
		)
		(property "Value" "BT169D"
			(at 2.54 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 2.54 -1.905 0)
		)
		(property "Datasheet" "https://media.digikey.com/pdf/Data%20Sheets/NXP%20PDFs/BT169_Series.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.5A Ion, 400V Voff, Thyristors logic level, Silicon Controlled Rectifier (Thyristor), TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "thyristor logic level"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*Inline*Narrow*"
			(at 0 0 0)
		)
	)
	(symbol "BT169G"
		(extends "BT169B")
		(property "Reference" "Q"
			(at 2.54 1.905 0)
		)
		(property "Value" "BT169G"
			(at 2.54 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 2.54 -1.905 0)
		)
		(property "Datasheet" "https://media.digikey.com/pdf/Data%20Sheets/NXP%20PDFs/BT169_Series.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.5A Ion, 600V Voff, Thyristors logic level, Silicon Controlled Rectifier (Thyristor), TO-92"
			(at 0 0 0)
		)
		(property "ki_keywords" "thyristor logic level"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?92*Inline*Narrow*"
			(at 0 0 0)
		)
	)
	(symbol "BTA16-600B"
		(extends "TIC226")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BTA16-600B"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/bta16.pdf"
			(at 0 0 0)
		)
		(property "Description" "16A RMS, 600V Off-State Voltage, 50mA Sensitivity, Insulated, Triac, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BTA16-600BW"
		(extends "TIC226")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BTA16-600BW"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/bta16.pdf"
			(at 0 0 0)
		)
		(property "Description" "16A RMS, 600V Off-State Voltage, 50mA Sensitivity, Snubberless, Insulated, Triac, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BTA16-600C"
		(extends "TIC226")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BTA16-600C"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/bta16.pdf"
			(at 0 0 0)
		)
		(property "Description" "16A RMS, 600V Off-State Voltage, 35mA Sensitivity, Insulated, Triac, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BTA16-600CW"
		(extends "TIC226")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BTA16-600CW"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/bta16.pdf"
			(at 0 0 0)
		)
		(property "Description" "16A RMS, 600V Off-State Voltage, 35mA Sensitivity, Snubberless, Insulated, Triac, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BTA16-600SW"
		(extends "TIC226")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BTA16-600SW"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/bta16.pdf"
			(at 0 0 0)
		)
		(property "Description" "16A RMS, 600V Off-State Voltage, 10mA Sensitivity, Snubberless, Insulated, Triac, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BTA16-800B"
		(extends "TIC226")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BTA16-800B"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/bta16.pdf"
			(at 0 0 0)
		)
		(property "Description" "16A RMS, 800V Off-State Voltage, 50mA Sensitivity, Insulated, Triac, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BTA16-800BW"
		(extends "TIC226")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BTA16-800BW"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/bta16.pdf"
			(at 0 0 0)
		)
		(property "Description" "16A RMS, 800V Off-State Voltage, 50mA Sensitivity, Snubberless, Insulated, Triac, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BTA16-800C"
		(extends "TIC226")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BTA16-800C"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/bta16.pdf"
			(at 0 0 0)
		)
		(property "Description" "16A RMS, 800V Off-State Voltage, 35mA Sensitivity, Insulated, Triac, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BTA16-800CW"
		(extends "TIC226")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BTA16-800CW"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/bta16.pdf"
			(at 0 0 0)
		)
		(property "Description" "16A RMS, 800V Off-State Voltage, 35mA Sensitivity, Snubberless, Insulated, Triac, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BTA16-800SW"
		(extends "TIC226")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BTA16-800SW"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/bta16.pdf"
			(at 0 0 0)
		)
		(property "Description" "16A RMS, 800V Off-State Voltage, 10mA Sensitivity, Snubberless, Insulated, Triac, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BTB16-600B"
		(extends "TIC226")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BTB16-600B"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/bta16.pdf"
			(at 0 0 0)
		)
		(property "Description" "16A RMS, 600V Off-State Voltage, 50mA Sensitivity, Non-Insulated, Triac, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BTB16-600BW"
		(extends "TIC226")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BTB16-600BW"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/bta16.pdf"
			(at 0 0 0)
		)
		(property "Description" "16A RMS, 600V Off-State Voltage, 50mA Sensitivity, Snubberless, Non-Insulated, Triac, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BTB16-600C"
		(extends "TIC226")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BTB16-600C"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/bta16.pdf"
			(at 0 0 0)
		)
		(property "Description" "16A RMS, 600V Off-State Voltage, 35mA Sensitivity, Non-Insulated, Triac, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BTB16-600CW"
		(extends "TIC226")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BTB16-600CW"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/bta16.pdf"
			(at 0 0 0)
		)
		(property "Description" "16A RMS, 600V Off-State Voltage, 35mA Sensitivity, Snubberless, Non-Insulated, Triac, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BTB16-600SW"
		(extends "TIC226")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BTB16-600SW"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/bta16.pdf"
			(at 0 0 0)
		)
		(property "Description" "16A RMS, 600V Off-State Voltage, 10mA Sensitivity, Snubberless, Non-Insulated, Triac, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BTB16-800B"
		(extends "TIC226")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BTB16-800B"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/bta16.pdf"
			(at 0 0 0)
		)
		(property "Description" "16A RMS, 800V Off-State Voltage, 50mA Sensitivity, Non-Insulated, Triac, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BTB16-800BW"
		(extends "TIC226")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BTB16-800BW"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/bta16.pdf"
			(at 0 0 0)
		)
		(property "Description" "16A RMS, 800V Off-State Voltage, 50mA Sensitivity, Snubberless, Non-Insulated, Triac, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BTB16-800C"
		(extends "TIC226")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BTB16-800C"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/bta16.pdf"
			(at 0 0 0)
		)
		(property "Description" "16A RMS, 800V Off-State Voltage, 35mA Sensitivity, Non-Insulated, Triac, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BTB16-800CW"
		(extends "TIC226")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BTB16-800CW"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/bta16.pdf"
			(at 0 0 0)
		)
		(property "Description" "16A RMS, 800V Off-State Voltage, 35mA Sensitivity, Snubberless, Non-Insulated, Triac, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "BTB16-800SW"
		(extends "TIC226")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "BTB16-800SW"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/bta16.pdf"
			(at 0 0 0)
		)
		(property "Description" "16A RMS, 800V Off-State Voltage, 10mA Sensitivity, Snubberless, Non-Insulated, Triac, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "CT401T"
		(extends "TIC226")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "CT401T"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "https://www.jscj-elec.com/gallery//file/CT401T-600%20SOT-223-3LK%20V1.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A RMS, 600-800V Off-State Voltage, 1.55V On-State Voltage, Triac, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "TIC116"
		(extends "TIC106")
		(property "Reference" "Q"
			(at 2.54 1.905 0)
		)
		(property "Value" "TIC116"
			(at 2.54 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 2.54 -1.905 0)
		)
		(property "Datasheet" "https://www.princeton.edu/~mae412/HANDOUTS/Datasheets/TIC116.pdf"
			(at 0 0 0)
		)
		(property "Description" "8A Ion, 400-800V Voff, Silicon Controlled Rectifier (Thyristor), TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "thyristor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "TIC126"
		(extends "TIC106")
		(property "Reference" "Q"
			(at 2.54 1.905 0)
		)
		(property "Value" "TIC126"
			(at 2.54 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 2.54 -1.905 0)
		)
		(property "Datasheet" "https://cdn-reichelt.de/documents/datenblatt/A400/TIC126.pdf"
			(at 0 0 0)
		)
		(property "Description" "12A Ion, 400-800V Voff, Silicon Controlled Rectifier (Thyristor), TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "thyristor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "TIC206"
		(extends "TIC226")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "TIC206"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.farnell.com/datasheets/56922.pdf"
			(at 0 0 0)
		)
		(property "Description" "4A RMS, 400-700V Off-State Voltage, Sensitive Gate Triac, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "TIC216"
		(extends "TIC226")
		(property "Reference" "Q"
			(at 5.08 1.905 0)
		)
		(property "Value" "TIC216"
			(at 5.08 0 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 5.08 -1.905 0)
		)
		(property "Datasheet" "http://www.mouser.com/ds/2/54/tic216-37811.pdf"
			(at 0 0 0)
		)
		(property "Description" "6A RMS, 400-800V Off-State Voltage, Triac, TO-220"
			(at 0 0 0)
		)
		(property "ki_keywords" "Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?220*"
			(at 0 0 0)
		)
	)
	(symbol "X0202NN"
		(extends "X0202MN")
		(property "Reference" "Q"
			(at 2.54 1.905 0)
		)
		(property "Value" "X0202NN"
			(at 2.54 0 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223"
			(at 2.54 -1.905 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/x02.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.25A Ion, 800 Voff, Silicon Controlled Rectifier (Thyristor), SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "thyristor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?223*"
			(at 0 0 0)
		)
	)
	(symbol "Z0103NN"
		(extends "Z0103MN")
		(property "Reference" "D"
			(at 3.175 0.635 0)
		)
		(property "Value" "Z0103NN"
			(at 3.175 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223"
			(at 19.05 -3.81 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/z01.pdf"
			(at 3.81 7.62 0)
		)
		(property "Description" "4Q Triac, 1A RMS, 800V VDRM, 3mA Igt, 7mA Ih, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Q Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*223*"
			(at 0 0 0)
		)
	)
	(symbol "Z0107MN"
		(extends "Z0103MN")
		(property "Reference" "D"
			(at 3.175 0.635 0)
		)
		(property "Value" "Z0107MN"
			(at 3.175 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223"
			(at 19.05 -3.81 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/z01.pdf"
			(at 3.81 7.62 0)
		)
		(property "Description" "4Q Triac, 1A RMS, 600V VDRM, 5mA Igt, 10mA Ih, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Q Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*223*"
			(at 0 0 0)
		)
	)
	(symbol "Z0107NN"
		(extends "Z0103MN")
		(property "Reference" "D"
			(at 3.175 0.635 0)
		)
		(property "Value" "Z0107NN"
			(at 3.175 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223"
			(at 19.05 -3.81 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/z01.pdf"
			(at 3.81 7.62 0)
		)
		(property "Description" "4Q Triac, 1A RMS, 800V VDRM, 5mA Igt, 10mA Ih, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Q Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*223*"
			(at 0 0 0)
		)
	)
	(symbol "Z0109MN"
		(extends "Z0103MN")
		(property "Reference" "D"
			(at 3.175 0.635 0)
		)
		(property "Value" "Z0109MN"
			(at 3.175 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223"
			(at 19.05 -3.81 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/z01.pdf"
			(at 3.81 7.62 0)
		)
		(property "Description" "4Q Triac, 1A RMS, 600V VDRM, 10mA Igt, 10mA Ih, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Q Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*223*"
			(at 0 0 0)
		)
	)
	(symbol "Z0109NN"
		(extends "Z0103MN")
		(property "Reference" "D"
			(at 3.175 0.635 0)
		)
		(property "Value" "Z0109NN"
			(at 3.175 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223"
			(at 19.05 -3.81 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/z01.pdf"
			(at 3.81 7.62 0)
		)
		(property "Description" "4Q Triac, 1A RMS, 800V VDRM, 10mA Igt, 10mA Ih, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Q Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*223*"
			(at 0 0 0)
		)
	)
	(symbol "Z0110MN"
		(extends "Z0103MN")
		(property "Reference" "D"
			(at 3.175 0.635 0)
		)
		(property "Value" "Z0110MN"
			(at 3.175 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223"
			(at 19.05 -3.81 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/z01.pdf"
			(at 3.81 7.62 0)
		)
		(property "Description" "4Q Triac, 1A RMS, 600V VDRM, 25mA Igt, 25mA Ih, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Q Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*223*"
			(at 0 0 0)
		)
	)
	(symbol "Z0110NN"
		(extends "Z0103MN")
		(property "Reference" "D"
			(at 3.175 0.635 0)
		)
		(property "Value" "Z0110NN"
			(at 3.175 -1.27 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223"
			(at 19.05 -3.81 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/z01.pdf"
			(at 3.81 7.62 0)
		)
		(property "Description" "4Q Triac, 1A RMS, 800V VDRM, 25mA Igt, 25mA Ih, SOT-223"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Q Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*223*"
			(at 0 0 0)
		)
	)
)
