(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "CK6418"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.096 10.16 0)
		)
		(property "Value" "CK6418"
			(at 8.128 8.382 0)
		)
		(property "Footprint" "Valve:Valve_Mini_Pentode_Linear"
			(at 13.208 0.762 0)
		)
		(property "Datasheet" "https://frank.pocnet.net/sheets/127/6/6418.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Subminiature Pentode"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "subminiature pentode valve"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VALVE*MINI*PENTODE*LINEAR*"
			(at 0 0 0)
		)
		(symbol "CK6418_0_1"
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "F+,G3")
				(number "3")
			)
		)
		(symbol "CK6418_1_0")
		(symbol "CK6418_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "G1")
				(number "4")
			)
			(pin output line
				(at 0 12.7 270)
				(length 2.54)
				(name "P")
				(number "1")
			)
			(pin input line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "G2")
				(number "2")
			)
		)
		(symbol "CK6418_2_1"
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "F+,G3")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EABC80"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 6.35 0)
		)
		(property "Value" "EABC80"
			(at 7.62 -8.89 0)
		)
		(property "Footprint" "Valve:Valve_Noval_P"
			(at 4.318 -10.414 0)
		)
		(property "Datasheet" "https://frank.pocnet.net/sheets/082/e/EABC80.pdf"
			(at 0 0 0)
		)
		(property "Description" "triple diode triode"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "diode triode valve"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VALVE*NOVAL*P*"
			(at 0 0 0)
		)
		(symbol "EABC80_0_1")
		(symbol "EABC80_1_0")
		(symbol "EABC80_1_1"
			(pin input line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "K")
				(number "3")
			)
			(pin output line
				(at 0 10.16 270)
				(length 2.54)
				(name "A2")
				(number "2")
			)
		)
		(symbol "EABC80_2_1"
			(pin input line
				(at -2.54 10.16 270)
				(length 3.81)
				(name "A1")
				(number "1")
			)
			(pin input line
				(at -2.54 -10.16 90)
				(length 3.81)
				(name "K")
				(number "7")
			)
			(pin output line
				(at 2.54 10.16 270)
				(length 3.81)
				(name "A3")
				(number "6")
			)
		)
		(symbol "EABC80_3_0")
		(symbol "EABC80_3_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "G")
				(number "8")
			)
			(pin input line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "K")
				(number "7")
			)
			(pin output line
				(at 0 10.16 270)
				(length 2.54)
				(name "A2")
				(number "9")
			)
		)
		(symbol "EABC80_4_1"
			(pin input line
				(at -2.54 -8.89 90)
				(length 2.54)
				(name "F1")
				(number "4")
			)
			(pin input line
				(at 2.54 -8.89 90)
				(length 2.54)
				(name "F2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EC92"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.048 7.874 0)
		)
		(property "Value" "EC92"
			(at 4.318 -8.128 0)
		)
		(property "Footprint" "Valve:Valve_Mini_P"
			(at 6.858 -9.652 0)
		)
		(property "Datasheet" "http://www.r-type.org/pdfs/ec92.pdf"
			(at 0 0 0)
		)
		(property "Description" "single triode"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "triode valve"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VALVE*MINI*P*"
			(at 0 0 0)
		)
		(symbol "EC92_0_1")
		(symbol "EC92_1_0")
		(symbol "EC92_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "G")
				(number "6")
			)
			(pin bidirectional line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "K")
				(number "7")
			)
			(pin output line
				(at 0 10.16 270)
				(length 2.54)
				(name "A")
				(number "1")
			)
		)
		(symbol "EC92_2_1"
			(pin power_in line
				(at -2.54 -8.89 90)
				(length 2.54)
				(name "F1")
				(number "3")
			)
			(pin power_in line
				(at 2.54 -8.89 90)
				(length 2.54)
				(name "F2")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ECC81"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.302 7.874 0)
		)
		(property "Value" "ECC81"
			(at 8.89 -7.62 0)
		)
		(property "Footprint" "Valve:Valve_Noval_P"
			(at 6.858 -10.16 0)
		)
		(property "Datasheet" "http://www.r-type.org/pdfs/ecc81.pdf"
			(at 0 0 0)
		)
		(property "Description" "double triode"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "triode valve"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VALVE*NOVAL*P*"
			(at 0 0 0)
		)
		(symbol "ECC81_0_1")
		(symbol "ECC81_1_0")
		(symbol "ECC81_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "G")
				(number "7")
			)
			(pin bidirectional line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "K")
				(number "8")
			)
			(pin output line
				(at 0 10.16 270)
				(length 2.54)
				(name "A")
				(number "6")
			)
		)
		(symbol "ECC81_2_0")
		(symbol "ECC81_2_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin bidirectional line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "K")
				(number "3")
			)
			(pin output line
				(at 0 10.16 270)
				(length 2.54)
				(name "A")
				(number "1")
			)
		)
		(symbol "ECC81_3_1"
			(pin power_in line
				(at -2.54 -11.43 90)
				(length 5.08)
				(name "F1")
				(number "4")
			)
			(pin power_in line
				(at 0 -11.43 90)
				(length 5.08)
				(name "F2")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -11.43 90)
				(length 5.08)
				(name "F1")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ECC88"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 4.318 7.112 0)
		)
		(property "Value" "ECC88"
			(at 5.08 -7.62 0)
		)
		(property "Footprint" "Valve:Valve_Noval_P"
			(at 6.858 -10.16 0)
		)
		(property "Datasheet" "http://www.r-type.org/pdfs/ecc88.pdf"
			(at 0 0 0)
		)
		(property "Description" "double triode, low-noise"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "triode valve"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VALVE*NOVAL*P*"
			(at 0 0 0)
		)
		(symbol "ECC88_0_1")
		(symbol "ECC88_1_0")
		(symbol "ECC88_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "G")
				(number "2")
			)
			(pin bidirectional line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "K")
				(number "3")
			)
			(pin output line
				(at 0 10.16 270)
				(length 2.54)
				(name "A")
				(number "1")
			)
		)
		(symbol "ECC88_2_0")
		(symbol "ECC88_2_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "G")
				(number "7")
			)
			(pin bidirectional line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "K")
				(number "8")
			)
			(pin output line
				(at 0 10.16 270)
				(length 2.54)
				(name "A")
				(number "6")
			)
		)
		(symbol "ECC88_3_1"
			(pin power_in line
				(at -2.54 -11.43 90)
				(length 5.08)
				(name "F1")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -11.43 90)
				(length 5.08)
				(name "F2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ECH81"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 12.7 0)
		)
		(property "Value" "ECH81"
			(at 5.715 -9.525 0)
		)
		(property "Footprint" "Valve:Valve_Noval_P"
			(at 7.62 -11.43 0)
		)
		(property "Datasheet" "http://www.r-type.org/pdfs/ech81.pdf"
			(at 0 0 0)
		)
		(property "Description" "triode heptode"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "triode heptode valve"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VALVE*NOVAL*P*"
			(at 0 0 0)
		)
		(symbol "ECH81_0_1")
		(symbol "ECH81_1_0")
		(symbol "ECH81_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "G")
				(number "9")
			)
			(pin bidirectional line
				(at -2.54 -12.7 90)
				(length 3.81)
				(name "K")
				(number "3")
			)
			(pin output line
				(at 0 13.97 270)
				(length 2.54)
				(name "A")
				(number "8")
			)
		)
		(symbol "ECH81_2_0")
		(symbol "ECH81_2_1"
			(pin input line
				(at -7.62 1.27 0)
				(length 2.54)
				(name "G3")
				(number "7")
			)
			(pin input line
				(at -7.62 -3.81 0)
				(length 2.54)
				(name "G1")
				(number "2")
			)
			(pin bidirectional line
				(at -2.54 -11.43 90)
				(length 2.54)
				(name "K_G5")
				(number "~")
			)
			(pin output line
				(at 0 13.97 270)
				(length 2.54)
				(name "A")
				(number "6")
			)
			(pin input line
				(at 7.62 3.81 180)
				(length 2.54)
				(name "G2_G4")
				(number "1")
			)
		)
		(symbol "ECH81_3_1"
			(pin power_in line
				(at -2.54 -13.97 90)
				(length 7.62)
				(name "F1")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -13.97 90)
				(length 7.62)
				(name "F2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ECL82"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 7.62 0)
		)
		(property "Value" "ECL82"
			(at 7.62 -8.89 0)
		)
		(property "Footprint" "Valve:Valve_Noval_P"
			(at 0 3.81 0)
		)
		(property "Datasheet" "http://www.r-type.org/pdfs/ecl82.pdf"
			(at 0 0 0)
		)
		(property "Description" "triode pentode"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "triode pentode valve"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Valve*Noval*P*"
			(at 0 0 0)
		)
		(symbol "ECL82_0_1")
		(symbol "ECL82_1_0")
		(symbol "ECL82_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin bidirectional line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "K")
				(number "8")
			)
			(pin output line
				(at 0 10.16 270)
				(length 2.54)
				(name "A")
				(number "9")
			)
		)
		(symbol "ECL82_2_0")
		(symbol "ECL82_2_1"
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "G1")
				(number "3")
			)
			(pin bidirectional line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "K_G3")
				(number "2")
			)
			(pin output line
				(at 0 10.16 270)
				(length 2.54)
				(name "A")
				(number "6")
			)
			(pin input line
				(at 7.62 0 180)
				(length 2.54)
				(name "G2")
				(number "7")
			)
		)
		(symbol "ECL82_3_1"
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 3.81)
				(name "F1")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 3.81)
				(name "F2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ECL86"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 7.62 0)
		)
		(property "Value" "ECL86"
			(at 7.62 -7.62 0)
		)
		(property "Footprint" "Valve:Valve_Noval_P"
			(at 0 3.81 0)
		)
		(property "Datasheet" "http://www.r-type.org/pdfs/ecl86.pdf"
			(at 0 0 0)
		)
		(property "Description" "triode pentode"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "triode pentode valve"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Valve*Noval*P*"
			(at 0 0 0)
		)
		(symbol "ECL86_0_1")
		(symbol "ECL86_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin bidirectional line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "K")
				(number "2")
			)
			(pin output line
				(at 0 10.16 270)
				(length 2.54)
				(name "A")
				(number "9")
			)
		)
		(symbol "ECL86_2_0")
		(symbol "ECL86_2_1"
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "G1")
				(number "8")
			)
			(pin bidirectional line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "K_G3")
				(number "7")
			)
			(pin output line
				(at 0 10.16 270)
				(length 2.54)
				(name "A")
				(number "6")
			)
			(pin input line
				(at 7.62 0 180)
				(length 2.54)
				(name "G2")
				(number "3")
			)
		)
		(symbol "ECL86_3_1"
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 3.81)
				(name "F1")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 3.81)
				(name "F2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EF80"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.556 8.89 0)
		)
		(property "Value" "EF80"
			(at 5.08 -8.89 0)
		)
		(property "Footprint" "Valve:Valve_Noval_P"
			(at 8.89 -8.89 0)
		)
		(property "Datasheet" "http://www.r-type.org/pdfs/ef80.pdf"
			(at 0 0 0)
		)
		(property "Description" "pentode"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "pentode valve"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VALVE*NOVAL*P*"
			(at 0 0 0)
		)
		(symbol "EF80_0_1")
		(symbol "EF80_1_0")
		(symbol "EF80_1_1"
			(pin input line
				(at -7.62 -1.27 0)
				(length 2.54)
				(name "G1")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 3.302)
				(name "F1")
				(number "3")
			)
			(pin output line
				(at 0 11.43 270)
				(length 2.54)
				(name "A")
				(number "7")
			)
			(pin input line
				(at 7.62 3.81 180)
				(length 2.54)
				(name "G3")
				(number "9")
			)
			(pin input line
				(at 7.62 1.27 180)
				(length 2.54)
				(name "G2")
				(number "8")
			)
			(pin input line
				(at 7.62 -3.81 180)
				(length 2.54)
				(name "S")
				(number "6")
			)
		)
		(symbol "EF80_2_1"
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 3.302)
				(name "F1")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 3.302)
				(name "F2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EF83"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 10.16 0)
		)
		(property "Value" "EF83"
			(at 6.35 -8.89 0)
		)
		(property "Footprint" "Valve:Valve_Noval_P"
			(at 12.7 -7.62 0)
		)
		(property "Datasheet" "http://www.r-type.org/pdfs/ef83.pdf"
			(at 0 0 0)
		)
		(property "Description" "pentode"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "pentode valve"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VALVE*NOVAL*P*"
			(at 0 0 0)
		)
		(symbol "EF83_0_1")
		(symbol "EF83_1_0")
		(symbol "EF83_1_1"
			(pin input line
				(at -7.62 -1.27 0)
				(length 2.54)
				(name "G1")
				(number "9")
			)
			(pin bidirectional line
				(at -2.54 -8.89 90)
				(length 2.54)
				(name "K")
				(number "3")
			)
			(pin output line
				(at 0 11.43 270)
				(length 2.54)
				(name "A")
				(number "6")
			)
			(pin input line
				(at 7.62 3.81 180)
				(length 2.54)
				(name "G3")
				(number "8")
			)
			(pin input line
				(at 7.62 1.27 180)
				(length 2.54)
				(name "G2")
				(number "1")
			)
			(pin input line
				(at 7.62 -3.81 180)
				(length 2.54)
				(name "S")
				(number "7")
			)
		)
		(symbol "EF83_2_1"
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 3.81)
				(name "F1")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 3.81)
				(name "F2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EL34"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 8.89 0)
		)
		(property "Value" "EL34"
			(at 6.35 -7.62 0)
		)
		(property "Footprint" "Valve:Valve_Octal"
			(at 7.62 -8.89 0)
		)
		(property "Datasheet" "http://www.r-type.org/pdfs/el34.pdf"
			(at 0 0 0)
		)
		(property "Description" "pentode, 25W"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "pentode valve"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VALVE*OCTAL*"
			(at 0 0 0)
		)
		(symbol "EL34_0_1")
		(symbol "EL34_1_0")
		(symbol "EL34_1_1"
			(pin input line
				(at -7.62 -1.27 0)
				(length 2.54)
				(name "G1")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -8.89 90)
				(length 3.81)
				(name "F1")
				(number "8")
			)
			(pin output line
				(at 0 11.43 270)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin input line
				(at 7.62 3.81 180)
				(length 2.54)
				(name "G3")
				(number "1")
			)
			(pin input line
				(at 7.62 1.27 180)
				(length 2.54)
				(name "G2")
				(number "4")
			)
		)
		(symbol "EL34_2_1"
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 3.81)
				(name "F1")
				(number "2")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 3.81)
				(name "F2")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EL84"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 10.16 0)
		)
		(property "Value" "EL84"
			(at 7.62 -7.62 0)
		)
		(property "Footprint" "Valve:Valve_Noval_P"
			(at 7.62 -10.16 0)
		)
		(property "Datasheet" "http://www.r-type.org/pdfs/el84.pdf"
			(at 0 0 0)
		)
		(property "Description" "pentode, 12W"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "pentode valve"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VALVE*NOVAL*P*"
			(at 0 0 0)
		)
		(symbol "EL84_0_1")
		(symbol "EL84_1_0")
		(symbol "EL84_1_1"
			(pin input line
				(at -7.62 -1.27 0)
				(length 2.54)
				(name "G1")
				(number "2")
			)
			(pin bidirectional line
				(at -2.54 -8.89 90)
				(length 2.54)
				(name "K_G3")
				(number "3")
			)
			(pin output line
				(at 0 11.43 270)
				(length 2.54)
				(name "A")
				(number "7")
			)
			(pin input line
				(at 7.62 1.27 180)
				(length 2.54)
				(name "G2")
				(number "9")
			)
		)
		(symbol "EL84_2_1"
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 3.81)
				(name "F1")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 3.81)
				(name "F2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EM84"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 7.62 0)
		)
		(property "Value" "EM84"
			(at 6.35 -7.62 0)
		)
		(property "Footprint" "Valve:Valve_Noval_P"
			(at 10.16 -8.89 0)
		)
		(property "Datasheet" "http://www.r-type.org/pdfs/em84.pdf"
			(at 0 0 0)
		)
		(property "Description" "indicator tube \"magic eye\""
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "indicator tube valve magic eye"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VALVE*NOVAL*P*"
			(at 0 0 0)
		)
		(symbol "EM84_0_1")
		(symbol "EM84_1_0")
		(symbol "EM84_1_1"
			(pin bidirectional line
				(at -2.54 -8.89 90)
				(length 2.54)
				(name "K")
				(number "2")
			)
			(pin output line
				(at 0 11.43 270)
				(length 3.81)
				(name "L")
				(number "6")
			)
			(pin input line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "ST")
				(number "7")
			)
		)
		(symbol "EM84_2_0")
		(symbol "EM84_2_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "G")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 3.81)
				(name "F1")
				(number "~")
			)
			(pin output line
				(at 0 10.16 270)
				(length 2.54)
				(name "A")
				(number "9")
			)
		)
		(symbol "EM84_3_1"
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 3.81)
				(name "F1")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 3.81)
				(name "F2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STABI"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 5.715 0)
		)
		(property "Value" "STABI"
			(at 5.715 -5.715 0)
		)
		(property "Footprint" "Valve:Valve_Glimm"
			(at 0 3.81 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VALVE*GLIMM*"
			(at 0 0 0)
		)
		(symbol "STABI_1_0")
		(symbol "STABI_1_1"
			(pin passive line
				(at 0 7.62 270)
				(length 2.54)
				(name "K")
				(number "7")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(name "A")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "6AK8"
		(extends "EABC80")
		(property "Reference" "U"
			(at 5.08 6.35 0)
		)
		(property "Value" "6AK8"
			(at 7.62 -8.89 0)
		)
		(property "Footprint" "Valve:Valve_Noval_P"
			(at 4.318 -10.414 0)
		)
		(property "Datasheet" "https://frank.pocnet.net/sheets/082/e/EABC80.pdf"
			(at 0 0 0)
		)
		(property "Description" "triple diode triode"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode triode valve"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VALVE*NOVAL*P*"
			(at 0 0 0)
		)
	)
	(symbol "9AK8"
		(extends "EABC80")
		(property "Reference" "U"
			(at 5.08 6.35 0)
		)
		(property "Value" "9AK8"
			(at 7.62 -8.89 0)
		)
		(property "Footprint" "Valve:Valve_Noval_P"
			(at 4.318 -10.414 0)
		)
		(property "Datasheet" "https://frank.pocnet.net/sheets/082/e/EABC80.pdf"
			(at 0 0 0)
		)
		(property "Description" "triple diode triode"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode triode valve"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VALVE*NOVAL*P*"
			(at 0 0 0)
		)
	)
	(symbol "CK548DX"
		(extends "CK6418")
		(property "Reference" "U"
			(at 6.096 10.16 0)
		)
		(property "Value" "CK548DX"
			(at 8.128 8.382 0)
		)
		(property "Footprint" "Valve:Valve_Mini_Pentode_Linear"
			(at 13.208 0.762 0)
		)
		(property "Datasheet" ""
			(at 0 1.27 0)
		)
		(property "Description" "Subminiature Pentode"
			(at 0 0 0)
		)
		(property "ki_keywords" "subminiature pentode valve"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VALVE*MINI*PENTODE*LINEAR*"
			(at 0 0 0)
		)
	)
	(symbol "ECC83"
		(extends "ECC81")
		(property "Reference" "U"
			(at 3.302 7.874 0)
		)
		(property "Value" "ECC83"
			(at 8.89 -7.62 0)
		)
		(property "Footprint" "Valve:Valve_Noval_P"
			(at 6.858 -10.16 0)
		)
		(property "Datasheet" "http://www.r-type.org/pdfs/ecc83.pdf"
			(at 0 0 0)
		)
		(property "Description" "double triode"
			(at 0 0 0)
		)
		(property "ki_keywords" "triode valve"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VALVE*NOVAL*P*"
			(at 0 0 0)
		)
	)
	(symbol "EF85"
		(extends "EF80")
		(property "Reference" "U"
			(at 3.556 8.89 0)
		)
		(property "Value" "EF85"
			(at 5.08 -8.89 0)
		)
		(property "Footprint" "Valve:Valve_Noval_P"
			(at 8.89 -8.89 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "pentode"
			(at 0 0 0)
		)
		(property "ki_keywords" "pentode valve"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VALVE*NOVAL*P*"
			(at 0 0 0)
		)
	)
	(symbol "EF86"
		(extends "EF83")
		(property "Reference" "U"
			(at 3.81 10.16 0)
		)
		(property "Value" "EF86"
			(at 6.35 -8.89 0)
		)
		(property "Footprint" "Valve:Valve_Noval_P"
			(at 12.7 -7.62 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "pentode"
			(at 0 0 0)
		)
		(property "ki_keywords" "pentode valve"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VALVE*NOVAL*P*"
			(at 0 0 0)
		)
	)
	(symbol "JAN6418"
		(extends "CK6418")
		(property "Reference" "U"
			(at 6.096 10.16 0)
		)
		(property "Value" "JAN6418"
			(at 8.128 8.382 0)
		)
		(property "Footprint" "Valve:Valve_Mini_Pentode_Linear"
			(at 13.208 0.762 0)
		)
		(property "Datasheet" "https://frank.pocnet.net/sheets/127/6/6418.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Subminiature Pentode"
			(at 0 0 0)
		)
		(property "ki_keywords" "subminiature pentode valve"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VALVE*MINI*PENTODE*LINEAR*"
			(at 0 0 0)
		)
	)
	(symbol "NOS-6418"
		(extends "CK6418")
		(property "Reference" "U"
			(at 6.096 10.16 0)
		)
		(property "Value" "NOS-6418"
			(at 8.128 8.382 0)
		)
		(property "Footprint" "Valve:Valve_Mini_Pentode_Linear"
			(at 13.208 0.762 0)
		)
		(property "Datasheet" "https://frank.pocnet.net/sheets/127/6/6418.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Subminiature Pentode"
			(at 0 0 0)
		)
		(property "ki_keywords" "subminiature pentode valve"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VALVE*MINI*PENTODE*LINEAR*"
			(at 0 0 0)
		)
	)
	(symbol "PABC80"
		(extends "EABC80")
		(property "Reference" "U"
			(at 5.08 6.35 0)
		)
		(property "Value" "PABC80"
			(at 7.62 -8.89 0)
		)
		(property "Footprint" "Valve:Valve_Noval_P"
			(at 4.318 -10.414 0)
		)
		(property "Datasheet" "https://frank.pocnet.net/sheets/082/e/EABC80.pdf"
			(at 0 0 0)
		)
		(property "Description" "triple diode triode"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode triode valve"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VALVE*NOVAL*P*"
			(at 0 0 0)
		)
	)
	(symbol "UABC80"
		(extends "EABC80")
		(property "Reference" "U"
			(at 5.08 6.35 0)
		)
		(property "Value" "UABC80"
			(at 7.62 -8.89 0)
		)
		(property "Footprint" "Valve:Valve_Noval_P"
			(at 4.318 -10.414 0)
		)
		(property "Datasheet" "https://frank.pocnet.net/sheets/082/e/EABC80.pdf"
			(at 0 0 0)
		)
		(property "Description" "triple diode triode"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode triode valve"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VALVE*NOVAL*P*"
			(at 0 0 0)
		)
	)
)
