(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "AD725"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 13.97 0)
		)
		(property "Value" "AD725"
			(at 12.7 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 19.05 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD725.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low Cost RGB to NTSC/PAL Encoder with Luma Trap Port"
			(at 0 0 0)
		)
		(property "ki_keywords" "Video"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AD725_0_1")
		(symbol "AD725_1_1"
			(pin power_in line
				(at -22.86 10.16 0)
				(length 7.62)
				(name "CE")
				(number "5")
			)
			(pin input line
				(at -22.86 7.62 0)
				(length 7.62)
				(name "NTSC/PAL")
				(number "1")
			)
			(pin input line
				(at -22.86 5.08 0)
				(length 7.62)
				(name "HSYNC")
				(number "16")
			)
			(pin input line
				(at -22.86 2.54 0)
				(length 7.62)
				(name "VSYNC")
				(number "15")
			)
			(pin input line
				(at -22.86 0 0)
				(length 7.62)
				(name "4FSC_CLK")
				(number "3")
			)
			(pin input line
				(at -22.86 -5.08 0)
				(length 7.62)
				(name "RED")
				(number "6")
			)
			(pin input line
				(at -22.86 -7.62 0)
				(length 7.62)
				(name "GREEN")
				(number "7")
			)
			(pin input line
				(at -22.86 -10.16 0)
				(length 7.62)
				(name "BLUE")
				(number "8")
			)
			(pin power_in line
				(at -2.54 16.51 270)
				(length 3.81)
				(name "AVCC")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 3.81)
				(name "AGND")
				(number "2")
			)
			(pin power_in line
				(at 1.27 16.51 270)
				(length 3.81)
				(name "DVCC")
				(number "14")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 3.81)
				(name "DGND")
				(number "13")
			)
			(pin output line
				(at 22.86 7.62 180)
				(length 7.62)
				(name "LUM_OUT")
				(number "11")
			)
			(pin output line
				(at 22.86 2.54 180)
				(length 7.62)
				(name "CHROM_OUT")
				(number "9")
			)
			(pin output line
				(at 22.86 -2.54 180)
				(length 7.62)
				(name "CVBS_OUT")
				(number "10")
			)
			(pin input line
				(at 22.86 -7.62 180)
				(length 7.62)
				(name "TRAP")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD9708AR"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 20.32 0)
		)
		(property "Value" "AD9708AR"
			(at 7.62 20.32 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD9708.pdf"
			(at 0 0 0)
		)
		(property "Description" "Video DAC (32 MHz), SOIC/TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "DAC CNA VIDEO"
			(at 0 0 0)
		)
		(symbol "AD9708AR_0_1")
		(symbol "AD9708AR_1_1"
			(pin input line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "DB0")
				(number "8")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "DB1")
				(number "7")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "DB2")
				(number "6")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "DB3")
				(number "5")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "DB4")
				(number "4")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "DB5")
				(number "3")
			)
			(pin input line
				(at -17.78 0 0)
				(length 3.81)
				(name "DB6")
				(number "2")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "DB7")
				(number "1")
			)
			(pin input clock
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "Clock")
				(number "28")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "SLEEP")
				(number "15")
			)
			(pin power_in line
				(at -5.08 22.86 270)
				(length 3.81)
				(name "DVDD")
				(number "27")
			)
			(pin power_in line
				(at -2.54 -22.86 90)
				(length 3.81)
				(name "DCOM")
				(number "26")
			)
			(pin power_in line
				(at 2.54 -22.86 90)
				(length 3.81)
				(name "ACOM")
				(number "20")
			)
			(pin power_in line
				(at 5.08 22.86 270)
				(length 3.81)
				(name "AVDD")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "REFIO")
				(number "17")
			)
			(pin power_in line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "REFLO")
				(number "16")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "FS_ADJ")
				(number "18")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "IOUTA")
				(number "22")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "IOUTB")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "COMP1")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "COMP2")
				(number "23")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD9891"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 59.69 0)
		)
		(property "Value" "AD9891"
			(at -13.97 57.15 0)
		)
		(property "Footprint" "Package_BGA:BGA-64_9.0x9.0mm_Layout10x10_P0.8mm"
			(at -16.51 57.15 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD9891_9895.pdf"
			(at 0 0 0)
		)
		(property "Description" "CCD Signal Processor, 20MHz 10bits, CSPBGA-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "CCD Signal Processor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BGA*9.0x9.0mm*Layout10x10*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "AD9891_0_1")
		(symbol "AD9891_1_1"
			(pin input line
				(at -17.78 48.26 0)
				(length 3.81)
				(name "SL")
				(number "B5")
			)
			(pin input line
				(at -17.78 45.72 0)
				(length 3.81)
				(name "SDI")
				(number "A4")
			)
			(pin input clock
				(at -17.78 43.18 0)
				(length 3.81)
				(name "SCK")
				(number "B4")
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 3.81)
				(name "VD")
				(number "A1")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 3.81)
				(name "HD")
				(number "B1")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 3.81)
				(name "SYNC")
				(number "C1")
			)
			(pin input clock
				(at -17.78 20.32 0)
				(length 3.81)
				(name "CLI")
				(number "C10")
			)
			(pin output clock
				(at -17.78 17.78 0)
				(length 3.81)
				(name "CLO")
				(number "D10")
			)
			(pin power_out line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "DRVDD")
				(number "K3")
			)
			(pin power_out line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "DRVSS")
				(number "K4")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "CDD-IN")
				(number "A8")
			)
			(pin power_in line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "RGVDD")
				(number "E10")
			)
			(pin power_in line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "RGVSS")
				(number "E9")
			)
			(pin power_in line
				(at -17.78 -12.7 0)
				(length 3.81)
				(name "HVDD")
				(number "G10")
			)
			(pin power_in line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "HVSS")
				(number "G9")
			)
			(pin power_in line
				(at -17.78 -20.32 0)
				(length 3.81)
				(name "TCVDD")
				(number "B10")
			)
			(pin power_in line
				(at -17.78 -22.86 0)
				(length 3.81)
				(name "TCVSS")
				(number "C9")
			)
			(pin power_in line
				(at -17.78 -27.94 0)
				(length 3.81)
				(name "AVDD1")
				(number "A10")
			)
			(pin power_in line
				(at -17.78 -30.48 0)
				(length 3.81)
				(name "AVDD2")
				(number "B7")
			)
			(pin power_in line
				(at -17.78 -35.56 0)
				(length 3.81)
				(name "AVSS1")
				(number "B9")
			)
			(pin power_in line
				(at -17.78 -38.1 0)
				(length 3.81)
				(name "AVSS2")
				(number "B6")
			)
			(pin power_in line
				(at -17.78 -43.18 0)
				(length 3.81)
				(name "DVDD")
				(number "A2")
			)
			(pin power_in line
				(at -17.78 -45.72 0)
				(length 3.81)
				(name "DVSS")
				(number "B2")
			)
			(pin output line
				(at -17.78 -50.8 0)
				(length 3.81)
				(name "REFB")
				(number "A6")
			)
			(pin output line
				(at -17.78 -53.34 0)
				(length 3.81)
				(name "REFT")
				(number "A5")
			)
			(pin output line
				(at 17.78 53.34 180)
				(length 3.81)
				(name "D0/SD0")
				(number "F2")
			)
			(pin output line
				(at 17.78 50.8 180)
				(length 3.81)
				(name "D1")
				(number "F1")
			)
			(pin output line
				(at 17.78 48.26 180)
				(length 3.81)
				(name "D2")
				(number "G2")
			)
			(pin output line
				(at 17.78 45.72 180)
				(length 3.81)
				(name "D3")
				(number "G1")
			)
			(pin output line
				(at 17.78 43.18 180)
				(length 3.81)
				(name "D4")
				(number "H2")
			)
			(pin output line
				(at 17.78 40.64 180)
				(length 3.81)
				(name "D5")
				(number "H1")
			)
			(pin output line
				(at 17.78 38.1 180)
				(length 3.81)
				(name "D6")
				(number "J2")
			)
			(pin output line
				(at 17.78 35.56 180)
				(length 3.81)
				(name "D7")
				(number "J1")
			)
			(pin output line
				(at 17.78 33.02 180)
				(length 3.81)
				(name "D8")
				(number "K2")
			)
			(pin input line
				(at 17.78 30.48 180)
				(length 3.81)
				(name "D9")
				(number "K1")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "LD/FD")
				(number "C2")
			)
			(pin output clock
				(at 17.78 17.78 180)
				(length 3.81)
				(name "DCLK")
				(number "D1")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "PBLK/CLPOB")
				(number "D2")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "MSHUT")
				(number "A3")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "STROBE")
				(number "B3")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "RG")
				(number "D9")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "H1")
				(number "H10")
			)
			(pin output line
				(at 17.78 0 180)
				(length 3.81)
				(name "H2")
				(number "H9")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "H3")
				(number "F10")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "H4")
				(number "F9")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "V1")
				(number "K5")
			)
			(pin output line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "V2")
				(number "J5")
			)
			(pin output line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "V3")
				(number "K6")
			)
			(pin output line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "V4")
				(number "J6")
			)
			(pin output line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "VSG1/V5")
				(number "K7")
			)
			(pin output line
				(at 17.78 -20.32 180)
				(length 3.81)
				(name "VSG2/V6")
				(number "J7")
			)
			(pin output line
				(at 17.78 -22.86 180)
				(length 3.81)
				(name "VSG3/V7")
				(number "K8")
			)
			(pin output line
				(at 17.78 -25.4 180)
				(length 3.81)
				(name "VSG4/V8")
				(number "J8")
			)
			(pin output line
				(at 17.78 -27.94 180)
				(length 3.81)
				(name "VSG5")
				(number "K9")
			)
			(pin output line
				(at 17.78 -30.48 180)
				(length 3.81)
				(name "VSG6")
				(number "J9")
			)
			(pin output line
				(at 17.78 -33.02 180)
				(length 3.81)
				(name "VSG7")
				(number "K10")
			)
			(pin output line
				(at 17.78 -35.56 180)
				(length 3.81)
				(name "VSG8")
				(number "J10")
			)
			(pin output line
				(at 17.78 -40.64 180)
				(length 3.81)
				(name "VSUB")
				(number "J3")
			)
			(pin output clock
				(at 17.78 -43.18 180)
				(length 3.81)
				(name "SUBCK")
				(number "J4")
			)
			(pin output line
				(at 17.78 -48.26 180)
				(length 3.81)
				(name "BYP1")
				(number "A9")
			)
			(pin output line
				(at 17.78 -50.8 180)
				(length 3.81)
				(name "BYP2")
				(number "B8")
			)
			(pin output line
				(at 17.78 -53.34 180)
				(length 3.81)
				(name "BYP3")
				(number "A7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD9895"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 59.69 0)
		)
		(property "Value" "AD9895"
			(at -13.97 57.15 0)
		)
		(property "Footprint" "Package_BGA:BGA-64_9.0x9.0mm_Layout10x10_P0.8mm"
			(at -16.51 57.15 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD9891_9895.pdf"
			(at 0 0 0)
		)
		(property "Description" "CCD Signal Processor, 30MHz 12bits, CSPBGA-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "CCD Signal Processor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BGA*9.0x9.0mm*Layout10x10*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "AD9895_0_1")
		(symbol "AD9895_1_1"
			(pin input line
				(at -17.78 48.26 0)
				(length 3.81)
				(name "SL")
				(number "B5")
			)
			(pin input line
				(at -17.78 45.72 0)
				(length 3.81)
				(name "SDI")
				(number "A4")
			)
			(pin input clock
				(at -17.78 43.18 0)
				(length 3.81)
				(name "SCK")
				(number "B4")
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 3.81)
				(name "VD")
				(number "A1")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 3.81)
				(name "HD")
				(number "B1")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 3.81)
				(name "SYNC")
				(number "C1")
			)
			(pin input clock
				(at -17.78 20.32 0)
				(length 3.81)
				(name "CLI")
				(number "C10")
			)
			(pin output clock
				(at -17.78 17.78 0)
				(length 3.81)
				(name "CLO")
				(number "D10")
			)
			(pin power_out line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "DRVDD")
				(number "K3")
			)
			(pin power_out line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "DRVSS")
				(number "K4")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "CDD-IN")
				(number "A8")
			)
			(pin power_in line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "RGVDD")
				(number "E10")
			)
			(pin power_in line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "RGVSS")
				(number "E9")
			)
			(pin power_in line
				(at -17.78 -12.7 0)
				(length 3.81)
				(name "HVDD")
				(number "G10")
			)
			(pin power_in line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "HVSS")
				(number "G9")
			)
			(pin power_in line
				(at -17.78 -20.32 0)
				(length 3.81)
				(name "TCVDD")
				(number "B10")
			)
			(pin power_in line
				(at -17.78 -22.86 0)
				(length 3.81)
				(name "TCVSS")
				(number "C9")
			)
			(pin power_in line
				(at -17.78 -27.94 0)
				(length 3.81)
				(name "AVDD1")
				(number "A10")
			)
			(pin power_in line
				(at -17.78 -30.48 0)
				(length 3.81)
				(name "AVDD2")
				(number "B7")
			)
			(pin power_in line
				(at -17.78 -35.56 0)
				(length 3.81)
				(name "AVSS1")
				(number "B9")
			)
			(pin power_in line
				(at -17.78 -38.1 0)
				(length 3.81)
				(name "AVSS2")
				(number "B6")
			)
			(pin power_in line
				(at -17.78 -43.18 0)
				(length 3.81)
				(name "DVDD")
				(number "A2")
			)
			(pin power_in line
				(at -17.78 -45.72 0)
				(length 3.81)
				(name "DVSS")
				(number "B2")
			)
			(pin output line
				(at -17.78 -50.8 0)
				(length 3.81)
				(name "REFB")
				(number "A6")
			)
			(pin output line
				(at -17.78 -53.34 0)
				(length 3.81)
				(name "REFT")
				(number "A5")
			)
			(pin output line
				(at 17.78 53.34 180)
				(length 3.81)
				(name "D0")
				(number "E2")
			)
			(pin output line
				(at 17.78 50.8 180)
				(length 3.81)
				(name "D1")
				(number "E1")
			)
			(pin output line
				(at 17.78 48.26 180)
				(length 3.81)
				(name "D2/SD0")
				(number "F2")
			)
			(pin output line
				(at 17.78 45.72 180)
				(length 3.81)
				(name "D3")
				(number "F1")
			)
			(pin output line
				(at 17.78 43.18 180)
				(length 3.81)
				(name "D4")
				(number "G2")
			)
			(pin output line
				(at 17.78 40.64 180)
				(length 3.81)
				(name "D5")
				(number "G1")
			)
			(pin output line
				(at 17.78 38.1 180)
				(length 3.81)
				(name "D6")
				(number "H2")
			)
			(pin output line
				(at 17.78 35.56 180)
				(length 3.81)
				(name "D7")
				(number "H1")
			)
			(pin output line
				(at 17.78 33.02 180)
				(length 3.81)
				(name "D8")
				(number "J2")
			)
			(pin output line
				(at 17.78 30.48 180)
				(length 3.81)
				(name "D9")
				(number "J1")
			)
			(pin output line
				(at 17.78 27.94 180)
				(length 3.81)
				(name "D10")
				(number "K2")
			)
			(pin input line
				(at 17.78 25.4 180)
				(length 3.81)
				(name "D11")
				(number "K1")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "LD/FD")
				(number "C2")
			)
			(pin output clock
				(at 17.78 17.78 180)
				(length 3.81)
				(name "DCLK")
				(number "D1")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "PBLK/CLPOB")
				(number "D2")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "MSHUT")
				(number "A3")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "STROBE")
				(number "B3")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "RG")
				(number "D9")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "H1")
				(number "H10")
			)
			(pin output line
				(at 17.78 0 180)
				(length 3.81)
				(name "H2")
				(number "H9")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "H3")
				(number "F10")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "H4")
				(number "F9")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "V1")
				(number "K5")
			)
			(pin output line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "V2")
				(number "J5")
			)
			(pin output line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "V3")
				(number "K6")
			)
			(pin output line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "V4")
				(number "J6")
			)
			(pin output line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "VSG1/V5")
				(number "K7")
			)
			(pin output line
				(at 17.78 -20.32 180)
				(length 3.81)
				(name "VSG2/V6")
				(number "J7")
			)
			(pin output line
				(at 17.78 -22.86 180)
				(length 3.81)
				(name "VSG3/V7")
				(number "K8")
			)
			(pin output line
				(at 17.78 -25.4 180)
				(length 3.81)
				(name "VSG4/V8")
				(number "J8")
			)
			(pin output line
				(at 17.78 -27.94 180)
				(length 3.81)
				(name "VSG5")
				(number "K9")
			)
			(pin output line
				(at 17.78 -30.48 180)
				(length 3.81)
				(name "VSG6")
				(number "J9")
			)
			(pin output line
				(at 17.78 -33.02 180)
				(length 3.81)
				(name "VSG7")
				(number "K10")
			)
			(pin output line
				(at 17.78 -35.56 180)
				(length 3.81)
				(name "VSG8")
				(number "J10")
			)
			(pin output line
				(at 17.78 -40.64 180)
				(length 3.81)
				(name "VSUB")
				(number "J3")
			)
			(pin output clock
				(at 17.78 -43.18 180)
				(length 3.81)
				(name "SUBCK")
				(number "J4")
			)
			(pin output line
				(at 17.78 -48.26 180)
				(length 3.81)
				(name "BYP1")
				(number "A9")
			)
			(pin output line
				(at 17.78 -50.8 180)
				(length 3.81)
				(name "BYP2")
				(number "B8")
			)
			(pin output line
				(at 17.78 -53.34 180)
				(length 3.81)
				(name "BYP3")
				(number "A7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD9984AKST"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 55.88 0)
		)
		(property "Value" "AD9984AKST"
			(at 12.7 58.42 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_14x14mm_P0.65mm"
			(at 30.48 53.34 0)
		)
		(property "Datasheet" "http://www.analog.com/media/en/technical-documentation/data-sheets/AD9984A.pdf"
			(at 31.75 36.83 0)
		)
		(property "Description" "High Performance 10-Bit Display Interface 140/170MSPS LQFP"
			(at 0 0 0)
		)
		(property "ki_keywords" "10bit video display interface"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*"
			(at 0 0 0)
		)
		(symbol "AD9984AKST_0_1")
		(symbol "AD9984AKST_0_2")
		(symbol "AD9984AKST_1_1"
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 5.08)
				(name "SDA")
				(number "66")
			)
			(pin input line
				(at -20.32 38.1 0)
				(length 5.08)
				(name "SCL")
				(number "67")
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 5.08)
				(name "VSOUT/A0")
				(number "22")
			)
			(pin input line
				(at -20.32 25.4 0)
				(length 5.08)
				(name "R_AIN0")
				(number "14")
			)
			(pin input line
				(at -20.32 22.86 0)
				(length 5.08)
				(name "R_AIN1")
				(number "16")
			)
			(pin input line
				(at -20.32 17.78 0)
				(length 5.08)
				(name "G_AIN0")
				(number "6")
			)
			(pin input line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "G_AIN1")
				(number "10")
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 5.08)
				(name "B_AIN0")
				(number "2")
			)
			(pin input line
				(at -20.32 7.62 0)
				(length 5.08)
				(name "B_AIN1")
				(number "4")
			)
			(pin input line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "HSYNC0")
				(number "70")
			)
			(pin input line
				(at -20.32 0 0)
				(length 5.08)
				(name "HSYNC1")
				(number "68")
			)
			(pin input line
				(at -20.32 -5.08 0)
				(length 5.08)
				(name "VSYNC0")
				(number "71")
			)
			(pin input line
				(at -20.32 -7.62 0)
				(length 5.08)
				(name "VSYNC1")
				(number "69")
			)
			(pin input line
				(at -20.32 -12.7 0)
				(length 5.08)
				(name "SOGIN0")
				(number "8")
			)
			(pin input line
				(at -20.32 -15.24 0)
				(length 5.08)
				(name "SOGIN1")
				(number "12")
			)
			(pin input line
				(at -20.32 -20.32 0)
				(length 5.08)
				(name "EXTCK/COAST")
				(number "72")
			)
			(pin input line
				(at -20.32 -22.86 0)
				(length 5.08)
				(name "CLAMP")
				(number "73")
			)
			(pin input line
				(at -20.32 -25.4 0)
				(length 5.08)
				(name "PWR_DN")
				(number "17")
			)
			(pin input line
				(at -20.32 -35.56 0)
				(length 5.08)
				(name "FILT")
				(number "78")
			)
			(pin input line
				(at -20.32 -38.1 0)
				(length 5.08)
				(name "REF_LO")
				(number "18")
			)
			(pin input line
				(at -20.32 -40.64 0)
				(length 5.08)
				(name "REF_HI")
				(number "20")
			)
			(pin power_in line
				(at -5.08 55.88 270)
				(length 5.08)
				(name "DAV_DD")
				(number "41")
			)
			(pin power_in line
				(at -2.54 55.88 270)
				(length 5.08)
				(name "PV_D")
				(number "74")
			)
			(pin passive line
				(at -2.54 55.88 270)
				(length 5.08)
				(hide yes)
				(name "PV_D")
				(number "76")
			)
			(pin passive line
				(at -2.54 55.88 270)
				(length 5.08)
				(hide yes)
				(name "PV_D")
				(number "79")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "27")
			)
			(pin power_in line
				(at -2.54 -55.88 90)
				(length 5.08)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "39")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "40")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "53")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "65")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "75")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "77")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "80")
			)
			(pin power_in line
				(at 0 55.88 270)
				(length 5.08)
				(name "VDD")
				(number "26")
			)
			(pin passive line
				(at 0 55.88 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "38")
			)
			(pin passive line
				(at 0 55.88 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "52")
			)
			(pin passive line
				(at 0 55.88 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "64")
			)
			(pin power_in line
				(at 2.54 55.88 270)
				(length 5.08)
				(name "VD")
				(number "1")
			)
			(pin passive line
				(at 2.54 55.88 270)
				(length 5.08)
				(hide yes)
				(name "VD")
				(number "13")
			)
			(pin passive line
				(at 2.54 55.88 270)
				(length 5.08)
				(hide yes)
				(name "VD")
				(number "5")
			)
			(pin passive line
				(at 2.54 55.88 270)
				(length 5.08)
				(hide yes)
				(name "VD")
				(number "9")
			)
			(pin no_connect line
				(at 12.7 -48.26 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "19")
			)
			(pin output line
				(at 17.78 48.26 180)
				(length 5.08)
				(name "RED_0")
				(number "37")
			)
			(pin output line
				(at 17.78 45.72 180)
				(length 5.08)
				(name "RED_1")
				(number "36")
			)
			(pin output line
				(at 17.78 43.18 180)
				(length 5.08)
				(name "RED_2")
				(number "35")
			)
			(pin output line
				(at 17.78 40.64 180)
				(length 5.08)
				(name "RED_3")
				(number "34")
			)
			(pin output line
				(at 17.78 38.1 180)
				(length 5.08)
				(name "RED_4")
				(number "33")
			)
			(pin output line
				(at 17.78 35.56 180)
				(length 5.08)
				(name "RED_5")
				(number "32")
			)
			(pin output line
				(at 17.78 33.02 180)
				(length 5.08)
				(name "RED_6")
				(number "31")
			)
			(pin output line
				(at 17.78 30.48 180)
				(length 5.08)
				(name "RED_7")
				(number "30")
			)
			(pin output line
				(at 17.78 27.94 180)
				(length 5.08)
				(name "RED_8")
				(number "29")
			)
			(pin output line
				(at 17.78 25.4 180)
				(length 5.08)
				(name "RED_9")
				(number "28")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 5.08)
				(name "GREEN_0")
				(number "51")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 5.08)
				(name "GREEN_1")
				(number "50")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "GREEN_2")
				(number "49")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "GREEN_3")
				(number "48")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "GREEN_4")
				(number "47")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "GREEN_5")
				(number "46")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "GREEN_6")
				(number "45")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "GREEN_7")
				(number "44")
			)
			(pin output line
				(at 17.78 0 180)
				(length 5.08)
				(name "GREEN_8")
				(number "43")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "GREEN_9")
				(number "42")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "BLUE_0")
				(number "63")
			)
			(pin output line
				(at 17.78 -10.16 180)
				(length 5.08)
				(name "BLUE_1")
				(number "62")
			)
			(pin output line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "BLUE_2")
				(number "61")
			)
			(pin output line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "BLUE_3")
				(number "60")
			)
			(pin output line
				(at 17.78 -17.78 180)
				(length 5.08)
				(name "BLUE_4")
				(number "59")
			)
			(pin output line
				(at 17.78 -20.32 180)
				(length 5.08)
				(name "BLUE_5")
				(number "58")
			)
			(pin output line
				(at 17.78 -22.86 180)
				(length 5.08)
				(name "BLUE_6")
				(number "57")
			)
			(pin output line
				(at 17.78 -25.4 180)
				(length 5.08)
				(name "BLUE_7")
				(number "56")
			)
			(pin output line
				(at 17.78 -27.94 180)
				(length 5.08)
				(name "BLUE_8")
				(number "55")
			)
			(pin output line
				(at 17.78 -30.48 180)
				(length 5.08)
				(name "BLUE_9")
				(number "54")
			)
			(pin output line
				(at 17.78 -35.56 180)
				(length 5.08)
				(name "DATACK")
				(number "25")
			)
			(pin output line
				(at 17.78 -38.1 180)
				(length 5.08)
				(name "HSOUT")
				(number "23")
			)
			(pin output line
				(at 17.78 -40.64 180)
				(length 5.08)
				(name "SOGOUT")
				(number "24")
			)
			(pin output line
				(at 17.78 -43.18 180)
				(length 5.08)
				(name "O/E_FIELD")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADA4430-1YKSZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 8.89 0)
		)
		(property "Value" "ADA4430-1YKSZ"
			(at 8.89 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADA4430-1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Ultralow Power, Video Filter, Power-Down, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "Video Filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
		(symbol "ADA4430-1YKSZ_0_1")
		(symbol "ADA4430-1YKSZ_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "V_{IN}")
				(number "1")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~{DIS}")
				(number "5")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V_{S}")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "V_{OUT}")
				(number "4")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "SAG")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADV7280xCP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 24.13 0)
		)
		(property "Value" "ADV7280xCP"
			(at 11.43 -24.13 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-32-1EP_5x5mm_P0.5mm_EP3.6x3.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADV7280.PDF"
			(at 60.96 -63.5 0)
		)
		(property "Description" "10-Bit, 4x Oversampled SDTV Video Decoder with Deinterlacer, LFCSP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "video decoder"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ADV7280xCP_0_1")
		(symbol "ADV7280xCP_1_1"
			(pin input line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "AIN1")
				(number "17")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "AIN2")
				(number "18")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "AIN2")
				(number "22")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "AIN3")
				(number "23")
			)
			(pin output line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "VREFP")
				(number "19")
			)
			(pin output line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "VREFN")
				(number "20")
			)
			(pin output line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "XTALP")
				(number "14")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "XTALN")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "SDATA")
				(number "27")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "SCLK")
				(number "28")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "ALSB")
				(number "26")
			)
			(pin power_in line
				(at -7.62 25.4 270)
				(length 2.54)
				(name "DVDDIO")
				(number "2")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "DVDD")
				(number "3")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "DVDD")
				(number "13")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "DGND")
				(number "1")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "DGND")
				(number "33")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "DGND")
				(number "4")
			)
			(pin power_in line
				(at 5.08 25.4 270)
				(length 2.54)
				(name "PVDD")
				(number "16")
			)
			(pin power_in line
				(at 10.16 25.4 270)
				(length 2.54)
				(name "AVDD")
				(number "21")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "P0")
				(number "12")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "P1")
				(number "11")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "P2")
				(number "10")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "P3")
				(number "9")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "P4")
				(number "8")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "P5")
				(number "7")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "P6")
				(number "6")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "P7")
				(number "5")
			)
			(pin input line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "~PWRDWN")
				(number "31")
			)
			(pin input line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "~RESET")
				(number "25")
			)
			(pin output line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "LLC")
				(number "32")
			)
			(pin output line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "~INTRQ")
				(number "24")
			)
			(pin output line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "VS/FIELD/SFL")
				(number "29")
			)
			(pin output line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "HS")
				(number "30")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADV7390BCPZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 26.67 0)
		)
		(property "Value" "ADV7390BCPZ"
			(at 13.97 26.67 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADV7390_7391_7392_7393.pdf"
			(at 0 0 0)
		)
		(property "Description" "10-Bit SD/HD Video Encoder, Macrovision Antitaping, LFCSP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Video Encoder"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ADV7390BCPZ_0_1")
		(symbol "ADV7390BCPZ_1_1"
			(pin input line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "P0")
				(number "30")
			)
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "P1")
				(number "31")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "P2")
				(number "2")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "P3")
				(number "3")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "P4")
				(number "4")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "P5")
				(number "7")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "P6")
				(number "8")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "P7")
				(number "9")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "CLKIN")
				(number "13")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{HSYNC}")
				(number "27")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{VSYNC}")
				(number "26")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "~{RESET}")
				(number "14")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "SCL")
				(number "12")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "SDA")
				(number "11")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "ALSB")
				(number "10")
			)
			(pin input line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "SFL")
				(number "25")
			)
			(pin passive line
				(at -5.08 27.94 270)
				(length 2.54)
				(hide yes)
				(name "V_{DD}")
				(number "28")
			)
			(pin power_in line
				(at -5.08 27.94 270)
				(length 2.54)
				(name "V_{DD}")
				(number "5")
			)
			(pin passive line
				(at -5.08 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "DGND")
				(number "29")
			)
			(pin power_in line
				(at -5.08 -27.94 90)
				(length 2.54)
				(name "DGND")
				(number "6")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "V_{DD_IO}")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 2.54)
				(name "GND_IO")
				(number "32")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "P_{VDD}")
				(number "17")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 2.54)
				(name "PGND")
				(number "15")
			)
			(pin power_in line
				(at 5.08 27.94 270)
				(length 2.54)
				(name "V_{AA}")
				(number "19")
			)
			(pin power_in line
				(at 5.08 -27.94 90)
				(length 2.54)
				(name "AGND")
				(number "18")
			)
			(pin passive line
				(at 5.08 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "33")
			)
			(pin output line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "COMP")
				(number "23")
			)
			(pin passive line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "EXT_LF")
				(number "16")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "DAC1")
				(number "22")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "DAC2")
				(number "21")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "DAC3")
				(number "20")
			)
			(pin input line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "R_{SET}")
				(number "24")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AV9173"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 10.16 0)
		)
		(property "Value" "AV9173"
			(at 6.35 10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ibselectronics.com/ibsstore/datasheet/Others/AV9173-01CN08.pdf"
			(at 0 0 0)
		)
		(property "Description" "Video Genlock PLL"
			(at 0 0 0)
		)
		(property "ki_keywords" "video pll"
			(at 0 0 0)
		)
		(symbol "AV9173_0_1")
		(symbol "AV9173_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "FREFIN")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "FSIGIN")
				(number "1")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "FS0")
				(number "4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "OE")
				(number "5")
			)
			(pin input line
				(at 0 12.7 270)
				(length 3.81)
				(name "VCC")
				(number "7")
			)
			(pin input line
				(at 0 -12.7 90)
				(length 3.81)
				(name "GND")
				(number "3")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CKKOUT")
				(number "6")
			)
			(pin tri_state line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CLK/2")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CX7930"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 20.32 0)
		)
		(property "Value" "CX7930"
			(at 8.89 20.32 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "CX7930_0_1")
		(symbol "CX7930_1_1"
			(pin input line
				(at -20.32 13.97 0)
				(length 7.62)
				(name "4FSCI")
				(number "10")
			)
			(pin output line
				(at -20.32 11.43 0)
				(length 7.62)
				(name "4FSCO")
				(number "9")
			)
			(pin input line
				(at -20.32 8.89 0)
				(length 7.62)
				(name "VDD")
				(number "28")
			)
			(pin input line
				(at -20.32 6.35 0)
				(length 7.62)
				(name "VSS")
				(number "14")
			)
			(pin input line
				(at -20.32 3.81 0)
				(length 7.62)
				(name "TEST")
				(number "16")
			)
			(pin input line
				(at -20.32 1.27 0)
				(length 7.62)
				(name "CLIN")
				(number "26")
			)
			(pin output line
				(at -20.32 -1.27 0)
				(length 7.62)
				(name "CLOUT")
				(number "25")
			)
			(pin input line
				(at -20.32 -3.81 0)
				(length 7.62)
				(name "MODE1")
				(number "21")
			)
			(pin input line
				(at -20.32 -6.35 0)
				(length 7.62)
				(name "MODE2")
				(number "22")
			)
			(pin input line
				(at -20.32 -8.89 0)
				(length 7.62)
				(name "EXT")
				(number "20")
			)
			(pin input line
				(at -20.32 -11.43 0)
				(length 7.62)
				(name "LALTRI")
				(number "15")
			)
			(pin input line
				(at -20.32 -13.97 0)
				(length 7.62)
				(name "HRI")
				(number "23")
			)
			(pin input line
				(at -20.32 -16.51 0)
				(length 7.62)
				(name "VRI")
				(number "1")
			)
			(pin output line
				(at 20.32 13.97 180)
				(length 7.62)
				(name "OSC")
				(number "19")
			)
			(pin output line
				(at 20.32 8.89 180)
				(length 7.62)
				(name "HCOMO")
				(number "24")
			)
			(pin output line
				(at 20.32 3.81 180)
				(length 7.62)
				(name "OFLD1")
				(number "2")
			)
			(pin output line
				(at 20.32 1.27 180)
				(length 7.62)
				(name "OFLD")
				(number "5")
			)
			(pin output line
				(at 20.32 -1.27 180)
				(length 7.62)
				(name "OLALT")
				(number "7")
			)
			(pin output line
				(at 20.32 -3.81 180)
				(length 7.62)
				(name "OBF")
				(number "3")
			)
			(pin output line
				(at 20.32 -6.35 180)
				(length 7.62)
				(name "OBLK")
				(number "6")
			)
			(pin output line
				(at 20.32 -8.89 180)
				(length 7.62)
				(name "OSYNC")
				(number "4")
			)
			(pin output line
				(at 20.32 -11.43 180)
				(length 7.62)
				(name "OVD")
				(number "12")
			)
			(pin output line
				(at 20.32 -13.97 180)
				(length 7.62)
				(name "OHD")
				(number "8")
			)
			(pin output line
				(at 20.32 -16.51 180)
				(length 7.62)
				(name "OFH")
				(number "27")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CXD3400N"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 21.59 0)
		)
		(property "Value" "CXD3400N"
			(at 3.81 -20.32 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "video\\cxd3400n.pdf"
			(at 0 0 0)
		)
		(property "Description" "6-channel Vertical Clock Driver for CCD Image Sensor, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "CCD Clock Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*"
			(at 0 0 0)
		)
		(symbol "CXD3400N_0_1")
		(symbol "CXD3400N_1_1"
			(pin input line
				(at -15.24 17.78 0)
				(length 3.81)
				(name "XSHT")
				(number "2")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 3.81)
				(name "XV3")
				(number "3")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 3.81)
				(name "XSG3B")
				(number "4")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "XSG3A")
				(number "5")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "XV1")
				(number "6")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "XSG1B")
				(number "7")
			)
			(pin input line
				(at -15.24 0 0)
				(length 3.81)
				(name "XSG1A")
				(number "8")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "XV4")
				(number "9")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "XV2")
				(number "10")
			)
			(pin power_in line
				(at -15.24 -12.7 0)
				(length 3.81)
				(name "VL")
				(number "18")
			)
			(pin power_in line
				(at -15.24 -16.51 0)
				(length 3.81)
				(name "VH")
				(number "15")
			)
			(pin power_in line
				(at 0 24.13 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 3.81)
				(name "GND")
				(number "11")
			)
			(pin output line
				(at 15.24 17.78 180)
				(length 3.81)
				(name "SHT")
				(number "20")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 3.81)
				(name "V3B")
				(number "19")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 3.81)
				(name "V3A")
				(number "17")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "V1B")
				(number "16")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "V1A")
				(number "14")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "V4")
				(number "13")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 3.81)
				(name "V2")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HD63484"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "HD63484"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "HD63484_0_1")
		(symbol "HD63484_1_1"
			(pin output inverted
				(at -27.94 48.26 0)
				(length 7.62)
				(name "DREQ")
				(number "8")
			)
			(pin input inverted
				(at -27.94 45.72 0)
				(length 7.62)
				(name "DACK")
				(number "9")
			)
			(pin input inverted
				(at -27.94 43.18 0)
				(length 7.62)
				(name "DONE")
				(number "7")
			)
			(pin output inverted
				(at -27.94 38.1 0)
				(length 7.62)
				(name "IRQ")
				(number "11")
			)
			(pin tri_state line
				(at -27.94 33.02 0)
				(length 7.62)
				(name "D0")
				(number "17")
			)
			(pin tri_state line
				(at -27.94 30.48 0)
				(length 7.62)
				(name "D1")
				(number "18")
			)
			(pin tri_state line
				(at -27.94 27.94 0)
				(length 7.62)
				(name "D2")
				(number "19")
			)
			(pin tri_state line
				(at -27.94 25.4 0)
				(length 7.62)
				(name "D3")
				(number "20")
			)
			(pin tri_state line
				(at -27.94 22.86 0)
				(length 7.62)
				(name "D4")
				(number "21")
			)
			(pin tri_state line
				(at -27.94 20.32 0)
				(length 7.62)
				(name "D5")
				(number "22")
			)
			(pin tri_state line
				(at -27.94 17.78 0)
				(length 7.62)
				(name "D6")
				(number "23")
			)
			(pin tri_state line
				(at -27.94 15.24 0)
				(length 7.62)
				(name "D7")
				(number "24")
			)
			(pin tri_state line
				(at -27.94 12.7 0)
				(length 7.62)
				(name "D8")
				(number "25")
			)
			(pin tri_state line
				(at -27.94 10.16 0)
				(length 7.62)
				(name "D9")
				(number "26")
			)
			(pin tri_state line
				(at -27.94 7.62 0)
				(length 7.62)
				(name "D10")
				(number "27")
			)
			(pin tri_state line
				(at -27.94 5.08 0)
				(length 7.62)
				(name "D11")
				(number "28")
			)
			(pin tri_state line
				(at -27.94 2.54 0)
				(length 7.62)
				(name "D12")
				(number "29")
			)
			(pin tri_state line
				(at -27.94 0 0)
				(length 7.62)
				(name "D13")
				(number "30")
			)
			(pin tri_state line
				(at -27.94 -2.54 0)
				(length 7.62)
				(name "D14")
				(number "31")
			)
			(pin tri_state line
				(at -27.94 -5.08 0)
				(length 7.62)
				(name "D15")
				(number "32")
			)
			(pin input inverted
				(at -27.94 -10.16 0)
				(length 7.62)
				(name "CS")
				(number "4")
			)
			(pin input line
				(at -27.94 -15.24 0)
				(length 7.62)
				(name "RS")
				(number "5")
			)
			(pin input line
				(at -27.94 -20.32 0)
				(length 7.62)
				(name "R/W")
				(number "3")
			)
			(pin output inverted
				(at -27.94 -25.4 0)
				(length 7.62)
				(name "DTACK")
				(number "10")
			)
			(pin input line
				(at -27.94 -30.48 0)
				(length 7.62)
				(name "LPSTB")
				(number "64")
			)
			(pin input inverted
				(at -27.94 -38.1 0)
				(length 7.62)
				(name "RESET")
				(number "6")
			)
			(pin input line
				(at -5.08 58.42 270)
				(length 7.62)
				(name "VCC")
				(number "14")
			)
			(pin input line
				(at -5.08 -58.42 90)
				(length 7.62)
				(name "GND")
				(number "16")
			)
			(pin input line
				(at -2.54 58.42 270)
				(length 7.62)
				(name "VCC")
				(number "49")
			)
			(pin input line
				(at -2.54 -58.42 90)
				(length 7.62)
				(name "GND")
				(number "51")
			)
			(pin output inverted
				(at 27.94 48.26 180)
				(length 7.62)
				(name "DRAW")
				(number "54")
			)
			(pin output line
				(at 27.94 45.72 180)
				(length 7.62)
				(name "MRD")
				(number "55")
			)
			(pin tri_state line
				(at 27.94 40.64 180)
				(length 7.62)
				(name "MAD0")
				(number "61")
			)
			(pin tri_state line
				(at 27.94 38.1 180)
				(length 7.62)
				(name "MAD1")
				(number "60")
			)
			(pin tri_state line
				(at 27.94 35.56 180)
				(length 7.62)
				(name "MAD2")
				(number "59")
			)
			(pin tri_state line
				(at 27.94 33.02 180)
				(length 7.62)
				(name "MAD3")
				(number "58")
			)
			(pin tri_state line
				(at 27.94 30.48 180)
				(length 7.62)
				(name "MAD4")
				(number "57")
			)
			(pin tri_state line
				(at 27.94 27.94 180)
				(length 7.62)
				(name "MAD5")
				(number "48")
			)
			(pin tri_state line
				(at 27.94 25.4 180)
				(length 7.62)
				(name "MAD6")
				(number "47")
			)
			(pin tri_state line
				(at 27.94 22.86 180)
				(length 7.62)
				(name "MAD7")
				(number "46")
			)
			(pin tri_state line
				(at 27.94 20.32 180)
				(length 7.62)
				(name "MAD8")
				(number "45")
			)
			(pin tri_state line
				(at 27.94 17.78 180)
				(length 7.62)
				(name "MAD9")
				(number "44")
			)
			(pin tri_state line
				(at 27.94 15.24 180)
				(length 7.62)
				(name "MAD10")
				(number "43")
			)
			(pin tri_state line
				(at 27.94 12.7 180)
				(length 7.62)
				(name "MAD11")
				(number "42")
			)
			(pin tri_state line
				(at 27.94 10.16 180)
				(length 7.62)
				(name "MAD12")
				(number "41")
			)
			(pin tri_state line
				(at 27.94 7.62 180)
				(length 7.62)
				(name "MAD13")
				(number "40")
			)
			(pin tri_state line
				(at 27.94 5.08 180)
				(length 7.62)
				(name "MAD14")
				(number "39")
			)
			(pin tri_state line
				(at 27.94 2.54 180)
				(length 7.62)
				(name "MAD15")
				(number "38")
			)
			(pin output line
				(at 27.94 0 180)
				(length 7.62)
				(name "MA16/RA0")
				(number "37")
			)
			(pin output line
				(at 27.94 -2.54 180)
				(length 7.62)
				(name "MA17/RA1")
				(number "36")
			)
			(pin output line
				(at 27.94 -5.08 180)
				(length 7.62)
				(name "MA18/RA2")
				(number "35")
			)
			(pin output line
				(at 27.94 -7.62 180)
				(length 7.62)
				(name "MA19/RA3")
				(number "34")
			)
			(pin output line
				(at 27.94 -10.16 180)
				(length 7.62)
				(name "RA4")
				(number "33")
			)
			(pin output line
				(at 27.94 -15.24 180)
				(length 7.62)
				(name "CHR")
				(number "56")
			)
			(pin output inverted
				(at 27.94 -17.78 180)
				(length 7.62)
				(name "CUD1")
				(number "1")
			)
			(pin output inverted
				(at 27.94 -20.32 180)
				(length 7.62)
				(name "CUD2")
				(number "2")
			)
			(pin output inverted
				(at 27.94 -25.4 180)
				(length 7.62)
				(name "HSYNC")
				(number "12")
			)
			(pin output inverted
				(at 27.94 -27.94 180)
				(length 7.62)
				(name "VSYNC")
				(number "13")
			)
			(pin input inverted
				(at 27.94 -30.48 180)
				(length 7.62)
				(name "EXTSYNC")
				(number "15")
			)
			(pin output inverted
				(at 27.94 -35.56 180)
				(length 7.62)
				(name "DISP1")
				(number "63")
			)
			(pin output inverted
				(at 27.94 -38.1 180)
				(length 7.62)
				(name "DISP2")
				(number "62")
			)
			(pin output line
				(at 27.94 -43.18 180)
				(length 7.62)
				(name "MCYC")
				(number "52")
			)
			(pin output inverted
				(at 27.94 -45.72 180)
				(length 7.62)
				(name "AS")
				(number "53")
			)
			(pin input clock
				(at 27.94 -48.26 180)
				(length 7.62)
				(name "2CLK")
				(number "50")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HD63484_PLCC"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "HD63484_PLCC"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "HD63484_PLCC_0_1")
		(symbol "HD63484_PLCC_1_1"
			(pin output inverted
				(at -27.94 48.26 0)
				(length 7.62)
				(name "DREQ")
				(number "9")
			)
			(pin input inverted
				(at -27.94 45.72 0)
				(length 7.62)
				(name "DACK")
				(number "10")
			)
			(pin input inverted
				(at -27.94 43.18 0)
				(length 7.62)
				(name "DONE")
				(number "8")
			)
			(pin output inverted
				(at -27.94 38.1 0)
				(length 7.62)
				(name "IRQ")
				(number "12")
			)
			(pin tri_state line
				(at -27.94 33.02 0)
				(length 7.62)
				(name "D0")
				(number "19")
			)
			(pin tri_state line
				(at -27.94 30.48 0)
				(length 7.62)
				(name "D1")
				(number "20")
			)
			(pin tri_state line
				(at -27.94 27.94 0)
				(length 7.62)
				(name "D2")
				(number "21")
			)
			(pin tri_state line
				(at -27.94 25.4 0)
				(length 7.62)
				(name "D3")
				(number "22")
			)
			(pin tri_state line
				(at -27.94 22.86 0)
				(length 7.62)
				(name "D4")
				(number "23")
			)
			(pin tri_state line
				(at -27.94 20.32 0)
				(length 7.62)
				(name "D5")
				(number "24")
			)
			(pin tri_state line
				(at -27.94 17.78 0)
				(length 7.62)
				(name "D6")
				(number "25")
			)
			(pin tri_state line
				(at -27.94 15.24 0)
				(length 7.62)
				(name "D7")
				(number "26")
			)
			(pin tri_state line
				(at -27.94 12.7 0)
				(length 7.62)
				(name "D8")
				(number "27")
			)
			(pin tri_state line
				(at -27.94 10.16 0)
				(length 7.62)
				(name "D9")
				(number "28")
			)
			(pin tri_state line
				(at -27.94 7.62 0)
				(length 7.62)
				(name "D10")
				(number "29")
			)
			(pin tri_state line
				(at -27.94 5.08 0)
				(length 7.62)
				(name "D11")
				(number "30")
			)
			(pin tri_state line
				(at -27.94 2.54 0)
				(length 7.62)
				(name "D12")
				(number "31")
			)
			(pin tri_state line
				(at -27.94 0 0)
				(length 7.62)
				(name "D13")
				(number "32")
			)
			(pin tri_state line
				(at -27.94 -2.54 0)
				(length 7.62)
				(name "D14")
				(number "33")
			)
			(pin tri_state line
				(at -27.94 -5.08 0)
				(length 7.62)
				(name "D15")
				(number "34")
			)
			(pin input inverted
				(at -27.94 -10.16 0)
				(length 7.62)
				(name "CS")
				(number "5")
			)
			(pin input line
				(at -27.94 -15.24 0)
				(length 7.62)
				(name "RS")
				(number "6")
			)
			(pin input line
				(at -27.94 -20.32 0)
				(length 7.62)
				(name "R/W")
				(number "4")
			)
			(pin output inverted
				(at -27.94 -25.4 0)
				(length 7.62)
				(name "DTACK")
				(number "11")
			)
			(pin input line
				(at -27.94 -30.48 0)
				(length 7.62)
				(name "LPSTB")
				(number "68")
			)
			(pin input inverted
				(at -27.94 -38.1 0)
				(length 7.62)
				(name "RESET")
				(number "7")
			)
			(pin input line
				(at -5.08 58.42 270)
				(length 7.62)
				(name "VCC")
				(number "1")
			)
			(pin input line
				(at -5.08 -58.42 90)
				(length 7.62)
				(name "GND")
				(number "17")
			)
			(pin input line
				(at -2.54 58.42 270)
				(length 7.62)
				(name "VCC")
				(number "15")
			)
			(pin input line
				(at -2.54 -58.42 90)
				(length 7.62)
				(name "GND")
				(number "18")
			)
			(pin input line
				(at 0 58.42 270)
				(length 7.62)
				(name "VCC")
				(number "52")
			)
			(pin input line
				(at 0 -58.42 90)
				(length 7.62)
				(name "GND")
				(number "35")
			)
			(pin input line
				(at 2.54 -58.42 90)
				(length 7.62)
				(name "GND")
				(number "54")
			)
			(pin input line
				(at 5.08 -58.42 90)
				(length 7.62)
				(name "GND")
				(number "55")
			)
			(pin output inverted
				(at 27.94 48.26 180)
				(length 7.62)
				(name "DRAW")
				(number "58")
			)
			(pin output line
				(at 27.94 45.72 180)
				(length 7.62)
				(name "MRD")
				(number "59")
			)
			(pin tri_state line
				(at 27.94 40.64 180)
				(length 7.62)
				(name "MAD0")
				(number "65")
			)
			(pin tri_state line
				(at 27.94 38.1 180)
				(length 7.62)
				(name "MAD1")
				(number "64")
			)
			(pin tri_state line
				(at 27.94 35.56 180)
				(length 7.62)
				(name "MAD2")
				(number "63")
			)
			(pin tri_state line
				(at 27.94 33.02 180)
				(length 7.62)
				(name "MAD3")
				(number "62")
			)
			(pin tri_state line
				(at 27.94 30.48 180)
				(length 7.62)
				(name "MAD4")
				(number "61")
			)
			(pin tri_state line
				(at 27.94 27.94 180)
				(length 7.62)
				(name "MAD5")
				(number "51")
			)
			(pin tri_state line
				(at 27.94 25.4 180)
				(length 7.62)
				(name "MAD6")
				(number "50")
			)
			(pin tri_state line
				(at 27.94 22.86 180)
				(length 7.62)
				(name "MAD7")
				(number "49")
			)
			(pin tri_state line
				(at 27.94 20.32 180)
				(length 7.62)
				(name "MAD8")
				(number "48")
			)
			(pin tri_state line
				(at 27.94 17.78 180)
				(length 7.62)
				(name "MAD9")
				(number "47")
			)
			(pin tri_state line
				(at 27.94 15.24 180)
				(length 7.62)
				(name "MAD10")
				(number "46")
			)
			(pin tri_state line
				(at 27.94 12.7 180)
				(length 7.62)
				(name "MAD11")
				(number "45")
			)
			(pin tri_state line
				(at 27.94 10.16 180)
				(length 7.62)
				(name "MAD12")
				(number "44")
			)
			(pin tri_state line
				(at 27.94 7.62 180)
				(length 7.62)
				(name "MAD13")
				(number "43")
			)
			(pin tri_state line
				(at 27.94 5.08 180)
				(length 7.62)
				(name "MAD14")
				(number "42")
			)
			(pin tri_state line
				(at 27.94 2.54 180)
				(length 7.62)
				(name "MAD15")
				(number "41")
			)
			(pin output line
				(at 27.94 0 180)
				(length 7.62)
				(name "MA16/RA0")
				(number "40")
			)
			(pin output line
				(at 27.94 -2.54 180)
				(length 7.62)
				(name "MA17/RA1")
				(number "39")
			)
			(pin output line
				(at 27.94 -5.08 180)
				(length 7.62)
				(name "MA18/RA2")
				(number "38")
			)
			(pin output line
				(at 27.94 -7.62 180)
				(length 7.62)
				(name "MA19/RA3")
				(number "37")
			)
			(pin output line
				(at 27.94 -10.16 180)
				(length 7.62)
				(name "RA4")
				(number "36")
			)
			(pin output line
				(at 27.94 -15.24 180)
				(length 7.62)
				(name "CHR")
				(number "60")
			)
			(pin output inverted
				(at 27.94 -17.78 180)
				(length 7.62)
				(name "CUD1")
				(number "2")
			)
			(pin output inverted
				(at 27.94 -20.32 180)
				(length 7.62)
				(name "CUD2")
				(number "3")
			)
			(pin output inverted
				(at 27.94 -25.4 180)
				(length 7.62)
				(name "HSYNC")
				(number "13")
			)
			(pin output inverted
				(at 27.94 -27.94 180)
				(length 7.62)
				(name "VSYNC")
				(number "14")
			)
			(pin input inverted
				(at 27.94 -30.48 180)
				(length 7.62)
				(name "EXTSYNC")
				(number "16")
			)
			(pin output inverted
				(at 27.94 -35.56 180)
				(length 7.62)
				(name "DISP1")
				(number "67")
			)
			(pin output inverted
				(at 27.94 -38.1 180)
				(length 7.62)
				(name "DISP2")
				(number "66")
			)
			(pin output line
				(at 27.94 -43.18 180)
				(length 7.62)
				(name "MCYC")
				(number "56")
			)
			(pin output inverted
				(at 27.94 -45.72 180)
				(length 7.62)
				(name "AS")
				(number "57")
			)
			(pin input clock
				(at 27.94 -48.26 180)
				(length 7.62)
				(name "2CLK")
				(number "53")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ICX415AQ"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 20.32 0)
		)
		(property "Value" "ICX415AQ"
			(at 6.35 -20.32 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Diagonal 8mm B/W Progressive Scan CCD Image Sensor with Square Pixel, CERDIP-22"
			(at 0 0 0)
		)
		(property "ki_keywords" "CCD B/W Image Sensor"
			(at 0 0 0)
		)
		(symbol "ICX415AQ_0_1")
		(symbol "ICX415AQ_1_1"
			(pin input clock
				(at -17.78 15.24 0)
				(length 3.81)
				(name "V1")
				(number "5")
			)
			(pin input clock
				(at -17.78 12.7 0)
				(length 3.81)
				(name "V2")
				(number "4")
			)
			(pin input clock
				(at -17.78 10.16 0)
				(length 3.81)
				(name "V3")
				(number "3")
			)
			(pin input clock
				(at -17.78 5.08 0)
				(length 3.81)
				(name "SUB")
				(number "15")
			)
			(pin input clock
				(at -17.78 0 0)
				(length 3.81)
				(name "H1")
				(number "16")
			)
			(pin input clock
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "H2")
				(number "17")
			)
			(pin input clock
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "RG")
				(number "13")
			)
			(pin power_in line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "VL")
				(number "14")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 3.81)
				(name "VDD")
				(number "12")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 3.81)
				(name "GND")
				(number "7")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "VOUT")
				(number "9")
			)
			(pin power_in line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "SUBCIR")
				(number "21")
			)
			(pin input line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "CGG")
				(number "10")
			)
			(pin input line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "CSUB")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISL59885"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "ISL59885"
			(at 5.08 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.renesas.com/us/en/document/dst/isl59885-datasheet?r=533081"
			(at 0 0 0)
		)
		(property "Description" "Sync Separator for HD and SD Video, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "video sync separator csync hsync vsync"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ISL59885_0_1")
		(symbol "ISL59885_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "CVBS")
				(number "2")
			)
			(pin passive line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "CSET")
				(number "6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "CSYNC")
				(number "1")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "VSYNC")
				(number "3")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "HSYNC")
				(number "7")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "~{HD}")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LM1881"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "LM1881"
			(at 6.35 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "LM1881_0_1")
		(symbol "LM1881_1_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VIDEO")
				(number "2")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "INT")
				(number "6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "CSYNC")
				(number "1")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "FRAME")
				(number "3")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "BURST")
				(number "5")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "O/E")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX310"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "MAX310"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX310-MAX311.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-Channel CMOS RF Video Multiplexer"
			(at 0 0 0)
		)
		(property "ki_keywords" "video rf"
			(at 0 0 0)
		)
		(symbol "MAX310_0_1")
		(symbol "MAX310_1_1"
			(pin input line
				(at -19.05 8.89 0)
				(length 7.62)
				(name "S1")
				(number "1")
			)
			(pin input line
				(at -19.05 6.35 0)
				(length 7.62)
				(name "S2")
				(number "2")
			)
			(pin input line
				(at -19.05 3.81 0)
				(length 7.62)
				(name "S3")
				(number "3")
			)
			(pin input line
				(at -19.05 1.27 0)
				(length 7.62)
				(name "S4")
				(number "4")
			)
			(pin input line
				(at -19.05 -1.27 0)
				(length 7.62)
				(name "S5")
				(number "5")
			)
			(pin input line
				(at -19.05 -3.81 0)
				(length 7.62)
				(name "S6")
				(number "6")
			)
			(pin input line
				(at -19.05 -6.35 0)
				(length 7.62)
				(name "S7")
				(number "7")
			)
			(pin input line
				(at -19.05 -8.89 0)
				(length 7.62)
				(name "S8")
				(number "8")
			)
			(pin input line
				(at 19.05 8.89 180)
				(length 7.62)
				(name "GND")
				(number "16")
			)
			(pin input line
				(at 19.05 6.35 180)
				(length 7.62)
				(name "A2")
				(number "15")
			)
			(pin input line
				(at 19.05 3.81 180)
				(length 7.62)
				(name "A1")
				(number "14")
			)
			(pin input line
				(at 19.05 1.27 180)
				(length 7.62)
				(name "A0")
				(number "13")
			)
			(pin input line
				(at 19.05 -1.27 180)
				(length 7.62)
				(name "EN")
				(number "12")
			)
			(pin input line
				(at 19.05 -3.81 180)
				(length 7.62)
				(name "V+")
				(number "11")
			)
			(pin input line
				(at 19.05 -6.35 180)
				(length 7.62)
				(name "OUT")
				(number "10")
			)
			(pin input line
				(at 19.05 -8.89 180)
				(length 7.62)
				(name "V-")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX311"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "MAX311"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX310-MAX311.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-Channel CMOS RF Video Multiplexer"
			(at 0 0 0)
		)
		(property "ki_keywords" "video rf"
			(at 0 0 0)
		)
		(symbol "MAX311_0_1")
		(symbol "MAX311_1_1"
			(pin input line
				(at -19.05 8.89 0)
				(length 7.62)
				(name "S1A")
				(number "1")
			)
			(pin input line
				(at -19.05 6.35 0)
				(length 7.62)
				(name "S2A")
				(number "2")
			)
			(pin input line
				(at -19.05 3.81 0)
				(length 7.62)
				(name "S3A")
				(number "3")
			)
			(pin input line
				(at -19.05 1.27 0)
				(length 7.62)
				(name "S4A")
				(number "4")
			)
			(pin input line
				(at -19.05 -1.27 0)
				(length 7.62)
				(name "S1B")
				(number "5")
			)
			(pin input line
				(at -19.05 -3.81 0)
				(length 7.62)
				(name "S2B")
				(number "6")
			)
			(pin input line
				(at -19.05 -6.35 0)
				(length 7.62)
				(name "S3B")
				(number "7")
			)
			(pin input line
				(at -19.05 -8.89 0)
				(length 7.62)
				(name "S4B")
				(number "8")
			)
			(pin output line
				(at 19.05 8.89 180)
				(length 7.62)
				(name "OUTA")
				(number "16")
			)
			(pin input line
				(at 19.05 6.35 180)
				(length 7.62)
				(name "GND")
				(number "15")
			)
			(pin input line
				(at 19.05 3.81 180)
				(length 7.62)
				(name "A1")
				(number "14")
			)
			(pin input line
				(at 19.05 1.27 180)
				(length 7.62)
				(name "A0")
				(number "13")
			)
			(pin input line
				(at 19.05 -1.27 180)
				(length 7.62)
				(name "EN")
				(number "12")
			)
			(pin input line
				(at 19.05 -3.81 180)
				(length 7.62)
				(name "V+")
				(number "11")
			)
			(pin input line
				(at 19.05 -6.35 180)
				(length 7.62)
				(name "OUTB")
				(number "10")
			)
			(pin input line
				(at 19.05 -8.89 180)
				(length 7.62)
				(name "V-")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MB88303P"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "MB88303P"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "MB88303P_0_1")
		(symbol "MB88303P_1_1"
			(pin input line
				(at -20.32 16.51 0)
				(length 7.62)
				(name "DA0")
				(number "14")
			)
			(pin input line
				(at -20.32 13.97 0)
				(length 7.62)
				(name "DA1")
				(number "15")
			)
			(pin input line
				(at -20.32 11.43 0)
				(length 7.62)
				(name "DA2")
				(number "16")
			)
			(pin input line
				(at -20.32 8.89 0)
				(length 7.62)
				(name "DA3")
				(number "17")
			)
			(pin input line
				(at -20.32 6.35 0)
				(length 7.62)
				(name "DA4")
				(number "18")
			)
			(pin input line
				(at -20.32 3.81 0)
				(length 7.62)
				(name "DA5")
				(number "19")
			)
			(pin input line
				(at -20.32 1.27 0)
				(length 7.62)
				(name "DA6")
				(number "20")
			)
			(pin input line
				(at -20.32 -1.27 0)
				(length 7.62)
				(name "DA7")
				(number "21")
			)
			(pin input line
				(at -20.32 -6.35 0)
				(length 7.62)
				(name "ADM")
				(number "13")
			)
			(pin input line
				(at -20.32 -11.43 0)
				(length 7.62)
				(name "LDI")
				(number "12")
			)
			(pin input inverted
				(at -20.32 -16.51 0)
				(length 7.62)
				(name "RESET")
				(number "1")
			)
			(pin power_in line
				(at 0 21.59 270)
				(length 2.54)
				(name "VCC")
				(number "22")
			)
			(pin power_in line
				(at 0 -21.59 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin input line
				(at 20.32 16.51 180)
				(length 7.62)
				(name "EX/RC")
				(number "9")
			)
			(pin output line
				(at 20.32 11.43 180)
				(length 7.62)
				(name "X/R")
				(number "10")
			)
			(pin output line
				(at 20.32 3.81 180)
				(length 7.62)
				(name "VOW")
				(number "5")
			)
			(pin output inverted
				(at 20.32 -1.27 180)
				(length 7.62)
				(name "VOB")
				(number "6")
			)
			(pin input inverted
				(at 20.32 -11.43 180)
				(length 7.62)
				(name "VSYNC")
				(number "7")
			)
			(pin input inverted
				(at 20.32 -16.51 180)
				(length 7.62)
				(name "HSYNC")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "S178"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "S178"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "S178_0_1")
		(symbol "S178_1_1"
			(pin input line
				(at -20.32 15.24 0)
				(length 7.62)
				(name "2.9")
				(number "2")
			)
			(pin input line
				(at -20.32 12.7 0)
				(length 7.62)
				(name "2.8")
				(number "3")
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 7.62)
				(name "2.7")
				(number "4")
			)
			(pin input line
				(at -20.32 7.62 0)
				(length 7.62)
				(name "2.6")
				(number "5")
			)
			(pin input line
				(at -20.32 5.08 0)
				(length 7.62)
				(name "2.5")
				(number "6")
			)
			(pin input line
				(at -20.32 2.54 0)
				(length 7.62)
				(name "2.4")
				(number "7")
			)
			(pin input line
				(at -20.32 0 0)
				(length 7.62)
				(name "2.3")
				(number "8")
			)
			(pin input line
				(at -20.32 -2.54 0)
				(length 7.62)
				(name "2.2")
				(number "9")
			)
			(pin input line
				(at -20.32 -5.08 0)
				(length 7.62)
				(name "2.1")
				(number "10")
			)
			(pin input line
				(at -20.32 -7.62 0)
				(length 7.62)
				(name "2.0")
				(number "11")
			)
			(pin input line
				(at -20.32 -10.16 0)
				(length 7.62)
				(name "N.A")
				(number "25")
			)
			(pin input line
				(at -20.32 -12.7 0)
				(length 7.62)
				(name "N.B")
				(number "24")
			)
			(pin input line
				(at -20.32 -15.24 0)
				(length 7.62)
				(name "N.C")
				(number "23")
			)
			(pin input inverted
				(at -7.62 -33.02 90)
				(length 7.62)
				(name "SH")
				(number "19")
			)
			(pin input line
				(at -5.08 33.02 270)
				(length 7.62)
				(name "+VCC")
				(number "1")
			)
			(pin input inverted
				(at -2.54 -33.02 90)
				(length 7.62)
				(name "V")
				(number "18")
			)
			(pin input clock
				(at 0 33.02 270)
				(length 7.62)
				(name "CP")
				(number "17")
			)
			(pin input inverted
				(at 2.54 -33.02 90)
				(length 7.62)
				(name "VR")
				(number "12")
			)
			(pin input line
				(at 5.08 33.02 270)
				(length 7.62)
				(name "-VCC")
				(number "15")
			)
			(pin input inverted
				(at 7.62 -33.02 90)
				(length 7.62)
				(name "SV")
				(number "13")
			)
			(pin output inverted
				(at 20.32 15.24 180)
				(length 7.62)
				(name "SUP")
				(number "28")
			)
			(pin output inverted
				(at 20.32 10.16 180)
				(length 7.62)
				(name "VD")
				(number "27")
			)
			(pin output inverted
				(at 20.32 5.08 180)
				(length 7.62)
				(name "SUP")
				(number "26")
			)
			(pin output inverted
				(at 20.32 0 180)
				(length 7.62)
				(name "CLAMP")
				(number "22")
			)
			(pin output inverted
				(at 20.32 -5.08 180)
				(length 7.62)
				(name "CS")
				(number "21")
			)
			(pin output inverted
				(at 20.32 -10.16 180)
				(length 7.62)
				(name "HD")
				(number "20")
			)
			(pin output line
				(at 20.32 -15.24 180)
				(length 7.62)
				(name "H2")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SAA7182"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -26.67 48.26 0)
		)
		(property "Value" "SAA7182"
			(at 17.78 -48.26 0)
		)
		(property "Footprint" ""
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://rcl-radio.ru/wp-content/uploads/2014/11/SAA7182.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "Digital Video Encoder, Obsolete"
			(at 0 0 0)
		)
		(property "ki_keywords" "Video Encoder"
			(at 0 0 0)
		)
		(symbol "SAA7182_0_1")
		(symbol "SAA7182_1_1"
			(pin input line
				(at -30.48 43.18 0)
				(length 3.81)
				(name "~RESN~")
				(number "1")
			)
			(pin input line
				(at -30.48 40.64 0)
				(length 3.81)
				(name "SA")
				(number "4")
			)
			(pin input line
				(at -30.48 38.1 0)
				(length 3.81)
				(name "SCL")
				(number "83")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 3.81)
				(name "SDA")
				(number "84")
			)
			(pin bidirectional clock
				(at -30.48 30.48 0)
				(length 3.81)
				(name "LCC")
				(number "48")
			)
			(pin input line
				(at -30.48 27.94 0)
				(length 3.81)
				(name "XTALI")
				(number "44")
			)
			(pin output line
				(at -30.48 25.4 0)
				(length 3.81)
				(name "XTAL")
				(number "45")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 3.81)
				(name "CREF")
				(number "47")
			)
			(pin output line
				(at -30.48 20.32 0)
				(length 3.81)
				(name "TTXRQ")
				(number "20")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 3.81)
				(name "RCV2")
				(number "36")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 3.81)
				(name "RCV1")
				(number "35")
			)
			(pin input line
				(at -30.48 12.7 0)
				(length 3.81)
				(name "CDIR")
				(number "50")
			)
			(pin input line
				(at -30.48 7.62 0)
				(length 3.81)
				(name "TTX")
				(number "21")
			)
			(pin input line
				(at -30.48 5.08 0)
				(length 3.81)
				(name "KEY")
				(number "9")
			)
			(pin input line
				(at -30.48 2.54 0)
				(length 3.81)
				(name "OVL2")
				(number "6")
			)
			(pin input line
				(at -30.48 0 0)
				(length 3.81)
				(name "OVL1")
				(number "7")
			)
			(pin input line
				(at -30.48 -2.54 0)
				(length 3.81)
				(name "OVL0")
				(number "8")
			)
			(pin input line
				(at -30.48 -5.08 0)
				(length 3.81)
				(name "DP0")
				(number "10")
			)
			(pin input line
				(at -30.48 -7.62 0)
				(length 3.81)
				(name "DP1")
				(number "11")
			)
			(pin input line
				(at -30.48 -10.16 0)
				(length 3.81)
				(name "DP2")
				(number "12")
			)
			(pin input line
				(at -30.48 -12.7 0)
				(length 3.81)
				(name "DP3")
				(number "13")
			)
			(pin input line
				(at -30.48 -15.24 0)
				(length 3.81)
				(name "DP4")
				(number "16")
			)
			(pin input line
				(at -30.48 -17.78 0)
				(length 3.81)
				(name "DP5")
				(number "17")
			)
			(pin input line
				(at -30.48 -20.32 0)
				(length 3.81)
				(name "DP6")
				(number "18")
			)
			(pin input line
				(at -30.48 -22.86 0)
				(length 3.81)
				(name "DP7")
				(number "19")
			)
			(pin input line
				(at -30.48 -25.4 0)
				(length 3.81)
				(name "MP7")
				(number "25")
			)
			(pin input line
				(at -30.48 -27.94 0)
				(length 3.81)
				(name "MP6")
				(number "26")
			)
			(pin input line
				(at -30.48 -30.48 0)
				(length 3.81)
				(name "MP5")
				(number "27")
			)
			(pin input line
				(at -30.48 -33.02 0)
				(length 3.81)
				(name "MP4")
				(number "28")
			)
			(pin input line
				(at -30.48 -35.56 0)
				(length 3.81)
				(name "MP3")
				(number "31")
			)
			(pin input line
				(at -30.48 -38.1 0)
				(length 3.81)
				(name "MP2")
				(number "32")
			)
			(pin input line
				(at -30.48 -40.64 0)
				(length 3.81)
				(name "MP1")
				(number "33")
			)
			(pin input line
				(at -30.48 -43.18 0)
				(length 3.81)
				(name "MP0")
				(number "34")
			)
			(pin power_in line
				(at -20.32 50.8 270)
				(length 3.81)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at -17.78 50.8 270)
				(length 3.81)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at -15.24 50.8 270)
				(length 3.81)
				(name "VDD")
				(number "22")
			)
			(pin power_in line
				(at -15.24 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "3")
			)
			(pin power_in line
				(at -12.7 50.8 270)
				(length 3.81)
				(name "VDD")
				(number "29")
			)
			(pin power_in line
				(at -12.7 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "15")
			)
			(pin power_in line
				(at -10.16 50.8 270)
				(length 3.81)
				(name "VDD")
				(number "38")
			)
			(pin power_in line
				(at -10.16 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "24")
			)
			(pin power_in line
				(at -7.62 50.8 270)
				(length 3.81)
				(name "VDD")
				(number "41")
			)
			(pin power_in line
				(at -7.62 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "30")
			)
			(pin power_in line
				(at -5.08 50.8 270)
				(length 3.81)
				(name "VDD")
				(number "49")
			)
			(pin power_in line
				(at -5.08 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "39")
			)
			(pin power_in line
				(at -2.54 50.8 270)
				(length 3.81)
				(name "VDD")
				(number "80")
			)
			(pin power_in line
				(at -2.54 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "42")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 3.81)
				(name "VDD")
				(number "82")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "51")
			)
			(pin power_in line
				(at 2.54 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "79")
			)
			(pin power_in line
				(at 5.08 50.8 270)
				(length 3.81)
				(name "VDDA")
				(number "54")
			)
			(pin power_in line
				(at 5.08 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "81")
			)
			(pin power_in line
				(at 7.62 50.8 270)
				(length 3.81)
				(name "VDDA")
				(number "57")
			)
			(pin power_in line
				(at 10.16 50.8 270)
				(length 3.81)
				(name "VDDA")
				(number "60")
			)
			(pin power_in line
				(at 12.7 50.8 270)
				(length 3.81)
				(name "VDDA")
				(number "64")
			)
			(pin power_in line
				(at 12.7 -50.8 90)
				(length 3.81)
				(name "VSSA")
				(number "67")
			)
			(pin power_in line
				(at 15.24 50.8 270)
				(length 3.81)
				(name "VDDA")
				(number "70")
			)
			(pin power_in line
				(at 17.78 50.8 270)
				(length 3.81)
				(name "VDDA")
				(number "72")
			)
			(pin power_in line
				(at 20.32 50.8 270)
				(length 3.81)
				(name "VDDA")
				(number "74")
			)
			(pin input line
				(at 30.48 40.64 180)
				(length 3.81)
				(name "SP")
				(number "78")
			)
			(pin input line
				(at 30.48 38.1 180)
				(length 3.81)
				(name "AP")
				(number "77")
			)
			(pin passive line
				(at 30.48 33.02 180)
				(length 3.81)
				(name "VREFL")
				(number "76")
			)
			(pin passive line
				(at 30.48 30.48 180)
				(length 3.81)
				(name "VREFH")
				(number "75")
			)
			(pin output line
				(at 30.48 20.32 180)
				(length 3.81)
				(name "CVBS")
				(number "73")
			)
			(pin output line
				(at 30.48 15.24 180)
				(length 3.81)
				(name "Y")
				(number "71")
			)
			(pin output line
				(at 30.48 10.16 180)
				(length 3.81)
				(name "C")
				(number "69")
			)
			(pin output line
				(at 30.48 5.08 180)
				(length 3.81)
				(name "R")
				(number "61")
			)
			(pin output line
				(at 30.48 0 180)
				(length 3.81)
				(name "G")
				(number "58")
			)
			(pin output line
				(at 30.48 -5.08 180)
				(length 3.81)
				(name "B")
				(number "55")
			)
			(pin passive line
				(at 30.48 -12.7 180)
				(length 3.81)
				(name "VREFH")
				(number "53")
			)
			(pin passive line
				(at 30.48 -15.24 180)
				(length 3.81)
				(name "VREFL")
				(number "52")
			)
			(pin input line
				(at 30.48 -40.64 180)
				(length 3.81)
				(name "CUR")
				(number "68")
			)
			(pin input line
				(at 30.48 -43.18 180)
				(length 3.81)
				(name "CUR")
				(number "63")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SI582"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "SI582"
			(at 7.62 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "SI582_0_1")
		(symbol "SI582_1_1"
			(pin input line
				(at -17.78 5.08 0)
				(length 7.62)
				(name "OFS")
				(number "1")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 7.62)
				(name "IN+")
				(number "3")
			)
			(pin input inverted
				(at -17.78 -2.54 0)
				(length 7.62)
				(name "IN-")
				(number "2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V+")
				(number "7")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "V-")
				(number "4")
			)
			(pin input inverted
				(at 17.78 5.08 180)
				(length 7.62)
				(name "DIS")
				(number "8")
			)
			(pin input line
				(at 17.78 0 180)
				(length 7.62)
				(name "OUT")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TDA1950"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "TDA1950"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "TDA1950_0_1")
		(symbol "TDA1950_1_1"
			(pin input line
				(at -30.48 8.89 0)
				(length 7.62)
				(name "NIVSEP")
				(number "8")
			)
			(pin output line
				(at -30.48 1.27 0)
				(length 7.62)
				(name "NIVV")
				(number "10")
			)
			(pin output line
				(at -30.48 -3.81 0)
				(length 7.62)
				(name "NIVH")
				(number "12")
			)
			(pin input inverted
				(at -30.48 -8.89 0)
				(length 7.62)
				(name "VIDEO")
				(number "11")
			)
			(pin output line
				(at -17.78 24.13 270)
				(length 7.62)
				(name "CS")
				(number "9")
			)
			(pin output line
				(at -12.7 24.13 270)
				(length 7.62)
				(name "MUTE")
				(number "7")
			)
			(pin input line
				(at -7.62 -24.13 90)
				(length 7.62)
				(name "VR")
				(number "5")
			)
			(pin output line
				(at -2.54 24.13 270)
				(length 7.62)
				(name "SW")
				(number "6")
			)
			(pin input inverted
				(at -2.54 -24.13 90)
				(length 7.62)
				(name "FLYH")
				(number "3")
			)
			(pin output line
				(at 2.54 24.13 270)
				(length 7.62)
				(name "PHCMP")
				(number "13")
			)
			(pin input line
				(at 2.54 -24.13 90)
				(length 7.62)
				(name "PHASE")
				(number "17")
			)
			(pin output line
				(at 7.62 24.13 270)
				(length 7.62)
				(name "R")
				(number "16")
			)
			(pin output line
				(at 12.7 24.13 270)
				(length 7.62)
				(name "C")
				(number "14")
			)
			(pin input line
				(at 30.48 13.97 180)
				(length 7.62)
				(name "+12")
				(number "14")
			)
			(pin input line
				(at 30.48 6.35 180)
				(length 7.62)
				(name "FLYV")
				(number "18")
			)
			(pin output line
				(at 30.48 1.27 180)
				(length 7.62)
				(name "SANDCASTLE")
				(number "4")
			)
			(pin output line
				(at 30.48 -3.81 180)
				(length 7.62)
				(name "HD")
				(number "2")
			)
			(pin input line
				(at 30.48 -13.97 180)
				(length 7.62)
				(name "GND")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TDA2593"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "TDA2593"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "TDA2593_0_1")
		(symbol "TDA2593_1_1"
			(pin input line
				(at -27.94 2.54 0)
				(length 7.62)
				(name "VIDEO")
				(number "9")
			)
			(pin input line
				(at -27.94 -2.54 0)
				(length 7.62)
				(name "NS")
				(number "10")
			)
			(pin input line
				(at -12.7 20.32 270)
				(length 7.62)
				(name "FW")
				(number "6")
			)
			(pin input inverted
				(at -12.7 -20.32 90)
				(length 7.62)
				(name "VCR")
				(number "11")
			)
			(pin input line
				(at -7.62 20.32 270)
				(length 7.62)
				(name "~")
				(number "5")
			)
			(pin input line
				(at -7.62 -20.32 90)
				(length 7.62)
				(name "F")
				(number "12")
			)
			(pin input line
				(at -2.54 20.32 270)
				(length 7.62)
				(name "PD")
				(number "4")
			)
			(pin input line
				(at -2.54 -20.32 90)
				(length 7.62)
				(name "F")
				(number "13")
			)
			(pin input line
				(at 2.54 20.32 270)
				(length 7.62)
				(name "V0")
				(number "2")
			)
			(pin input line
				(at 2.54 -20.32 90)
				(length 7.62)
				(name "C")
				(number "14")
			)
			(pin input line
				(at 7.62 20.32 270)
				(length 7.62)
				(name "VCC")
				(number "1")
			)
			(pin input line
				(at 7.62 -20.32 90)
				(length 7.62)
				(name "R")
				(number "15")
			)
			(pin input line
				(at 12.7 -20.32 90)
				(length 7.62)
				(name "GND")
				(number "16")
			)
			(pin output line
				(at 27.94 5.08 180)
				(length 7.62)
				(name "SANDC")
				(number "7")
			)
			(pin output line
				(at 27.94 0 180)
				(length 7.62)
				(name "HD")
				(number "3")
			)
			(pin output line
				(at 27.94 -5.08 180)
				(length 7.62)
				(name "VD")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TDA7260"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "TDA7260"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "TDA7260_0_1")
		(symbol "TDA7260_1_1"
			(pin input inverted
				(at -33.02 3.81 0)
				(length 7.62)
				(name "E-")
				(number "5")
			)
			(pin input line
				(at -33.02 -1.27 0)
				(length 7.62)
				(name "E+")
				(number "6")
			)
			(pin output line
				(at -33.02 -8.89 0)
				(length 7.62)
				(name "LIM")
				(number "7")
			)
			(pin output line
				(at -17.78 26.67 270)
				(length 7.62)
				(name "S0")
				(number "4")
			)
			(pin input line
				(at -12.7 26.67 270)
				(length 7.62)
				(name "I+")
				(number "3")
			)
			(pin power_in line
				(at -12.7 -26.67 90)
				(length 7.62)
				(name "GNDA")
				(number "8")
			)
			(pin input inverted
				(at -7.62 26.67 270)
				(length 7.62)
				(name "I-")
				(number "2")
			)
			(pin output line
				(at -5.08 -26.67 90)
				(length 7.62)
				(name "+10")
				(number "9")
			)
			(pin output line
				(at 0 26.67 270)
				(length 7.62)
				(name "SI")
				(number "1")
			)
			(pin input line
				(at 2.54 -26.67 90)
				(length 7.62)
				(name "CD")
				(number "10")
			)
			(pin input line
				(at 5.08 26.67 270)
				(length 7.62)
				(name "MUTE")
				(number "20")
			)
			(pin input line
				(at 12.7 26.67 270)
				(length 7.62)
				(name "VP+")
				(number "19")
			)
			(pin power_in line
				(at 15.24 -26.67 90)
				(length 7.62)
				(name "GND")
				(number "11")
			)
			(pin input line
				(at 33.02 16.51 180)
				(length 7.62)
				(name "CL")
				(number "18")
			)
			(pin output line
				(at 33.02 11.43 180)
				(length 7.62)
				(name "G1")
				(number "17")
			)
			(pin input line
				(at 33.02 6.35 180)
				(length 7.62)
				(name "POMPE1")
				(number "16")
			)
			(pin output line
				(at 33.02 1.27 180)
				(length 7.62)
				(name "G2")
				(number "15")
			)
			(pin output line
				(at 33.02 -6.35 180)
				(length 7.62)
				(name "G3")
				(number "14")
			)
			(pin input line
				(at 33.02 -11.43 180)
				(length 7.62)
				(name "POMPE2")
				(number "13")
			)
			(pin output line
				(at 33.02 -16.51 180)
				(length 7.62)
				(name "G4")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TDA8501"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 25.4 0)
		)
		(property "Value" "TDA8501"
			(at 6.35 25.4 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/TDA8501.pdf"
			(at 0 0 0)
		)
		(property "Description" "PAL/NTSC Encoder, RGB or Y/Y-R/Y-B Inputs, DIP/SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Video Encoder"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SOIC*"
			(at 0 0 0)
		)
		(symbol "TDA8501_0_1")
		(symbol "TDA8501_1_1"
			(pin input line
				(at -17.78 20.32 0)
				(length 3.81)
				(name "CS")
				(number "24")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "-R.Y")
				(number "1")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "-B.Y")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "H/2")
				(number "4")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "Y")
				(number "5")
			)
			(pin output line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "UOFF")
				(number "6")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "MCTR")
				(number "2")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "R")
				(number "7")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "G")
				(number "9")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "B")
				(number "11")
			)
			(pin output line
				(at -17.78 -12.7 0)
				(length 3.81)
				(name "VOFF")
				(number "12")
			)
			(pin output line
				(at -17.78 -17.78 0)
				(length 3.81)
				(name "OSC")
				(number "23")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 3.81)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 3.81)
				(name "VSS")
				(number "10")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "Y+SOUT")
				(number "22")
			)
			(pin input line
				(at 17.78 17.78 180)
				(length 3.81)
				(name "Y+SIN")
				(number "20")
			)
			(pin passive line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "VREF")
				(number "13")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "Y/OUT")
				(number "19")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "CVBS")
				(number "16")
			)
			(pin output line
				(at 17.78 0 180)
				(length 3.81)
				(name "C/OUT")
				(number "14")
			)
			(pin passive line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "B/ADJ")
				(number "21")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "NOTCH")
				(number "18")
			)
			(pin input line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "NTSC/PAL")
				(number "17")
			)
			(pin passive line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "FLT")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TDA8702"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 17.78 0)
		)
		(property "Value" "TDA8702"
			(at 5.08 17.78 0)
		)
		(property "Footprint" ""
			(at 0 -2.54 0)
		)
		(property "Datasheet" "philips/tda8702.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "8bit Video DAC (32 MHz), DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "DAC CNA VIDEO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO* SOIC*"
			(at 0 0 0)
		)
		(symbol "TDA8702_0_1")
		(symbol "TDA8702_1_1"
			(pin input line
				(at -15.24 12.7 0)
				(length 3.81)
				(name "DB0")
				(number "12")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 3.81)
				(name "DB1")
				(number "11")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "DB2")
				(number "3")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "DB3")
				(number "4")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "DB4")
				(number "10")
			)
			(pin input line
				(at -15.24 0 0)
				(length 3.81)
				(name "DB5")
				(number "9")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "DB6")
				(number "8")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "DB7")
				(number "7")
			)
			(pin input clock
				(at -15.24 -12.7 0)
				(length 3.81)
				(name "CLK")
				(number "5")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 3.81)
				(name "VCCD")
				(number "13")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 3.81)
				(name "DGND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 3.81)
				(name "VCCA")
				(number "16")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 3.81)
				(name "AGND")
				(number "2")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 3.81)
				(name "~VOUT~")
				(number "15")
			)
			(pin output line
				(at 15.24 0 180)
				(length 3.81)
				(name "VOUT")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 3.81)
				(name "VREF")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TDA8772"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -16.51 38.1 0)
		)
		(property "Value" "TDA8772"
			(at 8.89 38.1 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.pa0qy.nl/pdf/TDA8772.PDF"
			(at 0 0 0)
		)
		(property "Description" "Triple 8bit Video DAC, QFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Video DAC Colour 8bit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFP*"
			(at 0 0 0)
		)
		(symbol "TDA8772_0_1")
		(symbol "TDA8772_1_1"
			(pin input line
				(at -20.32 33.02 0)
				(length 3.81)
				(name "R0")
				(number "8")
			)
			(pin input line
				(at -20.32 30.48 0)
				(length 3.81)
				(name "R1")
				(number "7")
			)
			(pin input line
				(at -20.32 27.94 0)
				(length 3.81)
				(name "R2")
				(number "6")
			)
			(pin input line
				(at -20.32 25.4 0)
				(length 3.81)
				(name "R3")
				(number "5")
			)
			(pin input line
				(at -20.32 22.86 0)
				(length 3.81)
				(name "R4")
				(number "4")
			)
			(pin input line
				(at -20.32 20.32 0)
				(length 3.81)
				(name "R5")
				(number "3")
			)
			(pin input line
				(at -20.32 17.78 0)
				(length 3.81)
				(name "R6")
				(number "2")
			)
			(pin input line
				(at -20.32 15.24 0)
				(length 3.81)
				(name "R7")
				(number "1")
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 3.81)
				(name "G0")
				(number "20")
			)
			(pin input line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "G1")
				(number "19")
			)
			(pin input line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "G2")
				(number "18")
			)
			(pin input line
				(at -20.32 2.54 0)
				(length 3.81)
				(name "G3")
				(number "17")
			)
			(pin input line
				(at -20.32 0 0)
				(length 3.81)
				(name "G4")
				(number "16")
			)
			(pin input line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "G5")
				(number "15")
			)
			(pin input line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "G6")
				(number "14")
			)
			(pin input line
				(at -20.32 -7.62 0)
				(length 3.81)
				(name "G7")
				(number "13")
			)
			(pin input line
				(at -20.32 -12.7 0)
				(length 3.81)
				(name "B0")
				(number "31")
			)
			(pin input line
				(at -20.32 -15.24 0)
				(length 3.81)
				(name "B1")
				(number "30")
			)
			(pin input line
				(at -20.32 -17.78 0)
				(length 3.81)
				(name "B2")
				(number "29")
			)
			(pin input line
				(at -20.32 -20.32 0)
				(length 3.81)
				(name "B3")
				(number "28")
			)
			(pin input line
				(at -20.32 -22.86 0)
				(length 3.81)
				(name "B4")
				(number "27")
			)
			(pin input line
				(at -20.32 -25.4 0)
				(length 3.81)
				(name "B5")
				(number "26")
			)
			(pin input line
				(at -20.32 -27.94 0)
				(length 3.81)
				(name "B6")
				(number "25")
			)
			(pin input line
				(at -20.32 -30.48 0)
				(length 3.81)
				(name "B7")
				(number "24")
			)
			(pin power_in line
				(at -7.62 40.64 270)
				(length 3.81)
				(name "VCC")
				(number "10")
			)
			(pin power_in line
				(at -7.62 -40.64 90)
				(length 3.81)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 3.81)
				(name "VCC")
				(number "32")
			)
			(pin power_in line
				(at -5.08 -40.64 90)
				(length 3.81)
				(name "GND")
				(number "33")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 3.81)
				(name "VCCA")
				(number "35")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 3.81)
				(name "GNDA")
				(number "37")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 3.81)
				(name "VCCA")
				(number "39")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 3.81)
				(name "GNDA")
				(number "42")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 3.81)
				(name "VCCA")
				(number "43")
			)
			(pin output line
				(at 20.32 27.94 180)
				(length 3.81)
				(name "RED")
				(number "44")
			)
			(pin output line
				(at 20.32 22.86 180)
				(length 3.81)
				(name "GRE")
				(number "40")
			)
			(pin output line
				(at 20.32 17.78 180)
				(length 3.81)
				(name "BLU")
				(number "36")
			)
			(pin passive line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "IRFB")
				(number "41")
			)
			(pin passive line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "IRFA")
				(number "38")
			)
			(pin input line
				(at 20.32 0 180)
				(length 3.81)
				(name "VRD")
				(number "34")
			)
			(pin input line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "BLANK")
				(number "12")
			)
			(pin input line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "SYNC")
				(number "11")
			)
			(pin input clock
				(at 20.32 -20.32 180)
				(length 3.81)
				(name "CLKB")
				(number "23")
			)
			(pin input clock
				(at 20.32 -25.4 180)
				(length 3.81)
				(name "CLKG")
				(number "22")
			)
			(pin input clock
				(at 20.32 -30.48 180)
				(length 3.81)
				(name "CLKR")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TDA9500"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "TDA9500"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "TDA9500_0_1")
		(symbol "TDA9500_1_1"
			(pin power_in line
				(at -27.94 0 0)
				(length 7.62)
				(name "VIN")
				(number "6")
			)
			(pin output line
				(at -15.24 17.78 270)
				(length 7.62)
				(name "CS")
				(number "7")
			)
			(pin input line
				(at -15.24 -17.78 90)
				(length 7.62)
				(name "R")
				(number "16")
			)
			(pin output line
				(at -10.16 17.78 270)
				(length 7.62)
				(name "TOPV")
				(number "8")
			)
			(pin input line
				(at -10.16 -17.78 90)
				(length 7.62)
				(name "C")
				(number "15")
			)
			(pin passive line
				(at -5.08 17.78 270)
				(length 7.62)
				(name "~")
				(number "9")
			)
			(pin passive line
				(at -5.08 -17.78 90)
				(length 7.62)
				(name "COM")
				(number "14")
			)
			(pin passive line
				(at 0 17.78 270)
				(length 7.62)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 7.62)
				(name "~")
				(number "13")
			)
			(pin passive line
				(at 5.08 17.78 270)
				(length 7.62)
				(name "~")
				(number "12")
			)
			(pin input line
				(at 5.08 -17.78 90)
				(length 7.62)
				(name "FW")
				(number "11")
			)
			(pin output line
				(at 10.16 17.78 270)
				(length 7.62)
				(name "SANDC")
				(number "5")
			)
			(pin power_in line
				(at 15.24 17.78 270)
				(length 7.62)
				(name "VCC")
				(number "4")
			)
			(pin power_in line
				(at 15.24 -17.78 90)
				(length 7.62)
				(name "GND")
				(number "1")
			)
			(pin output line
				(at 27.94 0 180)
				(length 7.62)
				(name "SH")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TEA2014"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "TEA2014"
			(at 6.096 6.604 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://pdf1.alldatasheet.com/datasheet-pdf/view/123244/STMICROELECTRONICS/TEA2014.html"
			(at 7.62 -2.54 0)
		)
		(property "Description" "Video switching circuite for TV, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Video switching circuite for TV"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "TEA2014_0_1")
		(symbol "TEA2014_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "EVI")
				(number "8")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "IVI")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "2/1")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VO")
				(number "2")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SVO")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TEA5115"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -16.51 22.86 0)
		)
		(property "Value" "TEA5115"
			(at 10.16 22.86 0)
		)
		(property "Footprint" ""
			(at -1.27 -1.27 0)
		)
		(property "Datasheet" ""
			(at -1.27 -1.27 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "TEA5115_0_1")
		(symbol "TEA5115_1_1"
			(pin input line
				(at -25.4 17.78 0)
				(length 7.62)
				(name "ER1")
				(number "12")
			)
			(pin input line
				(at -25.4 15.24 0)
				(length 7.62)
				(name "ER2")
				(number "16")
			)
			(pin input line
				(at -25.4 10.16 0)
				(length 7.62)
				(name "EV1")
				(number "18")
			)
			(pin input line
				(at -25.4 7.62 0)
				(length 7.62)
				(name "EV2")
				(number "2")
			)
			(pin input line
				(at -25.4 2.54 0)
				(length 7.62)
				(name "EB1")
				(number "10")
			)
			(pin input line
				(at -25.4 0 0)
				(length 7.62)
				(name "EB2")
				(number "8")
			)
			(pin input line
				(at -25.4 -5.08 0)
				(length 7.62)
				(name "EFB1")
				(number "11")
			)
			(pin input line
				(at -25.4 -7.62 0)
				(length 7.62)
				(name "EFB2")
				(number "9")
			)
			(pin input line
				(at -25.4 -12.7 0)
				(length 7.62)
				(name "ES1")
				(number "17")
			)
			(pin input line
				(at -25.4 -15.24 0)
				(length 7.62)
				(name "ES2")
				(number "1")
			)
			(pin input line
				(at -25.4 -20.32 0)
				(length 7.62)
				(name "SEL1/2")
				(number "3")
			)
			(pin input line
				(at 0 27.94 270)
				(length 7.62)
				(name "VSP")
				(number "7")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 7.62)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 22.86 17.78 180)
				(length 7.62)
				(name "ROUT")
				(number "14")
			)
			(pin output line
				(at 22.86 10.16 180)
				(length 7.62)
				(name "VOUT")
				(number "4")
			)
			(pin output line
				(at 22.86 2.54 180)
				(length 7.62)
				(name "BOUT")
				(number "6")
			)
			(pin output line
				(at 22.86 -5.08 180)
				(length 7.62)
				(name "FBOUT")
				(number "13")
			)
			(pin output line
				(at 22.86 -12.7 180)
				(length 7.62)
				(name "SYOUT")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TFP410PAP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 57.15 0)
		)
		(property "Value" "TFP410PAP"
			(at 11.43 57.15 0)
		)
		(property "Footprint" "Package_QFP:HTQFP-64-1EP_10x10mm_P0.5mm_EP8x8mm_Mask4.4x4.4mm_ThermalVias"
			(at 1.27 -60.96 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tfp410.pdf"
			(at 1.27 -59.69 0)
		)
		(property "Description" "Digital Visual Interface Compliant PanelBus Digital Transmitter, HTQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "DVI Encoder Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTQFP*1EP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TFP410PAP_0_1")
		(symbol "TFP410PAP_1_1"
			(pin input line
				(at -17.78 53.34 0)
				(length 2.54)
				(name "IDCK-")
				(number "56")
			)
			(pin input line
				(at -17.78 50.8 0)
				(length 2.54)
				(name "IDCK+")
				(number "57")
			)
			(pin input line
				(at -17.78 45.72 0)
				(length 2.54)
				(name "DATA0")
				(number "63")
			)
			(pin input line
				(at -17.78 43.18 0)
				(length 2.54)
				(name "DATA1")
				(number "62")
			)
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "DATA2")
				(number "61")
			)
			(pin input line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "DATA3")
				(number "60")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "DATA4")
				(number "59")
			)
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "DATA5")
				(number "58")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "DATA6")
				(number "55")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "DATA7")
				(number "54")
			)
			(pin input line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "DATA8")
				(number "53")
			)
			(pin input line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "DATA9")
				(number "52")
			)
			(pin input line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "DATA10")
				(number "51")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "DATA11")
				(number "50")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "DATA12")
				(number "47")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "DATA13")
				(number "46")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "DATA14")
				(number "45")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "DATA15")
				(number "44")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "DATA16")
				(number "43")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "DATA17")
				(number "42")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "DATA18")
				(number "41")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "DATA19")
				(number "40")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "DATA20")
				(number "39")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "DATA21")
				(number "38")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "DATA22")
				(number "37")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "DATA23")
				(number "36")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "DE")
				(number "2")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "VSYNC")
				(number "5")
			)
			(pin input line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "HSYNC")
				(number "4")
			)
			(pin input line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "EDGE/HTPLG")
				(number "9")
			)
			(pin input line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "DKEN")
				(number "35")
			)
			(pin output line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "MSEN/PO1")
				(number "11")
			)
			(pin input line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "~PD")
				(number "10")
			)
			(pin input line
				(at -17.78 -40.64 0)
				(length 2.54)
				(name "ISEL/~RST")
				(number "13")
			)
			(pin input line
				(at -17.78 -43.18 0)
				(length 2.54)
				(name "CTL1/A1/DK1")
				(number "8")
			)
			(pin input line
				(at -17.78 -45.72 0)
				(length 2.54)
				(name "CTL2/A2/DK2")
				(number "7")
			)
			(pin input line
				(at -17.78 -48.26 0)
				(length 2.54)
				(name "CTL3/A3/DK3")
				(number "6")
			)
			(pin input line
				(at -17.78 -53.34 0)
				(length 2.54)
				(name "BSEL/SCL")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 -55.88 0)
				(length 2.54)
				(name "DSEL/SDA")
				(number "14")
			)
			(pin power_in line
				(at -2.54 58.42 270)
				(length 2.54)
				(name "TVDD")
				(number "23")
			)
			(pin passive line
				(at -2.54 58.42 270)
				(length 2.54)
				(hide yes)
				(name "TVDD")
				(number "29")
			)
			(pin power_in line
				(at -2.54 -60.96 90)
				(length 2.54)
				(name "TGND")
				(number "20")
			)
			(pin passive line
				(at -2.54 -60.96 90)
				(length 2.54)
				(hide yes)
				(name "TGND")
				(number "26")
			)
			(pin passive line
				(at -2.54 -60.96 90)
				(length 2.54)
				(hide yes)
				(name "TGND")
				(number "32")
			)
			(pin power_in line
				(at 0 58.42 270)
				(length 2.54)
				(name "DVDD")
				(number "1")
			)
			(pin passive line
				(at 0 58.42 270)
				(length 2.54)
				(hide yes)
				(name "DVDD")
				(number "12")
			)
			(pin passive line
				(at 0 58.42 270)
				(length 2.54)
				(hide yes)
				(name "DVDD")
				(number "33")
			)
			(pin power_in line
				(at 0 -60.96 90)
				(length 2.54)
				(name "DGND")
				(number "16")
			)
			(pin passive line
				(at 0 -60.96 90)
				(length 2.54)
				(hide yes)
				(name "DGND")
				(number "48")
			)
			(pin passive line
				(at 0 -60.96 90)
				(length 2.54)
				(hide yes)
				(name "DGND")
				(number "64")
			)
			(pin power_in line
				(at 2.54 58.42 270)
				(length 2.54)
				(name "PVDD")
				(number "18")
			)
			(pin power_in line
				(at 2.54 -60.96 90)
				(length 2.54)
				(name "PGND")
				(number "17")
			)
			(pin power_in line
				(at 5.08 -60.96 90)
				(length 2.54)
				(name "EP")
				(number "65")
			)
			(pin no_connect line
				(at 15.24 -33.02 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "49")
			)
			(pin input line
				(at 17.78 53.34 180)
				(length 2.54)
				(name "VREF")
				(number "3")
			)
			(pin input line
				(at 17.78 48.26 180)
				(length 2.54)
				(name "TFADJ")
				(number "19")
			)
			(pin output line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "TX0+")
				(number "25")
			)
			(pin output line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "TX0-")
				(number "24")
			)
			(pin output line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "TX1+")
				(number "28")
			)
			(pin output line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "TX1-")
				(number "27")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "TX2+")
				(number "31")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "TX2-")
				(number "30")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "TXC+")
				(number "22")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "TXC-")
				(number "21")
			)
			(pin input line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "RESERVED")
				(number "34")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADA4430-1WYRTZ"
		(extends "ADA4430-1YKSZ")
		(property "Reference" "U"
			(at -3.81 8.89 0)
		)
		(property "Value" "ADA4430-1WYRTZ"
			(at 8.89 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADA4430-1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Ultralow Power, Video Filter, Power-Down, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Video Filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "ADV7391BCPZ"
		(extends "ADV7390BCPZ")
		(property "Reference" "U"
			(at -13.97 26.67 0)
		)
		(property "Value" "ADV7391BCPZ"
			(at 13.97 26.67 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADV7390_7391_7392_7393.pdf"
			(at 0 0 0)
		)
		(property "Description" "10-Bit SD/HD Video Encoder, LFCSP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Video Encoder"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TDA1950F"
		(extends "TDA1950")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "TDA1950F"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
	)
	(symbol "TDA8702T"
		(extends "TDA8702")
		(property "Reference" "U"
			(at -11.43 17.78 0)
		)
		(property "Value" "TDA8702T"
			(at 5.08 17.78 0)
		)
		(property "Footprint" ""
			(at 0 -2.54 0)
		)
		(property "Datasheet" "philips/tda8702.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "8bit Video DAC (32 MHz), SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "DAC CNA VIDEO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO* SOIC*"
			(at 0 0 0)
		)
	)
	(symbol "TDA9503"
		(extends "TDA9500")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "TDA9503"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
	)
	(symbol "TDA9513"
		(extends "TDA9500")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "TDA9513"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
	)
)
