(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A4")
	(lib_symbols
		(symbol "Connector:Conn_01x02_Pin"
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0 2.54 0)
			)
			(property "Value" "Conn_01x02_Pin"
				(at 0 -5.08 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Generic connector, single row, 01x02, script generated"
				(at 0 0 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "connector"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Connector*:*_1x??_*"
				(at 0 0 0)
			)
			(symbol "Conn_01x02_Pin_1_1"
				(rectangle
					(start 0.8636 0.127)
					(end 0 -0.127)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 0.8636 -2.413)
					(end 0 -2.667)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 1.27 0) (xy 0.8636 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -2.54) (xy 0.8636 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 5.08 0 180)
					(length 3.81)
					(name "Pin_1")
					(number "1")
				)
				(pin passive line
					(at 5.08 -2.54 180)
					(length 3.81)
					(name "Pin_2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Connector:Conn_01x03_Pin"
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0 5.08 0)
			)
			(property "Value" "Conn_01x03_Pin"
				(at 0 -5.08 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Generic connector, single row, 01x03, script generated"
				(at 0 0 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "connector"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Connector*:*_1x??_*"
				(at 0 0 0)
			)
			(symbol "Conn_01x03_Pin_1_1"
				(rectangle
					(start 0.8636 2.667)
					(end 0 2.413)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 0.8636 0.127)
					(end 0 -0.127)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 0.8636 -2.413)
					(end 0 -2.667)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 1.27 2.54) (xy 0.8636 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 0) (xy 0.8636 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -2.54) (xy 0.8636 -2.54)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 5.08 2.54 180)
					(length 3.81)
					(name "Pin_1")
					(number "1")
				)
				(pin passive line
					(at 5.08 0 180)
					(length 3.81)
					(name "Pin_2")
					(number "2")
				)
				(pin passive line
					(at 5.08 -2.54 180)
					(length 3.81)
					(name "Pin_3")
					(number "3")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Connector_Generic:Conn_01x04"
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0 5.08 0)
			)
			(property "Value" "Conn_01x04"
				(at 0 -7.62 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
				(at 0 0 0)
			)
			(property "ki_keywords" "connector"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Connector*:*_1x??_*"
				(at 0 0 0)
			)
			(symbol "Conn_01x04_1_1"
				(rectangle
					(start -1.27 3.81)
					(end 1.27 -6.35)
					(fill
						(type background)
					)
				)
				(rectangle
					(start -1.27 2.667)
					(end 0 2.413)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 0.127)
					(end 0 -0.127)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 -2.413)
					(end 0 -2.667)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 -4.953)
					(end 0 -5.207)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at -5.08 2.54 0)
					(length 3.81)
					(name "Pin_1")
					(number "1")
				)
				(pin passive line
					(at -5.08 0 0)
					(length 3.81)
					(name "Pin_2")
					(number "2")
				)
				(pin passive line
					(at -5.08 -2.54 0)
					(length 3.81)
					(name "Pin_3")
					(number "3")
				)
				(pin passive line
					(at -5.08 -5.08 0)
					(length 3.81)
					(name "Pin_4")
					(number "4")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Device:R"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.032 0 90)
			)
			(property "Value" "R"
				(at 0 0 90)
			)
			(property "Footprint" ""
				(at -1.778 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_0_1"
				(rectangle
					(start -1.016 -2.54)
					(end 1.016 2.54)
					(fill
						(type none)
					)
				)
			)
			(symbol "R_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Diode:1N4448"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at 0 2.54 0)
			)
			(property "Value" "1N4448"
				(at 0 -2.54 0)
			)
			(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
				(at 0 -4.445 0)
			)
			(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/1N4148_1N4448.pdf"
				(at 0 0 0)
			)
			(property "Description" "100V 0.15A High-speed standard diode, DO-35"
				(at 0 0 0)
			)
			(property "Sim.Device" "D"
				(at 0 0 0)
			)
			(property "Sim.Pins" "1=K 2=A"
				(at 0 0 0)
			)
			(property "ki_keywords" "diode"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "D*DO?35*"
				(at 0 0 0)
			)
			(symbol "1N4448_0_1"
				(polyline
					(pts
						(xy -1.27 1.27) (xy -1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 1.27) (xy 1.27 -1.27) (xy -1.27 0) (xy 1.27 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 0) (xy -1.27 0)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "1N4448_1_1"
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "K")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "A")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Relay:SANYOU_SRD_Form_C"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "K"
				(at 11.43 3.81 0)
			)
			(property "Value" "SANYOU_SRD_Form_C"
				(at 11.43 1.27 0)
			)
			(property "Footprint" "Relay_THT:Relay_SPDT_SANYOU_SRD_Series_Form_C"
				(at 11.43 -1.27 0)
			)
			(property "Datasheet" "http://www.sanyourelay.ca/public/products/pdf/SRD.pdf"
				(at 0 0 0)
			)
			(property "Description" "Sanyo SRD relay, Single Pole Miniature Power Relay,"
				(at 0 0 0)
			)
			(property "ki_keywords" "Single Pole Relay SPDT"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Relay*SPDT*SANYOU*SRD*Series*Form*C*"
				(at 0 0 0)
			)
			(symbol "SANYOU_SRD_Form_C_0_0"
				(polyline
					(pts
						(xy 7.62 5.08) (xy 7.62 2.54) (xy 6.985 3.175) (xy 7.62 3.81)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "SANYOU_SRD_Form_C_0_1"
				(rectangle
					(start -10.16 5.08)
					(end 10.16 -5.08)
					(fill
						(type background)
					)
				)
				(rectangle
					(start -8.255 1.905)
					(end -1.905 -1.905)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -7.62 -1.905) (xy -2.54 1.905)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -5.08 5.08) (xy -5.08 1.905)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -5.08 -5.08) (xy -5.08 -1.905)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.905 0) (xy -1.27 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.635 0) (xy 0 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.635 0) (xy 1.27 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.905 0) (xy 2.54 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.175 0) (xy 3.81 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 -2.54) (xy 3.175 3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 -2.54) (xy 5.08 -5.08)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "SANYOU_SRD_Form_C_1_1"
				(polyline
					(pts
						(xy 2.54 3.81) (xy 3.175 3.175) (xy 2.54 2.54) (xy 2.54 5.08)
					)
					(fill
						(type outline)
					)
				)
				(pin passive line
					(at -5.08 7.62 270)
					(length 2.54)
					(name "~")
					(number "5")
				)
				(pin passive line
					(at -5.08 -7.62 90)
					(length 2.54)
					(name "~")
					(number "2")
				)
				(pin passive line
					(at 2.54 7.62 270)
					(length 2.54)
					(name "~")
					(number "4")
				)
				(pin passive line
					(at 5.08 -7.62 90)
					(length 2.54)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 7.62 7.62 270)
					(length 2.54)
					(name "~")
					(number "3")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Transistor_BJT:PN2222A"
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "Q"
				(at 5.08 1.905 0)
			)
			(property "Value" "PN2222A"
				(at 5.08 0 0)
			)
			(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
				(at 5.08 -1.905 0)
			)
			(property "Datasheet" "https://www.onsemi.com/pub/Collateral/PN2222-D.PDF"
				(at 0 0 0)
			)
			(property "Description" "1A Ic, 40V Vce, NPN Transistor, General Purpose Transistor, TO-92"
				(at 0 0 0)
			)
			(property "ki_keywords" "NPN Transistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "TO?92*"
				(at 0 0 0)
			)
			(symbol "PN2222A_0_1"
				(polyline
					(pts
						(xy -2.54 0) (xy 0.635 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.635 1.905) (xy 0.635 -1.905)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 1.27 0)
					(radius 2.8194)
					(fill
						(type none)
					)
				)
			)
			(symbol "PN2222A_1_1"
				(polyline
					(pts
						(xy 0.635 0.635) (xy 2.54 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.635 -0.635) (xy 2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -1.778) (xy 1.778 -1.27) (xy 2.286 -2.286) (xy 1.27 -1.778)
					)
					(fill
						(type outline)
					)
				)
				(pin input line
					(at -5.08 0 0)
					(length 2.54)
					(name "B")
					(number "2")
				)
				(pin passive line
					(at 2.54 5.08 270)
					(length 2.54)
					(name "C")
					(number "3")
				)
				(pin passive line
					(at 2.54 -5.08 90)
					(length 2.54)
					(name "E")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Transistor_BJT:S8050"
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "Q"
				(at 5.08 1.905 0)
			)
			(property "Value" "S8050"
				(at 5.08 0 0)
			)
			(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
				(at 5.08 -1.905 0)
			)
			(property "Datasheet" "http://www.unisonic.com.tw/datasheet/S8050.pdf"
				(at 0 0 0)
			)
			(property "Description" "0.7A Ic, 20V Vce, Low Voltage High Current NPN Transistor, TO-92"
				(at 0 0 0)
			)
			(property "ki_keywords" "S8050 NPN Low Voltage High Current Transistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "TO?92*"
				(at 0 0 0)
			)
			(symbol "S8050_0_1"
				(polyline
					(pts
						(xy -2.54 0) (xy 0.635 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.635 1.905) (xy 0.635 -1.905)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 1.27 0)
					(radius 2.8194)
					(fill
						(type none)
					)
				)
			)
			(symbol "S8050_1_1"
				(polyline
					(pts
						(xy 0.635 0.635) (xy 2.54 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.635 -0.635) (xy 2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -1.778) (xy 1.778 -1.27) (xy 2.286 -2.286) (xy 1.27 -1.778)
					)
					(fill
						(type outline)
					)
				)
				(pin input line
					(at -5.08 0 0)
					(length 2.54)
					(name "B")
					(number "2")
				)
				(pin passive line
					(at 2.54 5.08 270)
					(length 2.54)
					(name "C")
					(number "3")
				)
				(pin passive line
					(at 2.54 -5.08 90)
					(length 2.54)
					(name "E")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "radiateur-rescue:DS18B20-Sensor_Temperature"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -3.81 6.35 0)
			)
			(property "Value" "Sensor_Temperature_DS18B20"
				(at 6.35 6.35 0)
			)
			(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
				(at -25.4 -6.35 0)
			)
			(property "Datasheet" ""
				(at -3.81 6.35 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_fp_filters" "TO*92*"
				(at 0 0 0)
			)
			(symbol "DS18B20-Sensor_Temperature_0_1"
				(rectangle
					(start -5.08 5.08)
					(end 5.08 -5.08)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy -3.937 3.175) (xy -3.937 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.937 3.175) (xy -3.302 3.175)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.937 2.54) (xy -3.302 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.937 1.905) (xy -3.302 1.905)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.937 1.27) (xy -3.302 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.937 0.635) (xy -3.302 0.635)
					)
					(fill
						(type none)
					)
				)
				(arc
					(start -3.937 3.175)
					(mid -3.302 3.81)
					(end -2.667 3.175)
					(fill
						(type none)
					)
				)
				(circle
					(center -3.302 -2.54)
					(radius 1.27)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy -2.667 3.175) (xy -2.667 0)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -2.667 -1.905)
					(end -3.937 0)
					(fill
						(type outline)
					)
				)
			)
			(symbol "DS18B20-Sensor_Temperature_1_1"
				(pin power_in line
					(at 0 7.62 270)
					(length 2.54)
					(name "VDD")
					(number "3")
				)
				(pin power_in line
					(at 0 -7.62 90)
					(length 2.54)
					(name "GND")
					(number "1")
				)
				(pin bidirectional line
					(at 7.62 0 180)
					(length 2.54)
					(name "DQ")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "radiateur-rescue:GND-power"
			(power)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "power_GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(symbol "GND-power_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND-power_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(hide yes)
					(name "GND")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "radiateur-rescue:LED_RGBC-Device"
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D2"
				(at 0 12.6238 0)
			)
			(property "Value" "LED_RGBC"
				(at 0 10.3124 0)
			)
			(property "Footprint" "LED_THT:LED_RGB_5mm_amazon"
				(at 0 -1.27 0)
			)
			(property "Datasheet" "~"
				(at 0 -1.27 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*"
				(at 0 0 0)
			)
			(symbol "LED_RGBC-Device_0_0"
				(text "R"
					(at 1.905 3.81 0)
				)
				(text "G"
					(at 1.905 -1.27 0)
				)
				(text "B"
					(at 1.905 -6.35 0)
				)
			)
			(symbol "LED_RGBC-Device_0_1"
				(circle
					(center -2.032 0)
					(radius 0.254)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy -1.27 6.35) (xy -1.27 3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 6.35) (xy -1.27 3.81) (xy -1.27 3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 5.08) (xy 1.27 5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 5.08) (xy -2.032 5.08) (xy -2.032 -5.08) (xy -1.016 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 1.27) (xy -1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 1.27) (xy -1.27 -1.27) (xy -1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 0) (xy -2.54 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 -3.81) (xy -1.27 -6.35)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 -5.08) (xy 1.27 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.016 6.35) (xy 0.508 7.874) (xy -0.254 7.874) (xy 0.508 7.874) (xy 0.508 7.112)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.016 1.27) (xy 0.508 2.794) (xy -0.254 2.794) (xy 0.508 2.794) (xy 0.508 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.016 -3.81) (xy 0.508 -2.286) (xy -0.254 -2.286) (xy 0.508 -2.286) (xy 0.508 -3.048)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 6.35) (xy 1.524 7.874) (xy 0.762 7.874) (xy 1.524 7.874) (xy 1.524 7.112)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 1.27) (xy 1.524 2.794) (xy 0.762 2.794) (xy 1.524 2.794) (xy 1.524 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -3.81) (xy 1.524 -2.286) (xy 0.762 -2.286) (xy 1.524 -2.286) (xy 1.524 -3.048)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 6.35) (xy 1.27 3.81) (xy -1.27 5.08) (xy 1.27 6.35)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 1.27 6.35)
					(end 1.27 6.35)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 5.08) (xy 2.54 5.08)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 1.27 3.81)
					(end 1.27 6.35)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 1.27) (xy 1.27 -1.27) (xy -1.27 0) (xy 1.27 1.27)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 1.27 1.27)
					(end 1.27 1.27)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 0) (xy -1.27 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 0) (xy 2.54 0)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 1.27 -1.27)
					(end 1.27 1.27)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -3.81) (xy 1.27 -6.35) (xy -1.27 -5.08) (xy 1.27 -3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -5.08) (xy 2.54 -5.08)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 2.794 8.382)
					(end -2.794 -7.62)
					(fill
						(type background)
					)
				)
			)
			(symbol "LED_RGBC-Device_1_1"
				(pin passive line
					(at -5.08 0 0)
					(length 2.54)
					(name "K")
					(number "2")
				)
				(pin passive line
					(at 5.08 5.08 180)
					(length 2.54)
					(name "RA")
					(number "1")
				)
				(pin passive line
					(at 5.08 0 180)
					(length 2.54)
					(name "GA")
					(number "3")
				)
				(pin passive line
					(at 5.08 -5.08 180)
					(length 2.54)
					(name "BA")
					(number "4")
				)
			)
			(embedded_fonts no)
		)
		(symbol "radiateur-rescue:LINE-power"
			(power)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -3.81 0)
			)
			(property "Value" "power_LINE"
				(at 0 3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(symbol "LINE-power_0_1"
				(polyline
					(pts
						(xy -0.762 1.27) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "LINE-power_1_1"
				(pin power_in line
					(at 0 0 90)
					(length 0)
					(hide yes)
					(name "LINE")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "radiateur-rescue:NEUT-power"
			(power)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -3.81 0)
			)
			(property "Value" "power_NEUT"
				(at 0 3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(symbol "NEUT-power_0_1"
				(polyline
					(pts
						(xy -0.762 1.27) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "NEUT-power_1_1"
				(pin power_in line
					(at 0 0 90)
					(length 0)
					(hide yes)
					(name "NEUT")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "radiateur-rescue:PWR_FLAG-power"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#FLG"
				(at 0 1.905 0)
			)
			(property "Value" "power_PWR_FLAG"
				(at 0 3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(symbol "PWR_FLAG-power_0_0"
				(pin power_out line
					(at 0 0 90)
					(length 0)
					(name "pwr")
					(number "1")
				)
			)
			(symbol "PWR_FLAG-power_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 1.27) (xy -1.016 1.905) (xy 0 2.54) (xy 1.016 1.905) (xy 0 1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(embedded_fonts no)
		)
		(symbol "radiateur-rescue:Raspberry_Pi_2_3-Connector"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at -17.78 31.75 0)
			)
			(property "Value" "Connector_Raspberry_Pi_2_3"
				(at 10.16 -31.75 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_fp_filters" "PinHeader*2x20*P2.54mm*Vertical* PinSocket*2x20*P2.54mm*Vertical*"
				(at 0 0 0)
			)
			(symbol "Raspberry_Pi_2_3-Connector_0_1"
				(rectangle
					(start -17.78 30.48)
					(end 17.78 -30.48)
					(fill
						(type background)
					)
				)
			)
			(symbol "Raspberry_Pi_2_3-Connector_1_1"
				(rectangle
					(start -16.891 23.114)
					(end -17.78 22.606)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -16.891 20.574)
					(end -17.78 20.066)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -16.891 15.494)
					(end -17.78 14.986)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -16.891 12.954)
					(end -17.78 12.446)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -16.891 10.414)
					(end -17.78 9.906)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -16.891 5.334)
					(end -17.78 4.826)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -16.891 2.794)
					(end -17.78 2.286)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -16.891 0.254)
					(end -17.78 -0.254)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -16.891 -4.826)
					(end -17.78 -5.334)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -16.891 -7.366)
					(end -17.78 -7.874)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -16.891 -9.906)
					(end -17.78 -10.414)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -16.891 -12.446)
					(end -17.78 -12.954)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -16.891 -14.986)
					(end -17.78 -15.494)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -16.891 -17.526)
					(end -17.78 -18.034)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -10.414 -29.591)
					(end -9.906 -30.48)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -7.874 -29.591)
					(end -7.366 -30.48)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -5.334 30.48)
					(end -4.826 29.591)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -5.334 -29.591)
					(end -4.826 -30.48)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -2.794 30.48)
					(end -2.286 29.591)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -2.794 -29.591)
					(end -2.286 -30.48)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -0.254 -29.591)
					(end 0.254 -30.48)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 2.286 30.48)
					(end 2.794 29.591)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 2.286 -29.591)
					(end 2.794 -30.48)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 4.826 30.48)
					(end 5.334 29.591)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 4.826 -29.591)
					(end 5.334 -30.48)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 7.366 -29.591)
					(end 7.874 -30.48)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 17.78 23.114)
					(end 16.891 22.606)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 17.78 20.574)
					(end 16.891 20.066)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 17.78 15.494)
					(end 16.891 14.986)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 17.78 12.954)
					(end 16.891 12.446)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 17.78 7.874)
					(end 16.891 7.366)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 17.78 5.334)
					(end 16.891 4.826)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 17.78 2.794)
					(end 16.891 2.286)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 17.78 -2.286)
					(end 16.891 -2.794)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 17.78 -4.826)
					(end 16.891 -5.334)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 17.78 -7.366)
					(end 16.891 -7.874)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 17.78 -9.906)
					(end 16.891 -10.414)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 17.78 -12.446)
					(end 16.891 -12.954)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 17.78 -17.526)
					(end 16.891 -18.034)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 17.78 -20.066)
					(end 16.891 -20.574)
					(fill
						(type none)
					)
				)
				(pin bidirectional line
					(at -20.32 22.86 0)
					(length 2.54)
					(name "GPIO14/TXD")
					(number "8")
				)
				(pin bidirectional line
					(at -20.32 20.32 0)
					(length 2.54)
					(name "GPIO15/RXD")
					(number "10")
				)
				(pin bidirectional line
					(at -20.32 15.24 0)
					(length 2.54)
					(name "GPIO16")
					(number "36")
				)
				(pin bidirectional line
					(at -20.32 12.7 0)
					(length 2.54)
					(name "GPIO17")
					(number "11")
				)
				(pin bidirectional line
					(at -20.32 10.16 0)
					(length 2.54)
					(name "GPIO18/PWM0")
					(number "12")
				)
				(pin bidirectional line
					(at -20.32 5.08 0)
					(length 2.54)
					(name "GPIO19/MISO1")
					(number "35")
				)
				(pin bidirectional line
					(at -20.32 2.54 0)
					(length 2.54)
					(name "GPIO20/MOSI1")
					(number "38")
				)
				(pin bidirectional line
					(at -20.32 0 0)
					(length 2.54)
					(name "GPIO21/SCLK1")
					(number "40")
				)
				(pin bidirectional line
					(at -20.32 -5.08 0)
					(length 2.54)
					(name "GPIO22")
					(number "15")
				)
				(pin bidirectional line
					(at -20.32 -7.62 0)
					(length 2.54)
					(name "GPIO23")
					(number "16")
				)
				(pin bidirectional line
					(at -20.32 -10.16 0)
					(length 2.54)
					(name "GPIO24")
					(number "18")
				)
				(pin bidirectional line
					(at -20.32 -12.7 0)
					(length 2.54)
					(name "GPIO25")
					(number "22")
				)
				(pin bidirectional line
					(at -20.32 -15.24 0)
					(length 2.54)
					(name "GPIO26")
					(number "37")
				)
				(pin bidirectional line
					(at -20.32 -17.78 0)
					(length 2.54)
					(name "GPIO27")
					(number "13")
				)
				(pin power_in line
					(at -10.16 -33.02 90)
					(length 2.54)
					(name "GND")
					(number "6")
				)
				(pin power_in line
					(at -7.62 -33.02 90)
					(length 2.54)
					(name "GND")
					(number "9")
				)
				(pin power_in line
					(at -5.08 33.02 270)
					(length 2.54)
					(name "5V")
					(number "2")
				)
				(pin power_in line
					(at -5.08 -33.02 90)
					(length 2.54)
					(name "GND")
					(number "14")
				)
				(pin power_in line
					(at -2.54 33.02 270)
					(length 2.54)
					(name "5V")
					(number "4")
				)
				(pin power_in line
					(at -2.54 -33.02 90)
					(length 2.54)
					(name "GND")
					(number "20")
				)
				(pin power_in line
					(at 0 -33.02 90)
					(length 2.54)
					(name "GND")
					(number "25")
				)
				(pin power_in line
					(at 2.54 33.02 270)
					(length 2.54)
					(name "3V3")
					(number "1")
				)
				(pin power_in line
					(at 2.54 -33.02 90)
					(length 2.54)
					(name "GND")
					(number "30")
				)
				(pin power_in line
					(at 5.08 33.02 270)
					(length 2.54)
					(name "3V3")
					(number "17")
				)
				(pin power_in line
					(at 5.08 -33.02 90)
					(length 2.54)
					(name "GND")
					(number "34")
				)
				(pin power_in line
					(at 7.62 -33.02 90)
					(length 2.54)
					(name "GND")
					(number "39")
				)
				(pin bidirectional line
					(at 20.32 22.86 180)
					(length 2.54)
					(name "ID_SD/GPIO0")
					(number "27")
				)
				(pin bidirectional line
					(at 20.32 20.32 180)
					(length 2.54)
					(name "ID_SC/GPIO1")
					(number "28")
				)
				(pin bidirectional line
					(at 20.32 15.24 180)
					(length 2.54)
					(name "SDA/GPIO2")
					(number "3")
				)
				(pin bidirectional line
					(at 20.32 12.7 180)
					(length 2.54)
					(name "SCL/GPIO3")
					(number "5")
				)
				(pin bidirectional line
					(at 20.32 7.62 180)
					(length 2.54)
					(name "GCLK0/GPIO4")
					(number "7")
				)
				(pin bidirectional line
					(at 20.32 5.08 180)
					(length 2.54)
					(name "GCLK1/GPIO5")
					(number "29")
				)
				(pin bidirectional line
					(at 20.32 2.54 180)
					(length 2.54)
					(name "GCLK2/GPIO6")
					(number "31")
				)
				(pin bidirectional line
					(at 20.32 -2.54 180)
					(length 2.54)
					(name "~{CE1}/GPIO7")
					(number "26")
				)
				(pin bidirectional line
					(at 20.32 -5.08 180)
					(length 2.54)
					(name "~{CE0}/GPIO8")
					(number "24")
				)
				(pin bidirectional line
					(at 20.32 -7.62 180)
					(length 2.54)
					(name "MISO0/GPIO9")
					(number "21")
				)
				(pin bidirectional line
					(at 20.32 -10.16 180)
					(length 2.54)
					(name "MOSI0/GPIO10")
					(number "19")
				)
				(pin bidirectional line
					(at 20.32 -12.7 180)
					(length 2.54)
					(name "SCLK0/GPIO11")
					(number "23")
				)
				(pin bidirectional line
					(at 20.32 -17.78 180)
					(length 2.54)
					(name "PWM0/GPIO12")
					(number "32")
				)
				(pin bidirectional line
					(at 20.32 -20.32 180)
					(length 2.54)
					(name "PWM1/GPIO13")
					(number "33")
				)
			)
			(embedded_fonts no)
		)
		(symbol "radiateur-rescue:VCC-power"
			(power)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -3.81 0)
			)
			(property "Value" "power_VCC"
				(at 0 3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(symbol "VCC-power_0_1"
				(polyline
					(pts
						(xy -0.762 1.27) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "VCC-power_1_1"
				(pin power_in line
					(at 0 0 90)
					(length 0)
					(hide yes)
					(name "VCC")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
	)
	(junction
		(at 36.83 57.15)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 143.51 147.32)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 88.9 76.2)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 106.68 60.96)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 138.43 153.67)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 140.97 147.32)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 148.59 147.32)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 36.83 71.12)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 148.59 72.39)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 151.13 147.32)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 186.69 153.67)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 173.99 104.14)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 45.72 49.53)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 186.69 91.44)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 186.69 152.4)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 138.43 147.32)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 146.05 147.32)
		(diameter 0)
		(color 0 0 0 0)
	)
	(no_connect
		(at 166.37 88.9)
	)
	(no_connect
		(at 125.73 106.68)
	)
	(no_connect
		(at 166.37 91.44)
	)
	(no_connect
		(at 125.73 129.54)
	)
	(no_connect
		(at 166.37 109.22)
	)
	(no_connect
		(at 166.37 124.46)
	)
	(no_connect
		(at 166.37 106.68)
	)
	(no_connect
		(at 125.73 88.9)
	)
	(no_connect
		(at 166.37 99.06)
	)
	(no_connect
		(at 125.73 111.76)
	)
	(no_connect
		(at 125.73 124.46)
	)
	(no_connect
		(at 151.13 78.74)
	)
	(no_connect
		(at 125.73 91.44)
	)
	(no_connect
		(at 71.12 76.2)
	)
	(no_connect
		(at 166.37 132.08)
	)
	(no_connect
		(at 125.73 127)
	)
	(no_connect
		(at 140.97 78.74)
	)
	(no_connect
		(at 166.37 114.3)
	)
	(no_connect
		(at 166.37 129.54)
	)
	(no_connect
		(at 166.37 96.52)
	)
	(no_connect
		(at 125.73 109.22)
	)
	(no_connect
		(at 166.37 116.84)
	)
	(no_connect
		(at 125.73 101.6)
	)
	(wire
		(pts
			(xy 40.64 25.4) (xy 40.64 49.53)
		)
	)
	(wire
		(pts
			(xy 99.06 40.64) (xy 95.25 40.64)
		)
	)
	(wire
		(pts
			(xy 138.43 153.67) (xy 138.43 147.32)
		)
	)
	(wire
		(pts
			(xy 140.97 147.32) (xy 140.97 144.78)
		)
	)
	(wire
		(pts
			(xy 33.02 81.28) (xy 33.02 78.74)
		)
	)
	(wire
		(pts
			(xy 148.59 147.32) (xy 151.13 147.32)
		)
	)
	(wire
		(pts
			(xy 121.92 97.79) (xy 121.92 99.06)
		)
	)
	(wire
		(pts
			(xy 95.25 38.1) (xy 99.06 38.1)
		)
	)
	(wire
		(pts
			(xy 120.65 119.38) (xy 125.73 119.38)
		)
	)
	(wire
		(pts
			(xy 125.73 116.84) (xy 119.38 116.84)
		)
	)
	(wire
		(pts
			(xy 119.38 116.84) (xy 119.38 123.19)
		)
	)
	(wire
		(pts
			(xy 99.06 44.45) (xy 99.06 40.64)
		)
	)
	(wire
		(pts
			(xy 88.9 76.2) (xy 106.68 76.2)
		)
	)
	(wire
		(pts
			(xy 119.38 123.19) (xy 118.11 123.19)
		)
	)
	(wire
		(pts
			(xy 173.99 91.44) (xy 173.99 104.14)
		)
	)
	(wire
		(pts
			(xy 135.89 147.32) (xy 138.43 147.32)
		)
	)
	(wire
		(pts
			(xy 60.96 22.86) (xy 68.58 22.86)
		)
	)
	(wire
		(pts
			(xy 120.65 96.52) (xy 125.73 96.52)
		)
	)
	(wire
		(pts
			(xy 153.67 147.32) (xy 153.67 144.78)
		)
	)
	(wire
		(pts
			(xy 186.69 91.44) (xy 186.69 72.39)
		)
	)
	(wire
		(pts
			(xy 181.61 91.44) (xy 186.69 91.44)
		)
	)
	(wire
		(pts
			(xy 36.83 73.66) (xy 36.83 71.12)
		)
	)
	(wire
		(pts
			(xy 203.2 152.4) (xy 186.69 152.4)
		)
	)
	(wire
		(pts
			(xy 118.11 133.35) (xy 121.92 133.35)
		)
	)
	(wire
		(pts
			(xy 148.59 147.32) (xy 148.59 144.78)
		)
	)
	(wire
		(pts
			(xy 36.83 27.94) (xy 34.29 27.94)
		)
	)
	(wire
		(pts
			(xy 138.43 147.32) (xy 140.97 147.32)
		)
	)
	(wire
		(pts
			(xy 121.92 133.35) (xy 121.92 121.92)
		)
	)
	(wire
		(pts
			(xy 120.65 52.07) (xy 144.78 52.07)
		)
	)
	(wire
		(pts
			(xy 48.26 57.15) (xy 36.83 57.15)
		)
	)
	(wire
		(pts
			(xy 186.69 153.67) (xy 138.43 153.67)
		)
	)
	(wire
		(pts
			(xy 88.9 76.2) (xy 88.9 88.9)
		)
	)
	(wire
		(pts
			(xy 148.59 72.39) (xy 186.69 72.39)
		)
	)
	(wire
		(pts
			(xy 203.2 152.4) (xy 203.2 124.46)
		)
	)
	(wire
		(pts
			(xy 143.51 147.32) (xy 143.51 144.78)
		)
	)
	(wire
		(pts
			(xy 36.83 71.12) (xy 49.53 71.12)
		)
	)
	(wire
		(pts
			(xy 151.13 147.32) (xy 151.13 144.78)
		)
	)
	(wire
		(pts
			(xy 33.02 73.66) (xy 36.83 73.66)
		)
	)
	(wire
		(pts
			(xy 143.51 147.32) (xy 146.05 147.32)
		)
	)
	(wire
		(pts
			(xy 118.11 128.27) (xy 120.65 128.27)
		)
	)
	(wire
		(pts
			(xy 106.68 57.15) (xy 106.68 60.96)
		)
	)
	(wire
		(pts
			(xy 60.96 17.78) (xy 68.58 17.78)
		)
	)
	(wire
		(pts
			(xy 153.67 68.58) (xy 148.59 68.58)
		)
	)
	(wire
		(pts
			(xy 142.24 78.74) (xy 143.51 78.74)
		)
	)
	(wire
		(pts
			(xy 36.83 57.15) (xy 36.83 71.12)
		)
	)
	(wire
		(pts
			(xy 66.04 76.2) (xy 66.04 81.28)
		)
	)
	(wire
		(pts
			(xy 175.26 38.1) (xy 167.64 38.1)
		)
	)
	(wire
		(pts
			(xy 109.22 97.79) (xy 96.52 97.79)
		)
	)
	(wire
		(pts
			(xy 151.13 147.32) (xy 153.67 147.32)
		)
	)
	(wire
		(pts
			(xy 78.74 60.96) (xy 106.68 60.96)
		)
	)
	(wire
		(pts
			(xy 152.4 52.07) (xy 160.02 52.07)
		)
	)
	(wire
		(pts
			(xy 142.24 71.12) (xy 142.24 78.74)
		)
	)
	(wire
		(pts
			(xy 167.64 57.15) (xy 167.64 62.23)
		)
	)
	(wire
		(pts
			(xy 116.84 97.79) (xy 121.92 97.79)
		)
	)
	(wire
		(pts
			(xy 99.06 38.1) (xy 99.06 35.56)
		)
	)
	(wire
		(pts
			(xy 166.37 121.92) (xy 214.63 121.92)
		)
	)
	(wire
		(pts
			(xy 186.69 96.52) (xy 186.69 91.44)
		)
	)
	(wire
		(pts
			(xy 167.64 46.99) (xy 167.64 40.64)
		)
	)
	(wire
		(pts
			(xy 214.63 119.38) (xy 166.37 119.38)
		)
	)
	(wire
		(pts
			(xy 140.97 147.32) (xy 143.51 147.32)
		)
	)
	(wire
		(pts
			(xy 203.2 124.46) (xy 214.63 124.46)
		)
	)
	(wire
		(pts
			(xy 167.64 38.1) (xy 167.64 35.56)
		)
	)
	(wire
		(pts
			(xy 107.95 123.19) (xy 110.49 123.19)
		)
	)
	(wire
		(pts
			(xy 186.69 152.4) (xy 186.69 153.67)
		)
	)
	(wire
		(pts
			(xy 107.95 133.35) (xy 110.49 133.35)
		)
	)
	(wire
		(pts
			(xy 146.05 147.32) (xy 146.05 144.78)
		)
	)
	(wire
		(pts
			(xy 106.68 76.2) (xy 106.68 72.39)
		)
	)
	(wire
		(pts
			(xy 106.68 60.96) (xy 106.68 64.77)
		)
	)
	(wire
		(pts
			(xy 107.95 128.27) (xy 110.49 128.27)
		)
	)
	(wire
		(pts
			(xy 160.02 35.56) (xy 167.64 35.56)
		)
	)
	(wire
		(pts
			(xy 146.05 147.32) (xy 148.59 147.32)
		)
	)
	(wire
		(pts
			(xy 68.58 53.34) (xy 68.58 60.96)
		)
	)
	(wire
		(pts
			(xy 45.72 49.53) (xy 45.72 53.34)
		)
	)
	(wire
		(pts
			(xy 88.9 106.68) (xy 88.9 110.49)
		)
	)
	(wire
		(pts
			(xy 40.64 49.53) (xy 45.72 49.53)
		)
	)
	(wire
		(pts
			(xy 78.74 76.2) (xy 88.9 76.2)
		)
	)
	(wire
		(pts
			(xy 167.64 40.64) (xy 175.26 40.64)
		)
	)
	(wire
		(pts
			(xy 138.43 147.32) (xy 138.43 144.78)
		)
	)
	(wire
		(pts
			(xy 96.52 97.79) (xy 96.52 101.6)
		)
	)
	(wire
		(pts
			(xy 173.99 104.14) (xy 166.37 104.14)
		)
	)
	(wire
		(pts
			(xy 121.92 121.92) (xy 125.73 121.92)
		)
	)
	(wire
		(pts
			(xy 36.83 57.15) (xy 36.83 27.94)
		)
	)
	(wire
		(pts
			(xy 34.29 25.4) (xy 40.64 25.4)
		)
	)
	(wire
		(pts
			(xy 33.02 81.28) (xy 66.04 81.28)
		)
	)
	(wire
		(pts
			(xy 186.69 111.76) (xy 186.69 152.4)
		)
	)
	(wire
		(pts
			(xy 120.65 52.07) (xy 120.65 96.52)
		)
	)
	(wire
		(pts
			(xy 148.59 78.74) (xy 148.59 72.39)
		)
	)
	(wire
		(pts
			(xy 120.65 128.27) (xy 120.65 119.38)
		)
	)
	(wire
		(pts
			(xy 179.07 104.14) (xy 173.99 104.14)
		)
	)
	(wire
		(pts
			(xy 45.72 53.34) (xy 68.58 53.34)
		)
	)
	(wire
		(pts
			(xy 45.72 49.53) (xy 48.26 49.53)
		)
	)
	(wire
		(pts
			(xy 121.92 99.06) (xy 125.73 99.06)
		)
	)
	(wire
		(pts
			(xy 148.59 68.58) (xy 148.59 72.39)
		)
	)
	(wire
		(pts
			(xy 135.89 144.78) (xy 135.89 147.32)
		)
	)
	(label "Line1"
		(at 57.15 53.34 0)
	)
	(label "LineRadiateur"
		(at 44.45 81.28 0)
	)
	(label "NeutralOut"
		(at 39.37 71.12 0)
	)
	(label "Line1"
		(at 40.64 49.53 0)
	)
	(label "NeutralIn"
		(at 40.64 57.15 0)
	)
	(symbol
		(lib_id "radiateur-rescue:LINE-power")
		(at 48.26 49.53 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR03"
			(at 44.45 49.53 0)
		)
		(property "Value" "LINE"
			(at 51.5112 49.9618 90)
		)
		(property "Footprint" ""
			(at 48.26 49.53 0)
		)
		(property "Datasheet" ""
			(at 48.26 49.53 0)
		)
		(property "Description" ""
			(at 48.26 49.53 0)
		)
		(pin "1")
		(instances
			(project "Radiateur V2"
				(path
					(reference "#PWR03")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Relay:SANYOU_SRD_Form_C")
		(at 73.66 68.58 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "K1"
			(at 84.582 67.4116 0)
		)
		(property "Value" "5V Relais / coil 70"
			(at 84.582 69.723 0)
		)
		(property "Footprint" "Relay_THT:Relay_SPDT_SANYOU_SRD_Series_Form_C"
			(at 62.23 67.31 0)
		)
		(property "Datasheet" "http://www.sanyourelay.ca/public/products/pdf/SRD.pdf"
			(at 73.66 68.58 0)
		)
		(property "Description" "Sanyo SRD relay, Single Pole Miniature Power Relay,"
			(at 73.66 68.58 0)
		)
		(pin "2")
		(pin "3")
		(pin "5")
		(pin "4")
		(pin "1")
		(instances
			(project "Radiateur V2"
				(path
					(reference "K1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "radiateur-rescue:NEUT-power")
		(at 48.26 57.15 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR04"
			(at 44.45 57.15 0)
		)
		(property "Value" "NEUT"
			(at 51.5112 57.5818 90)
		)
		(property "Footprint" ""
			(at 48.26 57.15 0)
		)
		(property "Datasheet" ""
			(at 48.26 57.15 0)
		)
		(property "Description" ""
			(at 48.26 57.15 0)
		)
		(pin "1")
		(instances
			(project "Radiateur V2"
				(path
					(reference "#PWR04")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "radiateur-rescue:NEUT-power")
		(at 49.53 71.12 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR05"
			(at 45.72 71.12 0)
		)
		(property "Value" "NEUT"
			(at 52.7812 71.5518 90)
		)
		(property "Footprint" ""
			(at 49.53 71.12 0)
		)
		(property "Datasheet" ""
			(at 49.53 71.12 0)
		)
		(property "Description" ""
			(at 49.53 71.12 0)
		)
		(pin "1")
		(instances
			(project "Radiateur V2"
				(path
					(reference "#PWR05")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "radiateur-rescue:Raspberry_Pi_2_3-Connector")
		(at 146.05 111.76 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J5"
			(at 146.05 74.1426 0)
		)
		(property "Value" "ZeroHeader"
			(at 146.05 76.454 0)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x20_P2.54mm_Vertical"
			(at 146.05 111.76 0)
		)
		(property "Datasheet" "https://www.raspberrypi.org/documentation/hardware/raspberrypi/schematics/rpi_SCH_3bplus_1p0_reduced.pdf"
			(at 146.05 111.76 0)
		)
		(property "Description" ""
			(at 146.05 111.76 0)
		)
		(pin "18")
		(pin "4")
		(pin "36")
		(pin "40")
		(pin "10")
		(pin "38")
		(pin "11")
		(pin "35")
		(pin "15")
		(pin "16")
		(pin "37")
		(pin "22")
		(pin "12")
		(pin "13")
		(pin "8")
		(pin "6")
		(pin "9")
		(pin "2")
		(pin "14")
		(pin "20")
		(pin "25")
		(pin "1")
		(pin "30")
		(pin "17")
		(pin "34")
		(pin "39")
		(pin "27")
		(pin "28")
		(pin "7")
		(pin "23")
		(pin "29")
		(pin "3")
		(pin "21")
		(pin "24")
		(pin "32")
		(pin "5")
		(pin "33")
		(pin "31")
		(pin "19")
		(pin "26")
		(instances
			(project "Radiateur V2"
				(path
					(reference "J5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "radiateur-rescue:VCC-power")
		(at 142.24 71.12 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR011"
			(at 142.24 74.93 0)
		)
		(property "Value" "VCC"
			(at 142.6718 66.7258 0)
		)
		(property "Footprint" ""
			(at 142.24 71.12 0)
		)
		(property "Datasheet" ""
			(at 142.24 71.12 0)
		)
		(property "Description" ""
			(at 142.24 71.12 0)
		)
		(pin "1")
		(instances
			(project "Radiateur V2"
				(path
					(reference "#PWR011")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "radiateur-rescue:DS18B20-Sensor_Temperature")
		(at 186.69 104.14 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "U2"
			(at 192.532 102.9716 0)
		)
		(property "Value" "DS18B20"
			(at 192.532 105.283 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 212.09 110.49 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/DS18B20.pdf"
			(at 190.5 97.79 0)
		)
		(property "Description" ""
			(at 186.69 104.14 0)
		)
		(pin "1")
		(pin "3")
		(pin "2")
		(instances
			(project "Radiateur V2"
				(path
					(reference "U2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "radiateur-rescue:GND-power")
		(at 186.69 153.67 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR012"
			(at 186.69 160.02 0)
		)
		(property "Value" "GND"
			(at 186.817 158.0642 0)
		)
		(property "Footprint" ""
			(at 186.69 153.67 0)
		)
		(property "Datasheet" ""
			(at 186.69 153.67 0)
		)
		(property "Description" ""
			(at 186.69 153.67 0)
		)
		(pin "1")
		(instances
			(project "Radiateur V2"
				(path
					(reference "#PWR012")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Diode:1N4448")
		(at 106.68 68.58 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "D3"
			(at 108.6866 67.4116 90)
		)
		(property "Value" "1N4448"
			(at 108.6866 69.723 90)
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
			(at 102.235 68.58 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/1N4148_1N4448.pdf"
			(at 106.68 68.58 0)
		)
		(property "Description" "100V 0.15A High-speed standard diode, DO-35"
			(at 106.68 68.58 0)
		)
		(property "Sim.Device" "D"
			(at 106.68 68.58 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 106.68 68.58 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Radiateur V2"
				(path
					(reference "D3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "radiateur-rescue:VCC-power")
		(at 106.68 57.15 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR08"
			(at 106.68 60.96 0)
		)
		(property "Value" "VCC"
			(at 107.1118 52.7558 0)
		)
		(property "Footprint" ""
			(at 106.68 57.15 0)
		)
		(property "Datasheet" ""
			(at 106.68 57.15 0)
		)
		(property "Description" ""
			(at 106.68 57.15 0)
		)
		(pin "1")
		(instances
			(project "Radiateur V2"
				(path
					(reference "#PWR08")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 113.03 97.79 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R2"
			(at 113.03 92.5322 90)
		)
		(property "Value" "3.3K"
			(at 113.03 94.8436 90)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 113.03 96.012 90)
		)
		(property "Datasheet" "~"
			(at 113.03 97.79 0)
		)
		(property "Description" "Resistor"
			(at 113.03 97.79 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Radiateur V2"
				(path
					(reference "R2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Transistor_BJT:S8050")
		(at 91.44 101.6 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "Q1"
			(at 86.5886 100.4316 0)
		)
		(property "Value" "2N2222"
			(at 86.5886 102.743 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 86.36 103.505 0)
		)
		(property "Datasheet" "http://www.unisonic.com.tw/datasheet/S8050.pdf"
			(at 91.44 101.6 0)
		)
		(property "Description" "0.7A Ic, 20V Vce, Low Voltage High Current NPN Transistor, TO-92"
			(at 91.44 101.6 0)
		)
		(pin "3")
		(pin "2")
		(pin "1")
		(instances
			(project "Radiateur V2"
				(path
					(reference "Q1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "radiateur-rescue:GND-power")
		(at 88.9 110.49 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR06"
			(at 88.9 116.84 0)
		)
		(property "Value" "GND"
			(at 89.027 114.8842 0)
		)
		(property "Footprint" ""
			(at 88.9 110.49 0)
		)
		(property "Datasheet" ""
			(at 88.9 110.49 0)
		)
		(property "Description" ""
			(at 88.9 110.49 0)
		)
		(pin "1")
		(instances
			(project "Radiateur V2"
				(path
					(reference "#PWR06")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "radiateur-rescue:LED_RGBC-Device")
		(at 102.87 128.27 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "D2"
			(at 102.87 115.6462 0)
		)
		(property "Value" "LED_RGBC"
			(at 102.87 117.9576 0)
		)
		(property "Footprint" "LED_THT:LED_D5.0mm-4_RGB_Wide_Pins"
			(at 102.87 129.54 0)
		)
		(property "Datasheet" "~"
			(at 102.87 129.54 0)
		)
		(property "Description" ""
			(at 102.87 128.27 0)
		)
		(pin "1")
		(pin "4")
		(pin "2")
		(pin "3")
		(instances
			(project "Radiateur V2"
				(path
					(reference "D2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "radiateur-rescue:GND-power")
		(at 97.79 128.27 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR07"
			(at 91.44 128.27 0)
		)
		(property "Value" "GND"
			(at 94.5388 128.397 90)
		)
		(property "Footprint" ""
			(at 97.79 128.27 0)
		)
		(property "Datasheet" ""
			(at 97.79 128.27 0)
		)
		(property "Description" ""
			(at 97.79 128.27 0)
		)
		(pin "1")
		(instances
			(project "Radiateur V2"
				(path
					(reference "#PWR07")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 114.3 123.19 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R3"
			(at 114.3 117.9322 90)
		)
		(property "Value" "1K"
			(at 114.3 120.2436 90)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 114.3 121.412 90)
		)
		(property "Datasheet" "~"
			(at 114.3 123.19 0)
		)
		(property "Description" "Resistor"
			(at 114.3 123.19 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Radiateur V2"
				(path
					(reference "R3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 114.3 128.27 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R4"
			(at 114.3 123.0122 90)
		)
		(property "Value" "1K"
			(at 114.3 125.3236 90)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 114.3 126.492 90)
		)
		(property "Datasheet" "~"
			(at 114.3 128.27 0)
		)
		(property "Description" "Resistor"
			(at 114.3 128.27 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Radiateur V2"
				(path
					(reference "R4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 114.3 133.35 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R5"
			(at 114.3 128.0922 90)
		)
		(property "Value" "1K"
			(at 114.3 130.4036 90)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 114.3 131.572 90)
		)
		(property "Datasheet" "~"
			(at 114.3 133.35 0)
		)
		(property "Description" "Resistor"
			(at 114.3 133.35 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Radiateur V2"
				(path
					(reference "R5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 88.9 92.71 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R1"
			(at 94.1578 92.71 90)
		)
		(property "Value" "27"
			(at 91.8464 92.71 90)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 90.678 92.71 90)
		)
		(property "Datasheet" "~"
			(at 88.9 92.71 0)
		)
		(property "Description" "Resistor"
			(at 88.9 92.71 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Radiateur V2"
				(path
					(reference "R1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 177.8 91.44 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R6"
			(at 177.8 86.1822 90)
		)
		(property "Value" "4.7K"
			(at 177.8 88.4936 90)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 177.8 89.662 90)
		)
		(property "Datasheet" "~"
			(at 177.8 91.44 0)
		)
		(property "Description" "Resistor"
			(at 177.8 91.44 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Radiateur V2"
				(path
					(reference "R6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "radiateur-rescue:PWR_FLAG-power")
		(at 153.67 68.58 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#FLG0102"
			(at 153.67 66.675 0)
		)
		(property "Value" "PWR_FLAG"
			(at 153.67 64.1858 0)
		)
		(property "Footprint" ""
			(at 153.67 68.58 0)
		)
		(property "Datasheet" "~"
			(at 153.67 68.58 0)
		)
		(property "Description" ""
			(at 153.67 68.58 0)
		)
		(pin "1")
		(instances
			(project "Radiateur V2"
				(path
					(reference "#FLG0102")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector_Generic:Conn_01x04")
		(at 219.71 124.46 0)
		(mirror x)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J6"
			(at 217.6272 113.665 0)
		)
		(property "Value" "VCC/GND/10/9"
			(at 217.6272 115.9764 0)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
			(at 219.71 124.46 0)
		)
		(property "Datasheet" "~"
			(at 219.71 124.46 0)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 219.71 124.46 0)
		)
		(pin "4")
		(pin "2")
		(pin "1")
		(pin "3")
		(instances
			(project "Radiateur V2"
				(path
					(reference "J6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "radiateur-rescue:PWR_FLAG-power")
		(at 138.43 153.67 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#FLG0103"
			(at 138.43 155.575 0)
		)
		(property "Value" "PWR_FLAG"
			(at 138.43 158.0642 0)
		)
		(property "Footprint" ""
			(at 138.43 153.67 0)
		)
		(property "Datasheet" "~"
			(at 138.43 153.67 0)
		)
		(property "Description" ""
			(at 138.43 153.67 0)
		)
		(pin "1")
		(instances
			(project "Radiateur V2"
				(path
					(reference "#FLG0103")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "radiateur-rescue:VCC-power")
		(at 214.63 127 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR0102"
			(at 214.63 123.19 0)
		)
		(property "Value" "VCC"
			(at 214.1982 131.3942 0)
		)
		(property "Footprint" ""
			(at 214.63 127 0)
		)
		(property "Datasheet" ""
			(at 214.63 127 0)
		)
		(property "Description" ""
			(at 214.63 127 0)
		)
		(pin "1")
		(instances
			(project "Radiateur V2"
				(path
					(reference "#PWR0102")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x02_Pin")
		(at 180.34 40.64 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J9"
			(at 179.705 45.72 0)
		)
		(property "Value" "FAN"
			(at 179.705 43.18 0)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
			(at 180.34 40.64 0)
		)
		(property "Datasheet" "~"
			(at 180.34 40.64 0)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 180.34 40.64 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Radiateur V2"
				(path
					(reference "J9")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x03_Pin")
		(at 73.66 20.32 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J2"
			(at 74.93 19.0499 0)
		)
		(property "Value" "ToTransfo"
			(at 74.93 21.5899 0)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
			(at 73.66 20.32 0)
		)
		(property "Datasheet" "~"
			(at 73.66 20.32 0)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 73.66 20.32 0)
		)
		(pin "1")
		(pin "3")
		(pin "2")
		(instances
			(project "Radiateur V2"
				(path
					(reference "J2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Transistor_BJT:PN2222A")
		(at 165.1 52.07 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "Q2"
			(at 170.18 50.7999 0)
		)
		(property "Value" "PN2222A"
			(at 170.18 53.3399 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 170.18 53.975 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/PN2222-D.PDF"
			(at 165.1 52.07 0)
		)
		(property "Description" "1A Ic, 40V Vce, NPN Transistor, General Purpose Transistor, TO-92"
			(at 165.1 52.07 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(instances
			(project "Radiateur V2"
				(path
					(reference "Q2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x02_Pin")
		(at 29.21 25.4 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J7"
			(at 29.845 20.32 0)
		)
		(property "Value" "230V IN"
			(at 29.845 22.86 0)
		)
		(property "Footprint" "Connector_Phoenix_MC_HighVoltage:PhoenixContact_MCV_1,5_2-G-5.08_1x02_P5.08mm_Vertical"
			(at 29.21 25.4 0)
		)
		(property "Datasheet" "~"
			(at 29.21 25.4 0)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 29.21 25.4 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Radiateur V2"
				(path
					(reference "J7")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x02_Pin")
		(at 90.17 38.1 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J8"
			(at 90.805 33.02 0)
		)
		(property "Value" "5V IN"
			(at 90.805 35.56 0)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
			(at 90.17 38.1 0)
		)
		(property "Datasheet" "~"
			(at 90.17 38.1 0)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 90.17 38.1 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Radiateur V2"
				(path
					(reference "J8")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x03_Pin")
		(at 27.94 76.2 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J1"
			(at 28.575 68.58 0)
		)
		(property "Value" "Radiateur Out"
			(at 28.575 71.12 0)
		)
		(property "Footprint" "Connector_Phoenix_MC_HighVoltage:PhoenixContact_MCV_1,5_3-G-5.08_1x03_P5.08mm_Vertical"
			(at 27.94 76.2 0)
		)
		(property "Datasheet" "~"
			(at 27.94 76.2 0)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 27.94 76.2 0)
		)
		(pin "2")
		(pin "3")
		(pin "1")
		(instances
			(project "Radiateur V2"
				(path
					(reference "J1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "radiateur-rescue:VCC-power")
		(at 99.06 35.56 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR013"
			(at 99.06 39.37 0)
		)
		(property "Value" "VCC"
			(at 99.4918 31.1658 0)
		)
		(property "Footprint" ""
			(at 99.06 35.56 0)
		)
		(property "Datasheet" ""
			(at 99.06 35.56 0)
		)
		(property "Description" ""
			(at 99.06 35.56 0)
		)
		(pin "1")
		(instances
			(project "Radiateur V2"
				(path
					(reference "#PWR013")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "radiateur-rescue:LINE-power")
		(at 60.96 17.78 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR01"
			(at 64.77 17.78 0)
		)
		(property "Value" "LINE"
			(at 57.7088 17.3228 90)
		)
		(property "Footprint" ""
			(at 60.96 17.78 0)
		)
		(property "Datasheet" ""
			(at 60.96 17.78 0)
		)
		(property "Description" ""
			(at 60.96 17.78 0)
		)
		(pin "1")
		(instances
			(project "Radiateur V2"
				(path
					(reference "#PWR01")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "radiateur-rescue:GND-power")
		(at 99.06 44.45 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR09"
			(at 99.06 50.8 0)
		)
		(property "Value" "GND"
			(at 99.187 48.8442 0)
		)
		(property "Footprint" ""
			(at 99.06 44.45 0)
		)
		(property "Datasheet" ""
			(at 99.06 44.45 0)
		)
		(property "Description" ""
			(at 99.06 44.45 0)
		)
		(pin "1")
		(instances
			(project "Radiateur V2"
				(path
					(reference "#PWR09")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "radiateur-rescue:GND-power")
		(at 167.64 62.23 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR010"
			(at 167.64 68.58 0)
		)
		(property "Value" "GND"
			(at 167.767 66.6242 0)
		)
		(property "Footprint" ""
			(at 167.64 62.23 0)
		)
		(property "Datasheet" ""
			(at 167.64 62.23 0)
		)
		(property "Description" ""
			(at 167.64 62.23 0)
		)
		(pin "1")
		(instances
			(project "Radiateur V2"
				(path
					(reference "#PWR010")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "radiateur-rescue:NEUT-power")
		(at 60.96 22.86 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR02"
			(at 64.77 22.86 0)
		)
		(property "Value" "NEUT"
			(at 57.7088 22.4028 90)
		)
		(property "Footprint" ""
			(at 60.96 22.86 0)
		)
		(property "Datasheet" ""
			(at 60.96 22.86 0)
		)
		(property "Description" ""
			(at 60.96 22.86 0)
		)
		(pin "1")
		(instances
			(project "Radiateur V2"
				(path
					(reference "#PWR02")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 148.59 52.07 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R7"
			(at 148.59 45.72 90)
		)
		(property "Value" "1K"
			(at 148.59 48.26 90)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 148.59 53.848 90)
		)
		(property "Datasheet" "~"
			(at 148.59 52.07 0)
		)
		(property "Description" "Resistor"
			(at 148.59 52.07 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Radiateur V2"
				(path
					(reference "R7")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "radiateur-rescue:VCC-power")
		(at 160.02 35.56 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR014"
			(at 163.83 35.56 0)
		)
		(property "Value" "VCC"
			(at 155.6258 35.1282 0)
		)
		(property "Footprint" ""
			(at 160.02 35.56 0)
		)
		(property "Datasheet" ""
			(at 160.02 35.56 0)
		)
		(property "Description" ""
			(at 160.02 35.56 0)
		)
		(pin "1")
		(instances
			(project "Radiateur V2"
				(path
					(reference "#PWR014")
					(unit 1)
				)
			)
		)
	)
	(sheet_instances
		(path
			(page "1")
		)
	)
	(embedded_fonts no)
)
