(module Relay_SPDT_Finder_36.11 (layer F.Cu) (tedit 5D3F5A07)
  (descr "FINDER 36.11, SPDT relay, 10A, https://gfinder.findernet.com/public/attachments/36/EN/S36EN.pdf")
  (tags "spdt relay")
  (fp_text reference REF** (at 8.1 9.2) (layer F.SilkS))
  (fp_text value Relay_SPDT_Finder_36.11 (at 8 -9.6) (layer F.Fab))
  (fp_text user %R (at 7.1 0.025) (layer F.Fab))
  (pad A1 thru_hole circle (at 2 6) (size 3 3) (drill 1.3) (layers *.Cu *.Mask))
  (pad 14 thru_hole circle (at 14.2 6) (size 3 3) (drill 1.3) (layers *.Cu *.Mask))
  (pad 12 thru_hole circle (at 14.2 -6) (size 3 3) (drill 1.3) (layers *.Cu *.Mask))
  (pad A2 thru_hole circle (at 2 -6) (size 3 3) (drill 1.3) (layers *.Cu *.Mask))
  (pad 11 thru_hole circle (at 0 0) (size 3 3) (drill 1.3) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Relay_THT.3dshapes/Relay_SPDT_Finder_36.11.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
