(footprint "BatteryHolder_Eagle_12BH611-GR"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "https://eu.mouser.com/datasheet/2/209/EPD-200766-1274481.pdf")
	(tags "9V Battery Holder")
	(property "Reference" "REF**"
		(at -24.13 -24.13 0)
		(layer "F.SilkS")
	)
	(property "Value" "BatteryHolder_Eagle_12BH611-GR"
		(at -24.13 11.43 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "-"
		(at -7 -12.7 0)
		(layer "F.Fab")
	)
	(fp_text user "+"
		(at -7 0 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -24.13 -6.35 180)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -38.9 -17.45)
		(size 2.6 2.6)
		(drill 2.6)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -24.15 4.75)
		(size 2.6 2.6)
		(drill 2.6)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -10.9 -17.45)
		(size 2.6 2.6)
		(drill 2.6)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 3 3)
		(drill 2.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 -12.7)
		(size 3 3)
		(drill 2.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Battery.3dshapes/BatteryHolder_Eagle_12BH611-GR.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
