(footprint "BatteryHolder_Keystone_1057_1x2032"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SMT (Auto-In/Ultra-Low) Holder for 2032 Cell, 33.2 x 23.9mm, 2mm height above PCB, https://www.keyelco.com/userAssets/file/M65p4.pdf")
	(tags "Keystone type 1057 coin cell holder CR2032")
	(property "Reference" "REF**"
		(at -14.1 -4.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "BatteryHolder_Keystone_1057_1x2032"
		(at 0 12.65 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_line
		(start -14.7 -2.08505)
		(end -14.7 -3.285)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -14.7 3.284899)
		(end -14.7 2.084949)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -14.3 -3.685)
		(end -12.244621 -3.685)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -14.3 1.684949)
		(end -13.5 1.684949)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -13.5 -1.68505)
		(end -14.3 -1.68505)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -13.5 1.684949)
		(end -13.5 -1.68505)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -12.244621 -3.685)
		(end -11.921437 -3.711285)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -12.244621 3.684999)
		(end -14.3 3.684899)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -11.921437 -3.711285)
		(end -11.606747 -3.789448)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -11.921437 3.711284)
		(end -12.244621 3.684999)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -11.606747 -3.789448)
		(end -11.308824 -3.917435)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -11.606747 3.789447)
		(end -11.921437 3.711284)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -11.308824 -3.917435)
		(end -11.035498 -4.091883)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -11.308824 3.917434)
		(end -11.606747 3.789447)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -11.035498 -4.091883)
		(end -10.793954 -4.308205)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -11.035498 4.091882)
		(end -11.308824 3.917434)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -10.793954 -4.308205)
		(end -10.59054 -4.560716)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -10.793954 4.308204)
		(end -11.035498 4.091882)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -10.59054 -4.560716)
		(end -10.430603 -4.842778)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -10.59054 4.560715)
		(end -10.793954 4.308204)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -10.430603 -4.842778)
		(end -9.510966 -6.464636)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -10.430603 4.842777)
		(end -10.59054 4.560715)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -9.510966 -6.464636)
		(end -8.341335 -7.916572)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -9.510966 6.464635)
		(end -10.430603 4.842777)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -8.341335 -7.916572)
		(end -6.952454 -9.160424)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -8.341335 7.916571)
		(end -9.510966 6.464635)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -6.952454 -9.160424)
		(end -5.38083 -10.163496)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -6.952454 9.160423)
		(end -8.341335 7.916571)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -5.38083 -10.163496)
		(end -3.667773 -10.899424)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -5.38083 10.163495)
		(end -6.952454 9.160423)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -3.667773 -10.899424)
		(end -1.858308 -11.348863)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -3.667773 10.899423)
		(end -5.38083 10.163495)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -1.858308 -11.348863)
		(end 0 -11.5)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -1.858308 11.348862)
		(end -3.667773 10.899423)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 0 -11.5)
		(end 1.858309 -11.348863)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 0 11.499999)
		(end -1.858308 11.348862)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 1.858309 -11.348863)
		(end 3.667774 -10.899424)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 1.858309 11.348862)
		(end 0 11.499999)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 3.667774 -10.899424)
		(end 5.380831 -10.163496)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 3.667774 10.899423)
		(end 1.858309 11.348862)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 5.380831 -10.163496)
		(end 6.952455 -9.160424)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 5.380831 10.163495)
		(end 3.667774 10.899423)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 6.952455 -9.160424)
		(end 8.341336 -7.916572)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 6.952455 9.160423)
		(end 5.380831 10.163495)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 8.341336 -7.916572)
		(end 9.510967 -6.464636)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 8.341336 7.916571)
		(end 6.952455 9.160423)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 9.510967 -6.464636)
		(end 10.430604 -4.842778)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 9.510967 6.464635)
		(end 8.341336 7.916571)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 10.430604 -4.842778)
		(end 10.590541 -4.560716)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 10.430604 4.842777)
		(end 9.510967 6.464635)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 10.590541 -4.560716)
		(end 10.793955 -4.308205)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 10.590541 4.560715)
		(end 10.430604 4.842777)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 10.793955 -4.308205)
		(end 11.035499 -4.091883)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 10.793955 4.308204)
		(end 10.590541 4.560715)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 11.035499 -4.091883)
		(end 11.308825 -3.917435)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 11.035499 4.091882)
		(end 10.793955 4.308204)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 11.308825 -3.917435)
		(end 11.606748 -3.789448)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 11.308825 3.917434)
		(end 11.035499 4.091882)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 11.606748 -3.789448)
		(end 11.921438 -3.711285)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 11.606748 3.789447)
		(end 11.308825 3.917434)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 11.921438 -3.711285)
		(end 12.244622 -3.685)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 11.921438 3.711284)
		(end 11.606748 3.789447)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 12.244622 -3.685)
		(end 14.3 -3.685)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 12.244622 3.684999)
		(end 11.921438 3.711284)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 13.5 -1.68505)
		(end 13.5 1.684949)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 13.5 1.684949)
		(end 14.3 1.68505)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 14.3 -1.68505)
		(end 13.5 -1.68505)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 14.3 3.682793)
		(end 12.244622 3.684999)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 14.7 -3.285)
		(end 14.7 -2.08505)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 14.7 2.082843)
		(end 14.7 3.282793)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -14.7 -3.285)
		(mid -14.582843 -3.567843)
		(end -14.3 -3.685)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -14.7 2.084949)
		(mid -14.582843 1.802106)
		(end -14.3 1.684949)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -14.3 -1.68505)
		(mid -14.582843 -1.802207)
		(end -14.7 -2.08505)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -14.3 3.684899)
		(mid -14.582843 3.567742)
		(end -14.7 3.284899)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 14.3 -3.685)
		(mid 14.582843 -3.567843)
		(end 14.7 -3.285)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 14.3 1.68505)
		(mid 14.582843 1.802207)
		(end 14.7 2.08505)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 14.7 -2.08505)
		(mid 14.582843 -1.802207)
		(end 14.3 -1.68505)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 14.7 3.282793)
		(mid 14.582843 3.565636)
		(end 14.3 3.682793)
		(layer "Edge.Cuts")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd custom
		(at -15.15 -0.1)
		(size 1 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.2 -1.65) (xy 0.271537 -1.594563) (xy 0.343074 -1.539127) (xy 0.500662 -1.450081) (xy 0.58506 -1.417404)
					(xy 0.669458 -1.384728) (xy 0.757691 -1.364583) (xy 0.845923 -1.344438) (xy 1.026357 -1.330056)
					(xy 1.235196 -1.330056) (xy 1.444035 -1.330057) (xy 1.444034 1.539942) (xy 1.044035 1.539967) (xy 0.86174 1.553331)
					(xy 0.683343 1.593137) (xy 0.512659 1.658535) (xy 0.353336 1.748125) (xy 0.28106 1.804058) (xy 0.208783 1.859992)
					(xy -1.65 1.859992) (xy -1.65 -1.650007)
				)
				(width 0.12)
				(fill yes)
			)
		)
	)
	(pad "2" smd custom
		(at 15.15 0.1 180)
		(size 1 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.2 -1.65) (xy 0.271537 -1.594563) (xy 0.343074 -1.539127) (xy 0.500662 -1.450081) (xy 0.58506 -1.417404)
					(xy 0.669458 -1.384728) (xy 0.757691 -1.364583) (xy 0.845923 -1.344438) (xy 1.026357 -1.330056)
					(xy 1.235196 -1.330056) (xy 1.444035 -1.330057) (xy 1.444034 1.539942) (xy 1.044035 1.539967) (xy 0.86174 1.553331)
					(xy 0.683343 1.593137) (xy 0.512659 1.658535) (xy 0.353336 1.748125) (xy 0.28106 1.804058) (xy 0.208783 1.859992)
					(xy -1.65 1.859992) (xy -1.65 -1.650007)
				)
				(width 0.12)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Battery.3dshapes/BatteryHolder_Keystone_1057_1x2032.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
