(footprint "BatteryHolder_Keystone_2460_1xAA"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "https://www.keyelco.com/product-pdf.cfm?p=1025")
	(tags "AA battery cell holder")
	(property "Reference" "REF**"
		(at -0.02 -9.42 180)
		(layer "F.SilkS")
	)
	(property "Value" "BatteryHolder_Keystone_2460_1xAA"
		(at 24.5 0 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "+"
		(at -3.4 -0.06 0)
		(layer "F.SilkS")
	)
	(fp_text user "-"
		(at 55.37 -0.06 0)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 0.01 -0.06 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 2.75 -5.995 90)
		(size 2.64 2.64)
		(drill 2.64)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 49.23 5.995)
		(size 2.64 2.64)
		(drill 2.64)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole rect
		(at 0 0 180)
		(size 2 2)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 51.99 0 180)
		(size 2 2)
		(drill 1.02)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Battery.3dshapes/BatteryHolder_Keystone_2460_1xAA.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
