(footprint "BatteryHolder_Keystone_2479_3xAAA"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Keystone Battery Holder, 2479, Battery Type 3xAAA (Script generated with StandardBox.py) (Keystone Battery Holder, 2479, Battery Type 3xAAA)")
	(tags "Keystone Battery Holder 2479 Battery Type 3xAAA")
	(property "Reference" "REF**"
		(at -0.09 -8.195 0)
		(layer "F.SilkS")
	)
	(property "Value" "BatteryHolder_Keystone_2479_3xAAA"
		(at 23.725 31.495 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "+"
		(at -4.5 0.05 0)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 23.725 11.75 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 23.72 0)
		(size 3.45 3.45)
		(drill 3.45)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 23.72 23.5)
		(size 3.45 3.45)
		(drill 3.45)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 3 3)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 12.7)
		(size 3 3)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Battery.3dshapes/BatteryHolder_Keystone_2479_3xAAA.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
