(footprint "BatteryHolder_Keystone_590"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "AA CR2 A battery holder with leaf spring, Keystone, https://ken.keyeuro.eu/cat/590.pdf")
	(tags "AA battery holder Keystone")
	(property "Reference" "REF**"
		(at 0 5.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "BatteryHolder_Keystone_590"
		(at 0 -8 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 0 -2 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole oval
		(at -4.445 -3.05 90)
		(size 1.9 1.4)
		(drill oval 1.3 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole oval
		(at 0 0)
		(size 1.9 1.4)
		(drill oval 1.3 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole oval
		(at 4.445 -3.05 90)
		(size 1.9 1.4)
		(drill oval 1.3 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KISYS3DMOD}/Battery.3dshapes/BatteryHolder_Keystone_590.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
