(footprint "BatteryHolder_Multicomp_BC-2001_1x2032"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "CR2032 retainer clip, SMT ( http://www.farnell.com/datasheets/1505853.pdf )")
	(tags "BC-2001 CR2032 2032 Battery Holder")
	(property "Reference" "REF**"
		(at 0 11.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "BatteryHolder_Multicomp_BC-2001_1x2032"
		(at 0 -10.6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0.33 4.89 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -12.95 0)
		(size 5 5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1" smd rect
		(at 12.95 0)
		(size 5 5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 0 0)
		(size 4 4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.Fab")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 0.969387 -28.403453) (xy 1.614245 -28.323602) (xy 2.252964 -28.204205) (xy 2.883122 -28.045714)
				(xy 3.502328 -27.848731) (xy 4.108232 -27.614002) (xy 4.698538 -27.342418) (xy 5.271004 -27.03501)
				(xy 5.823461 -26.692943) (xy 6.353812 -26.317516) (xy 6.860045 -25.910151) (xy 7.340241 -25.472395)
				(xy 7.792577 -25.005908) (xy 8.215338 -24.51246) (xy 8.60692 -23.993922) (xy 8.965837 -23.452261)
				(xy 9.290728 -22.889532) (xy 9.580362 -22.30787) (xy 9.833638 -21.709482) (xy 10.049597 -21.096636)
				(xy 10.227418 -20.471658) (xy 10.366428 -19.836918) (xy 10.466099 -19.194825) (xy 10.526054 -18.547814)
				(xy 10.546064 -17.898339) (xy 10.526054 -17.248864) (xy 10.466099 -16.601853) (xy 10.366428 -15.95976)
				(xy 10.227418 -15.32502) (xy 10.049597 -14.700042) (xy 9.833638 -14.087196) (xy 9.580362 -13.488808)
				(xy 9.290728 -12.907146) (xy 8.965837 -12.344417) (xy 8.60692 -11.802756) (xy 8.215338 -11.284218)
				(xy 7.792577 -10.79077) (xy 7.340241 -10.324283) (xy 6.860045 -9.886527) (xy 6.353812 -9.479162)
				(xy 5.823461 -9.103735) (xy 5.271004 -8.761668) (xy 4.698538 -8.45426) (xy 4.108232 -8.182676) (xy 3.502328 -7.947947)
				(xy 2.883122 -7.750964) (xy 2.252964 -7.592473) (xy 1.614245 -7.473076) (xy 0.969387 -7.393225)
				(xy 0.320837 -7.353224) (xy -0.328947 -7.353224) (xy -0.977497 -7.393225) (xy -1.622355 -7.473076)
				(xy -2.261074 -7.592473) (xy -2.891232 -7.750964) (xy -3.510438 -7.947947) (xy -4.116342 -8.182676)
				(xy -4.706648 -8.45426) (xy -5.279114 -8.761668) (xy -5.831571 -9.103735) (xy -6.361922 -9.479162)
				(xy -6.868155 -9.886527) (xy -7.348351 -10.324283) (xy -7.800687 -10.79077) (xy -8.223448 -11.284218)
				(xy -8.61503 -11.802756) (xy -8.973947 -12.344417) (xy -9.298838 -12.907146) (xy -9.588472 -13.488808)
				(xy -9.841748 -14.087196) (xy -10.057707 -14.700042) (xy -10.235528 -15.32502) (xy -10.374538 -15.95976)
				(xy -10.474209 -16.601853) (xy -10.534164 -17.248864) (xy -10.554174 -17.898339) (xy -10.534164 -18.547814)
				(xy -10.474209 -19.194825) (xy -10.374538 -19.836918) (xy -10.235528 -20.471658) (xy -10.057707 -21.096636)
				(xy -9.841748 -21.709482) (xy -9.588472 -22.30787) (xy -9.298838 -22.889532) (xy -8.973947 -23.452261)
				(xy -8.61503 -23.993922) (xy -8.223448 -24.51246) (xy -7.800687 -25.005908) (xy -7.348351 -25.472395)
				(xy -6.868155 -25.910151) (xy -6.361922 -26.317516) (xy -5.831571 -26.692943) (xy -5.279115 -27.03501)
				(xy -4.706648 -27.342418) (xy -4.116342 -27.614002) (xy -3.510438 -27.848731) (xy -2.891232 -28.045714)
				(xy -2.261074 -28.204205) (xy -1.622355 -28.323602) (xy -0.977497 -28.403453) (xy -0.328947 -28.443454)
				(xy 0.320837 -28.443454)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Battery.3dshapes/BatteryHolder_Multicomp_BC-2001_1x2032.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
