(footprint "BatteryHolder_Renata_SMTU2032-LF_1x2032"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "https://www.renata.com/fr/downloads/?product=smtu2032-lf&fileid=6a9833a4d49dfb7b550194fe0f")
	(tags "Renata SMT battery holder coin cell 2032")
	(property "Reference" "REF**"
		(at 0 -9 0)
		(layer "F.SilkS")
	)
	(property "Value" "BatteryHolder_Renata_SMTU2032-LF_1x2032"
		(at 0 11 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "+"
		(at -15.3 -2.785 0)
		(layer "F.SilkS")
	)
	(fp_text user "Adhesive fixation"
		(at 0 -3.6 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -14.7 0)
		(size 2.6 3.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.07692307692)
	)
	(pad "2" smd roundrect
		(at 14.7 0)
		(size 2.6 3.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.07692307692)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Battery.3dshapes/BatteryHolder_Renata_SMTU2032-LF_1x2032.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
