(footprint "BatteryHolder_TruPower_BH-331P_3xAA"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Keystone Battery Holder BH-331P Battery Type 3xAA (Script generated with StandardBox.py) (Keystone Battery Holder BH-331P Battery Type 3xAA)")
	(tags "Battery Holder BH-331P Battery Type 3xAA")
	(property "Reference" "REF**"
		(at 0.2 -10.35 0)
		(layer "F.SilkS")
	)
	(property "Value" "BatteryHolder_TruPower_BH-331P_3xAA"
		(at 26.7 40.15 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "+"
		(at -4.5 0 0)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 26.7 15 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 26.7 0)
		(size 3.5 3.5)
		(drill 3.5)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 26.7 30)
		(size 3.5 3.5)
		(drill 3.5)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 12.8)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Battery.3dshapes/BatteryHolder_TruPower_BH-331P_3xAA.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
