(footprint "Battery_Panasonic_CR2032-HFN_Horizontal_CircularHoles"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Panasonic CR-2032/HFN battery, https://industrial.panasonic.com/cdbs/www-data/pdf2/AAA4000/AAA4000D166.PDF")
	(tags "battery CR-2032 coin cell")
	(property "Reference" "REF**"
		(at 11 -11 0)
		(layer "F.SilkS")
	)
	(property "Value" "Battery_Panasonic_CR2032-HFN_Horizontal_CircularHoles"
		(at 10.5 11 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "+"
		(at 2.032 -0.127 0)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 10.5 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.6 2)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 20.5 0)
		(size 1.6 2)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Battery.3dshapes/Battery_Panasonic_CR2032-HFN_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
