(footprint "SW_SPST_PTS647_Sx50"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "C&K Components SPST SMD PTS647 Series 4.5mm Tact Switch, 5.0mm Height, see https://www.ckswitches.com/media/2567/pts647.pdf")
	(tags "SPST Button Switch")
	(property "Reference" "REF**"
		(at 0 -4.05 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_SPST_PTS647_Sx50"
		(at 0 4.15 0)
		(layer "F.Fab")
	)
	(property "Datasheet" "https://www.ckswitches.com/media/2567/pts647.pdf"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 5.85 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 -4.05 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -2.625 -1.6)
		(size 1.55 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "1" smd roundrect
		(at 2.625 -1.6)
		(size 1.55 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -2.625 1.6)
		(size 1.55 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at 2.625 1.6)
		(size 1.55 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_PTS647Sx50.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
