(footprint "SW_XKB_DM1-16UP-1"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "1A 30V SPDT Micro Switch rated for one million cycles, W12.7xD5.7xH6.6, https://www.helloxkb.com/public/images/pdf/DMX-XXXP-X.pdf")
	(tags "SPDT endstop limit switch vertical hook lever XKB DM1-16UP-1")
	(property "Reference" "REF**"
		(at 5.08 -4.064 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "SW_XKB_DM1-16UP-1"
		(at 5.08 6 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(attr through_hole)
	(fp_text user "NC"
		(at 10.16 4 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "C"
		(at 0 4 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "NO"
		(at 5.08 4 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 5.08 -2.032 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 2 2)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 5.08 0)
		(size 2 2)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 10.16 0)
		(size 2 2)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_XKB_DM1-16UP-1.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
