(footprint "Buzzer_D14mm_H7mm_P10mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Generic Buzzer, D14mm height 7mm with pitch 10mm")
	(tags "buzzer")
	(property "Reference" "REF**"
		(at 5.16 -8.23 0)
		(layer "F.SilkS")
	)
	(property "Value" "Buzzer_D14mm_H7mm_P10mm"
		(at 4.69 8.41 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "+"
		(at -0.01 -2.54 0)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 5.32 2.27 0)
		(layer "F.Fab")
	)
	(fp_text user "+"
		(at -0.01 -2.54 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 10 0)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Buzzer_Beeper.3dshapes/Buzzer_D14mm_H7mm_P10mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
