(footprint "MagneticBuzzer_Kobitone_254-EMB73-RO"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "MagneticBuzzer_Kobitone_254-EMB73-RO https://www.mouser.es/datasheet/2/209/joytech_11092018_KT-400379-1501513.pdf")
	(tags "MagneticBuzzer_Kobitone_254-EMB73-RO")
	(property "Reference" "REF**"
		(at 1.95 -4.55 0)
		(layer "F.SilkS")
	)
	(property "Value" "MagneticBuzzer_Kobitone_254-EMB73-RO"
		(at 1.9 5.35 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "+"
		(at -2.7 -0.05 0)
		(layer "F.SilkS")
	)
	(fp_text user "+"
		(at -2.7 -0.05 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at 1.8 -1.85 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 2 2)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 3 0)
		(size 2 2)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Buzzer_Beeper.3dshapes/MagneticBuzzer_Kobitone_254-EMB73-RO.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
