(footprint "C_1808_4520Metric"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Capacitor SMD 1808 (4520 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: datasheet page 3, https://product.tdk.com/system/files/dam/doc/product/capacitor/ceramic/mlcc/catalog/mlcc_commercial_soft_en.pdf), generated with kicad-footprint-generator")
	(tags "capacitor")
	(property "Reference" "REF**"
		(at 0 -2.1 0)
		(layer "F.SilkS")
	)
	(property "Value" "C_1808_4520Metric"
		(at 0 2.1 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -2.075 0)
		(size 1.55 2.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.16129)
	)
	(pad "2" smd roundrect
		(at 2.075 0)
		(size 1.55 2.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.16129)
	)
	(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1808_4520Metric.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
