(footprint "CP_Radial_D30.0mm_P10.00mm_3pin_SnapIn"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "CP, Radial series, Radial, pin pitch=10.00mm, diameter=30mm, height=45mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf")
	(tags "CP Radial series Radial pin pitch 10.00mm diameter 30mm height 45mm Electrolytic Capacitor")
	(property "Reference" "REF**"
		(at 5 -16.25 0)
		(layer "F.SilkS")
	)
	(property "Value" "CP_Radial_D30.0mm_P10.00mm_3pin_SnapIn"
		(at 5 16.25 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 5 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 4 4)
		(drill 2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 6.7 4.75)
		(size 5 5)
		(drill 2.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 10 0)
		(size 4 4)
		(drill 2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D30.0mm_P10.00mm_3pin_SnapIn.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
