(footprint "DX_5R5HxxxxU_D11.5mm_P10.00mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "CP, Radial series, Radial, pin pitch=10.00mm, diameter=11.5mm, Supercapacitor, http://www.elna.co.jp/en/capacitor/double_layer/catalog/pdf/dx_e.pdf")
	(tags "CP Radial series Radial pin pitch 10.00mm diameter 11.5mm supercapacitor")
	(property "Reference" "REF**"
		(at 4 -7 0)
		(layer "F.SilkS")
	)
	(property "Value" "DX_5R5HxxxxU_D11.5mm_P10.00mm"
		(at 4 8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 5 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.35 2.15)
		(drill oval 0.35 1.15)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 10 0)
		(size 1.35 2.15)
		(drill oval 0.35 1.15)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Capacitor_THT.3dshapes/DX_5R5HxxxxU_D11.5mm_P10.00mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
