(footprint "Banana_Cliff_FCR7350B_S16N-PC_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Cliff single 4mm shrouded banana panel socket, through-hole, horizontal, black, https://www.cliffuk.co.uk/products/testleads/sockets/S16NPC.pdf")
	(tags "cliff 4mm socket jack banana black")
	(property "Reference" "REF**"
		(at 0 -7.25 0)
		(layer "F.SilkS")
	)
	(property "Value" "Banana_Cliff_FCR7350B_S16N-PC_Horizontal"
		(at 0 7.25 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -6.36 -5.08)
		(size 1.7 1.7)
		(drill 1.2)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -6.36 5.08)
		(size 1.7 1.7)
		(drill 1.2)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 3.8 -5.08)
		(size 1.7 1.7)
		(drill 1.2)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 3.8 5.08)
		(size 1.7 1.7)
		(drill 1.2)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 3.5 3.5)
		(drill 2.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector.3dshapes/Banana_Cliff_FCR7350B_S16N-PC_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
