(footprint "Banana_Jack_1Pin"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Single banana socket, footprint - 6mm drill")
	(tags "banana socket")
	(property "Reference" "REF**"
		(at 0 -6.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Banana_Jack_1Pin"
		(at -0.25 6.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 10.16 10.16)
		(drill 6.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector.3dshapes/Banana_Jack_1Pin.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 2 2 2)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
