(footprint "CUI_PD-30"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "3 pin connector, PD-30, http://www.cui.com/product/resource/pd-30.pdf")
	(tags "connector 3-pin PD-30 power DIN")
	(property "Reference" "REF**"
		(at 2.5 -3.35 0)
		(layer "F.SilkS")
	)
	(property "Value" "CUI_PD-30"
		(at 2.5 16.15 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 2.5 6.15 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 0 7.15 180)
		(size 1.7 1.7)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 5 7.15 180)
		(size 1.7 1.7)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole rect
		(at 0 0 180)
		(size 3.7 3.7)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 5 0 180)
		(size 3.7 3.7)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 8.5 3.15 180)
		(size 2.1 2.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 2.5 9.15 180)
		(size 3.2 3.2)
		(drill 2.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector.3dshapes/CUI_PD-30.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
