(footprint "NS-Tech_Grove_1x04_P2mm_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "https://statics3.seeedstudio.com/images/opl/datasheet/3470130P1.pdf")
	(tags "Grove-1x04")
	(property "Reference" "REF**"
		(at -1.5 -4 0)
		(layer "F.SilkS")
	)
	(property "Value" "NS-Tech_Grove_1x04_P2mm_Vertical"
		(at 4.19 2.83 90)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at -2 2 90)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 2)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 4)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 0 6)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector.3dshapes/NS-Tech_Grove_1x04_P2mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 0.3937 0.3937 0.3937)
		)
		(rotate
			(xyz 0 0 -90)
		)
	)
)
