(footprint "Jack_3.5mm_Switronic_ST-005-G_horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "3.5mm horizontal headphones jack, http://akizukidenshi.com/download/ds/switronic/ST-005-G.pdf")
	(tags "Connector Audio Switronic ST-005-G")
	(property "Reference" "REF**"
		(at 0 -4.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Jack_3.5mm_Switronic_ST-005-G_horizontal"
		(at 0 4.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 2.5 -2.5)
		(size 1 1)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 2.5 2.5)
		(size 1 1)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "R" thru_hole rect
		(at 6.5 -2.25)
		(size 1.9 1.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "S" thru_hole circle
		(at 6.5 2.25)
		(size 1.9 1.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "T" thru_hole circle
		(at -1 -2.9)
		(size 1.9 1.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "T" thru_hole circle
		(at -1 2.9)
		(size 1.9 1.9)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_Switronic_ST-005-G_horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
