(footprint "Jack_speakON_Neutrik_NL8MDXX-V-3_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "speakON Chassis Connectors, 8 pole chassis connector, nickel metal square G-size flange, self tapping screw holes (A-screw), vertical PCB mount, replaces NL8MD-V-1, https://www.neutrik.com/en/product/nl8mdxx-v-3")
	(tags "neutrik speakon")
	(property "Reference" "REF**"
		(at 0.75 -15.15 0)
		(layer "F.SilkS")
	)
	(property "Value" "Jack_speakON_Neutrik_NL8MDXX-V-3_Vertical"
		(at 0.75 25.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 0.75 5.05 0)
		(layer "F.Fab")
	)
	(pad "1+" thru_hole circle
		(at 0 0)
		(size 3.4 3.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1-" thru_hole circle
		(at -4.8 -1.55)
		(size 3.4 3.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2+" thru_hole circle
		(at -4.3 4.3)
		(size 3.4 3.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2-" thru_hole circle
		(at -5.85 10.6)
		(size 3.4 3.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3+" thru_hole circle
		(at 0 10.1)
		(size 3.4 3.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3-" thru_hole circle
		(at 6.3 11.65)
		(size 3.4 3.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4+" thru_hole circle
		(at 5.8 5.8)
		(size 3.4 3.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4-" thru_hole circle
		(at 7.35 -0.5)
		(size 3.4 3.4)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_speakON_Neutrik_NL8MDXX-V-3_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
