(footprint "MiniXLR-5_Switchcraft_TRAPC_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "http://www.switchcraft.com/ProductSummary.aspx?Parent=620 http://www.switchcraft.com/Drawings/TRAPC_X-TRASM_X_SERIES_CD.PDF")
	(tags "THT Mini XLR 5Pin right angle")
	(property "Reference" "REF**"
		(at 8 -5 180)
		(layer "F.SilkS")
	)
	(property "Value" "MiniXLR-5_Switchcraft_TRAPC_Horizontal"
		(at 0 17.14 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "PCB Edge"
		(at 3.355 8.763 180)
		(layer "Dwgs.User")
	)
	(fp_text user "${REFERENCE}"
		(at 3.556 5.588 180)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -2.794 5.334 180)
		(size 1.778 1.778)
		(drill 1.778)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 9.144 5.334 180)
		(size 1.778 1.778)
		(drill 1.778)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole rect
		(at 0 0 180)
		(size 1.8 1.8)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 1.27 2.54 180)
		(size 1.8 1.8)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 3.81 2.54 180)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 5.08 0 180)
		(size 1.8 1.8)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 2.54 0 180)
		(size 1.8 1.8)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Audio.3dshapes/MiniXLR-5_Switchcraft_TRAPC_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
