(footprint "MMCX_Molex_73415-1471_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "http://www.molex.com/pdm_docs/sd/734151471_sd.pdf")
	(tags "Molex MMCX Coaxial Connector 50 ohms Female Jack Vertical THT")
	(property "Reference" "REF**"
		(at -0.04 -3.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "MMCX_Molex_73415-1471_Vertical"
		(at 0 3.2 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 1.24 1.24)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at -1.27 -1.27)
		(size 1.24 1.24)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at -1.27 1.27)
		(size 1.24 1.24)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 1.27 -1.27)
		(size 1.24 1.24)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 1.27 1.27)
		(size 1.24 1.24)
		(drill 0.84)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/MMCX_Molex_73415-1471_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
