(footprint "WR-MMCX_Wuerth_66012102111404_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Würth WR-MMCX PCB SMT Jack, Vertical (https://www.we-online.com/components/products/datasheet/66012102111404.pdf)")
	(tags "Coaxial Connector 50 ohms Female")
	(property "Reference" "REF**"
		(at 0 -2.75 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "WR-MMCX_Wuerth_66012102111404_Vertical"
		(at 0 6.05 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd circle
		(at 0 0)
		(size 1.47 1.47)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd custom
		(at -1.71 0)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.395 -2.11) (xy -0.395 2.11) (xy 1.175 2.11) (xy 1.175 1.1793) (xy 1.072058 1.129954) (xy 0.883921 1.000689)
					(xy 0.721347 0.840456) (xy 0.589367 0.654213) (xy 0.492065 0.447725) (xy 0.432453 0.227381) (xy 0.412375 0)
					(xy 0.432453 -0.227381) (xy 0.492065 -0.447725) (xy 0.589367 -0.654213) (xy 0.721347 -0.840456)
					(xy 0.883921 -1.000689) (xy 1.072058 -1.129954) (xy 1.175 -1.1793) (xy 1.175 -2.11)
				)
				(width 0.001)
				(fill yes)
			)
		)
	)
	(pad "2" smd custom
		(at 1.67 0)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.452065 -0.447725) (xy -0.392453 -0.227381) (xy -0.372375 0) (xy -0.392453 0.227381) (xy -0.452065 0.447725)
					(xy -0.549367 0.654213) (xy -0.681347 0.840456) (xy -0.843921 1.000689) (xy -1.032058 1.129954)
					(xy -1.135 1.1793) (xy -1.135 2.11) (xy 0.435 2.11) (xy 0.435 -2.11) (xy -1.135 -2.11) (xy -1.135 -1.1793)
					(xy -1.032058 -1.129954) (xy -0.843921 -1.000689) (xy -0.681347 -0.840456) (xy -0.549367 -0.654213)
				)
				(width 0.001)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/WR-MMCX_Wuerth_66012102111404_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
