(footprint "Hirose_DF13-10P-1.25DSA_1x10_P1.25mm_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Hirose DF13 through hole, DF13-10P-1.25DSA, 10 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13-2P-1.25DSA%2850%29/), generated with kicad-footprint-generator")
	(tags "connector Hirose DF13 vertical")
	(property "Reference" "REF**"
		(at 5.62 -3.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "Hirose_DF13-10P-1.25DSA_1x10_P1.25mm_Vertical"
		(at 5.62 2.4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 5.62 -1.5 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 0.9 1.4)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "2" thru_hole oval
		(at 1.25 0)
		(size 0.9 1.4)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 2.5 0)
		(size 0.9 1.4)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at 3.75 0)
		(size 0.9 1.4)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole oval
		(at 5 0)
		(size 0.9 1.4)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole oval
		(at 6.25 0)
		(size 0.9 1.4)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole oval
		(at 7.5 0)
		(size 0.9 1.4)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole oval
		(at 8.75 0)
		(size 0.9 1.4)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole oval
		(at 10 0)
		(size 0.9 1.4)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole oval
		(at 11.25 0)
		(size 0.9 1.4)
		(drill 0.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Hirose.3dshapes/Hirose_DF13-10P-1.25DSA_1x10_P1.25mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
