(footprint "Hirose_DF13C_CL535-0411-3-51_1x11-1MP_P1.25mm_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Hirose DF13C SMD, CL535-0411-3-51, 11 Pins per row (https://www.hirose.com/product/en/products/DF13/DF13C-10P-1.25V%2851%29/), generated with kicad-footprint-generator")
	(tags "connector Hirose DF13C vertical")
	(property "Reference" "REF**"
		(at 0 -3.55 0)
		(layer "F.SilkS")
	)
	(property "Value" "Hirose_DF13C_CL535-0411-3-51_1x11-1MP_P1.25mm_Vertical"
		(at 0 4.15 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "KEEPOUT"
		(at 0 0.735 0)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.25 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -6.25 -1.45)
		(size 0.7 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -5 -1.45)
		(size 0.7 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -3.75 -1.45)
		(size 0.7 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -2.5 -1.45)
		(size 0.7 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -1.25 -1.45)
		(size 0.7 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 0 -1.45)
		(size 0.7 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 1.25 -1.45)
		(size 0.7 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 2.5 -1.45)
		(size 0.7 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 3.75 -1.45)
		(size 0.7 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 5 -1.45)
		(size 0.7 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 6.25 -1.45)
		(size 0.7 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "MP" smd rect
		(at -8.5 1.25)
		(size 1.6 2.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "MP" smd rect
		(at 8.5 1.25)
		(size 1.6 2.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Hirose.3dshapes/Hirose_DF13C_CL535-0411-3-51_1x11-1MP_P1.25mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
