(footprint "JAE_LY20-8P-DLT1_2x04_P2.00mm_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Molex LY 20 series connector, LY20-8P-DLT1, 4 Circuits (http://www.jae.com/z-en/pdf_download_exec.cfm?param=SJ038187.pdf), generated with kicad-footprint-generator")
	(tags "connector JAE  top entry")
	(property "Reference" "REF**"
		(at 3.2 -3 0)
		(layer "F.SilkS")
	)
	(property "Value" "JAE_LY20-8P-DLT1_2x04_P2.00mm_Horizontal"
		(at 3.2 9 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 3.2 7.1 0)
		(layer "F.Fab")
	)
	(pad "a1" thru_hole roundrect
		(at 0 0)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.208333)
	)
	(pad "a2" thru_hole circle
		(at 0 2)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a3" thru_hole circle
		(at 0 4)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "a4" thru_hole circle
		(at 0 6)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b1" thru_hole circle
		(at 2 0)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b2" thru_hole circle
		(at 2 2)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b3" thru_hole circle
		(at 2 4)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "b4" thru_hole circle
		(at 2 6)
		(size 1.2 1.2)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_JAE.3dshapes/JAE_LY20-8P-DLT1_2x04_P2.00mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
