(footprint "Molex_Micro-Fit_3.0_43650-1010_1x10-1MP_P3.00mm_Horizontal"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Molex Micro-Fit 3.0 Connector System, 43650-1010 (compatible alternatives: 43650-1011, 43650-1009), 10 Pins per row (https://www.molex.com/pdm_docs/sd/436500210_sd.pdf), generated with kicad-footprint-generator")
	(tags "connector Molex Micro-Fit_3.0 horizontal")
	(property "Reference" "REF**"
		(at 0 -6.15 0)
		(layer "F.SilkS")
	)
	(property "Value" "Molex_Micro-Fit_3.0_43650-1010_1x10-1MP_P3.00mm_Horizontal"
		(at 0 7.78 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 -4.25 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -13.5 5.12)
		(size 1.27 2.92)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "2" smd rect
		(at -10.5 5.12)
		(size 1.27 2.92)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "3" smd rect
		(at -7.5 5.12)
		(size 1.27 2.92)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "4" smd rect
		(at -4.5 5.12)
		(size 1.27 2.92)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "5" smd rect
		(at -1.5 5.12)
		(size 1.27 2.92)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "6" smd rect
		(at 1.5 5.12)
		(size 1.27 2.92)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "7" smd rect
		(at 4.5 5.12)
		(size 1.27 2.92)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "8" smd rect
		(at 7.5 5.12)
		(size 1.27 2.92)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "9" smd rect
		(at 10.5 5.12)
		(size 1.27 2.92)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "10" smd rect
		(at 13.5 5.12)
		(size 1.27 2.92)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "MP" thru_hole circle
		(at -15.65 -0.35)
		(size 2.71 2.71)
		(drill 2.41)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
	)
	(pad "MP" thru_hole circle
		(at 15.65 -0.35)
		(size 2.71 2.71)
		(drill 2.41)
		(property pad_prop_heatsink)
		(layers "*.Cu" "*.Mask")
	)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Micro-Fit_3.0_43650-1010_1x10-1MP_P3.00mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
