(footprint "Molex_Pico-Lock_205338-0008_1x08-1MP_P2.00mm_Horizontal"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Molex Pico-Lock series connector, 205338-0008 (https://www.molex.com/pdm_docs/sd/2053380002_sd.pdf), generated with kicad-footprint-generator")
	(tags "connector Molex Pico-Lock horizontal")
	(property "Reference" "REF**"
		(at 0 -5.28 0)
		(layer "F.SilkS")
	)
	(property "Value" "Molex_Pico-Lock_205338-0008_1x08-1MP_P2.00mm_Horizontal"
		(at 0 5.36 0)
		(layer "F.Fab")
	)
	(attr smd)
	(pad "1" smd roundrect
		(at -7 -3.36)
		(size 1.1 1.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.227273)
	)
	(pad "2" smd roundrect
		(at -5 -3.36)
		(size 1.1 1.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.227273)
	)
	(pad "3" smd roundrect
		(at -3 -3.36)
		(size 1.1 1.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.227273)
	)
	(pad "4" smd roundrect
		(at -1 -3.36)
		(size 1.1 1.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.227273)
	)
	(pad "5" smd roundrect
		(at 1 -3.36)
		(size 1.1 1.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.227273)
	)
	(pad "6" smd roundrect
		(at 3 -3.36)
		(size 1.1 1.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.227273)
	)
	(pad "7" smd roundrect
		(at 5 -3.36)
		(size 1.1 1.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.227273)
	)
	(pad "8" smd roundrect
		(at 7 -3.36)
		(size 1.1 1.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.227273)
	)
	(pad "MP" smd roundrect
		(at -9.895 2.635)
		(size 1.35 2.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.185185)
	)
	(pad "MP" smd roundrect
		(at 9.895 2.635)
		(size 1.35 2.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.185185)
	)
	(fp_text user "${REFERENCE}"
		(at 0 0.37 0)
		(layer "F.Fab")
	)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Pico-Lock_205338-0008_1x08-1MP_P2.00mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
