(footprint "BUS_PCI"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "PCI bus Edge Connector")
	(tags "PCI bus Edge Connector")
	(property "Reference" "REF**"
		(at -11.81 -5.78 0)
		(layer "F.SilkS")
	)
	(property "Value" "BUS_PCI"
		(at 18.29 -5.78 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(fp_text user "${REFERENCE}"
		(at 0 -0.76 0)
		(layer "F.Fab")
	)
	(pad "A1" connect rect
		(at -38.73 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A1" connect rect
		(at -38.73 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A2" connect rect
		(at -37.46 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A2" connect rect
		(at -37.46 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A3" connect rect
		(at -36.2 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A3" connect rect
		(at -36.2 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A4" connect rect
		(at -34.92 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A4" connect rect
		(at -34.92 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A5" connect rect
		(at -33.65 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A5" connect rect
		(at -33.65 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A6" connect rect
		(at -32.38 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A6" connect rect
		(at -32.38 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A7" connect rect
		(at -31.11 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A7" connect rect
		(at -31.11 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A8" connect rect
		(at -29.84 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A8" connect rect
		(at -29.84 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A9" connect rect
		(at -28.57 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A9" connect rect
		(at -28.57 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A10" connect rect
		(at -27.3 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A10" connect rect
		(at -27.3 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A11" connect rect
		(at -26.03 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A11" connect rect
		(at -26.03 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A12" connect rect
		(at -24.77 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A12" connect rect
		(at -24.77 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A13" connect rect
		(at -23.49 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A13" connect rect
		(at -23.49 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A14" connect rect
		(at -22.22 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A14" connect rect
		(at -22.22 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A15" connect rect
		(at -20.95 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A15" connect rect
		(at -20.95 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A16" connect rect
		(at -19.68 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A16" connect rect
		(at -19.68 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A17" connect rect
		(at -18.41 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A17" connect rect
		(at -18.41 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A18" connect rect
		(at -17.14 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A18" connect rect
		(at -17.14 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A19" connect rect
		(at -15.88 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A19" connect rect
		(at -15.88 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A20" connect rect
		(at -14.6 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A20" connect rect
		(at -14.6 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A21" connect rect
		(at -13.34 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A21" connect rect
		(at -13.34 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A22" connect rect
		(at -12.06 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A22" connect rect
		(at -12.06 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A23" connect rect
		(at -10.79 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A23" connect rect
		(at -10.79 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A24" connect rect
		(at -9.52 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A24" connect rect
		(at -9.52 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A25" connect rect
		(at -8.25 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A25" connect rect
		(at -8.25 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A26" connect rect
		(at -6.98 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A26" connect rect
		(at -6.98 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A27" connect rect
		(at -5.71 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A27" connect rect
		(at -5.71 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A28" connect rect
		(at -4.44 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A28" connect rect
		(at -4.44 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A29" connect rect
		(at -3.17 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A29" connect rect
		(at -3.17 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A30" connect rect
		(at -1.9 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A30" connect rect
		(at -1.9 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A31" connect rect
		(at -0.63 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A31" connect rect
		(at -0.63 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A32" connect rect
		(at 0.64 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A32" connect rect
		(at 0.64 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A33" connect rect
		(at 1.91 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A33" connect rect
		(at 1.91 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A34" connect rect
		(at 3.18 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A34" connect rect
		(at 3.18 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A35" connect rect
		(at 4.45 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A35" connect rect
		(at 4.45 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A36" connect rect
		(at 5.72 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A36" connect rect
		(at 5.72 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A37" connect rect
		(at 6.99 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A37" connect rect
		(at 6.99 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A38" connect rect
		(at 8.26 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A38" connect rect
		(at 8.26 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A39" connect rect
		(at 9.53 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A39" connect rect
		(at 9.53 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A40" connect rect
		(at 10.8 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A40" connect rect
		(at 10.8 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A41" connect rect
		(at 12.07 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A41" connect rect
		(at 12.07 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A42" connect rect
		(at 13.34 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A42" connect rect
		(at 13.34 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A43" connect rect
		(at 14.61 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A43" connect rect
		(at 14.61 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A44" connect rect
		(at 15.88 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A44" connect rect
		(at 15.88 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A45" connect rect
		(at 17.15 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A45" connect rect
		(at 17.15 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A46" connect rect
		(at 18.42 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A46" connect rect
		(at 18.42 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A47" connect rect
		(at 19.69 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A47" connect rect
		(at 19.69 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A48" connect rect
		(at 20.96 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A48" connect rect
		(at 20.96 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A49" connect rect
		(at 22.23 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A49" connect rect
		(at 22.23 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A52" connect rect
		(at 26.04 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A52" connect rect
		(at 26.04 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A53" connect rect
		(at 27.31 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A53" connect rect
		(at 27.31 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A54" connect rect
		(at 28.58 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A54" connect rect
		(at 28.58 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A55" connect rect
		(at 29.85 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A55" connect rect
		(at 29.85 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A56" connect rect
		(at 31.12 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A56" connect rect
		(at 31.12 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A57" connect rect
		(at 32.39 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A57" connect rect
		(at 32.39 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A58" connect rect
		(at 33.66 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A58" connect rect
		(at 33.66 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A59" connect rect
		(at 34.93 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A59" connect rect
		(at 34.93 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A60" connect rect
		(at 36.2 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A60" connect rect
		(at 36.2 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A61" connect rect
		(at 37.47 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A61" connect rect
		(at 37.47 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A62" connect rect
		(at 38.73 -1.33)
		(size 1.02 4.57)
		(layers "B.Cu" "B.Mask")
	)
	(pad "A62" connect rect
		(at 38.73 1.33)
		(size 0.51 0.76)
		(layers "B.Cu" "B.Mask")
	)
	(pad "B1" connect rect
		(at -38.73 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B1" connect rect
		(at -38.73 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B2" connect rect
		(at -37.46 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B2" connect rect
		(at -37.46 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B3" connect rect
		(at -36.2 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B3" connect rect
		(at -36.2 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B4" connect rect
		(at -34.92 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B4" connect rect
		(at -34.92 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B5" connect rect
		(at -33.65 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B5" connect rect
		(at -33.65 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B6" connect rect
		(at -32.38 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B6" connect rect
		(at -32.38 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B7" connect rect
		(at -31.11 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B7" connect rect
		(at -31.11 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B8" connect rect
		(at -29.84 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B8" connect rect
		(at -29.84 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B9" connect rect
		(at -28.57 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B9" connect rect
		(at -28.57 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B10" connect rect
		(at -27.3 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B10" connect rect
		(at -27.3 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B11" connect rect
		(at -26.03 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B11" connect rect
		(at -26.03 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B12" connect rect
		(at -24.77 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B12" connect rect
		(at -24.77 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B13" connect rect
		(at -23.49 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B13" connect rect
		(at -23.49 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B14" connect rect
		(at -22.22 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B14" connect rect
		(at -22.22 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B15" connect rect
		(at -20.95 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B15" connect rect
		(at -20.95 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B16" connect rect
		(at -19.68 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B16" connect rect
		(at -19.68 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B17" connect rect
		(at -18.41 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B17" connect rect
		(at -18.41 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B18" connect rect
		(at -17.14 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B18" connect rect
		(at -17.14 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B19" connect rect
		(at -15.88 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B19" connect rect
		(at -15.88 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B20" connect rect
		(at -14.6 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B20" connect rect
		(at -14.6 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B21" connect rect
		(at -13.34 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B21" connect rect
		(at -13.34 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B22" connect rect
		(at -12.06 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B22" connect rect
		(at -12.06 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B23" connect rect
		(at -10.79 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B23" connect rect
		(at -10.79 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B24" connect rect
		(at -9.52 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B24" connect rect
		(at -9.52 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B25" connect rect
		(at -8.25 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B25" connect rect
		(at -8.25 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B26" connect rect
		(at -6.98 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B26" connect rect
		(at -6.98 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B27" connect rect
		(at -5.71 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B27" connect rect
		(at -5.71 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B28" connect rect
		(at -4.44 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B28" connect rect
		(at -4.44 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B29" connect rect
		(at -3.17 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B29" connect rect
		(at -3.17 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B30" connect rect
		(at -1.9 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B30" connect rect
		(at -1.9 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B31" connect rect
		(at -0.63 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B31" connect rect
		(at -0.63 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B32" connect rect
		(at 0.64 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B32" connect rect
		(at 0.64 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B33" connect rect
		(at 1.91 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B33" connect rect
		(at 1.91 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B34" connect rect
		(at 3.18 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B34" connect rect
		(at 3.18 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B35" connect rect
		(at 4.45 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B35" connect rect
		(at 4.45 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B36" connect rect
		(at 5.72 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B36" connect rect
		(at 5.72 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B37" connect rect
		(at 6.99 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B37" connect rect
		(at 6.99 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B38" connect rect
		(at 8.26 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B38" connect rect
		(at 8.26 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B39" connect rect
		(at 9.53 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B39" connect rect
		(at 9.53 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B40" connect rect
		(at 10.8 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B40" connect rect
		(at 10.8 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B41" connect rect
		(at 12.07 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B41" connect rect
		(at 12.07 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B42" connect rect
		(at 13.34 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B42" connect rect
		(at 13.34 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B43" connect rect
		(at 14.61 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B43" connect rect
		(at 14.61 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B44" connect rect
		(at 15.88 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B44" connect rect
		(at 15.88 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B45" connect rect
		(at 17.15 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B45" connect rect
		(at 17.15 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B46" connect rect
		(at 18.42 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B46" connect rect
		(at 18.42 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B47" connect rect
		(at 19.69 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B47" connect rect
		(at 19.69 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B48" connect rect
		(at 20.96 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B48" connect rect
		(at 20.96 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B49" connect rect
		(at 22.23 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B49" connect rect
		(at 22.23 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B52" connect rect
		(at 26.04 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B52" connect rect
		(at 26.04 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B53" connect rect
		(at 27.31 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B53" connect rect
		(at 27.31 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B54" connect rect
		(at 28.58 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B54" connect rect
		(at 28.58 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B55" connect rect
		(at 29.85 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B55" connect rect
		(at 29.85 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B56" connect rect
		(at 31.12 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B56" connect rect
		(at 31.12 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B57" connect rect
		(at 32.39 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B57" connect rect
		(at 32.39 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B58" connect rect
		(at 33.66 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B58" connect rect
		(at 33.66 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B59" connect rect
		(at 34.93 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B59" connect rect
		(at 34.93 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B60" connect rect
		(at 36.2 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B60" connect rect
		(at 36.2 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B61" connect rect
		(at 37.47 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B61" connect rect
		(at 37.47 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B62" connect rect
		(at 38.73 -1.33)
		(size 1.02 4.57)
		(layers "F.Cu" "F.Mask")
	)
	(pad "B62" connect rect
		(at 38.73 1.33)
		(size 0.51 0.76)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
)
