(footprint "Samtec_MECF-05-0_-L-DV_2x05_P1.27mm_Polarized_Edge"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Highspeed card edge connector for PCB's with 05 contacts (polarized)")
	(tags "conn samtec card-edge high-speed")
	(property "Reference" "REF**"
		(at 0 -5.95 0)
		(layer "F.SilkS")
	)
	(property "Value" "Samtec_MECF-05-0_-L-DV_2x05_P1.27mm_Polarized_Edge"
		(at 0 5.7 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(fp_line
		(start -4.5 -5)
		(end -4.05 -5)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -4.05 5)
		(end -4.05 -5)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -4.05 5)
		(end -1.88 5)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -1.88 -2)
		(end -0.64 -2)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -1.88 5)
		(end -1.88 -2)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -0.64 5)
		(end -0.64 -2)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -0.64 5)
		(end 4.05 5)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 4.05 5)
		(end 4.05 -5)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 4.5 -5)
		(end 4.05 -5)
		(layer "Edge.Cuts")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -2.54 0)
		(layer "F.Fab")
	)
	(pad "1" connect rect
		(at -2.53 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "2" connect rect
		(at -2.53 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "5" connect rect
		(at 0.01 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "6" connect rect
		(at 0.01 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "7" connect rect
		(at 1.28 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "8" connect rect
		(at 1.28 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(pad "9" connect rect
		(at 2.55 2.5)
		(size 0.56 4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "10" connect rect
		(at 2.55 2.5)
		(size 0.56 4)
		(layers "B.Cu" "B.Mask")
	)
	(embedded_fonts no)
)
