(footprint "PhoenixContact_SPT_2.5_9-V-5.0-EX_1x09_P5.0mm_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Connector Phoenix Contact, SPT 2.5/9-V-5.0-EX Terminal Block, 1732564 (https://www.phoenixcontact.com/online/portal/gb/?uri=pxc-oc-itemdetail:pid=1732564), generated with kicad-footprint-generator")
	(tags "Connector Phoenix Contact SPT 2.5/9-V-5.0-EX 1732564")
	(property "Reference" "REF**"
		(at 20.9 -3.95 0)
		(layer "F.SilkS")
	)
	(property "Value" "PhoenixContact_SPT_2.5_9-V-5.0-EX_1x09_P5.0mm_Vertical"
		(at 20.9 12.15 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 20.9 -2.05 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 1.8 3.3)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.138889)
	)
	(pad "1" thru_hole roundrect
		(at 0 8.2)
		(size 1.8 3.3)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.138889)
	)
	(pad "2" thru_hole oval
		(at 5 0)
		(size 1.8 3.3)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 5 8.2)
		(size 1.8 3.3)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 10 0)
		(size 1.8 3.3)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 10 8.2)
		(size 1.8 3.3)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at 15 0)
		(size 1.8 3.3)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at 15 8.2)
		(size 1.8 3.3)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole oval
		(at 20 0)
		(size 1.8 3.3)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole oval
		(at 20 8.2)
		(size 1.8 3.3)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole oval
		(at 25 0)
		(size 1.8 3.3)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole oval
		(at 25 8.2)
		(size 1.8 3.3)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole oval
		(at 30 0)
		(size 1.8 3.3)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole oval
		(at 30 8.2)
		(size 1.8 3.3)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole oval
		(at 35 0)
		(size 1.8 3.3)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole oval
		(at 35 8.2)
		(size 1.8 3.3)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole oval
		(at 40 0)
		(size 1.8 3.3)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole oval
		(at 40 8.2)
		(size 1.8 3.3)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Phoenix_SPT.3dshapes/PhoenixContact_SPT_2.5_9-V-5.0-EX_1x09_P5.0mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
