(footprint "PhoenixContact_SPT_5_6-V-7.5-ZB_1x06_P7.5mm_Vertical"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Connector Phoenix Contact, SPT 5/6-V-7.5-ZB Terminal Block, 1719354 (https://www.phoenixcontact.com/online/portal/gb/?uri=pxc-oc-itemdetail:pid=1719354), generated with kicad-footprint-generator")
	(tags "Connector Phoenix Contact SPT 5/6-V-7.5-ZB 1719354")
	(property "Reference" "REF**"
		(at 16.85 -3.78 0)
		(layer "F.SilkS")
	)
	(property "Value" "PhoenixContact_SPT_5_6-V-7.5-ZB_1x06_P7.5mm_Vertical"
		(at 16.85 17.32 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 16.85 -1.88 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 2.8 4.3)
		(drill 2.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.089286)
	)
	(pad "2" thru_hole oval
		(at 7.5 14)
		(size 2.8 4.3)
		(drill 2.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 15 0)
		(size 2.8 4.3)
		(drill 2.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at 22.5 14)
		(size 2.8 4.3)
		(drill 2.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole oval
		(at 30 0)
		(size 2.8 4.3)
		(drill 2.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole oval
		(at 37.5 14)
		(size 2.8 4.3)
		(drill 2.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Connector_Phoenix_SPT.3dshapes/PhoenixContact_SPT_5_6-V-7.5-ZB_1x06_P7.5mm_Vertical.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
